May 27 05:26:22 raspberrypi bash[460]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 05:26:27 raspberrypi systemd[1]: session-176.scope: Succeeded.
May 27 05:27:23 raspberrypi bash[460]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 05:28:22 raspberrypi bash[460]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 05:29:02 raspberrypi systemd[1]: Starting Daily apt download activities...
May 27 05:29:03 raspberrypi systemd[1]: apt-daily.service: Succeeded.
May 27 05:29:03 raspberrypi systemd[1]: Started Daily apt download activities.
May 27 05:29:22 raspberrypi bash[460]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 05:30:23 raspberrypi bash[460]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 05:31:23 raspberrypi bash[460]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 05:31:26 raspberrypi PackageKit: daemon quit
May 27 05:31:26 raspberrypi systemd[1]: packagekit.service: Main process exited, code=killed, status=15/TERM
May 27 05:31:26 raspberrypi systemd[1]: packagekit.service: Succeeded.
May 27 05:31:27 raspberrypi systemd[1]: Started Session 177 of user pi.
May 27 05:31:28 raspberrypi dbus-daemon[357]: [system] Activating via systemd: service name='org.freedesktop.PackageKit' unit='packagekit.service' requested by ':1.851' (uid=0 pid=19605 comm="/usr/bin/gdbus call --system --dest org.freedeskto")
May 27 05:31:28 raspberrypi systemd[1]: Starting PackageKit Daemon...
May 27 05:31:28 raspberrypi PackageKit: daemon start
May 27 05:31:28 raspberrypi dbus-daemon[357]: [system] Successfully activated service 'org.freedesktop.PackageKit'
May 27 05:31:28 raspberrypi systemd[1]: Started PackageKit Daemon.
May 27 05:31:34 raspberrypi systemd[1]: session-177.scope: Succeeded.
May 27 05:32:23 raspberrypi bash[460]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 05:33:23 raspberrypi bash[460]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 05:34:23 raspberrypi bash[460]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 05:35:23 raspberrypi bash[460]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 05:36:23 raspberrypi bash[460]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 05:36:33 raspberrypi PackageKit: daemon quit
May 27 05:36:33 raspberrypi systemd[1]: packagekit.service: Main process exited, code=killed, status=15/TERM
May 27 05:36:33 raspberrypi systemd[1]: packagekit.service: Succeeded.
May 27 05:36:34 raspberrypi systemd[1]: Started Session 178 of user pi.
May 27 05:36:36 raspberrypi dbus-daemon[357]: [system] Activating via systemd: service name='org.freedesktop.PackageKit' unit='packagekit.service' requested by ':1.856' (uid=0 pid=21348 comm="/usr/bin/gdbus call --system --dest org.freedeskto")
May 27 05:36:36 raspberrypi systemd[1]: Starting PackageKit Daemon...
May 27 05:36:36 raspberrypi PackageKit: daemon start
May 27 05:36:36 raspberrypi dbus-daemon[357]: [system] Successfully activated service 'org.freedesktop.PackageKit'
May 27 05:36:36 raspberrypi systemd[1]: Started PackageKit Daemon.
May 27 05:36:42 raspberrypi systemd[1]: session-178.scope: Succeeded.
May 27 05:37:22 raspberrypi bash[460]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 05:38:23 raspberrypi bash[460]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 05:39:23 raspberrypi bash[460]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 05:40:23 raspberrypi bash[460]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 05:41:23 raspberrypi bash[460]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 05:41:41 raspberrypi PackageKit: daemon quit
May 27 05:41:41 raspberrypi systemd[1]: packagekit.service: Main process exited, code=killed, status=15/TERM
May 27 05:41:41 raspberrypi systemd[1]: packagekit.service: Succeeded.
May 27 05:41:42 raspberrypi systemd[1]: Started Session 179 of user pi.
May 27 05:41:44 raspberrypi dbus-daemon[357]: [system] Activating via systemd: service name='org.freedesktop.PackageKit' unit='packagekit.service' requested by ':1.861' (uid=0 pid=23095 comm="/usr/bin/gdbus call --system --dest org.freedeskto")
May 27 05:41:44 raspberrypi systemd[1]: Starting PackageKit Daemon...
May 27 05:41:44 raspberrypi PackageKit: daemon start
May 27 05:41:44 raspberrypi dbus-daemon[357]: [system] Successfully activated service 'org.freedesktop.PackageKit'
May 27 05:41:44 raspberrypi systemd[1]: Started PackageKit Daemon.
May 27 05:41:49 raspberrypi systemd[1]: session-179.scope: Succeeded.
May 27 05:42:23 raspberrypi bash[460]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 05:43:22 raspberrypi bash[460]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 05:44:23 raspberrypi bash[460]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 05:17:05 raspberrypi systemd-modules-load[106]: Inserted module 'i2c_dev'
May 27 05:17:05 raspberrypi fake-hwclock[108]: Do 27. Mai 03:17:01 UTC 2021
May 27 05:17:05 raspberrypi systemd-fsck[127]: e2fsck 1.44.5 (15-Dec-2018)
May 27 05:17:05 raspberrypi systemd-fsck[127]: rootfs: clean, 443241/7201152 files, 2129784/29238646 blocks
May 27 05:17:05 raspberrypi systemd[1]: Started File System Check on Root Device.
May 27 05:17:05 raspberrypi systemd[1]: Starting Remount Root and Kernel File Systems...
May 27 05:17:05 raspberrypi systemd[1]: Started udev Coldplug all Devices.
May 27 05:17:05 raspberrypi systemd[1]: Starting Helper to synchronize boot up for ifupdown...
May 27 05:17:05 raspberrypi systemd[1]: Started Set the console keyboard layout.
May 27 05:17:05 raspberrypi systemd[1]: Started Helper to synchronize boot up for ifupdown.
May 27 05:17:05 raspberrypi systemd[1]: Started Remount Root and Kernel File Systems.
May 27 05:17:05 raspberrypi systemd[1]: Starting Load/Save Random Seed...
May 27 05:17:05 raspberrypi systemd[1]: Starting Create System Users...
May 27 05:17:05 raspberrypi systemd[1]: Starting Flush Journal to Persistent Storage...
May 27 05:17:05 raspberrypi systemd[1]: Condition check resulted in Rebuild Hardware Database being skipped.
May 27 05:17:05 raspberrypi systemd[1]: Started Load/Save Random Seed.
May 27 05:17:05 raspberrypi systemd[1]: Started Flush Journal to Persistent Storage.
May 27 05:17:05 raspberrypi systemd[1]: Started Create System Users.
May 27 05:17:05 raspberrypi systemd[1]: Starting Create Static Device Nodes in /dev...
May 27 05:17:05 raspberrypi systemd[1]: Started Create Static Device Nodes in /dev.
May 27 05:17:05 raspberrypi systemd[1]: Starting udev Kernel Device Manager...
May 27 05:17:05 raspberrypi systemd[1]: Reached target Local File Systems (Pre).
May 27 05:17:05 raspberrypi systemd[1]: Started udev Kernel Device Manager.
May 27 05:17:05 raspberrypi systemd[1]: Starting Show Plymouth Boot Screen...
May 27 05:17:05 raspberrypi systemd[1]: Received SIGRTMIN+20 from PID 157 (plymouthd).
May 27 05:17:05 raspberrypi systemd[1]: Started Show Plymouth Boot Screen.
May 27 05:17:05 raspberrypi systemd[1]: Condition check resulted in Dispatch Password Requests to Console Directory Watch being skipped.
May 27 05:17:05 raspberrypi systemd[1]: Reached target Local Encrypted Volumes.
May 27 05:17:05 raspberrypi systemd[1]: Started Forward Password Requests to Plymouth Directory Watch.
May 27 05:17:05 raspberrypi systemd-udevd[165]: Using default interface naming scheme 'v240'.
May 27 05:17:05 raspberrypi mtp-probe: checking bus 1, device 3: "/sys/devices/platform/scb/fd500000.pcie/pci0000:00/0000:00:00.0/0000:01:00.0/usb1/1-1/1-1.2"
May 27 05:17:05 raspberrypi mtp-probe: bus: 1, device: 3 was not an MTP device
May 27 05:17:05 raspberrypi systemd-udevd[150]: Using default interface naming scheme 'v240'.
May 27 05:17:05 raspberrypi systemd[1]: Found device CT120BX500SSD1 boot.
May 27 05:17:05 raspberrypi systemd[1]: Listening on Load/Save RF Kill Switch Status /dev/rfkill Watch.
May 27 05:17:05 raspberrypi systemd[1]: Condition check resulted in Set Up Additional Binary Formats being skipped.
May 27 05:17:05 raspberrypi kernel: [    0.000000] Booting Linux on physical CPU 0x0
May 27 05:17:05 raspberrypi systemd[1]: Condition check resulted in FUSE Control File System being skipped.
May 27 05:17:05 raspberrypi kernel: [    0.000000] Linux version 5.10.17-v7l+ (dom@buildbot) (arm-linux-gnueabihf-gcc-8 (Ubuntu/Linaro 8.4.0-3ubuntu1) 8.4.0, GNU ld (GNU Binutils for Ubuntu) 2.34) #1414 SMP Fri Apr 30 13:20:47 BST 2021
May 27 05:17:05 raspberrypi kernel: [    0.000000] CPU: ARMv7 Processor [410fd083] revision 3 (ARMv7), cr=30c5383d
May 27 05:17:05 raspberrypi kernel: [    0.000000] CPU: div instructions available: patching division code
May 27 05:17:05 raspberrypi kernel: [    0.000000] CPU: PIPT / VIPT nonaliasing data cache, PIPT instruction cache
May 27 05:17:05 raspberrypi kernel: [    0.000000] OF: fdt: Machine model: Raspberry Pi 4 Model B Rev 1.1
May 27 05:17:05 raspberrypi systemd[1]: Condition check resulted in Rebuild Hardware Database being skipped.
May 27 05:17:05 raspberrypi kernel: [    0.000000] Memory policy: Data cache writealloc
May 27 05:17:05 raspberrypi kernel: [    0.000000] Reserved memory: created CMA memory pool at 0x000000001ec00000, size 256 MiB
May 27 05:17:05 raspberrypi kernel: [    0.000000] OF: reserved mem: initialized node linux,cma, compatible id shared-dma-pool
May 27 05:17:05 raspberrypi kernel: [    0.000000] Zone ranges:
May 27 05:17:05 raspberrypi kernel: [    0.000000]   DMA      [mem 0x0000000000000000-0x000000002fffffff]
May 27 05:17:05 raspberrypi kernel: [    0.000000]   Normal   empty
May 27 05:17:05 raspberrypi kernel: [    0.000000]   HighMem  [mem 0x0000000030000000-0x00000000fbffffff]
May 27 05:17:05 raspberrypi systemd[1]: Starting File System Check on /dev/disk/by-partuuid/ec677da3-01...
May 27 05:17:05 raspberrypi kernel: [    0.000000] Movable zone start for each node
May 27 05:17:05 raspberrypi kernel: [    0.000000] Early memory node ranges
May 27 05:17:05 raspberrypi kernel: [    0.000000]   node   0: [mem 0x0000000000000000-0x000000003b2fffff]
May 27 05:17:05 raspberrypi systemd[1]: Condition check resulted in Dispatch Password Requests to Console Directory Watch being skipped.
May 27 05:17:05 raspberrypi kernel: [    0.000000]   node   0: [mem 0x0000000040000000-0x00000000fbffffff]
May 27 05:17:05 raspberrypi kernel: [    0.000000] Initmem setup node 0 [mem 0x0000000000000000-0x00000000fbffffff]
May 27 05:17:05 raspberrypi kernel: [    0.000000] On node 0 totalpages: 1012480
May 27 05:17:05 raspberrypi kernel: [    0.000000]   DMA zone: 2304 pages used for memmap
May 27 05:17:05 raspberrypi kernel: [    0.000000]   DMA zone: 0 pages reserved
May 27 05:17:05 raspberrypi systemd[1]: Condition check resulted in Huge Pages File System being skipped.
May 27 05:17:05 raspberrypi kernel: [    0.000000]   DMA zone: 196608 pages, LIFO batch:63
May 27 05:17:05 raspberrypi kernel: [    0.000000]   HighMem zone: 815872 pages, LIFO batch:63
May 27 05:17:05 raspberrypi kernel: [    0.000000] percpu: Embedded 20 pages/cpu s50700 r8192 d23028 u81920
May 27 05:17:05 raspberrypi kernel: [    0.000000] pcpu-alloc: s50700 r8192 d23028 u81920 alloc=20*4096
May 27 05:17:05 raspberrypi kernel: [    0.000000] pcpu-alloc: [0] 0 [0] 1 [0] 2 [0] 3 
May 27 05:17:05 raspberrypi systemd[1]: Starting Load/Save RF Kill Switch Status...
May 27 05:17:05 raspberrypi kernel: [    0.000000] Built 1 zonelists, mobility grouping on.  Total pages: 1010176
May 27 05:17:05 raspberrypi kernel: [    0.000000] Kernel command line: coherent_pool=1M 8250.nr_uarts=0 snd_bcm2835.enable_compat_alsa=0 snd_bcm2835.enable_hdmi=1  smsc95xx.macaddr=DC:A6:32:4D:A9:C9 vc_mem.mem_base=0x3eb00000 vc_mem.mem_size=0x3ff00000  console=ttyS0,115200 console=tty1 root=PARTUUID=ec677da3-02 rootfstype=ext4 elevator=deadline fsck.repair=yes rootwait quiet splash plymouth.ignore-serial-consoles
May 27 05:17:05 raspberrypi systemd[1]: Started Load/Save RF Kill Switch Status.
May 27 05:17:05 raspberrypi kernel: [    0.000000] Kernel parameter elevator= does not have any effect anymore.
May 27 05:17:05 raspberrypi kernel: [    0.000000] Please use sysfs to set IO scheduler for individual devices.
May 27 05:17:05 raspberrypi kernel: [    0.000000] Dentry cache hash table entries: 131072 (order: 7, 524288 bytes, linear)
May 27 05:17:05 raspberrypi kernel: [    0.000000] Inode-cache hash table entries: 65536 (order: 6, 262144 bytes, linear)
May 27 05:17:05 raspberrypi kernel: [    0.000000] mem auto-init: stack:off, heap alloc:off, heap free:off
May 27 05:17:05 raspberrypi kernel: [    0.000000] software IO TLB: mapped [mem 0x0000000017cc0000-0x000000001bcc0000] (64MB)
May 27 05:17:05 raspberrypi systemd-fsck[284]: fsck.fat 4.1 (2017-01-24)
May 27 05:17:05 raspberrypi kernel: [    0.000000] Memory: 3653916K/4049920K available (10240K kernel code, 1358K rwdata, 3160K rodata, 2048K init, 890K bss, 133860K reserved, 262144K cma-reserved, 3263488K highmem)
May 27 05:17:05 raspberrypi kernel: [    0.000000] SLUB: HWalign=64, Order=0-3, MinObjects=0, CPUs=4, Nodes=1
May 27 05:17:05 raspberrypi kernel: [    0.000000] ftrace: allocating 33942 entries in 67 pages
May 27 05:17:05 raspberrypi systemd-fsck[284]: 0x41: Dirty bit is set. Fs was not properly unmounted and some data may be corrupt.
May 27 05:17:05 raspberrypi kernel: [    0.000000] ftrace: allocated 67 pages with 3 groups
May 27 05:17:05 raspberrypi kernel: [    0.000000] rcu: Hierarchical RCU implementation.
May 27 05:17:05 raspberrypi kernel: [    0.000000] 	Rude variant of Tasks RCU enabled.
May 27 05:17:05 raspberrypi kernel: [    0.000000] 	Tracing variant of Tasks RCU enabled.
May 27 05:17:05 raspberrypi kernel: [    0.000000] rcu: RCU calculated value of scheduler-enlistment delay is 10 jiffies.
May 27 05:17:05 raspberrypi kernel: [    0.000000] NR_IRQS: 16, nr_irqs: 16, preallocated irqs: 16
May 27 05:17:05 raspberrypi kernel: [    0.000000] GIC: Using split EOI/Deactivate mode
May 27 05:17:05 raspberrypi systemd-fsck[284]:  Automatically removing dirty bit.
May 27 05:17:05 raspberrypi kernel: [    0.000000] random: get_random_bytes called from start_kernel+0x3c8/0x59c with crng_init=0
May 27 05:17:05 raspberrypi kernel: [    0.000008] sched_clock: 32 bits at 1000kHz, resolution 1000ns, wraps every 2147483647500ns
May 27 05:17:05 raspberrypi kernel: [    0.000026] clocksource: timer: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 1911260446275 ns
May 27 05:17:05 raspberrypi kernel: [    0.000088] bcm2835: system timer (irq = 25)
May 27 05:17:05 raspberrypi systemd-fsck[284]: Performing changes.
May 27 05:17:05 raspberrypi kernel: [    0.000739] arch_timer: cp15 timer(s) running at 54.00MHz (phys).
May 27 05:17:05 raspberrypi kernel: [    0.000756] clocksource: arch_sys_counter: mask: 0xffffffffffffff max_cycles: 0xc743ce346, max_idle_ns: 440795203123 ns
May 27 05:17:05 raspberrypi kernel: [    0.000774] sched_clock: 56 bits at 54MHz, resolution 18ns, wraps every 4398046511102ns
May 27 05:17:05 raspberrypi kernel: [    0.000789] Switching to timer-based delay loop, resolution 18ns
May 27 05:17:05 raspberrypi systemd-fsck[284]: /dev/sda1: 261 files, 97561/516190 clusters
May 27 05:17:05 raspberrypi kernel: [    0.001040] Console: colour dummy device 80x30
May 27 05:17:05 raspberrypi kernel: [    0.001108] printk: console [tty1] enabled
May 27 05:17:05 raspberrypi kernel: [    0.001161] Calibrating delay loop (skipped), value calculated using timer frequency.. 108.00 BogoMIPS (lpj=540000)
May 27 05:17:05 raspberrypi kernel: [    0.001193] pid_max: default: 32768 minimum: 301
May 27 05:17:05 raspberrypi kernel: [    0.001362] LSM: Security Framework initializing
May 27 05:17:05 raspberrypi systemd[1]: Started File System Check on /dev/disk/by-partuuid/ec677da3-01.
May 27 05:17:05 raspberrypi kernel: [    0.001546] Mount-cache hash table entries: 2048 (order: 1, 8192 bytes, linear)
May 27 05:17:05 raspberrypi kernel: [    0.001572] Mountpoint-cache hash table entries: 2048 (order: 1, 8192 bytes, linear)
May 27 05:17:05 raspberrypi kernel: [    0.003127] Disabling memory control group subsystem
May 27 05:17:05 raspberrypi systemd[1]: Mounting /boot...
May 27 05:17:05 raspberrypi kernel: [    0.003244] CPU: Testing write buffer coherency: ok
May 27 05:17:05 raspberrypi kernel: [    0.003697] CPU0: thread -1, cpu 0, socket 0, mpidr 80000000
May 27 05:17:05 raspberrypi kernel: [    0.004903] Setting up static identity map for 0x200000 - 0x20003c
May 27 05:17:05 raspberrypi kernel: [    0.005101] rcu: Hierarchical SRCU implementation.
May 27 05:17:05 raspberrypi kernel: [    0.006023] smp: Bringing up secondary CPUs ...
May 27 05:17:05 raspberrypi systemd[1]: Mounted /boot.
May 27 05:17:05 raspberrypi kernel: [    0.007230] CPU1: thread -1, cpu 1, socket 0, mpidr 80000001
May 27 05:17:05 raspberrypi kernel: [    0.008598] CPU2: thread -1, cpu 2, socket 0, mpidr 80000002
May 27 05:17:05 raspberrypi kernel: [    0.009893] CPU3: thread -1, cpu 3, socket 0, mpidr 80000003
May 27 05:17:05 raspberrypi kernel: [    0.010050] smp: Brought up 1 node, 4 CPUs
May 27 05:17:05 raspberrypi systemd[1]: Reached target Local File Systems.
May 27 05:17:05 raspberrypi kernel: [    0.010071] SMP: Total of 4 processors activated (432.00 BogoMIPS).
May 27 05:17:05 raspberrypi kernel: [    0.010086] CPU: All CPU(s) started in HYP mode.
May 27 05:17:05 raspberrypi kernel: [    0.010108] CPU: Virtualization extensions available.
May 27 05:17:05 raspberrypi kernel: [    0.010988] devtmpfs: initialized
May 27 05:17:05 raspberrypi kernel: [    0.024948] VFP support v0.3: implementor 41 architecture 3 part 40 variant 8 rev 0
May 27 05:17:05 raspberrypi kernel: [    0.025179] clocksource: jiffies: mask: 0xffffffff max_cycles: 0xffffffff, max_idle_ns: 19112604462750000 ns
May 27 05:17:05 raspberrypi systemd[1]: Starting Set console font and keymap...
May 27 05:17:05 raspberrypi kernel: [    0.025210] futex hash table entries: 1024 (order: 4, 65536 bytes, linear)
May 27 05:17:05 raspberrypi kernel: [    0.032192] pinctrl core: initialized pinctrl subsystem
May 27 05:17:05 raspberrypi kernel: [    0.033250] NET: Registered protocol family 16
May 27 05:17:05 raspberrypi kernel: [    0.037302] DMA: preallocated 1024 KiB pool for atomic coherent allocations
May 27 05:17:05 raspberrypi kernel: [    0.038058] audit: initializing netlink subsys (disabled)
May 27 05:17:05 raspberrypi kernel: [    0.038349] audit: type=2000 audit(0.030:1): state=initialized audit_enabled=0 res=1
May 27 05:17:05 raspberrypi systemd[1]: Starting Raise network interfaces...
May 27 05:17:05 raspberrypi kernel: [    0.038907] thermal_sys: Registered thermal governor 'step_wise'
May 27 05:17:05 raspberrypi kernel: [    0.039672] hw-breakpoint: found 5 (+1 reserved) breakpoint and 4 watchpoint registers.
May 27 05:17:05 raspberrypi kernel: [    0.039689] hw-breakpoint: maximum watchpoint size is 8 bytes.
May 27 05:17:05 raspberrypi kernel: [    0.040077] Serial: AMBA PL011 UART driver
May 27 05:17:05 raspberrypi systemd[1]: Starting Preprocess NFS configuration...
May 27 05:17:05 raspberrypi kernel: [    0.071905] bcm2835-mbox fe00b880.mailbox: mailbox enabled
May 27 05:17:05 raspberrypi kernel: [    0.091092] raspberrypi-firmware soc:firmware: Attached to firmware from 2021-04-30T13:45:52, variant start
May 27 05:17:05 raspberrypi kernel: [    0.101104] raspberrypi-firmware soc:firmware: Firmware hash is d7f29d96450abfc77cd6cf011af1faf1e03e5e56
May 27 05:17:05 raspberrypi kernel: [    0.146275] bcm2835-dma fe007000.dma: DMA legacy API manager, dmachans=0x1
May 27 05:17:05 raspberrypi systemd[1]: Starting Tell Plymouth To Write Out Runtime Data...
May 27 05:17:05 raspberrypi kernel: [    0.150389] vgaarb: loaded
May 27 05:17:05 raspberrypi kernel: [    0.150837] SCSI subsystem initialized
May 27 05:17:05 raspberrypi kernel: [    0.151047] usbcore: registered new interface driver usbfs
May 27 05:17:05 raspberrypi kernel: [    0.151119] usbcore: registered new interface driver hub
May 27 05:17:05 raspberrypi systemd[1]: Starting Create Volatile Files and Directories...
May 27 05:17:05 raspberrypi kernel: [    0.151569] usbcore: registered new device driver usb
May 27 05:17:05 raspberrypi kernel: [    0.151907] usb_phy_generic phy: supply vcc not found, using dummy regulator
May 27 05:17:05 raspberrypi kernel: [    0.153864] clocksource: Switched to clocksource arch_sys_counter
May 27 05:17:05 raspberrypi kernel: [    1.153488] VFS: Disk quotas dquot_6.6.0
May 27 05:17:05 raspberrypi systemd[1]: Condition check resulted in Commit a transient machine-id on disk being skipped.
May 27 05:17:05 raspberrypi kernel: [    1.153589] VFS: Dquot-cache hash table entries: 1024 (order 0, 4096 bytes)
May 27 05:17:05 raspberrypi kernel: [    1.153754] FS-Cache: Loaded
May 27 05:17:05 raspberrypi kernel: [    1.154073] CacheFiles: Loaded
May 27 05:17:05 raspberrypi kernel: [    1.164518] NET: Registered protocol family 2
May 27 05:17:05 raspberrypi systemd[1]: Started Set console font and keymap.
May 27 05:17:05 raspberrypi kernel: [    1.165352] tcp_listen_portaddr_hash hash table entries: 512 (order: 0, 6144 bytes, linear)
May 27 05:17:05 raspberrypi systemd[1]: nfs-config.service: Succeeded.
May 27 05:17:05 raspberrypi kernel: [    1.165395] TCP established hash table entries: 8192 (order: 3, 32768 bytes, linear)
May 27 05:17:05 raspberrypi kernel: [    1.165559] TCP bind hash table entries: 8192 (order: 4, 65536 bytes, linear)
May 27 05:17:05 raspberrypi kernel: [    1.165629] TCP: Hash tables configured (established 8192 bind 8192)
May 27 05:17:05 raspberrypi kernel: [    1.165787] UDP hash table entries: 512 (order: 2, 16384 bytes, linear)
May 27 05:17:05 raspberrypi systemd[1]: Started Preprocess NFS configuration.
May 27 05:17:05 raspberrypi systemd[1]: plymouth-read-write.service: Succeeded.
May 27 05:17:05 raspberrypi systemd[1]: Started Tell Plymouth To Write Out Runtime Data.
May 27 05:17:05 raspberrypi systemd[1]: Received SIGRTMIN+20 from PID 157 (plymouthd).
May 27 05:17:05 raspberrypi systemd[1]: Condition check resulted in RPC security service for NFS client and server being skipped.
May 27 05:17:05 raspberrypi systemd[1]: Condition check resulted in RPC security service for NFS server being skipped.
May 27 05:17:05 raspberrypi systemd[1]: Reached target NFS client services.
May 27 05:17:05 raspberrypi systemd[1]: Reached target Remote File Systems (Pre).
May 27 05:17:05 raspberrypi systemd[1]: Reached target Remote File Systems.
May 27 05:17:05 raspberrypi systemd[1]: Started Create Volatile Files and Directories.
May 27 05:17:05 raspberrypi systemd[1]: Starting Network Time Synchronization...
May 27 05:17:05 raspberrypi systemd[1]: Starting Update UTMP about System Boot/Shutdown...
May 27 05:17:05 raspberrypi systemd[1]: Started Update UTMP about System Boot/Shutdown.
May 27 05:17:05 raspberrypi systemd[1]: Started Raise network interfaces.
May 27 05:17:05 raspberrypi systemd[1]: Started Network Time Synchronization.
May 27 05:17:05 raspberrypi systemd[1]: Reached target System Initialization.
May 27 05:17:05 raspberrypi systemd[1]: Listening on CUPS Scheduler.
May 27 05:17:05 raspberrypi systemd[1]: Started Daily Cleanup of Temporary Directories.
May 27 05:17:05 raspberrypi systemd[1]: Started CUPS Scheduler.
May 27 05:17:05 raspberrypi systemd[1]: Reached target Paths.
May 27 05:17:05 raspberrypi systemd[1]: Listening on D-Bus System Message Bus Socket.
May 27 05:17:05 raspberrypi systemd[1]: Listening on triggerhappy.socket.
May 27 05:17:05 raspberrypi systemd[1]: Listening on Avahi mDNS/DNS-SD Stack Activation Socket.
May 27 05:17:05 raspberrypi systemd[1]: Reached target Sockets.
May 27 05:17:05 raspberrypi systemd[1]: Reached target Basic System.
May 27 05:17:05 raspberrypi kernel: [    1.165823] UDP-Lite hash table entries: 512 (order: 2, 16384 bytes, linear)
May 27 05:17:05 raspberrypi kernel: [    1.166096] NET: Registered protocol family 1
May 27 05:17:05 raspberrypi kernel: [    1.166792] RPC: Registered named UNIX socket transport module.
May 27 05:17:05 raspberrypi systemd[1]: Condition check resulted in getty on tty2-tty6 if dbus and logind are not available being skipped.
May 27 05:17:05 raspberrypi kernel: [    1.166808] RPC: Registered udp transport module.
May 27 05:17:05 raspberrypi kernel: [    1.166823] RPC: Registered tcp transport module.
May 27 05:17:05 raspberrypi kernel: [    1.166838] RPC: Registered tcp NFSv4.1 backchannel transport module.
May 27 05:17:05 raspberrypi kernel: [    1.166861] PCI: CLS 0 bytes, default 64
May 27 05:17:05 raspberrypi systemd[1]: Starting rng-tools.service...
May 27 05:17:05 raspberrypi kernel: [    1.169810] Initialise system trusted keyrings
May 27 05:17:05 raspberrypi kernel: [    1.170040] workingset: timestamp_bits=14 max_order=20 bucket_order=6
May 27 05:17:05 raspberrypi kernel: [    1.178594] zbud: loaded
May 27 05:17:05 raspberrypi kernel: [    1.180501] FS-Cache: Netfs 'nfs' registered for caching
May 27 05:17:05 raspberrypi systemd[1]: Starting Disk Manager...
May 27 05:17:05 raspberrypi kernel: [    1.181276] NFS: Registering the id_resolver key type
May 27 05:17:05 raspberrypi kernel: [    1.181315] Key type id_resolver registered
May 27 05:17:05 raspberrypi kernel: [    1.181331] Key type id_legacy registered
May 27 05:17:05 raspberrypi systemd[1]: Started CUPS Scheduler.
May 27 05:17:05 raspberrypi kernel: [    1.181475] nfs4filelayout_init: NFSv4 File Layout Driver Registering...
May 27 05:17:05 raspberrypi kernel: [    1.182490] Key type asymmetric registered
May 27 05:17:05 raspberrypi kernel: [    1.182506] Asymmetric key parser 'x509' registered
May 27 05:17:05 raspberrypi kernel: [    1.182696] bounce: pool size: 64 pages
May 27 05:17:05 raspberrypi kernel: [    1.182740] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 249)
May 27 05:17:05 raspberrypi kernel: [    1.182949] io scheduler mq-deadline registered
May 27 05:17:05 raspberrypi systemd[1]: Starting triggerhappy global hotkey daemon...
May 27 05:17:05 raspberrypi kernel: [    1.182966] io scheduler kyber registered
May 27 05:17:05 raspberrypi kernel: [    1.187394] brcm-pcie fd500000.pcie: host bridge /scb/pcie@7d500000 ranges:
May 27 05:17:05 raspberrypi kernel: [    1.187425] brcm-pcie fd500000.pcie:   No bus range found for /scb/pcie@7d500000, using [bus 00-ff]
May 27 05:17:05 raspberrypi systemd[1]: Starting LSB: Switch to ondemand cpu governor (unless shift key is pressed)...
May 27 05:17:05 raspberrypi kernel: [    1.187505] brcm-pcie fd500000.pcie:      MEM 0x0600000000..0x063fffffff -> 0x00c0000000
May 27 05:17:05 raspberrypi kernel: [    1.187593] brcm-pcie fd500000.pcie:   IB MEM 0x0000000000..0x00bfffffff -> 0x0400000000
May 27 05:17:05 raspberrypi kernel: [    1.245968] brcm-pcie fd500000.pcie: link up, 5.0 GT/s PCIe x1 (SSC)
May 27 05:17:05 raspberrypi kernel: [    1.246332] brcm-pcie fd500000.pcie: PCI host bridge to bus 0000:00
May 27 05:17:05 raspberrypi kernel: [    1.246353] pci_bus 0000:00: root bus resource [bus 00-ff]
May 27 05:17:05 raspberrypi systemd[1]: Starting System Logging Service...
May 27 05:17:05 raspberrypi kernel: [    1.246374] pci_bus 0000:00: root bus resource [mem 0x600000000-0x63fffffff] (bus address [0xc0000000-0xffffffff])
May 27 05:17:05 raspberrypi kernel: [    1.246462] pci 0000:00:00.0: [14e4:2711] type 01 class 0x060400
May 27 05:17:05 raspberrypi kernel: [    1.246705] pci 0000:00:00.0: PME# supported from D0 D3hot
May 27 05:17:05 raspberrypi kernel: [    1.250203] PCI: bus0: Fast back to back transfers disabled
May 27 05:17:05 raspberrypi rng-tools[345]: Starting Hardware RNG entropy gatherer daemon: rngd.
May 27 05:17:05 raspberrypi kernel: [    1.250541] pci 0000:01:00.0: [1106:3483] type 00 class 0x0c0330
May 27 05:17:05 raspberrypi kernel: [    1.250669] pci 0000:01:00.0: reg 0x10: [mem 0x00000000-0x00000fff 64bit]
May 27 05:17:05 raspberrypi kernel: [    1.251103] pci 0000:01:00.0: PME# supported from D0 D3cold
May 27 05:17:05 raspberrypi kernel: [    1.254604] PCI: bus1: Fast back to back transfers disabled
May 27 05:17:05 raspberrypi kernel: [    1.254701] pci 0000:00:00.0: BAR 8: assigned [mem 0x600000000-0x6000fffff]
May 27 05:17:05 raspberrypi kernel: [    1.254726] pci 0000:01:00.0: BAR 0: assigned [mem 0x600000000-0x600000fff 64bit]
May 27 05:17:05 raspberrypi rngd[352]: rngd 2-unofficial-mt.14 starting up...
May 27 05:17:05 raspberrypi kernel: [    1.254810] pci 0000:00:00.0: PCI bridge to [bus 01]
May 27 05:17:05 raspberrypi kernel: [    1.254836] pci 0000:00:00.0:   bridge window [mem 0x600000000-0x6000fffff]
May 27 05:17:05 raspberrypi kernel: [    1.255256] pcieport 0000:00:00.0: enabling device (0140 -> 0142)
May 27 05:17:05 raspberrypi kernel: [    1.255481] pcieport 0000:00:00.0: PME: Signaling with IRQ 62
May 27 05:17:05 raspberrypi kernel: [    1.263781] iproc-rng200 fe104000.rng: hwrng registered
May 27 05:17:05 raspberrypi kernel: [    1.264127] vc-mem: phys_addr:0x00000000 mem_base=0x3eb00000 mem_size:0x3ff00000(1023 MiB)
May 27 05:17:05 raspberrypi systemd[1]: Started Regular background program processing daemon.
May 27 05:17:05 raspberrypi kernel: [    1.265000] gpiomem-bcm2835 fe200000.gpiomem: Initialised: Registers at 0xfe200000
May 27 05:17:05 raspberrypi kernel: [    1.277216] brd: module loaded
May 27 05:17:05 raspberrypi kernel: [    1.289477] loop: module loaded
May 27 05:17:05 raspberrypi kernel: [    1.291120] Loading iSCSI transport class v2.0-870.
May 27 05:17:05 raspberrypi systemd[1]: Started Manage Sound Card State (restore and store).
May 27 05:17:05 raspberrypi kernel: [    1.293531] libphy: Fixed MDIO Bus: probed
May 27 05:17:05 raspberrypi kernel: [    1.295321] bcmgenet fd580000.ethernet: GENET 5.0 EPHY: 0x0000
May 27 05:17:05 raspberrypi kernel: [    1.313941] libphy: bcmgenet MII bus: probed
May 27 05:17:05 raspberrypi kernel: [    1.394050] unimac-mdio unimac-mdio.-19: Broadcom UniMAC MDIO bus
May 27 05:17:05 raspberrypi systemd[1]: Starting Save/Restore Sound Card State...
May 27 05:17:05 raspberrypi kernel: [    1.395209] usbcore: registered new interface driver r8152
May 27 05:17:05 raspberrypi kernel: [    1.395277] usbcore: registered new interface driver lan78xx
May 27 05:17:05 raspberrypi kernel: [    1.395338] usbcore: registered new interface driver smsc95xx
May 27 05:17:05 raspberrypi kernel: [    1.396971] xhci_hcd 0000:01:00.0: enabling device (0140 -> 0142)
May 27 05:17:05 raspberrypi rngd[352]: entropy feed to the kernel ready
May 27 05:17:05 raspberrypi kernel: [    1.397132] xhci_hcd 0000:01:00.0: xHCI Host Controller
May 27 05:17:05 raspberrypi kernel: [    1.397168] xhci_hcd 0000:01:00.0: new USB bus registered, assigned bus number 1
May 27 05:17:05 raspberrypi kernel: [    1.400513] xhci_hcd 0000:01:00.0: hcc params 0x002841eb hci version 0x100 quirks 0x0000030000000890
May 27 05:17:05 raspberrypi kernel: [    1.401846] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002, bcdDevice= 5.10
May 27 05:17:05 raspberrypi alsactl[358]: alsactl 1.1.8 daemon started
May 27 05:17:05 raspberrypi kernel: [    1.401865] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1
May 27 05:17:05 raspberrypi kernel: [    1.401883] usb usb1: Product: xHCI Host Controller
May 27 05:17:05 raspberrypi kernel: [    1.401899] usb usb1: Manufacturer: Linux 5.10.17-v7l+ xhci-hcd
May 27 05:17:05 raspberrypi kernel: [    1.401915] usb usb1: SerialNumber: 0000:01:00.0
May 27 05:17:05 raspberrypi thd[349]: Found socket passed from systemd
May 27 05:17:05 raspberrypi kernel: [    1.402638] hub 1-0:1.0: USB hub found
May 27 05:17:05 raspberrypi kernel: [    1.402736] hub 1-0:1.0: 1 port detected
May 27 05:17:05 raspberrypi kernel: [    1.403410] xhci_hcd 0000:01:00.0: xHCI Host Controller
May 27 05:17:05 raspberrypi kernel: [    1.403438] xhci_hcd 0000:01:00.0: new USB bus registered, assigned bus number 2
May 27 05:17:05 raspberrypi systemd[1]: Starting Avahi mDNS/DNS-SD Stack...
May 27 05:17:05 raspberrypi kernel: [    1.403464] xhci_hcd 0000:01:00.0: Host supports USB 3.0 SuperSpeed
May 27 05:17:05 raspberrypi kernel: [    1.404061] usb usb2: New USB device found, idVendor=1d6b, idProduct=0003, bcdDevice= 5.10
May 27 05:17:05 raspberrypi kernel: [    1.404080] usb usb2: New USB device strings: Mfr=3, Product=2, SerialNumber=1
May 27 05:17:05 raspberrypi kernel: [    1.404097] usb usb2: Product: xHCI Host Controller
May 27 05:17:05 raspberrypi kernel: [    1.404113] usb usb2: Manufacturer: Linux 5.10.17-v7l+ xhci-hcd
May 27 05:17:05 raspberrypi kernel: [    1.404130] usb usb2: SerialNumber: 0000:01:00.0
May 27 05:17:05 raspberrypi kernel: [    1.404849] hub 2-0:1.0: USB hub found
May 27 05:17:05 raspberrypi cron[356]: (CRON) INFO (pidfile fd = 3)
May 27 05:17:05 raspberrypi kernel: [    1.404936] hub 2-0:1.0: 4 ports detected
May 27 05:17:05 raspberrypi kernel: [    1.406601] dwc_otg: version 3.00a 10-AUG-2012 (platform bus)
May 27 05:17:05 raspberrypi systemd[1]: Started D-Bus System Message Bus.
May 27 05:17:05 raspberrypi systemd[1]: Starting Configure Bluetooth Modems connected by UART...
May 27 05:17:05 raspberrypi kernel: [    1.406904] dwc_otg: FIQ enabled
May 27 05:17:05 raspberrypi kernel: [    1.406918] dwc_otg: NAK holdoff enabled
May 27 05:17:05 raspberrypi kernel: [    1.406932] dwc_otg: FIQ split-transaction FSM enabled
May 27 05:17:05 raspberrypi kernel: [    1.406950] Module dwc_common_port init
May 27 05:17:05 raspberrypi kernel: [    1.407391] usbcore: registered new interface driver uas
May 27 05:17:05 raspberrypi kernel: [    1.407496] usbcore: registered new interface driver usb-storage
May 27 05:17:05 raspberrypi systemd[1]: Starting Check for v3d driver...
May 27 05:17:05 raspberrypi kernel: [    1.407690] mousedev: PS/2 mouse device common for all mice
May 27 05:17:05 raspberrypi kernel: [    1.409332] bcm2835-wdt bcm2835-wdt: Broadcom BCM2835 watchdog timer
May 27 05:17:05 raspberrypi systemd[1]: Starting WPA supplicant...
May 27 05:17:05 raspberrypi kernel: [    1.412790] sdhci: Secure Digital Host Controller Interface driver
May 27 05:17:05 raspberrypi kernel: [    1.412805] sdhci: Copyright(c) Pierre Ossman
May 27 05:17:05 raspberrypi kernel: [    1.413502] mmc-bcm2835 fe300000.mmcnr: could not get clk, deferring probe
May 27 05:17:05 raspberrypi kernel: [    1.414204] sdhci-pltfm: SDHCI platform and OF driver helper
May 27 05:17:05 raspberrypi kernel: [    1.418343] ledtrig-cpu: registered to indicate activity on CPUs
May 27 05:17:05 raspberrypi systemd[1]: Starting Login Service...
May 27 05:17:05 raspberrypi kernel: [    1.418687] hid: raw HID events driver (C) Jiri Kosina
May 27 05:17:05 raspberrypi kernel: [    1.418881] usbcore: registered new interface driver usbhid
May 27 05:17:05 raspberrypi kernel: [    1.418896] usbhid: USB HID core driver
May 27 05:17:05 raspberrypi systemd[1]: Starting dphys-swapfile - set up, mount/unmount, and delete a swap file...
May 27 05:17:05 raspberrypi kernel: [    1.424648] Initializing XFRM netlink socket
May 27 05:17:05 raspberrypi kernel: [    1.424689] NET: Registered protocol family 17
May 27 05:17:05 raspberrypi kernel: [    1.424833] Key type dns_resolver registered
May 27 05:17:05 raspberrypi kernel: [    1.425270] Registering SWP/SWPB emulation handler
May 27 05:17:05 raspberrypi kernel: [    1.425450] registered taskstats version 1
May 27 05:17:05 raspberrypi kernel: [    1.425477] Loading compiled-in X.509 certificates
May 27 05:17:05 raspberrypi systemd[1]: Condition check resulted in Copy user wpa_supplicant.conf being skipped.
May 27 05:17:05 raspberrypi kernel: [    1.426314] Key type ._fscrypt registered
May 27 05:17:05 raspberrypi kernel: [    1.426331] Key type .fscrypt registered
May 27 05:17:05 raspberrypi kernel: [    1.426346] Key type fscrypt-provisioning registered
May 27 05:17:05 raspberrypi kernel: [    1.438018] uart-pl011 fe201000.serial: there is not valid maps for state default
May 27 05:17:05 raspberrypi kernel: [    1.438331] uart-pl011 fe201000.serial: cts_event_workaround enabled
May 27 05:17:05 raspberrypi systemd[1]: Starting dhcpcd on all interfaces...
May 27 05:17:05 raspberrypi kernel: [    1.438405] fe201000.serial: ttyAMA0 at MMIO 0xfe201000 (irq = 36, base_baud = 0) is a PL011 rev2
May 27 05:17:05 raspberrypi kernel: [    1.445165] bcm2835-power bcm2835-power: Broadcom BCM2835 power domains driver
May 27 05:17:05 raspberrypi kernel: [    1.446201] mmc-bcm2835 fe300000.mmcnr: mmc_debug:0 mmc_debug2:0
May 27 05:17:05 raspberrypi kernel: [    1.446218] mmc-bcm2835 fe300000.mmcnr: DMA channel allocated
May 27 05:17:05 raspberrypi kernel: [    1.476478] of_cfs_init
May 27 05:17:05 raspberrypi kernel: [    1.476729] of_cfs_init: OK
May 27 05:17:05 raspberrypi systemd[1]: Starting Check for Raspberry Pi EEPROM updates...
May 27 05:17:05 raspberrypi kernel: [    1.484009] mmc1: Controller never released inhibit bit(s).
May 27 05:17:05 raspberrypi kernel: [    1.502441] mmc1: queuing unknown CIS tuple 0x80 (2 bytes)
May 27 05:17:05 raspberrypi kernel: [    1.504224] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
May 27 05:17:05 raspberrypi kernel: [    1.505914] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
May 27 05:17:05 raspberrypi systemd[1]: Condition check resulted in Turn on SSH if /boot/ssh is present being skipped.
May 27 05:17:05 raspberrypi kernel: [    1.508934] mmc1: queuing unknown CIS tuple 0x80 (7 bytes)
May 27 05:17:05 raspberrypi kernel: [    1.510621] mmc1: queuing unknown CIS tuple 0x80 (3 bytes)
May 27 05:17:05 raspberrypi kernel: [    1.521445] mmc0: SDHCI controller on fe340000.emmc2 [fe340000.emmc2] using ADMA
May 27 05:17:05 raspberrypi kernel: [    1.522383] Waiting for root device PARTUUID=ec677da3-02...
May 27 05:17:05 raspberrypi systemd[1]: Reached target System Time Synchronized.
May 27 05:17:05 raspberrypi kernel: [    1.554535] random: fast init done
May 27 05:17:05 raspberrypi kernel: [    1.578181] mmc1: new high speed SDIO card at address 0001
May 27 05:17:05 raspberrypi kernel: [    1.763906] usb 1-1: new high-speed USB device number 2 using xhci_hcd
May 27 05:17:05 raspberrypi cron[356]: (CRON) INFO (Running @reboot jobs)
May 27 05:17:05 raspberrypi kernel: [    1.946526] usb 1-1: New USB device found, idVendor=2109, idProduct=3431, bcdDevice= 4.21
May 27 05:17:05 raspberrypi systemd[1]: Started Daily rotation of log files.
May 27 05:17:05 raspberrypi systemd[1]: Started Daily man-db regeneration.
May 27 05:17:05 raspberrypi systemd[1]: apt-daily.timer: Not using persistent file timestamp Thu 2021-05-27 05:29:02 CEST as it is in the future.
May 27 05:17:05 raspberrypi systemd[1]: Started Daily apt download activities.
May 27 05:17:05 raspberrypi systemd[1]: Started Daily apt upgrade and clean activities.
May 27 05:17:05 raspberrypi systemd[1]: Reached target Timers.
May 27 05:17:05 raspberrypi systemd[1]: Started triggerhappy global hotkey daemon.
May 27 05:17:05 raspberrypi systemd[1]: Started rng-tools.service.
May 27 05:17:05 raspberrypi systemd[1]: Started Save/Restore Sound Card State.
May 27 05:17:05 raspberrypi systemd[1]: Reached target Sound Card.
May 27 05:17:05 raspberrypi avahi-daemon[360]: Found user 'avahi' (UID 108) and group 'avahi' (GID 113).
May 27 05:17:05 raspberrypi avahi-daemon[360]: Successfully dropped root privileges.
May 27 05:17:05 raspberrypi avahi-daemon[360]: avahi-daemon 0.7 starting up.
May 27 05:17:05 raspberrypi rsyslogd: imuxsock: Acquired UNIX socket '/run/systemd/journal/syslog' (fd 3) from systemd.  [v8.1901.0]
May 27 05:17:05 raspberrypi rsyslogd:  [origin software="rsyslogd" swVersion="8.1901.0" x-pid="351" x-info="https://www.rsyslog.com"] start
May 27 05:17:05 raspberrypi kernel: [    1.946546] usb 1-1: New USB device strings: Mfr=0, Product=1, SerialNumber=0
May 27 05:17:05 raspberrypi kernel: [    1.946563] usb 1-1: Product: USB2.0 Hub
May 27 05:17:05 raspberrypi kernel: [    1.948311] hub 1-1:1.0: USB hub found
May 27 05:17:05 raspberrypi kernel: [    1.948631] hub 1-1:1.0: 4 ports detected
May 27 05:17:05 raspberrypi kernel: [    2.273903] usb 1-1.2: new high-speed USB device number 3 using xhci_hcd
May 27 05:17:05 raspberrypi kernel: [    2.405139] usb 1-1.2: New USB device found, idVendor=059b, idProduct=047a, bcdDevice= 1.00
May 27 05:17:05 raspberrypi kernel: [    2.405159] usb 1-1.2: New USB device strings: Mfr=10, Product=11, SerialNumber=5
May 27 05:17:05 raspberrypi kernel: [    2.405176] usb 1-1.2: Product: Iomega Select HDD
May 27 05:17:05 raspberrypi kernel: [    2.405193] usb 1-1.2: Manufacturer: Iomega
May 27 05:17:05 raspberrypi kernel: [    2.405209] usb 1-1.2: SerialNumber: 2106E417CD33
May 27 05:17:05 raspberrypi kernel: [    2.408159] usb-storage 1-1.2:1.0: USB Mass Storage device detected
May 27 05:17:05 raspberrypi kernel: [    2.408960] scsi host0: usb-storage 1-1.2:1.0
May 27 05:17:05 raspberrypi kernel: [    3.434679] scsi 0:0:0:0: Direct-Access     CT120BX5 00SSD1                PQ: 0 ANSI: 2 CCS
May 27 05:17:05 raspberrypi kernel: [    3.436071] sd 0:0:0:0: [sda] 234441648 512-byte logical blocks: (120 GB/112 GiB)
May 27 05:17:05 raspberrypi kernel: [    3.436831] sd 0:0:0:0: [sda] Write Protect is off
May 27 05:17:05 raspberrypi kernel: [    3.436851] sd 0:0:0:0: [sda] Mode Sense: 28 00 00 00
May 27 05:17:05 raspberrypi kernel: [    3.437539] sd 0:0:0:0: [sda] No Caching mode page found
May 27 05:17:05 raspberrypi kernel: [    3.437576] sd 0:0:0:0: [sda] Assuming drive cache: write through
May 27 05:17:05 raspberrypi kernel: [    3.438956]  sda: sda1 sda2
May 27 05:17:05 raspberrypi kernel: [    3.442160] sd 0:0:0:0: [sda] Attached SCSI disk
May 27 05:17:05 raspberrypi kernel: [    3.482573] EXT4-fs (sda2): INFO: recovery required on readonly filesystem
May 27 05:17:05 raspberrypi kernel: [    3.482591] EXT4-fs (sda2): write access will be enabled during recovery
May 27 05:17:05 raspberrypi kernel: [    3.899823] EXT4-fs (sda2): orphan cleanup on readonly fs
May 27 05:17:05 raspberrypi kernel: [    3.904250] EXT4-fs (sda2): 1 orphan inode deleted
May 27 05:17:05 raspberrypi kernel: [    3.904268] EXT4-fs (sda2): recovery complete
May 27 05:17:05 raspberrypi kernel: [    3.913535] EXT4-fs (sda2): mounted filesystem with ordered data mode. Opts: (null)
May 27 05:17:05 raspberrypi kernel: [    3.913618] VFS: Mounted root (ext4 filesystem) readonly on device 8:2.
May 27 05:17:05 raspberrypi kernel: [    3.914559] devtmpfs: mounted
May 27 05:17:05 raspberrypi kernel: [    3.923467] Freeing unused kernel memory: 2048K
May 27 05:17:05 raspberrypi kernel: [    3.944197] Run /sbin/init as init process
May 27 05:17:05 raspberrypi kernel: [    3.944212]   with arguments:
May 27 05:17:05 raspberrypi kernel: [    3.944226]     /sbin/init
May 27 05:17:05 raspberrypi kernel: [    3.944241]     splash
May 27 05:17:05 raspberrypi kernel: [    3.944254]   with environment:
May 27 05:17:05 raspberrypi kernel: [    3.944269]     HOME=/
May 27 05:17:05 raspberrypi kernel: [    3.944282]     TERM=linux
May 27 05:17:05 raspberrypi kernel: [    4.523295] NET: Registered protocol family 10
May 27 05:17:05 raspberrypi kernel: [    4.524675] Segment Routing with IPv6
May 27 05:17:05 raspberrypi kernel: [    5.342734] random: systemd: uninitialized urandom read (16 bytes read)
May 27 05:17:05 raspberrypi kernel: [    5.353819] random: systemd: uninitialized urandom read (16 bytes read)
May 27 05:17:05 raspberrypi kernel: [    5.354477] random: systemd: uninitialized urandom read (16 bytes read)
May 27 05:17:05 raspberrypi kernel: [    5.483607] i2c /dev entries driver
May 27 05:17:05 raspberrypi kernel: [    6.126427] EXT4-fs (sda2): re-mounted. Opts: (null)
May 27 05:17:05 raspberrypi kernel: [    6.913637] vc_sm_cma: module is from the staging directory, the quality is unknown, you have been warned.
May 27 05:17:05 raspberrypi kernel: [    6.921078] bcm2835_vc_sm_cma_probe: Videocore shared memory driver
May 27 05:17:05 raspberrypi kernel: [    6.921106] [vc_sm_connected_init]: start
May 27 05:17:05 raspberrypi kernel: [    6.922711] [vc_sm_connected_init]: installed successfully
May 27 05:17:05 raspberrypi kernel: [    6.932947] rpivid-mem feb00000.hevc-decoder: rpivid-hevcmem initialised: Registers at 0xfeb00000 length 0x00010000
May 27 05:17:05 raspberrypi kernel: [    6.933817] rpivid-mem feb10000.rpivid-local-intc: rpivid-intcmem initialised: Registers at 0xfeb10000 length 0x00001000
May 27 05:17:05 raspberrypi kernel: [    6.934650] rpivid-mem feb20000.h264-decoder: rpivid-h264mem initialised: Registers at 0xfeb20000 length 0x00010000
May 27 05:17:05 raspberrypi kernel: [    6.935231] rpivid-mem feb30000.vp9-decoder: rpivid-vp9mem initialised: Registers at 0xfeb30000 length 0x00010000
May 27 05:17:05 raspberrypi kernel: [    6.970390] mc: Linux media interface: v0.10
May 27 05:17:05 raspberrypi kernel: [    7.013305] snd_bcm2835: module is from the staging directory, the quality is unknown, you have been warned.
May 27 05:17:05 raspberrypi kernel: [    7.030644] bcm2835_audio bcm2835_audio: card created with 8 channels
May 27 05:17:05 raspberrypi kernel: [    7.032506] videodev: Linux video capture interface: v2.00
May 27 05:17:05 raspberrypi kernel: [    7.104353] bcm2835_mmal_vchiq: module is from the staging directory, the quality is unknown, you have been warned.
May 27 05:17:05 raspberrypi kernel: [    7.104360] bcm2835_mmal_vchiq: module is from the staging directory, the quality is unknown, you have been warned.
May 27 05:17:05 raspberrypi kernel: [    7.104516] bcm2835_mmal_vchiq: module is from the staging directory, the quality is unknown, you have been warned.
May 27 05:17:05 raspberrypi kernel: [    7.129460] bcm2835_codec: module is from the staging directory, the quality is unknown, you have been warned.
May 27 05:17:05 raspberrypi kernel: [    7.136136] bcm2835_v4l2: module is from the staging directory, the quality is unknown, you have been warned.
May 27 05:17:05 raspberrypi kernel: [    7.143481] bcm2835_isp: module is from the staging directory, the quality is unknown, you have been warned.
May 27 05:17:05 raspberrypi kernel: [    7.156911] bcm2835-codec bcm2835-codec: Device registered as /dev/video10
May 27 05:17:05 raspberrypi kernel: [    7.156960] bcm2835-codec bcm2835-codec: Loaded V4L2 decode
May 27 05:17:05 raspberrypi kernel: [    7.161940] bcm2835-isp bcm2835-isp: Device node output[0] registered as /dev/video13
May 27 05:17:05 raspberrypi kernel: [    7.165947] bcm2835-codec bcm2835-codec: Device registered as /dev/video11
May 27 05:17:05 raspberrypi kernel: [    7.165994] bcm2835-codec bcm2835-codec: Loaded V4L2 encode
May 27 05:17:05 raspberrypi kernel: [    7.166138] bcm2835-isp bcm2835-isp: Device node capture[0] registered as /dev/video14
May 27 05:17:05 raspberrypi kernel: [    7.166697] bcm2835-isp bcm2835-isp: Device node capture[1] registered as /dev/video15
May 27 05:17:05 raspberrypi kernel: [    7.168606] bcm2835-isp bcm2835-isp: Device node stats[2] registered as /dev/video16
May 27 05:17:05 raspberrypi kernel: [    7.168680] bcm2835-isp bcm2835-isp: Register output node 0 with media controller
May 27 05:17:05 raspberrypi kernel: [    7.168709] bcm2835-isp bcm2835-isp: Register capture node 1 with media controller
May 27 05:17:05 raspberrypi kernel: [    7.168790] bcm2835-isp bcm2835-isp: Register capture node 2 with media controller
May 27 05:17:05 raspberrypi kernel: [    7.168814] bcm2835-isp bcm2835-isp: Register capture node 3 with media controller
May 27 05:17:05 raspberrypi kernel: [    7.169190] bcm2835-isp bcm2835-isp: Loaded V4L2 bcm2835-isp
May 27 05:17:05 raspberrypi kernel: [    7.185805] bcm2835-codec bcm2835-codec: Device registered as /dev/video12
May 27 05:17:05 raspberrypi kernel: [    7.185851] bcm2835-codec bcm2835-codec: Loaded V4L2 isp
May 27 05:17:05 raspberrypi kernel: [    7.352949] cfg80211: Loading compiled-in X.509 certificates for regulatory database
May 27 05:17:05 raspberrypi kernel: [    7.376077] [drm] Initialized v3d 1.0.0 20180419 for fec00000.v3d on minor 0
May 27 05:17:05 raspberrypi kernel: [    7.482442] cfg80211: Loaded X.509 cert 'sforshee: 00b28ddf47aef9cea7'
May 27 05:17:05 raspberrypi kernel: [    7.577431] [drm] No displays found. Consider forcing hotplug if HDMI is attached
May 27 05:17:05 raspberrypi kernel: [    7.577557] vc4-drm gpu: bound fe600000.firmwarekms (ops vc4_fkms_ops [vc4])
May 27 05:17:05 raspberrypi kernel: [    7.582263] [drm] Initialized vc4 0.0.0 20140616 for gpu on minor 1
May 27 05:17:05 raspberrypi kernel: [    7.602152] brcmfmac: F1 signature read @0x18000000=0x15264345
May 27 05:17:05 raspberrypi kernel: [    7.618640] brcmfmac: brcmf_fw_alloc_request: using brcm/brcmfmac43455-sdio for chip BCM4345/6
May 27 05:17:05 raspberrypi kernel: [    7.620296] usbcore: registered new interface driver brcmfmac
May 27 05:17:05 raspberrypi kernel: [    7.649205] brcmfmac mmc1:0001:1: Direct firmware load for brcm/brcmfmac43455-sdio.raspberrypi,4-model-b.txt failed with error -2
May 27 05:17:05 raspberrypi kernel: [    7.696062] sd 0:0:0:0: Attached scsi generic sg0 type 0
May 27 05:17:05 raspberrypi kernel: [    7.891986] brcmfmac: brcmf_fw_alloc_request: using brcm/brcmfmac43455-sdio for chip BCM4345/6
May 27 05:17:05 raspberrypi kernel: [    7.904760] brcmfmac: brcmf_c_preinit_dcmds: Firmware: BCM4345/6 wl0: Jan  4 2021 19:56:29 version 7.45.229 (617f1f5 CY) FWID 01-2dbd9d2e
May 27 05:17:05 raspberrypi kernel: [    8.132153] random: crng init done
May 27 05:17:05 raspberrypi kernel: [    8.132168] random: 7 urandom warning(s) missed due to ratelimiting
May 27 05:17:05 raspberrypi dhcpcd[368]: dev: loaded udev
May 27 05:17:05 raspberrypi kernel: [   10.302241] uart-pl011 fe201000.serial: no DMA platform data
May 27 05:17:05 raspberrypi kernel: [   10.414634] 8021q: 802.1Q VLAN Support v1.8
May 27 05:17:05 raspberrypi dhcpcd[368]: forked to background, child pid 410
May 27 05:17:05 raspberrypi dphys-swapfile[367]: want /var/swap=100MByte, checking existing: keeping it
May 27 05:17:06 raspberrypi udisksd[346]: udisks daemon version 2.8.1 starting
May 27 05:17:06 raspberrypi systemd[1]: Started System Logging Service.
May 27 05:17:06 raspberrypi systemd[1]: Started Check for v3d driver.
May 27 05:17:06 raspberrypi avahi-daemon[360]: Successfully called chroot().
May 27 05:17:06 raspberrypi avahi-daemon[360]: Successfully dropped remaining capabilities.
May 27 05:17:06 raspberrypi avahi-daemon[360]: No service file found in /etc/avahi/services.
May 27 05:17:06 raspberrypi systemd[1]: Started dhcpcd on all interfaces.
May 27 05:17:06 raspberrypi avahi-daemon[360]: Network interface enumeration completed.
May 27 05:17:06 raspberrypi avahi-daemon[360]: Server startup complete. Host name is raspberrypi.local. Local service cookie is 4034207191.
May 27 05:17:06 raspberrypi wpa_supplicant[365]: Successfully initialized wpa_supplicant
May 27 05:17:06 raspberrypi systemd[1]: Started Login Service.
May 27 05:17:06 raspberrypi systemd[1]: Started Avahi mDNS/DNS-SD Stack.
May 27 05:17:06 raspberrypi systemd[1]: Started WPA supplicant.
May 27 05:17:06 raspberrypi systemd[1]: Started Make remote CUPS printers available locally.
May 27 05:17:06 raspberrypi udisksd[346]: failed to load module crypto: libbd_crypto.so.2: cannot open shared object file: No such file or directory
May 27 05:17:06 raspberrypi systemd[1]: Reached target Network.
May 27 05:17:06 raspberrypi udisksd[346]: failed to load module mdraid: libbd_mdraid.so.2: cannot open shared object file: No such file or directory
May 27 05:17:06 raspberrypi systemd[1]: Started ioBroker Server.
May 27 05:17:06 raspberrypi systemd[1]: Condition check resulted in fast remote file copy program daemon being skipped.
May 27 05:17:06 raspberrypi raspi-config[350]: Checking if shift key is held down:Error opening '/dev/input/event*': No such file or directory
May 27 05:17:06 raspberrypi systemd[1]: Starting /etc/rc.local Compatibility...
May 27 05:17:06 raspberrypi raspi-config[350]:  No. Switching to ondemand scaling governor.
May 27 05:17:06 raspberrypi systemd[1]: Starting OpenBSD Secure Shell server...
May 27 05:17:06 raspberrypi dhcpcd-run-hooks[458]: wlan0: starting wpa_supplicant
May 27 05:17:06 raspberrypi kernel: [   10.853911] Adding 102396k swap on /var/swap.  Priority:-2 extents:1 across:102396k FS
May 27 05:17:06 raspberrypi systemd[1]: Starting Permit User Sessions...
May 27 05:17:06 raspberrypi systemd[1]: Started LSB: Switch to ondemand cpu governor (unless shift key is pressed).
May 27 05:17:06 raspberrypi systemd[1]: Started dphys-swapfile - set up, mount/unmount, and delete a swap file.
May 27 05:17:06 raspberrypi systemd[1]: Started /etc/rc.local Compatibility.
May 27 05:17:06 raspberrypi systemd[1]: Started Permit User Sessions.
May 27 05:17:06 raspberrypi systemd[1]: Starting Hold until boot process finishes up...
May 27 05:17:06 raspberrypi systemd[1]: Starting Light Display Manager...
May 27 05:17:06 raspberrypi kernel: [   10.934772] brcmfmac: brcmf_cfg80211_set_power_mgmt: power save enabled
May 27 05:17:06 raspberrypi udisksd[346]: Failed to load the 'mdraid' libblockdev plugin
May 27 05:17:06 raspberrypi udisksd[346]: Failed to load the 'crypto' libblockdev plugin
May 27 05:17:06 raspberrypi dbus-daemon[362]: [system] Activating via systemd: service name='org.freedesktop.PolicyKit1' unit='polkit.service' requested by ':1.5' (uid=0 pid=346 comm="/usr/lib/udisks2/udisksd ")
May 27 05:17:06 raspberrypi systemd[1]: Starting Authorization Manager...
May 27 05:17:06 raspberrypi rpi-eeprom-update[369]: Skipping automatic bootloader upgrade. current 1599135103 >= min 1599135103
May 27 05:17:06 raspberrypi dhcpcd[410]: wlan0: connected to Access Point `'
May 27 05:17:06 raspberrypi dhcpcd[410]: eth0: waiting for carrier
May 27 05:17:06 raspberrypi dhcpcd[410]: wlan0: waiting for carrier
May 27 05:17:06 raspberrypi kernel: [   11.320469] bcmgenet fd580000.ethernet: configuring instance for external RGMII (RX delay)
May 27 05:17:06 raspberrypi kernel: [   11.320781] bcmgenet fd580000.ethernet eth0: Link is Down
May 27 05:17:06 raspberrypi systemd[1]: Started OpenBSD Secure Shell server.
May 27 05:17:06 raspberrypi lightdm[476]: Error getting user list from org.freedesktop.Accounts: GDBus.Error:org.freedesktop.DBus.Error.ServiceUnknown: The name org.freedesktop.Accounts was not provided by any .service files
May 27 05:17:06 raspberrypi rpi-eeprom-update[369]: BOOTLOADER: up to date
May 27 05:17:06 raspberrypi rpi-eeprom-update[369]:    CURRENT: Do 3. Sep 12:11:43 UTC 2020 (1599135103)
May 27 05:17:06 raspberrypi rpi-eeprom-update[369]:     LATEST: Do 29. Apr 16:11:25 UTC 2021 (1619712685)
May 27 05:17:06 raspberrypi rpi-eeprom-update[369]:    RELEASE: default (/lib/firmware/raspberrypi/bootloader/default)
May 27 05:17:06 raspberrypi rpi-eeprom-update[369]:             Use raspi-config to change the release.
May 27 05:17:06 raspberrypi rpi-eeprom-update[369]:   VL805_FW: Dedicated VL805 EEPROM
May 27 05:17:06 raspberrypi rpi-eeprom-update[369]:      VL805: up to date
May 27 05:17:06 raspberrypi rpi-eeprom-update[369]:    CURRENT: 000138a1
May 27 05:17:06 raspberrypi rpi-eeprom-update[369]:     LATEST: 000138a1
May 27 05:17:06 raspberrypi systemd[1]: Started Check for Raspberry Pi EEPROM updates.
May 27 05:17:06 raspberrypi polkitd[477]: started daemon version 0.105 using authority implementation `local' version `0.105'
May 27 05:17:06 raspberrypi dbus-daemon[362]: [system] Successfully activated service 'org.freedesktop.PolicyKit1'
May 27 05:17:06 raspberrypi systemd[1]: Started Authorization Manager.
May 27 05:17:06 raspberrypi systemd[1]: Received SIGRTMIN+21 from PID 157 (plymouthd).
May 27 05:17:06 raspberrypi systemd[1]: plymouth-quit-wait.service: Succeeded.
May 27 05:17:06 raspberrypi systemd[1]: Started Hold until boot process finishes up.
May 27 05:17:06 raspberrypi systemd[1]: plymouth-start.service: Succeeded.
May 27 05:17:06 raspberrypi systemd[1]: Started Getty on tty1.
May 27 05:17:06 raspberrypi systemd[1]: Reached target Login Prompts.
May 27 05:17:06 raspberrypi systemd[1]: Started Light Display Manager.
May 27 05:17:07 raspberrypi systemd[1]: Started Disk Manager.
May 27 05:17:07 raspberrypi udisksd[346]: Acquired the name org.freedesktop.UDisks2 on the system message bus
May 27 05:17:09 raspberrypi systemd[1]: systemd-rfkill.service: Succeeded.
May 27 05:17:09 raspberrypi kernel: [   13.859308] broken atomic modeset userspace detected, disabling atomic
May 27 05:17:09 raspberrypi kernel: [   14.555579] broken atomic modeset userspace detected, disabling atomic
May 27 05:17:09 raspberrypi systemd[1]: lightdm.service: Main process exited, code=exited, status=1/FAILURE
May 27 05:17:09 raspberrypi systemd[1]: lightdm.service: Failed with result 'exit-code'.
May 27 05:17:10 raspberrypi systemd[1]: lightdm.service: Service RestartSec=100ms expired, scheduling restart.
May 27 05:17:10 raspberrypi systemd[1]: lightdm.service: Scheduled restart job, restart counter is at 1.
May 27 05:17:10 raspberrypi systemd[1]: Stopped Light Display Manager.
May 27 05:17:10 raspberrypi systemd[1]: Starting Light Display Manager...
May 27 05:17:10 raspberrypi lightdm[540]: Error getting user list from org.freedesktop.Accounts: GDBus.Error:org.freedesktop.DBus.Error.ServiceUnknown: The name org.freedesktop.Accounts was not provided by any .service files
May 27 05:17:10 raspberrypi systemd[1]: Started Light Display Manager.
May 27 05:17:10 raspberrypi dhcpcd[410]: eth0: carrier acquired
May 27 05:17:10 raspberrypi dhcpcd[410]: DUID 00:01:00:01:27:d4:25:9f:dc:a6:32:4d:a9:c9
May 27 05:17:10 raspberrypi dhcpcd[410]: eth0: IAID 32:4d:a9:c9
May 27 05:17:10 raspberrypi dhcpcd[410]: eth0: adding address fe80::65d:ad68:fef2:77ea
May 27 05:17:10 raspberrypi avahi-daemon[360]: Joining mDNS multicast group on interface eth0.IPv6 with address fe80::65d:ad68:fef2:77ea.
May 27 05:17:10 raspberrypi avahi-daemon[360]: New relevant interface eth0.IPv6 for mDNS.
May 27 05:17:10 raspberrypi dhcpcd[410]: eth0: probing address 192.168.0.250/24
May 27 05:17:10 raspberrypi avahi-daemon[360]: Registering new address record for fe80::65d:ad68:fef2:77ea on eth0.*.
May 27 05:17:10 raspberrypi kernel: [   15.514030] bcmgenet fd580000.ethernet eth0: Link is Up - 1Gbps/Full - flow control rx/tx
May 27 05:17:10 raspberrypi kernel: [   15.514060] IPv6: ADDRCONF(NETDEV_CHANGE): eth0: link becomes ready
May 27 05:17:11 raspberrypi kernel: [   15.636785] broken atomic modeset userspace detected, disabling atomic
May 27 05:17:11 raspberrypi dhcpcd[410]: eth0: soliciting an IPv6 router
May 27 05:17:11 raspberrypi kernel: [   16.243494] broken atomic modeset userspace detected, disabling atomic
May 27 05:17:11 raspberrypi systemd[1]: lightdm.service: Main process exited, code=exited, status=1/FAILURE
May 27 05:17:11 raspberrypi systemd[1]: lightdm.service: Failed with result 'exit-code'.
May 27 05:17:11 raspberrypi bash[461]: ================================== > LOG REDIRECT system.adapter.admin.0 => true [starting]
May 27 05:17:11 raspberrypi systemd[1]: lightdm.service: Service RestartSec=100ms expired, scheduling restart.
May 27 05:17:11 raspberrypi systemd[1]: lightdm.service: Scheduled restart job, restart counter is at 2.
May 27 05:17:11 raspberrypi systemd[1]: Stopped Light Display Manager.
May 27 05:17:11 raspberrypi systemd[1]: Starting Light Display Manager...
May 27 05:17:12 raspberrypi lightdm[556]: Error getting user list from org.freedesktop.Accounts: GDBus.Error:org.freedesktop.DBus.Error.ServiceUnknown: The name org.freedesktop.Accounts was not provided by any .service files
May 27 05:17:12 raspberrypi systemd[1]: Started Light Display Manager.
May 27 05:17:12 raspberrypi dhcpcd[410]: eth0: Router Advertisement from fe80::10:18ff:fea0:d144
May 27 05:17:12 raspberrypi dhcpcd[410]: eth0: adding address 2a02:8109:9dc0:1ba4:6ecc:f236:6d1:757a/64
May 27 05:17:12 raspberrypi avahi-daemon[360]: Leaving mDNS multicast group on interface eth0.IPv6 with address fe80::65d:ad68:fef2:77ea.
May 27 05:17:12 raspberrypi avahi-daemon[360]: Joining mDNS multicast group on interface eth0.IPv6 with address 2a02:8109:9dc0:1ba4:6ecc:f236:6d1:757a.
May 27 05:17:12 raspberrypi avahi-daemon[360]: Registering new address record for 2a02:8109:9dc0:1ba4:6ecc:f236:6d1:757a on eth0.*.
May 27 05:17:12 raspberrypi dhcpcd[410]: eth0: adding route to 2a02:8109:9dc0:1ba4::/64
May 27 05:17:12 raspberrypi avahi-daemon[360]: Withdrawing address record for fe80::65d:ad68:fef2:77ea on eth0.
May 27 05:17:12 raspberrypi dhcpcd[410]: eth0: confirming prior DHCPv6 lease
May 27 05:17:12 raspberrypi dhcpcd[410]: eth0: adding default route via fe80::10:18ff:fea0:d144
May 27 05:17:12 raspberrypi kernel: [   16.637393] ICMPv6: process `dhcpcd' is using deprecated sysctl (syscall) net.ipv6.neigh.eth0.retrans_time - use net.ipv6.neigh.eth0.retrans_time_ms instead
May 27 05:17:12 raspberrypi systemd[1]: Created slice User Slice of UID 1000.
May 27 05:17:12 raspberrypi systemd[1]: Starting User Runtime Directory /run/user/1000...
May 27 05:17:12 raspberrypi systemd[1]: Started User Runtime Directory /run/user/1000.
May 27 05:17:12 raspberrypi systemd[1]: Starting User Manager for UID 1000...
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.admin.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.alexa2.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.backitup.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.bring.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.broadlink2.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.broadlink2.1" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.daswetter.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.deconz.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.discovery.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.fahrplan.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.feiertage.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.history.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.hs100.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.hue.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.ical.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.info.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.javascript.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.linux-control.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.material.0" for host "iobroker"
May 27 05:17:12 raspberrypi systemd[567]: Listening on GnuPG network certificate management daemon.
May 27 05:17:12 raspberrypi systemd[567]: Listening on Sound System.
May 27 05:17:12 raspberrypi systemd[567]: Listening on GnuPG cryptographic agent and passphrase cache (access for web browsers).
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.moma.0" for host "iobroker"
May 27 05:17:12 raspberrypi systemd[567]: Listening on GnuPG cryptographic agent (ssh-agent emulation).
May 27 05:17:12 raspberrypi systemd[567]: Reached target Timers.
May 27 05:17:12 raspberrypi systemd[567]: Listening on GnuPG cryptographic agent and passphrase cache (restricted).
May 27 05:17:12 raspberrypi systemd[567]: Listening on GnuPG cryptographic agent and passphrase cache.
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.mpd.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.mqtt.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.net-tools.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.onkyo.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.paw.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.pollenflug.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.radar2.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.rpi2.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.scenes.0" for host "iobroker"
May 27 05:17:12 raspberrypi systemd[567]: Starting D-Bus User Message Bus Socket.
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.sonoff.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.systeminfo.0" for host "iobroker"
May 27 05:17:12 raspberrypi systemd[567]: Reached target Paths.
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.telegram.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.vis-canvas-gauges.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.vis-colorpicker.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.vis-fancyswitch.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.vis-google-fonts.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.vis-history.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.vis-hqwidgets.0" for host "iobroker"
May 27 05:17:12 raspberrypi systemd[567]: Listening on D-Bus User Message Bus Socket.
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.vis-inventwo.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.vis-jqui-mfd.0" for host "iobroker"
May 27 05:17:12 raspberrypi systemd[567]: Reached target Sockets.
May 27 05:17:12 raspberrypi systemd[567]: Reached target Basic System.
May 27 05:17:12 raspberrypi systemd[567]: Reached target Default.
May 27 05:17:12 raspberrypi systemd[567]: Startup finished in 242ms.
May 27 05:17:12 raspberrypi systemd[1]: Started User Manager for UID 1000.
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.vis-justgage.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.vis-lcars.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.vis-map.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.vis-material-advanced.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.vis-metro.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.vis-players.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.vis-rgraph.0" for host "iobroker"
May 27 05:17:12 raspberrypi systemd[1]: Started Session 1 of user pi.
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.vis-timeandweather.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.vis-weather.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.vis.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.weatherunderground.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.web.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.ping.0" for host "iobroker"
May 27 05:17:12 raspberrypi bash[461]: host.iobroker check instance "system.adapter.countdown.0" for host "iobroker"
May 27 05:17:12 raspberrypi kernel: [   17.075356] Bluetooth: Core ver 2.22
May 27 05:17:12 raspberrypi kernel: [   17.075409] NET: Registered protocol family 31
May 27 05:17:12 raspberrypi kernel: [   17.075415] Bluetooth: HCI device and connection manager initialized
May 27 05:17:12 raspberrypi kernel: [   17.075429] Bluetooth: HCI socket layer initialized
May 27 05:17:12 raspberrypi kernel: [   17.075439] Bluetooth: L2CAP socket layer initialized
May 27 05:17:12 raspberrypi kernel: [   17.075454] Bluetooth: SCO socket layer initialized
May 27 05:17:12 raspberrypi kernel: [   17.093149] Bluetooth: HCI UART driver ver 2.3
May 27 05:17:12 raspberrypi kernel: [   17.093161] Bluetooth: HCI UART protocol H4 registered
May 27 05:17:12 raspberrypi kernel: [   17.093243] Bluetooth: HCI UART protocol Three-wire (H5) registered
May 27 05:17:12 raspberrypi kernel: [   17.093415] Bluetooth: HCI UART protocol Broadcom registered
May 27 05:17:12 raspberrypi btuart[363]: bcm43xx_init
May 27 05:17:12 raspberrypi btuart[363]: Flash firmware /lib/firmware/brcm/BCM4345C0.hcd
May 27 05:17:12 raspberrypi btuart[363]: Set Controller UART speed to 3000000 bit/s
May 27 05:17:12 raspberrypi btuart[363]: Device setup complete
May 27 05:17:12 raspberrypi systemd[1]: Starting Load/Save RF Kill Switch Status...
May 27 05:17:12 raspberrypi systemd[1]: Started Configure Bluetooth Modems connected by UART.
May 27 05:17:12 raspberrypi dhcpcd[410]: eth0: REPLY6 received from fe80::10:18ff:fea0:d144
May 27 05:17:12 raspberrypi dhcpcd[410]: eth0: adding address 2a02:8109:9dc0:1ba4::8536/128
May 27 05:17:12 raspberrypi dhcpcd[410]: eth0: renew in 302400, rebind in 483840, expire in 604800 seconds
May 27 05:17:12 raspberrypi avahi-daemon[360]: Registering new address record for 2a02:8109:9dc0:1ba4::8536 on eth0.*.
May 27 05:17:12 raspberrypi systemd[1]: Started Load/Save RF Kill Switch Status.
May 27 05:17:12 raspberrypi systemd[1]: Created slice system-bthelper.slice.
May 27 05:17:12 raspberrypi systemd[1]: Starting Raspberry Pi bluetooth helper...
May 27 05:17:12 raspberrypi systemd[1]: Reached target Multi-User System.
May 27 05:17:12 raspberrypi systemd[1]: Reached target Graphical Interface.
May 27 05:17:12 raspberrypi systemd[1]: Starting Update UTMP about System Runlevel Changes...
May 27 05:17:12 raspberrypi bthelper[590]: Raspberry Pi BDADDR already set
May 27 05:17:12 raspberrypi systemd[1]: Started Raspberry Pi bluetooth helper.
May 27 05:17:12 raspberrypi systemd[1]: Starting Bluetooth service...
May 27 05:17:12 raspberrypi systemd[1]: systemd-update-utmp-runlevel.service: Succeeded.
May 27 05:17:12 raspberrypi systemd[1]: Started Update UTMP about System Runlevel Changes.
May 27 05:17:12 raspberrypi kernel: [   17.286402] broken atomic modeset userspace detected, disabling atomic
May 27 05:17:12 raspberrypi bluetoothd[608]: Bluetooth daemon 5.50
May 27 05:17:12 raspberrypi systemd[1]: Started Bluetooth service.
May 27 05:17:12 raspberrypi systemd[1]: Reached target Bluetooth.
May 27 05:17:12 raspberrypi systemd[1]: Startup finished in 4.351s (kernel) + 12.990s (userspace) = 17.342s.
May 27 05:17:12 raspberrypi bluetoothd[608]: Starting SDP server
May 27 05:17:12 raspberrypi kernel: [   17.370023] Bluetooth: BNEP (Ethernet Emulation) ver 1.3
May 27 05:17:12 raspberrypi kernel: [   17.370033] Bluetooth: BNEP filters: protocol multicast
May 27 05:17:12 raspberrypi kernel: [   17.370048] Bluetooth: BNEP socket layer initialized
May 27 05:17:12 raspberrypi dbus-daemon[362]: [system] Activating via systemd: service name='org.freedesktop.hostname1' unit='dbus-org.freedesktop.hostname1.service' requested by ':1.23' (uid=0 pid=608 comm="/usr/lib/bluetooth/bluetoothd ")
May 27 05:17:12 raspberrypi bluetoothd[608]: Bluetooth management interface 1.18 initialized
May 27 05:17:12 raspberrypi bluetoothd[608]: Sap driver initialization failed.
May 27 05:17:12 raspberrypi bluetoothd[608]: sap-server: Operation not permitted (1)
May 27 05:17:12 raspberrypi systemd[1]: Starting Hostname Service...
May 27 05:17:12 raspberrypi bluetoothd[608]: Failed to set privacy: Rejected (0x0b)
May 27 05:17:12 raspberrypi dbus-daemon[362]: [system] Successfully activated service 'org.freedesktop.hostname1'
May 27 05:17:12 raspberrypi systemd[1]: Started Hostname Service.
May 27 05:17:13 raspberrypi kernel: [   17.911582] broken atomic modeset userspace detected, disabling atomic
May 27 05:17:13 raspberrypi systemd[1]: lightdm.service: Main process exited, code=exited, status=1/FAILURE
May 27 05:17:13 raspberrypi systemd[1]: lightdm.service: Failed with result 'exit-code'.
May 27 05:17:13 raspberrypi systemd[1]: lightdm.service: Service RestartSec=100ms expired, scheduling restart.
May 27 05:17:13 raspberrypi systemd[1]: lightdm.service: Scheduled restart job, restart counter is at 3.
May 27 05:17:13 raspberrypi systemd[1]: Stopped Light Display Manager.
May 27 05:17:13 raspberrypi systemd[1]: Starting Light Display Manager...
May 27 05:17:13 raspberrypi lightdm[623]: Error getting user list from org.freedesktop.Accounts: GDBus.Error:org.freedesktop.DBus.Error.ServiceUnknown: The name org.freedesktop.Accounts was not provided by any .service files
May 27 05:17:13 raspberrypi systemd[1]: Started Light Display Manager.
May 27 05:17:14 raspberrypi kernel: [   18.949339] broken atomic modeset userspace detected, disabling atomic
May 27 05:17:14 raspberrypi kernel: [   19.548199] broken atomic modeset userspace detected, disabling atomic
May 27 05:17:14 raspberrypi systemd[1]: lightdm.service: Main process exited, code=exited, status=1/FAILURE
May 27 05:17:14 raspberrypi systemd[1]: lightdm.service: Failed with result 'exit-code'.
May 27 05:17:15 raspberrypi bash[461]: ================================== > LOG REDIRECT system.adapter.admin.0 => false [Process stopped]
May 27 05:17:15 raspberrypi bash[461]: ================================== > LOG REDIRECT system.adapter.admin.0 => false [system.adapter.admin.0.logging]
May 27 05:17:15 raspberrypi systemd[1]: lightdm.service: Service RestartSec=100ms expired, scheduling restart.
May 27 05:17:15 raspberrypi systemd[1]: lightdm.service: Scheduled restart job, restart counter is at 4.
May 27 05:17:15 raspberrypi systemd[1]: Stopped Light Display Manager.
May 27 05:17:15 raspberrypi systemd[1]: Starting Light Display Manager...
May 27 05:17:15 raspberrypi lightdm[636]: Error getting user list from org.freedesktop.Accounts: GDBus.Error:org.freedesktop.DBus.Error.ServiceUnknown: The name org.freedesktop.Accounts was not provided by any .service files
May 27 05:17:15 raspberrypi systemd[1]: Started Light Display Manager.
May 27 05:17:15 raspberrypi dhcpcd[410]: eth0: using static address 192.168.0.250/24
May 27 05:17:15 raspberrypi dhcpcd[410]: eth0: adding route to 192.168.0.0/24
May 27 05:17:15 raspberrypi dhcpcd[410]: eth0: adding default route via 192.168.0.1
May 27 05:17:15 raspberrypi avahi-daemon[360]: Joining mDNS multicast group on interface eth0.IPv4 with address 192.168.0.250.
May 27 05:17:15 raspberrypi avahi-daemon[360]: New relevant interface eth0.IPv4 for mDNS.
May 27 05:17:15 raspberrypi avahi-daemon[360]: Registering new address record for 192.168.0.250 on eth0.IPv4.
May 27 05:17:16 raspberrypi kernel: [   20.585739] broken atomic modeset userspace detected, disabling atomic
May 27 05:17:16 raspberrypi kernel: [   21.204643] broken atomic modeset userspace detected, disabling atomic
May 27 05:17:16 raspberrypi systemd[1]: lightdm.service: Main process exited, code=exited, status=1/FAILURE
May 27 05:17:16 raspberrypi systemd[1]: lightdm.service: Failed with result 'exit-code'.
May 27 05:17:16 raspberrypi systemd[1]: lightdm.service: Service RestartSec=100ms expired, scheduling restart.
May 27 05:17:16 raspberrypi systemd[1]: lightdm.service: Scheduled restart job, restart counter is at 5.
May 27 05:17:16 raspberrypi systemd[1]: Stopped Light Display Manager.
May 27 05:17:16 raspberrypi systemd[1]: Starting Light Display Manager...
May 27 05:17:17 raspberrypi lightdm[701]: Error getting user list from org.freedesktop.Accounts: GDBus.Error:org.freedesktop.DBus.Error.ServiceUnknown: The name org.freedesktop.Accounts was not provided by any .service files
May 27 05:17:17 raspberrypi systemd[1]: Started Light Display Manager.
May 27 05:17:17 raspberrypi systemd[1]: systemd-rfkill.service: Succeeded.
May 27 05:17:17 raspberrypi bthelper[590]: Changing power off succeeded
May 27 05:17:17 raspberrypi kernel: [   22.270028] broken atomic modeset userspace detected, disabling atomic
May 27 05:17:17 raspberrypi bthelper[590]: Changing power on succeeded
May 27 05:17:18 raspberrypi kernel: [   22.882297] broken atomic modeset userspace detected, disabling atomic
May 27 05:17:18 raspberrypi systemd[1]: lightdm.service: Main process exited, code=exited, status=1/FAILURE
May 27 05:17:18 raspberrypi systemd[1]: lightdm.service: Failed with result 'exit-code'.
May 27 05:17:18 raspberrypi systemd[1]: lightdm.service: Service RestartSec=100ms expired, scheduling restart.
May 27 05:17:18 raspberrypi systemd[1]: lightdm.service: Scheduled restart job, restart counter is at 6.
May 27 05:17:18 raspberrypi systemd[1]: Stopped Light Display Manager.
May 27 05:17:18 raspberrypi systemd[1]: Starting Light Display Manager...
May 27 05:17:18 raspberrypi lightdm[721]: Error getting user list from org.freedesktop.Accounts: GDBus.Error:org.freedesktop.DBus.Error.ServiceUnknown: The name org.freedesktop.Accounts was not provided by any .service files
May 27 05:17:18 raspberrypi systemd[1]: Started Light Display Manager.
May 27 05:17:19 raspberrypi kernel: [   23.868702] broken atomic modeset userspace detected, disabling atomic
May 27 05:17:19 raspberrypi kernel: [   24.467995] broken atomic modeset userspace detected, disabling atomic
May 27 05:17:19 raspberrypi systemd[1]: lightdm.service: Main process exited, code=exited, status=1/FAILURE
May 27 05:17:19 raspberrypi systemd[1]: lightdm.service: Failed with result 'exit-code'.
May 27 05:17:20 raspberrypi systemd[1]: lightdm.service: Service RestartSec=100ms expired, scheduling restart.
May 27 05:17:20 raspberrypi systemd[1]: lightdm.service: Scheduled restart job, restart counter is at 7.
May 27 05:17:20 raspberrypi systemd[1]: Stopped Light Display Manager.
May 27 05:17:20 raspberrypi systemd[1]: Starting Light Display Manager...
May 27 05:17:20 raspberrypi lightdm[730]: Error getting user list from org.freedesktop.Accounts: GDBus.Error:org.freedesktop.DBus.Error.ServiceUnknown: The name org.freedesktop.Accounts was not provided by any .service files
May 27 05:17:20 raspberrypi systemd[1]: Started Light Display Manager.
May 27 05:17:20 raspberrypi kernel: [   25.518674] broken atomic modeset userspace detected, disabling atomic
May 27 05:17:21 raspberrypi kernel: [   26.112955] broken atomic modeset userspace detected, disabling atomic
May 27 05:17:21 raspberrypi systemd[1]: lightdm.service: Main process exited, code=exited, status=1/FAILURE
May 27 05:17:21 raspberrypi systemd[1]: lightdm.service: Failed with result 'exit-code'.
May 27 05:17:21 raspberrypi systemd[1]: lightdm.service: Service RestartSec=100ms expired, scheduling restart.
May 27 05:17:21 raspberrypi systemd[1]: lightdm.service: Scheduled restart job, restart counter is at 8.
May 27 05:17:21 raspberrypi systemd[1]: Stopped Light Display Manager.
May 27 05:17:21 raspberrypi systemd[1]: Starting Light Display Manager...
May 27 05:17:21 raspberrypi lightdm[746]: Error getting user list from org.freedesktop.Accounts: GDBus.Error:org.freedesktop.DBus.Error.ServiceUnknown: The name org.freedesktop.Accounts was not provided by any .service files
May 27 05:17:21 raspberrypi systemd[1]: Started Light Display Manager.
May 27 05:17:22 raspberrypi kernel: [   27.130341] broken atomic modeset userspace detected, disabling atomic
May 27 05:17:22 raspberrypi dhcpcd[410]: eth0: fe80::10:18ff:fea0:d144 is reachable again
May 27 05:17:22 raspberrypi dhcpcd[410]: eth0: fe80::10:18ff:fea0:d144 is reachable again
May 27 05:17:23 raspberrypi kernel: [   27.735130] broken atomic modeset userspace detected, disabling atomic
May 27 05:17:23 raspberrypi systemd[1]: lightdm.service: Main process exited, code=exited, status=1/FAILURE
May 27 05:17:23 raspberrypi systemd[1]: lightdm.service: Failed with result 'exit-code'.
May 27 05:17:23 raspberrypi systemd[1]: lightdm.service: Service RestartSec=100ms expired, scheduling restart.
May 27 05:17:23 raspberrypi systemd[1]: lightdm.service: Scheduled restart job, restart counter is at 9.
May 27 05:17:23 raspberrypi systemd[1]: Stopped Light Display Manager.
May 27 05:17:23 raspberrypi systemd[1]: Starting Light Display Manager...
May 27 05:17:23 raspberrypi lightdm[816]: Error getting user list from org.freedesktop.Accounts: GDBus.Error:org.freedesktop.DBus.Error.ServiceUnknown: The name org.freedesktop.Accounts was not provided by any .service files
May 27 05:17:23 raspberrypi systemd[1]: Started Light Display Manager.
May 27 05:17:24 raspberrypi kernel: [   28.784933] broken atomic modeset userspace detected, disabling atomic
May 27 05:17:24 raspberrypi kernel: [   29.395617] broken atomic modeset userspace detected, disabling atomic
May 27 05:17:24 raspberrypi systemd[1]: lightdm.service: Main process exited, code=exited, status=1/FAILURE
May 27 05:17:24 raspberrypi systemd[1]: lightdm.service: Failed with result 'exit-code'.
May 27 05:17:25 raspberrypi systemd[1]: lightdm.service: Service RestartSec=100ms expired, scheduling restart.
May 27 05:17:25 raspberrypi systemd[1]: lightdm.service: Scheduled restart job, restart counter is at 10.
May 27 05:17:25 raspberrypi systemd[1]: Stopped Light Display Manager.
May 27 05:17:25 raspberrypi systemd[1]: lightdm.service: Start request repeated too quickly.
May 27 05:17:25 raspberrypi systemd[1]: lightdm.service: Failed with result 'exit-code'.
May 27 05:17:25 raspberrypi systemd[1]: Failed to start Light Display Manager.
May 27 05:17:25 raspberrypi systemd[1]: lightdm.service: Triggering OnFailure= dependencies.
May 27 05:17:25 raspberrypi systemd[1]: Starting Terminate Plymouth Boot Screen...
May 27 05:17:25 raspberrypi systemd[1]: plymouth-quit.service: Succeeded.
May 27 05:17:25 raspberrypi systemd[1]: Started Terminate Plymouth Boot Screen.
May 27 05:17:34 raspberrypi systemd[1]: systemd-fsckd.service: Succeeded.
May 27 08:17:39 raspberrypi systemd-timesyncd[311]: Synchronized to time server for the first time [2a03:4000:28:365::1]:123 (2.debian.pool.ntp.org).
May 27 08:17:39 raspberrypi systemd[1]: Starting Daily apt upgrade and clean activities...
May 27 08:17:41 raspberrypi systemd[1]: apt-daily-upgrade.service: Succeeded.
May 27 08:17:41 raspberrypi systemd[1]: Started Daily apt upgrade and clean activities.
May 27 08:17:47 raspberrypi systemd[1]: systemd-hostnamed.service: Succeeded.
May 27 08:18:04 raspberrypi bash[461]: ================================== > LOG REDIRECT system.adapter.javascript.0 => false [Process stopped]
May 27 08:18:04 raspberrypi bash[461]: ================================== > LOG REDIRECT system.adapter.javascript.0 => false [system.adapter.javascript.0.logging]
May 27 08:18:28 raspberrypi systemd[1]: Started Session 3 of user pi.
May 27 08:18:41 raspberrypi systemd[1]: Started Session 4 of user pi.
May 27 08:18:43 raspberrypi dbus-daemon[362]: [system] Activating via systemd: service name='org.freedesktop.PackageKit' unit='packagekit.service' requested by ':1.53' (uid=0 pid=2269 comm="/usr/bin/gdbus call --system --dest org.freedeskto")
May 27 08:18:43 raspberrypi systemd[1]: Starting PackageKit Daemon...
May 27 08:18:43 raspberrypi PackageKit: daemon start
May 27 08:18:44 raspberrypi dbus-daemon[362]: [system] Successfully activated service 'org.freedesktop.PackageKit'
May 27 08:18:44 raspberrypi systemd[1]: Started PackageKit Daemon.
May 27 08:18:52 raspberrypi systemd[1]: session-4.scope: Succeeded.
May 27 08:19:04 raspberrypi bash[461]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 08:20:04 raspberrypi bash[461]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 08:21:04 raspberrypi bash[461]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 08:22:04 raspberrypi bash[461]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 08:23:04 raspberrypi bash[461]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 08:23:49 raspberrypi PackageKit: daemon quit
May 27 08:23:49 raspberrypi systemd[1]: packagekit.service: Main process exited, code=killed, status=15/TERM
May 27 08:23:49 raspberrypi systemd[1]: packagekit.service: Succeeded.
May 27 08:23:53 raspberrypi systemd[1]: Started Session 5 of user pi.
May 27 08:23:54 raspberrypi dbus-daemon[362]: [system] Activating via systemd: service name='org.freedesktop.PackageKit' unit='packagekit.service' requested by ':1.57' (uid=0 pid=4339 comm="/usr/bin/gdbus call --system --dest org.freedeskto")
May 27 08:23:54 raspberrypi systemd[1]: Starting PackageKit Daemon...
May 27 08:23:54 raspberrypi PackageKit: daemon start
May 27 08:23:54 raspberrypi dbus-daemon[362]: [system] Successfully activated service 'org.freedesktop.PackageKit'
May 27 08:23:54 raspberrypi systemd[1]: Started PackageKit Daemon.
May 27 08:24:00 raspberrypi systemd[1]: session-5.scope: Succeeded.
May 27 08:24:04 raspberrypi bash[461]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 08:25:04 raspberrypi bash[461]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 08:26:04 raspberrypi bash[461]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 08:27:04 raspberrypi bash[461]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 08:28:04 raspberrypi bash[461]: cat: /sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq: Keine Berechtigung
May 27 08:28:59 raspberrypi PackageKit: daemon quit
May 27 08:28:59 raspberrypi systemd[1]: packagekit.service: Main process exited, code=killed, status=15/TERM
May 27 08:28:59 raspberrypi systemd[1]: packagekit.service: Succeeded.