2021-12-16 16:31:01.712 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,2,97,19,1,0,113]	
2021-12-16 16:31:01.713 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 2 - 3 - 1 - 19 - [1,0] - 113	
2021-12-16 16:31:01.713 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- SYS - osalNvLength - {"length":1}	
2021-12-16 16:31:01.714 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:01.715 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> SYS - osalNvReadExt - {"id":96,"offset":0}	
2021-12-16 16:31:01.716 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,4,33,28,96,0,0,0,89]	
2021-12-16 16:31:01.722 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,97,28,0,1,85,42]	
2021-12-16 16:31:01.723 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,97,28,0,1,85,42]	
2021-12-16 16:31:01.724 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 3 - 1 - 28 - [0,1,85] - 42	
2021-12-16 16:31:01.724 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- SYS - osalNvReadExt - {"status":0,"len":1,"value":{"type":"Buffer","data":[85]}}	
2021-12-16 16:31:01.725 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:01.727 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> SYS - osalNvLength - {"id":33}	
2021-12-16 16:31:01.728 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,2,33,19,33,0,17]	
2021-12-16 16:31:01.732 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,2,97,19,116,0,4]	
2021-12-16 16:31:01.733 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,2,97,19,116,0,4]	
2021-12-16 16:31:01.734 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 2 - 3 - 1 - 19 - [116,0] - 4	
2021-12-16 16:31:01.734 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- SYS - osalNvLength - {"length":116}	
2021-12-16 16:31:01.735 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:01.736 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> SYS - osalNvReadExt - {"id":33,"offset":0}	
2021-12-16 16:31:01.736 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,4,33,28,33,0,0,0,24]	
2021-12-16 16:31:01.741 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,118,97,28,0,116,212,5]	
2021-12-16 16:31:01.742 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,118,97,28,0,116,212,5]	
2021-12-16 16:31:01.744 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [2,51,20,51,0,30,0,0,0,1,5,1,143,0,7,0,2,5,30,0,0,0,14,0]	
2021-12-16 16:31:01.745 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,118,97,28,0,116,212,5,2,51,20,51,0,30,0,0,0,1,5,1,143,0,7,0,2,5,30,0,0,0,14,0]	
2021-12-16 16:31:01.747 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [0,0,0,0,0,0,0,0,0,0,98,26,8,0,0,64,0,0,15,15,4,0,1,0,0,0,1,0,0,0,0,47]	
2021-12-16 16:31:01.747 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,118,97,28,0,116,212,5,2,51,20,51,0,30,0,0,0,1,5,1,143,0,7,0,2,5,30,0,0,0,14,0,0,0,0,0,0,0,0,0,0,0,98,26,8,0,0,64,0,0,15,15,4,0,1,0,0,0,1,0,0,0,0,47]	
2021-12-16 16:31:01.749 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [212,221,66,221,45,212,221,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]	
2021-12-16 16:31:01.750 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,118,97,28,0,116,212,5,2,51,20,51,0,30,0,0,0,1,5,1,143,0,7,0,2,5,30,0,0,0,14,0,0,0,0,0,0,0,0,0,0,0,98,26,8,0,0,64,0,0,15,15,4,0,1,0,0,0,1,0,0,0,0,47,212,221,66,221,45,212,221,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]	
2021-12-16 16:31:01.752 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [0,0,0,0,0,0,0,0,0,0,0,0,15,3,0,1,120,10,1,0,0,0,113,26,0,0,129]	
2021-12-16 16:31:01.753 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,118,97,28,0,116,212,5,2,51,20,51,0,30,0,0,0,1,5,1,143,0,7,0,2,5,30,0,0,0,14,0,0,0,0,0,0,0,0,0,0,0,98,26,8,0,0,64,0,0,15,15,4,0,1,0,0,0,1,0,0,0,0,47,212,221,66,221,45,212,221,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,3,0,1,120,10,1,0,0,0,113,26,0,0,129]	
2021-12-16 16:31:01.753 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 118 - 3 - 1 - 28 - [0,116,212,5,2,51,20,51,0,30,0,0,0,1,5,1,143,0,7,0,2,5,30,0,0,0,14,0,0,0,0,0,0,0,0,0,0,0,98,26,8,0,0,64,0,0,15,15,4,0,1,0,0,0,1,0,0,0,0,47,212,221,66,221,45,212,221,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,3,0,1,120,10,1,0,0,0,113,26,0,0] - 129	
2021-12-16 16:31:01.754 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- SYS - osalNvReadExt - {"status":0,"len":116,"value":{"type":"Buffer","data":[212,5,2,51,20,51,0,30,0,0,0,1,5,1,143,0,7,0,2,5,30,0,0,0,14,0,0,0,0,0,0,0,0,0,0,0,98,26,8,0,0,64,0,0,15,15,4,0,1,0,0,0,1,0,0,0,0,47,212,221,66,221,45,212,221,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,15,3,0,1,120,10,1,0,0,0,113,26,0,0]}}	
2021-12-16 16:31:01.754 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:01.757 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> SYS - osalNvLength - {"id":98}	
2021-12-16 16:31:01.757 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,2,33,19,98,0,82]	
2021-12-16 16:31:01.767 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,2,97,19,16,0,96]	
2021-12-16 16:31:01.767 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,2,97,19,16,0,96]	
2021-12-16 16:31:01.767 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 2 - 3 - 1 - 19 - [16,0] - 96	
2021-12-16 16:31:01.768 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- SYS - osalNvLength - {"length":16}	
2021-12-16 16:31:01.768 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:01.769 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> SYS - osalNvReadExt - {"id":98,"offset":0}	
2021-12-16 16:31:01.769 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,4,33,28,98,0,0,0,91]	
2021-12-16 16:31:01.784 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,18,97,28,0,16,1,3]	
2021-12-16 16:31:01.785 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,18,97,28,0,16,1,3]	
2021-12-16 16:31:01.786 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [5,7,9,11,13,15,0,2]	
2021-12-16 16:31:01.787 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,18,97,28,0,16,1,3,5,7,9,11,13,15,0,2]	
2021-12-16 16:31:01.789 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [4,6,8,10,12,13,124]	
2021-12-16 16:31:01.789 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,18,97,28,0,16,1,3,5,7,9,11,13,15,0,2,4,6,8,10,12,13,124]	
2021-12-16 16:31:01.790 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 18 - 3 - 1 - 28 - [0,16,1,3,5,7,9,11,13,15,0,2,4,6,8,10,12,13] - 124	
2021-12-16 16:31:01.790 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- SYS - osalNvReadExt - {"status":0,"len":16,"value":{"type":"Buffer","data":[1,3,5,7,9,11,13,15,0,2,4,6,8,10,12,13]}}	
2021-12-16 16:31:01.791 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:01.791 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> SYS - osalNvLength - {"id":58}	
2021-12-16 16:31:01.792 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,2,33,19,58,0,10]	
2021-12-16 16:31:01.797 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,2,97,19,17,0,97]	
2021-12-16 16:31:01.797 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,2,97,19,17,0,97]	
2021-12-16 16:31:01.798 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 2 - 3 - 1 - 19 - [17,0] - 97	
2021-12-16 16:31:01.799 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- SYS - osalNvLength - {"length":17}	
2021-12-16 16:31:01.800 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:01.800 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> SYS - osalNvReadExt - {"id":58,"offset":0}	
2021-12-16 16:31:01.801 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,4,33,28,58,0,0,0,3]	
2021-12-16 16:31:01.807 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,19,97,28,0,17,0,1]	
2021-12-16 16:31:01.807 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,19,97,28,0,17,0,1]	
2021-12-16 16:31:01.809 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [3,5,7,9,11,13,15,0,2,4,6,8,10,12,13,124]	
2021-12-16 16:31:01.810 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,19,97,28,0,17,0,1,3,5,7,9,11,13,15,0,2,4,6,8,10,12,13,124]	
2021-12-16 16:31:01.810 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 19 - 3 - 1 - 28 - [0,17,0,1,3,5,7,9,11,13,15,0,2,4,6,8,10,12,13] - 124	
2021-12-16 16:31:01.811 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- SYS - osalNvReadExt - {"status":0,"len":17,"value":{"type":"Buffer","data":[0,1,3,5,7,9,11,13,15,0,2,4,6,8,10,12,13]}}	
2021-12-16 16:31:01.811 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:01.812 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> SYS - osalNvLength - {"id":59}	
2021-12-16 16:31:01.812 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,2,33,19,59,0,11]	
2021-12-16 16:31:01.817 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,2,97,19,17,0,97]	
2021-12-16 16:31:01.817 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,2,97,19,17,0,97]	
2021-12-16 16:31:01.818 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 2 - 3 - 1 - 19 - [17,0] - 97	
2021-12-16 16:31:01.818 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- SYS - osalNvLength - {"length":17}	
2021-12-16 16:31:01.819 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:01.820 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> SYS - osalNvReadExt - {"id":59,"offset":0}	
2021-12-16 16:31:01.821 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,4,33,28,59,0,0,0,2]	
2021-12-16 16:31:01.826 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,19,97,28,0,17,0,1]	
2021-12-16 16:31:01.827 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,19,97,28,0,17,0,1]	
2021-12-16 16:31:01.829 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [3,5,7,9,11,13,15,0,2,4,6,8,10,12,13,124]	
2021-12-16 16:31:01.829 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,19,97,28,0,17,0,1,3,5,7,9,11,13,15,0,2,4,6,8,10,12,13,124]	
2021-12-16 16:31:01.830 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 19 - 3 - 1 - 28 - [0,17,0,1,3,5,7,9,11,13,15,0,2,4,6,8,10,12,13] - 124	
2021-12-16 16:31:01.830 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- SYS - osalNvReadExt - {"status":0,"len":17,"value":{"type":"Buffer","data":[0,1,3,5,7,9,11,13,15,0,2,4,6,8,10,12,13]}}	
2021-12-16 16:31:01.831 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:01.839 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:startup:strategy (stage-1) adapter is configured	
2021-12-16 16:31:01.839 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:startup:strategy (stage-2) extended pan id is reversed	
2021-12-16 16:31:01.840 - warn: zigbee.0 (26219) Extended PAN ID is reversed (expected=2fd4dd42dd2dd4dd, actual=ddd42ddd42ddd42f)	
2021-12-16 16:31:01.841 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:startup:strategy (stage-2) adapter state matches configuration	
2021-12-16 16:31:01.841 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:startup determined startup strategy: startup	
2021-12-16 16:31:01.842 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> UTIL - getDeviceInfo - {}	
2021-12-16 16:31:01.843 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,0,39,0,39]	
2021-12-16 16:31:01.851 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,46,103,0,0,140,193,159]	
2021-12-16 16:31:01.852 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,46,103,0,0,140,193,159]	
2021-12-16 16:31:01.853 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [33,0,75,18,0,0,0,7,9,16,148,248,142,241,241,69]	
2021-12-16 16:31:01.854 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,46,103,0,0,140,193,159,33,0,75,18,0,0,0,7,9,16,148,248,142,241,241,69]	
2021-12-16 16:31:01.856 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [11,40,144,237,132,179,49,116,91,206,165,62,157,213,211,168,126,240,122,16,109,194,187,209]	
2021-12-16 16:31:01.857 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,46,103,0,0,140,193,159,33,0,75,18,0,0,0,7,9,16,148,248,142,241,241,69,11,40,144,237,132,179,49,116,91,206,165,62,157,213,211,168,126,240,122,16,109,194,187,209]	
2021-12-16 16:31:01.858 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [162,173,101]	
2021-12-16 16:31:01.859 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,46,103,0,0,140,193,159,33,0,75,18,0,0,0,7,9,16,148,248,142,241,241,69,11,40,144,237,132,179,49,116,91,206,165,62,157,213,211,168,126,240,122,16,109,194,187,209,162,173,101]	
2021-12-16 16:31:01.860 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 46 - 3 - 7 - 0 - [0,140,193,159,33,0,75,18,0,0,0,7,9,16,148,248,142,241,241,69,11,40,144,237,132,179,49,116,91,206,165,62,157,213,211,168,126,240,122,16,109,194,187,209,162,173] - 101	
2021-12-16 16:31:01.860 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- UTIL - getDeviceInfo - {"status":0,"ieeeaddr":"0x00124b00219fc18c","shortaddr":0,"devicetype":7,"devicestate":9,"numassocdevices":16,"assocdeviceslist":[63636,61838,17905,10251,60816,45956,29745,52827,16037,54685,43219,61566,4218,49773,53691,44450]}	
2021-12-16 16:31:01.861 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:01.861 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:startup adapter is already running in coordinator mode	
2021-12-16 16:31:01.862 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - activeEpReq - {"dstaddr":0,"nwkaddrofinterest":0}	
2021-12-16 16:31:01.863 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,4,37,5,0,0,0,0,36]	
2021-12-16 16:31:01.867 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,5,0,97,254,20]	
2021-12-16 16:31:01.868 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,5,0,97,254,20]	
2021-12-16 16:31:01.868 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 5 - [0] - 97	
2021-12-16 16:31:01.869 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - activeEpReq - {"status":0}	
2021-12-16 16:31:01.870 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,20]	
2021-12-16 16:31:01.872 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [69,133,0,0,0,0,0,14,242,47,13,12,110,11,10,8,6,5,4,3,2,1,102]	
2021-12-16 16:31:01.873 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,20,69,133,0,0,0,0,0,14,242,47,13,12,110,11,10,8,6,5,4,3,2,1,102]	
2021-12-16 16:31:01.873 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 20 - 2 - 5 - 133 - [0,0,0,0,0,14,242,47,13,12,110,11,10,8,6,5,4,3,2,1] - 102	
2021-12-16 16:31:01.874 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - activeEpRsp - {"srcaddr":0,"status":0,"nwkaddr":0,"activeepcount":14,"activeeplist":[242,47,13,12,110,11,10,8,6,5,4,3,2,1]}	
2021-12-16 16:31:01.875 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:01.875 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:startup endpoint '1' already registered	
2021-12-16 16:31:01.875 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:startup endpoint '2' already registered	
2021-12-16 16:31:01.876 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:startup endpoint '3' already registered	
2021-12-16 16:31:01.876 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:startup endpoint '4' already registered	
2021-12-16 16:31:01.876 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:startup endpoint '5' already registered	
2021-12-16 16:31:01.877 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:startup endpoint '6' already registered	
2021-12-16 16:31:01.877 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:startup endpoint '8' already registered	
2021-12-16 16:31:01.877 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:startup endpoint '10' already registered	
2021-12-16 16:31:01.877 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:startup endpoint '11' already registered	
2021-12-16 16:31:01.878 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:startup endpoint '110' already registered	
2021-12-16 16:31:01.878 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:startup endpoint '12' already registered	
2021-12-16 16:31:01.878 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:startup endpoint '13' already registered	
2021-12-16 16:31:01.878 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:startup endpoint '47' already registered	
2021-12-16 16:31:01.879 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:startup endpoint '242' already registered	
2021-12-16 16:31:01.879 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - extFindGroup - {"endpoint":242,"groupid":2948}	
2021-12-16 16:31:01.880 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,74,242,132,11,17]	
2021-12-16 16:31:01.889 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,19,101,74,0,132,11,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,179]	
2021-12-16 16:31:01.889 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,19,101,74,0,132,11,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,179]	
2021-12-16 16:31:01.890 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 19 - 3 - 5 - 74 - [0,132,11,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0] - 179	
2021-12-16 16:31:01.891 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - extFindGroup - {"status":0,"groupid":2948,"namelen":0,"groupname":{"type":"Buffer","data":[]}}	
2021-12-16 16:31:01.891 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:01.892 - debug: zigbee.0 (26219) zigbee-herdsman:controller:log Started with result 'resumed'	
2021-12-16 16:31:01.893 - debug: zigbee.0 (26219) zigbee-herdsman:controller:log Injected database: true, adapter: true	
2021-12-16 16:31:01.894 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - activeEpReq - {"dstaddr":0,"nwkaddrofinterest":0}	
2021-12-16 16:31:01.895 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,4,37,5,0,0,0,0,36]	
2021-12-16 16:31:01.899 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,5,0,97,254,20]	
2021-12-16 16:31:01.900 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,5,0,97,254,20]	
2021-12-16 16:31:01.901 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 5 - [0] - 97	
2021-12-16 16:31:01.901 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - activeEpReq - {"status":0}	
2021-12-16 16:31:01.902 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,20]	
2021-12-16 16:31:01.904 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [69,133,0,0,0,0,0,14,242,47,13,12,110,11,10,8,6,5,4,3,2,1,102]	
2021-12-16 16:31:01.905 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,20,69,133,0,0,0,0,0,14,242,47,13,12,110,11,10,8,6,5,4,3,2,1,102]	
2021-12-16 16:31:01.906 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 20 - 2 - 5 - 133 - [0,0,0,0,0,14,242,47,13,12,110,11,10,8,6,5,4,3,2,1] - 102	
2021-12-16 16:31:01.906 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - activeEpRsp - {"srcaddr":0,"status":0,"nwkaddr":0,"activeepcount":14,"activeeplist":[242,47,13,12,110,11,10,8,6,5,4,3,2,1]}	
2021-12-16 16:31:01.907 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:01.907 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> UTIL - getDeviceInfo - {}	
2021-12-16 16:31:01.908 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,0,39,0,39]	
2021-12-16 16:31:01.916 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,46,103,0,0,140,193,159]	
2021-12-16 16:31:01.917 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,46,103,0,0,140,193,159]	
2021-12-16 16:31:01.918 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [33,0,75,18,0,0,0,7,9,16,148,248,142,241,241,69]	
2021-12-16 16:31:01.919 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,46,103,0,0,140,193,159,33,0,75,18,0,0,0,7,9,16,148,248,142,241,241,69]	
2021-12-16 16:31:01.921 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [11,40,144,237,132,179,49,116,91,206,165,62,157,213,211,168,126,240,122,16,109,194,187,209]	
2021-12-16 16:31:01.922 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,46,103,0,0,140,193,159,33,0,75,18,0,0,0,7,9,16,148,248,142,241,241,69,11,40,144,237,132,179,49,116,91,206,165,62,157,213,211,168,126,240,122,16,109,194,187,209]	
2021-12-16 16:31:01.923 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [162,173,101]	
2021-12-16 16:31:01.924 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,46,103,0,0,140,193,159,33,0,75,18,0,0,0,7,9,16,148,248,142,241,241,69,11,40,144,237,132,179,49,116,91,206,165,62,157,213,211,168,126,240,122,16,109,194,187,209,162,173,101]	
2021-12-16 16:31:01.925 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 46 - 3 - 7 - 0 - [0,140,193,159,33,0,75,18,0,0,0,7,9,16,148,248,142,241,241,69,11,40,144,237,132,179,49,116,91,206,165,62,157,213,211,168,126,240,122,16,109,194,187,209,162,173] - 101	
2021-12-16 16:31:01.925 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- UTIL - getDeviceInfo - {"status":0,"ieeeaddr":"0x00124b00219fc18c","shortaddr":0,"devicetype":7,"devicestate":9,"numassocdevices":16,"assocdeviceslist":[63636,61838,17905,10251,60816,45956,29745,52827,16037,54685,43219,61566,4218,49773,53691,44450]}	
2021-12-16 16:31:01.926 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:01.926 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - simpleDescReq - {"dstaddr":0,"nwkaddrofinterest":0,"endpoint":242}	
2021-12-16 16:31:01.926 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,5,37,4,0,0,0,0,242,214]	
2021-12-16 16:31:01.931 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,4,0,96,254,14]	
2021-12-16 16:31:01.931 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,4,0,96,254,14]	
2021-12-16 16:31:01.932 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 4 - [0] - 96	
2021-12-16 16:31:01.932 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - simpleDescReq - {"status":0}	
2021-12-16 16:31:01.933 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14]	
2021-12-16 16:31:01.935 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [69,132,0,0,0,0,0,8,242,224,161,5,0,0,0,0,113]	
2021-12-16 16:31:01.936 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14,69,132,0,0,0,0,0,8,242,224,161,5,0,0,0,0,113]	
2021-12-16 16:31:01.936 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 14 - 2 - 5 - 132 - [0,0,0,0,0,8,242,224,161,5,0,0,0,0] - 113	
2021-12-16 16:31:01.937 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - simpleDescRsp - {"srcaddr":0,"status":0,"nwkaddr":0,"len":8,"endpoint":242,"profileid":41440,"deviceid":5,"deviceversion":0,"numinclusters":0,"inclusterlist":[],"numoutclusters":0,"outclusterlist":[]}	
2021-12-16 16:31:01.938 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:01.938 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - simpleDescReq - {"dstaddr":0,"nwkaddrofinterest":0,"endpoint":47}	
2021-12-16 16:31:01.939 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,5,37,4,0,0,0,0,47,11]	
2021-12-16 16:31:01.943 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,4,0,96,254,14]	
2021-12-16 16:31:01.944 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,4,0,96,254,14]	
2021-12-16 16:31:01.944 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 4 - [0] - 96	
2021-12-16 16:31:01.945 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - simpleDescReq - {"status":0}	
2021-12-16 16:31:01.945 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14]	
2021-12-16 16:31:01.948 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [69,132,0,0,0,0,0,8,47,4,1,5,0,0,0,0,232]	
2021-12-16 16:31:01.951 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14,69,132,0,0,0,0,0,8,47,4,1,5,0,0,0,0,232]	
2021-12-16 16:31:01.952 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 14 - 2 - 5 - 132 - [0,0,0,0,0,8,47,4,1,5,0,0,0,0] - 232	
2021-12-16 16:31:01.952 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - simpleDescRsp - {"srcaddr":0,"status":0,"nwkaddr":0,"len":8,"endpoint":47,"profileid":260,"deviceid":5,"deviceversion":0,"numinclusters":0,"inclusterlist":[],"numoutclusters":0,"outclusterlist":[]}	
2021-12-16 16:31:01.953 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:01.953 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - simpleDescReq - {"dstaddr":0,"nwkaddrofinterest":0,"endpoint":13}	
2021-12-16 16:31:01.954 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,5,37,4,0,0,0,0,13,41]	
2021-12-16 16:31:01.961 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,4,0,96,254,16,69,132,0,0,0,0,0,10,13,4,1,5,0,0,1,25,0,0,206]	
2021-12-16 16:31:01.961 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,4,0,96,254,16,69,132,0,0,0,0,0,10,13,4,1,5,0,0,1,25,0,0,206]	
2021-12-16 16:31:01.962 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 4 - [0] - 96	
2021-12-16 16:31:01.962 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - simpleDescReq - {"status":0}	
2021-12-16 16:31:01.963 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,16,69,132,0,0,0,0,0,10,13,4,1,5,0,0,1,25,0,0,206]	
2021-12-16 16:31:01.963 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 16 - 2 - 5 - 132 - [0,0,0,0,0,10,13,4,1,5,0,0,1,25,0,0] - 206	
2021-12-16 16:31:01.963 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - simpleDescRsp - {"srcaddr":0,"status":0,"nwkaddr":0,"len":10,"endpoint":13,"profileid":260,"deviceid":5,"deviceversion":0,"numinclusters":1,"inclusterlist":[25],"numoutclusters":0,"outclusterlist":[]}	
2021-12-16 16:31:01.964 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:01.964 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - simpleDescReq - {"dstaddr":0,"nwkaddrofinterest":0,"endpoint":12}	
2021-12-16 16:31:01.965 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,5,37,4,0,0,0,0,12,40]	
2021-12-16 16:31:01.971 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,4,0,96,254,14,69,132,0,0,0,0,0,8,12,94,192,5,0,0,0,0,80]	
2021-12-16 16:31:01.971 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,4,0,96,254,14,69,132,0,0,0,0,0,8,12,94,192,5,0,0,0,0,80]	
2021-12-16 16:31:01.972 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 4 - [0] - 96	
2021-12-16 16:31:01.972 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - simpleDescReq - {"status":0}	
2021-12-16 16:31:01.973 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14,69,132,0,0,0,0,0,8,12,94,192,5,0,0,0,0,80]	
2021-12-16 16:31:01.973 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 14 - 2 - 5 - 132 - [0,0,0,0,0,8,12,94,192,5,0,0,0,0] - 80	
2021-12-16 16:31:01.974 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - simpleDescRsp - {"srcaddr":0,"status":0,"nwkaddr":0,"len":8,"endpoint":12,"profileid":49246,"deviceid":5,"deviceversion":0,"numinclusters":0,"inclusterlist":[],"numoutclusters":0,"outclusterlist":[]}	
2021-12-16 16:31:01.974 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:01.974 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - simpleDescReq - {"dstaddr":0,"nwkaddrofinterest":0,"endpoint":110}	
2021-12-16 16:31:01.975 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,5,37,4,0,0,0,0,110,74]	
2021-12-16 16:31:01.986 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,4,0,96,254,14,69,132,0,0,0,0,0,8,110,4,1,5,0,0,0,0,169]	
2021-12-16 16:31:01.986 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,4,0,96,254,14,69,132,0,0,0,0,0,8,110,4,1,5,0,0,0,0,169]	
2021-12-16 16:31:01.987 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 4 - [0] - 96	
2021-12-16 16:31:01.987 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - simpleDescReq - {"status":0}	
2021-12-16 16:31:01.987 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14,69,132,0,0,0,0,0,8,110,4,1,5,0,0,0,0,169]	
2021-12-16 16:31:01.988 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 14 - 2 - 5 - 132 - [0,0,0,0,0,8,110,4,1,5,0,0,0,0] - 169	
2021-12-16 16:31:01.988 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - simpleDescRsp - {"srcaddr":0,"status":0,"nwkaddr":0,"len":8,"endpoint":110,"profileid":260,"deviceid":5,"deviceversion":0,"numinclusters":0,"inclusterlist":[],"numoutclusters":0,"outclusterlist":[]}	
2021-12-16 16:31:01.988 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:01.989 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - simpleDescReq - {"dstaddr":0,"nwkaddrofinterest":0,"endpoint":11}	
2021-12-16 16:31:01.989 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,5,37,4,0,0,0,0,11,47]	
2021-12-16 16:31:01.999 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,4,0,96,254,20,69,132,0,0,0,0,0,14,11,4,1,0,4,0,1,1,5,2,0,5,2,5,212]	
2021-12-16 16:31:02.000 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,4,0,96,254,20,69,132,0,0,0,0,0,14,11,4,1,0,4,0,1,1,5,2,0,5,2,5,212]	
2021-12-16 16:31:02.000 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 4 - [0] - 96	
2021-12-16 16:31:02.001 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - simpleDescReq - {"status":0}	
2021-12-16 16:31:02.001 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,20,69,132,0,0,0,0,0,14,11,4,1,0,4,0,1,1,5,2,0,5,2,5,212]	
2021-12-16 16:31:02.001 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 20 - 2 - 5 - 132 - [0,0,0,0,0,14,11,4,1,0,4,0,1,1,5,2,0,5,2,5] - 212	
2021-12-16 16:31:02.002 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - simpleDescRsp - {"srcaddr":0,"status":0,"nwkaddr":0,"len":14,"endpoint":11,"profileid":260,"deviceid":1024,"deviceversion":0,"numinclusters":1,"inclusterlist":[1281],"numoutclusters":2,"outclusterlist":[1280,1282]}	
2021-12-16 16:31:02.002 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:02.002 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - simpleDescReq - {"dstaddr":0,"nwkaddrofinterest":0,"endpoint":10}	
2021-12-16 16:31:02.003 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,5,37,4,0,0,0,0,10,46]	
2021-12-16 16:31:02.007 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,4,0,96,254,14]	
2021-12-16 16:31:02.008 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,4,0,96,254,14]	
2021-12-16 16:31:02.009 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 4 - [0] - 96	
2021-12-16 16:31:02.009 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - simpleDescReq - {"status":0}	
2021-12-16 16:31:02.010 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14]	
2021-12-16 16:31:02.012 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [69,132,0,0,0,0,0,8,10,4,1,5,0,0,0,0,205]	
2021-12-16 16:31:02.013 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14,69,132,0,0,0,0,0,8,10,4,1,5,0,0,0,0,205]	
2021-12-16 16:31:02.014 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 14 - 2 - 5 - 132 - [0,0,0,0,0,8,10,4,1,5,0,0,0,0] - 205	
2021-12-16 16:31:02.014 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - simpleDescRsp - {"srcaddr":0,"status":0,"nwkaddr":0,"len":8,"endpoint":10,"profileid":260,"deviceid":5,"deviceversion":0,"numinclusters":0,"inclusterlist":[],"numoutclusters":0,"outclusterlist":[]}	
2021-12-16 16:31:02.015 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:02.015 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - simpleDescReq - {"dstaddr":0,"nwkaddrofinterest":0,"endpoint":8}	
2021-12-16 16:31:02.016 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,5,37,4,0,0,0,0,8,44]	
2021-12-16 16:31:02.021 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,4,0,96,254,14]	
2021-12-16 16:31:02.022 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,4,0,96,254,14]	
2021-12-16 16:31:02.022 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 4 - [0] - 96	
2021-12-16 16:31:02.023 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - simpleDescReq - {"status":0}	
2021-12-16 16:31:02.024 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14]	
2021-12-16 16:31:02.031 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [69,132,0,0,0,0,0,8,8,4,1,5,0,0,0,0,207]	
2021-12-16 16:31:02.031 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14,69,132,0,0,0,0,0,8,8,4,1,5,0,0,0,0,207]	
2021-12-16 16:31:02.032 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 14 - 2 - 5 - 132 - [0,0,0,0,0,8,8,4,1,5,0,0,0,0] - 207	
2021-12-16 16:31:02.032 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - simpleDescRsp - {"srcaddr":0,"status":0,"nwkaddr":0,"len":8,"endpoint":8,"profileid":260,"deviceid":5,"deviceversion":0,"numinclusters":0,"inclusterlist":[],"numoutclusters":0,"outclusterlist":[]}	
2021-12-16 16:31:02.033 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:02.033 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - simpleDescReq - {"dstaddr":0,"nwkaddrofinterest":0,"endpoint":6}	
2021-12-16 16:31:02.033 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,5,37,4,0,0,0,0,6,34]	
2021-12-16 16:31:02.038 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,4,0,96,254,14]	
2021-12-16 16:31:02.038 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,4,0,96,254,14]	
2021-12-16 16:31:02.039 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 4 - [0] - 96	
2021-12-16 16:31:02.039 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - simpleDescReq - {"status":0}	
2021-12-16 16:31:02.040 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14]	
2021-12-16 16:31:02.042 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [69,132,0,0,0,0,0,8,6,9,1,5,0,0,0,0,204]	
2021-12-16 16:31:02.043 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14,69,132,0,0,0,0,0,8,6,9,1,5,0,0,0,0,204]	
2021-12-16 16:31:02.043 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 14 - 2 - 5 - 132 - [0,0,0,0,0,8,6,9,1,5,0,0,0,0] - 204	
2021-12-16 16:31:02.044 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - simpleDescRsp - {"srcaddr":0,"status":0,"nwkaddr":0,"len":8,"endpoint":6,"profileid":265,"deviceid":5,"deviceversion":0,"numinclusters":0,"inclusterlist":[],"numoutclusters":0,"outclusterlist":[]}	
2021-12-16 16:31:02.045 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:02.045 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - simpleDescReq - {"dstaddr":0,"nwkaddrofinterest":0,"endpoint":5}	
2021-12-16 16:31:02.046 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,5,37,4,0,0,0,0,5,33]	
2021-12-16 16:31:02.050 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,4,0,96,254,14]	
2021-12-16 16:31:02.051 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,4,0,96,254,14]	
2021-12-16 16:31:02.051 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 4 - [0] - 96	
2021-12-16 16:31:02.052 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - simpleDescReq - {"status":0}	
2021-12-16 16:31:02.052 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14]	
2021-12-16 16:31:02.055 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [69,132,0,0,0,0,0,8,5,8,1,5,0,0,0,0,206]	
2021-12-16 16:31:02.055 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14,69,132,0,0,0,0,0,8,5,8,1,5,0,0,0,0,206]	
2021-12-16 16:31:02.056 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 14 - 2 - 5 - 132 - [0,0,0,0,0,8,5,8,1,5,0,0,0,0] - 206	
2021-12-16 16:31:02.057 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - simpleDescRsp - {"srcaddr":0,"status":0,"nwkaddr":0,"len":8,"endpoint":5,"profileid":264,"deviceid":5,"deviceversion":0,"numinclusters":0,"inclusterlist":[],"numoutclusters":0,"outclusterlist":[]}	
2021-12-16 16:31:02.057 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:02.058 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - simpleDescReq - {"dstaddr":0,"nwkaddrofinterest":0,"endpoint":4}	
2021-12-16 16:31:02.059 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,5,37,4,0,0,0,0,4,32]	
2021-12-16 16:31:02.064 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,4,0,96,254,14]	
2021-12-16 16:31:02.064 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,4,0,96,254,14]	
2021-12-16 16:31:02.065 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 4 - [0] - 96	
2021-12-16 16:31:02.065 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - simpleDescReq - {"status":0}	
2021-12-16 16:31:02.066 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14]	
2021-12-16 16:31:02.068 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [69,132,0,0,0,0,0,8,4,7,1,5,0,0,0,0,192]	
2021-12-16 16:31:02.069 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14,69,132,0,0,0,0,0,8,4,7,1,5,0,0,0,0,192]	
2021-12-16 16:31:02.070 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 14 - 2 - 5 - 132 - [0,0,0,0,0,8,4,7,1,5,0,0,0,0] - 192	
2021-12-16 16:31:02.070 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - simpleDescRsp - {"srcaddr":0,"status":0,"nwkaddr":0,"len":8,"endpoint":4,"profileid":263,"deviceid":5,"deviceversion":0,"numinclusters":0,"inclusterlist":[],"numoutclusters":0,"outclusterlist":[]}	
2021-12-16 16:31:02.071 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:02.071 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - simpleDescReq - {"dstaddr":0,"nwkaddrofinterest":0,"endpoint":3}	
2021-12-16 16:31:02.072 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,5,37,4,0,0,0,0,3,39]	
2021-12-16 16:31:02.078 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,4,0,96,254,14]	
2021-12-16 16:31:02.079 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,4,0,96,254,14]	
2021-12-16 16:31:02.079 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 4 - [0] - 96	
2021-12-16 16:31:02.080 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - simpleDescReq - {"status":0}	
2021-12-16 16:31:02.081 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14]	
2021-12-16 16:31:02.083 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [69,132,0,0,0,0,0,8,3,4,1,5,0,0,0,0,196]	
2021-12-16 16:31:02.084 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14,69,132,0,0,0,0,0,8,3,4,1,5,0,0,0,0,196]	
2021-12-16 16:31:02.084 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 14 - 2 - 5 - 132 - [0,0,0,0,0,8,3,4,1,5,0,0,0,0] - 196	
2021-12-16 16:31:02.085 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - simpleDescRsp - {"srcaddr":0,"status":0,"nwkaddr":0,"len":8,"endpoint":3,"profileid":260,"deviceid":5,"deviceversion":0,"numinclusters":0,"inclusterlist":[],"numoutclusters":0,"outclusterlist":[]}	
2021-12-16 16:31:02.086 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:02.087 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - simpleDescReq - {"dstaddr":0,"nwkaddrofinterest":0,"endpoint":2}	
2021-12-16 16:31:02.087 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,5,37,4,0,0,0,0,2,38]	
2021-12-16 16:31:02.091 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,4,0,96,254,14]	
2021-12-16 16:31:02.092 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,4,0,96,254,14]	
2021-12-16 16:31:02.093 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 4 - [0] - 96	
2021-12-16 16:31:02.093 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - simpleDescReq - {"status":0}	
2021-12-16 16:31:02.094 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14]	
2021-12-16 16:31:02.100 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [69,132,0,0,0,0,0,8,2,1,1,5,0,0,0,0,192]	
2021-12-16 16:31:02.100 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14,69,132,0,0,0,0,0,8,2,1,1,5,0,0,0,0,192]	
2021-12-16 16:31:02.101 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 14 - 2 - 5 - 132 - [0,0,0,0,0,8,2,1,1,5,0,0,0,0] - 192	
2021-12-16 16:31:02.101 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - simpleDescRsp - {"srcaddr":0,"status":0,"nwkaddr":0,"len":8,"endpoint":2,"profileid":257,"deviceid":5,"deviceversion":0,"numinclusters":0,"inclusterlist":[],"numoutclusters":0,"outclusterlist":[]}	
2021-12-16 16:31:02.102 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:02.102 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - simpleDescReq - {"dstaddr":0,"nwkaddrofinterest":0,"endpoint":1}	
2021-12-16 16:31:02.103 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,5,37,4,0,0,0,0,1,37]	
2021-12-16 16:31:02.108 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,4,0,96,254,14,69,132,0,0,0,0,0,8]	
2021-12-16 16:31:02.109 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,4,0,96,254,14,69,132,0,0,0,0,0,8]	
2021-12-16 16:31:02.109 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 4 - [0] - 96	
2021-12-16 16:31:02.110 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - simpleDescReq - {"status":0}	
2021-12-16 16:31:02.110 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14,69,132,0,0,0,0,0,8]	
2021-12-16 16:31:02.113 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [1,4,1,5,0,0,0,0,198]	
2021-12-16 16:31:02.114 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,14,69,132,0,0,0,0,0,8,1,4,1,5,0,0,0,0,198]	
2021-12-16 16:31:02.114 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 14 - 2 - 5 - 132 - [0,0,0,0,0,8,1,4,1,5,0,0,0,0] - 198	
2021-12-16 16:31:02.115 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - simpleDescRsp - {"srcaddr":0,"status":0,"nwkaddr":0,"len":8,"endpoint":1,"profileid":260,"deviceid":5,"deviceversion":0,"numinclusters":0,"inclusterlist":[],"numoutclusters":0,"outclusterlist":[]}	
2021-12-16 16:31:02.115 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:02.119 - debug: zigbee.0 (26219) zigbee-herdsman started	
2021-12-16 16:31:02.120 - info: zigbee.0 (26219) Coordinator firmware version: {"type":"zStack3x0","meta":{"transportrev":2,"product":1,"majorrel":2,"minorrel":7,"maintrel":1,"revision":20201026}}	
2021-12-16 16:31:02.121 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - extNwkInfo - {}	
2021-12-16 16:31:02.122 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,0,37,80,117]	
2021-12-16 16:31:02.127 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,24,101,80,0,0,9,98,26,0,0,47,212,221,66,221,45,212,221,0,0,0,0,0,0,0,0,14,207]	
2021-12-16 16:31:02.128 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,24,101,80,0,0,9,98,26,0,0,47,212,221,66,221,45,212,221,0,0,0,0,0,0,0,0,14,207]	
2021-12-16 16:31:02.129 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 24 - 3 - 5 - 80 - [0,0,9,98,26,0,0,47,212,221,66,221,45,212,221,0,0,0,0,0,0,0,0,14] - 207	
2021-12-16 16:31:02.130 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - extNwkInfo - {"shortaddr":0,"devstate":9,"panid":6754,"parentaddr":0,"extendedpanid":"0xddd42ddd42ddd42f","parentextaddr":"0x0000000000000000","channel":14}	
2021-12-16 16:31:02.130 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:02.131 - debug: zigbee.0 (26219) Zigbee network parameters: panID=6754 channel=14 extendedPanID=2fd4dd42dd2dd4dd	
2021-12-16 16:31:02.132 - info: zigbee.0 (26219) Unable to disable LED, unsupported function.	
2021-12-16 16:31:02.132 - info: zigbee.0 (26219) --> transmitPower : high	
2021-12-16 16:31:02.133 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> SYS - stackTune - {"operation":0,"value":"19"}	
2021-12-16 16:31:02.134 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,2,33,15,0,19,63]	
2021-12-16 16:31:02.138 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,97,15,0,111]	
2021-12-16 16:31:02.138 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,97,15,0,111]	
2021-12-16 16:31:02.139 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 1 - 15 - [0] - 111	
2021-12-16 16:31:02.140 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- SYS - stackTune - {"value":0}	
2021-12-16 16:31:02.140 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:02.146 - info: zigbee.0 (26219) Currently 40 devices are joined:	
2021-12-16 16:31:02.146 - debug: zigbee.0 (26219) Publish available for 0x00158d0002b54a17 = true	
2021-12-16 16:31:02.150 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002b54a17 = 10	
2021-12-16 16:31:02.154 - debug: zigbee.0 (26219) Publish available for 0x00158d0002130d3b = true	
2021-12-16 16:31:02.159 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002130d3b = 10	
2021-12-16 16:31:02.162 - debug: zigbee.0 (26219) Publish available for 0x00158d0002130f3a = true	
2021-12-16 16:31:02.166 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002130f3a = 10	
2021-12-16 16:31:02.167 - debug: zigbee.0 (26219) Publish available for 0x00158d0002f8d76c = true	
2021-12-16 16:31:02.169 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002f8d76c = 10	
2021-12-16 16:31:02.170 - debug: zigbee.0 (26219) Publish available for 0x00158d000274f4de = true	
2021-12-16 16:31:02.171 - debug: zigbee.0 (26219) Publish LQ for 0x00158d000274f4de = 10	
2021-12-16 16:31:02.173 - debug: zigbee.0 (26219) Publish available for 0x00158d0002135d9b = true	
2021-12-16 16:31:02.174 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002135d9b = 10	
2021-12-16 16:31:02.175 - debug: zigbee.0 (26219) Publish available for 0x00158d000274f4bf = true	
2021-12-16 16:31:02.177 - debug: zigbee.0 (26219) Publish LQ for 0x00158d000274f4bf = 10	
2021-12-16 16:31:02.178 - debug: zigbee.0 (26219) Publish available for 0x00158d000271c4b7 = true	
2021-12-16 16:31:02.179 - debug: zigbee.0 (26219) Publish LQ for 0x00158d000271c4b7 = 10	
2021-12-16 16:31:02.181 - debug: zigbee.0 (26219) Publish available for 0x00158d0002f8d5b4 = true	
2021-12-16 16:31:02.182 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002f8d5b4 = 10	
2021-12-16 16:31:02.183 - debug: zigbee.0 (26219) Publish available for 0x00158d0002e34b33 = true	
2021-12-16 16:31:02.185 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002e34b33 = 10	
2021-12-16 16:31:02.186 - debug: zigbee.0 (26219) Publish available for 0x00158d000521d656 = true	
2021-12-16 16:31:02.187 - debug: zigbee.0 (26219) Publish LQ for 0x00158d000521d656 = 10	
2021-12-16 16:31:02.189 - debug: zigbee.0 (26219) Publish available for 0x00158d00028aee30 = true	
2021-12-16 16:31:02.190 - debug: zigbee.0 (26219) Publish LQ for 0x00158d00028aee30 = 10	
2021-12-16 16:31:02.191 - debug: zigbee.0 (26219) Publish available for 0x00158d00021369f3 = true	
2021-12-16 16:31:02.193 - debug: zigbee.0 (26219) Publish LQ for 0x00158d00021369f3 = 10	
2021-12-16 16:31:02.194 - debug: zigbee.0 (26219) Publish available for 0x00158d0002b54752 = true	
2021-12-16 16:31:02.196 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002b54752 = 10	
2021-12-16 16:31:02.199 - debug: zigbee.0 (26219) Publish available for 0x00158d000274f643 = true	
2021-12-16 16:31:02.200 - debug: zigbee.0 (26219) Publish LQ for 0x00158d000274f643 = 10	
2021-12-16 16:31:02.202 - debug: zigbee.0 (26219) Publish available for 0x00158d000274f64d = true	
2021-12-16 16:31:02.203 - debug: zigbee.0 (26219) Publish LQ for 0x00158d000274f64d = 10	
2021-12-16 16:31:02.204 - debug: zigbee.0 (26219) Publish available for 0x00158d0002b51c42 = true	
2021-12-16 16:31:02.206 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002b51c42 = 10	
2021-12-16 16:31:02.207 - debug: zigbee.0 (26219) Publish available for 0x00158d000274f4f7 = true	
2021-12-16 16:31:02.208 - debug: zigbee.0 (26219) Publish LQ for 0x00158d000274f4f7 = 10	
2021-12-16 16:31:02.209 - debug: zigbee.0 (26219) Publish available for 0x00158d000274f4d3 = true	
2021-12-16 16:31:02.211 - debug: zigbee.0 (26219) Publish LQ for 0x00158d000274f4d3 = 10	
2021-12-16 16:31:02.212 - debug: zigbee.0 (26219) Publish available for 0x00158d0002722af7 = true	
2021-12-16 16:31:02.213 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002722af7 = 10	
2021-12-16 16:31:02.215 - debug: zigbee.0 (26219) Publish available for 0x847127fffed62092 = true	
2021-12-16 16:31:02.216 - debug: zigbee.0 (26219) Publish LQ for 0x847127fffed62092 = 10	
2021-12-16 16:31:02.217 - debug: zigbee.0 (26219) Publish available for 0x847127fffed0a598 = true	
2021-12-16 16:31:02.218 - debug: zigbee.0 (26219) Publish LQ for 0x847127fffed0a598 = 10	
2021-12-16 16:31:02.220 - debug: zigbee.0 (26219) Publish available for 0x847127fffecfc657 = true	
2021-12-16 16:31:02.221 - debug: zigbee.0 (26219) Publish LQ for 0x847127fffecfc657 = 10	
2021-12-16 16:31:02.222 - debug: zigbee.0 (26219) Publish available for 0x000d6ffffe2cd4b8 = true	
2021-12-16 16:31:02.224 - debug: zigbee.0 (26219) Publish LQ for 0x000d6ffffe2cd4b8 = 10	
2021-12-16 16:31:02.226 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d0002b54a17 lumi.weather not needed	
2021-12-16 16:31:02.226 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d0002130d3b lumi.sensor_switch.aq2 not needed	
2021-12-16 16:31:02.227 - debug: zigbee.0 (26219) DeviceConfigure 0x7cb03eaa00acb990 Plug 01 not needed	
2021-12-16 16:31:02.227 - debug: zigbee.0 (26219) DeviceConfigure 0x7cb03eaa0a00dfcb Plug 01 not needed	
2021-12-16 16:31:02.228 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d0002c65ed8 lumi.light.aqcn02 not needed	
2021-12-16 16:31:02.228 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d0002130f3a lumi.sensor_switch.aq2 not needed	
2021-12-16 16:31:02.228 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d0002f8d76c lumi.ctrl_neutral1 not needed	
2021-12-16 16:31:02.228 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d000274f4de lumi.sensor_magnet.aq2 not needed	
2021-12-16 16:31:02.229 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d0002135d9b lumi.sensor_switch.aq2 not needed	
2021-12-16 16:31:02.229 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d000274f4bf lumi.sensor_magnet.aq2 not needed	
2021-12-16 16:31:02.229 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d000271c4b7 lumi.sensor_wleak.aq1 not needed	
2021-12-16 16:31:02.229 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d0002f8d5b4 lumi.ctrl_neutral1 not needed	
2021-12-16 16:31:02.229 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d0002e34b33 lumi.ctrl_neutral1 not needed	
2021-12-16 16:31:02.230 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d000521d656 lumi.switch.b1lacn02 not needed	
2021-12-16 16:31:02.230 - debug: zigbee.0 (26219) DeviceConfigure 0x84182600000c7532 Plug 01 not needed	
2021-12-16 16:31:02.230 - debug: zigbee.0 (26219) DeviceConfigure 0x7cb03eaa0a025809 Plug 01 not needed	
2021-12-16 16:31:02.230 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d00028aee30 lumi.sensor_cube.aqgl01 not needed	
2021-12-16 16:31:02.231 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d00021369f3 lumi.sensor_switch.aq2 not needed	
2021-12-16 16:31:02.231 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d0002b54752 lumi.weather not needed	
2021-12-16 16:31:02.231 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d000274f643 lumi.sensor_magnet.aq2 not needed	
2021-12-16 16:31:02.231 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d000274f64d lumi.sensor_magnet.aq2 not needed	
2021-12-16 16:31:02.231 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d0002b51c42 lumi.weather not needed	
2021-12-16 16:31:02.232 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d000274f4f7 lumi.sensor_magnet.aq2 not needed	
2021-12-16 16:31:02.234 - debug: zigbee.0 (26219) DeviceConfigure 0x7cb03eaa00a36bed Plug 01 not needed	
2021-12-16 16:31:02.235 - debug: zigbee.0 (26219) DeviceConfigure 0x7cb03eaa0a019e9d Plug 01 not needed	
2021-12-16 16:31:02.235 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d0002b805e3 lumi.light.aqcn02 not needed	
2021-12-16 16:31:02.235 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d0002b7d87c lumi.light.aqcn02 not needed	
2021-12-16 16:31:02.236 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d0002b7d6a9 lumi.light.aqcn02 not needed	
2021-12-16 16:31:02.236 - debug: zigbee.0 (26219) DeviceConfigure 0x000b57fffe4436b0 TRADFRI bulb E27 WS opal 980lm not needed	
2021-12-16 16:31:02.236 - debug: zigbee.0 (26219) DeviceConfigure 0x90fd9ffffe02c40f TRADFRI bulb E27 WS opal 980lm not needed	
2021-12-16 16:31:02.237 - debug: zigbee.0 (26219) DeviceConfigure 0x90fd9ffffe7fe8c9 TRADFRI bulb E27 WS opal 980lm not needed	
2021-12-16 16:31:02.237 - debug: zigbee.0 (26219) DeviceConfigure 0x90fd9ffffe88755e TRADFRI bulb E27 WS opal 980lm not needed	
2021-12-16 16:31:02.237 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d000274f4d3 lumi.sensor_magnet.aq2 not needed	
2021-12-16 16:31:02.237 - debug: zigbee.0 (26219) DeviceConfigure 0x00158d0002722af7 lumi.sensor_magnet.aq2 not needed	
2021-12-16 16:31:02.238 - debug: zigbee.0 (26219) DeviceConfigure 0x847127fffed62092 TS0601 not needed	
2021-12-16 16:31:02.238 - debug: zigbee.0 (26219) DeviceConfigure 0x847127fffed0a598 TS0601 not needed	
2021-12-16 16:31:02.238 - debug: zigbee.0 (26219) DeviceConfigure 0x847127fffecfc657 TS0601 not needed	
2021-12-16 16:31:02.239 - debug: zigbee.0 (26219) DeviceConfigure 0xa4c138934ce2822b TS0001 not needed	
2021-12-16 16:31:02.239 - debug: zigbee.0 (26219) DeviceConfigure 0xa4c138ec0e4ef1cf TS0001 not needed	
2021-12-16 16:31:02.240 - debug: zigbee.0 (26219) DeviceConfigure 0x000d6ffffe2cd4b8 FYRTUR block-out roller blind not needed	
2021-12-16 16:31:02.242 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":2,"_type":"EndDevice","_ieeeAddr":"0x00158d0002b54a17","_networkAddress":63636,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":63636,"deviceIeeeAddress":"0x00158d0002b54a17","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2211}},"msRelativeHumidity":{"attributes":{"measuredValue":4686}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10314}},"genBasic":{"attributes":{"65281":{"1":2955,"4":17320,"5":35,"6":[0,1],"10":32268,"100":2206,"101":4686,"102":103143},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.weather","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":30,"_dateCode":"20161129","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668296512},"mapped":{"zigbeeModel":["lumi.weather"],"model":"WSDCGQ11LM","vendor":"Xiaomi","description":"Aqara temperature, humidity and pressure sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"msTemperatureMeasurement","options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}],"type":["attributeReport","readResponse"]},{"cluster":"msRelativeHumidity","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."}]},{"cluster":"msPressureMeasurement","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"humidity","property":"humidity","access":1,"unit":"%","description":"Measured relative humidity"},{"type":"numeric","name":"pressure","property":"pressure","access":1,"unit":"hPa","description":"The measured atmospheric pressure"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":["[Circular]","[Circular]","[Circular]","[Circular]","[Circular]","[Circular]"]},"name":"0x00158d0002b54a17"}	
2021-12-16 16:31:02.243 - info: zigbee.0 (26219) 0x00158d0002b54a17 (addr 63636): WSDCGQ11LM - Xiaomi Aqara temperature, humidity and pressure sensor (EndDevice)	
2021-12-16 16:31:02.248 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":3,"_type":"EndDevice","_ieeeAddr":"0x00158d0002130d3b","_networkAddress":61838,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":61838,"deviceIeeeAddress":"0x00158d0002130d3b","clusters":{"genBasic":{"attributes":{"65281":{"1":3005,"3":27,"4":17320,"5":48,"6":[0,1],"10":47504},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_switch.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639668545618},"mapped":{"zigbeeModel":["lumi.sensor_switch.aq2","lumi.remote.b1acn01"],"model":"WXKG11LM","vendor":"Xiaomi","description":"Aqara wireless switch","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"enum","name":"action","property":"action","access":1,"values":["single","double","triple","quadruple","hold","release"],"description":"Triggered action (e.g. a button click)"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genMultistateInput","type":["attributeReport"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genMultistateInput","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]}],"toZigbee":[],"options":["[Circular]"]},"name":"0x00158d0002130d3b"}	
2021-12-16 16:31:02.248 - info: zigbee.0 (26219) 0x00158d0002130d3b (addr 61838): WXKG11LM - Xiaomi Aqara wireless switch (EndDevice)	
2021-12-16 16:31:02.249 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":4,"_type":"Router","_ieeeAddr":"0x7cb03eaa00acb990","_networkAddress":47504,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":47504,"deviceIeeeAddress":"0x7cb03eaa00acb990","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668554590},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["Plug 01"],"model":"AB3257001NJ","description":"Smart+ plug","vendor":"OSRAM","whiteLabel":[{"vendor":"LEDVANCE","model":"AB3257001NJ"}],"ota":{},"options":[]},"name":"0x7cb03eaa00acb990"}	
2021-12-16 16:31:02.250 - info: zigbee.0 (26219) 0x7cb03eaa00acb990 (addr 47504): AB3257001NJ - OSRAM Smart+ plug (Router)	
2021-12-16 16:31:02.251 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":5,"_type":"Router","_ieeeAddr":"0x7cb03eaa0a00dfcb","_networkAddress":34528,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":34528,"deviceIeeeAddress":"0x7cb03eaa0a00dfcb","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1629886942483},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["Plug 01"],"model":"AB3257001NJ","description":"Smart+ plug","vendor":"OSRAM","whiteLabel":[{"vendor":"LEDVANCE","model":"AB3257001NJ"}],"ota":{},"options":[]},"name":"0x7cb03eaa0a00dfcb"}	
2021-12-16 16:31:02.252 - info: zigbee.0 (26219) 0x7cb03eaa0a00dfcb (addr 34528): AB3257001NJ - OSRAM Smart+ plug (Router)	
2021-12-16 16:31:02.253 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":6,"_type":"Router","_ieeeAddr":"0x00158d0002c65ed8","_networkAddress":41267,"_manufacturerID":4447,"_endpoints":[{"ID":1,"profileID":260,"deviceID":258,"inputClusters":[0,4,3,5,10,258,13,19,6,1,1030,8,768,1027,1029,1026],"outputClusters":[25,10,13,258,19,6,1,1030,8,768],"deviceNetworkAddress":41267,"deviceIeeeAddress":"0x00158d0002c65ed8","clusters":{"genBasic":{"attributes":{"65281":{"3":86,"5":430,"7":"0x0000000000000000","8":279,"9":1792,"10":0,"100":1,"101":254,"102":346},"modelId":"lumi.light.aqcn02","appVersion":23,"manufacturerName":"LUMI","powerSource":4,"zclVersion":1,"stackVersion":2,"hwVersion":1,"dateCode":"11-22-2018","swBuildId":"1.23\u0000"}},"genOnOff":{"attributes":{"61440":117440752,"onOff":1}},"msTemperatureMeasurement":{"attributes":{"measuredValue":2122}},"lightingColorCtrl":{"attributes":{"colorTemperature":346,"tuyaRgbMode":10564352,"colorMode":1}},"genLevelCtrl":{"attributes":{"61440":10564352,"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"DC Source","_modelID":"lumi.light.aqcn02","_applicationVersion":23,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"11-22-2018","_softwareBuildID":"1.23\u0000","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":2},"_lastSeen":1639597631149},"mapped":{"zigbeeModel":["lumi.light.aqcn02"],"model":"ZNLDP12LM","vendor":"Xiaomi","description":"Aqara smart LED bulb","toZigbee":[{"key":["state","brightness","brightness_percent"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp","color_temp_percent"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."},{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["transition"],"attr":[]},{"key":["rate"],"attr":[]},{"key":["brightness_move","brightness_move_onoff"]},{"key":["colortemp_move","color_temp_move"]},{"key":["brightness_step","brightness_step_onoff"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_step"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["level_config"]},{"key":["power_on_behavior"]},{"key":["color_options"]},{"key":["color_mode"]},{"key":["effect","alert","flash"]},{"key":["power_outage_memory"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"fromZigbee":[{"cluster":"lightingColorCtrl","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"msOccupancySensing","type":["attributeReport","readResponse"]},{"cluster":"msRelativeHumidity","type":["attributeReport","readResponse"]},{"cluster":"msPressureMeasurement","type":["attributeReport","readResponse"]},{"cluster":"msTemperatureMeasurement","type":["attributeReport","readResponse"]}],"exposes":[{"type":"light","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","value_toggle":"TOGGLE","description":"On/off state of this light"},{"type":"numeric","name":"brightness","property":"brightness","access":7,"value_min":0,"value_max":254,"description":"Brightness of this light"},{"type":"numeric","name":"color_temp","property":"color_temp","access":7,"unit":"mired","value_min":150,"value_max":500,"description":"Color temperature of this light","presets":[{"name":"coolest","value":150,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":500,"description":"Warmest temperature supported"}]}]},{"type":"enum","name":"effect","property":"effect","access":2,"values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)"},{"type":"binary","name":"power_outage_memory","property":"power_outage_memory","access":3,"value_on":true,"value_off":false,"description":"Enable/disable the power outage memory, this recovers the on/off mode after power failure"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"ota":{},"options":["[Circular]","[Circular]"]},"name":"0x00158d0002c65ed8"}	
2021-12-16 16:31:02.254 - info: zigbee.0 (26219) 0x00158d0002c65ed8 (addr 41267): ZNLDP12LM - Xiaomi Aqara smart LED bulb (Router)	
2021-12-16 16:31:02.254 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":7,"_type":"EndDevice","_ieeeAddr":"0x00158d0002130f3a","_networkAddress":60816,"_manufacturerID":4151,"_endpoints":[{"ID":1,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":60816,"deviceIeeeAddress":"0x00158d0002130f3a","clusters":{"genBasic":{"attributes":{"65281":{"1":3015,"3":26,"4":17320,"5":23,"6":[0,1],"10":47504},"modelId":"lumi.sensor_switch.aq2","appVersion":3}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_switch.aq2","_applicationVersion":3,"_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639665771838},"mapped":{"zigbeeModel":["lumi.sensor_switch.aq2","lumi.remote.b1acn01"],"model":"WXKG11LM","vendor":"Xiaomi","description":"Aqara wireless switch","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"enum","name":"action","property":"action","access":1,"values":["single","double","triple","quadruple","hold","release"],"description":"Triggered action (e.g. a button click)"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genMultistateInput","type":["attributeReport"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genMultistateInput","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]}],"toZigbee":[],"options":["[Circular]"]},"name":"0x00158d0002130f3a"}	
2021-12-16 16:31:02.255 - info: zigbee.0 (26219) 0x00158d0002130f3a (addr 60816): WXKG11LM - Xiaomi Aqara wireless switch (EndDevice)	
2021-12-16 16:31:02.256 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":8,"_type":"EndDevice","_ieeeAddr":"0x00158d0002f8d76c","_networkAddress":10251,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":6,"inputClusters":[0,3,1,2,25,10],"outputClusters":[0,10,25],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{"genBasic":{"attributes":{"65281":{"1":3300,"3":29,"5":799,"8":9750,"10":0,"100":0,"101":0,"110":0,"111":255,"153":0,"155":0},"manufacturerName":"LUMI","powerSource":4,"zclVersion":0,"stackVersion":2,"hwVersion":38,"dateCode":"04-25-2018"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":2,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{"genOnOff":{"attributes":{"61440":52956144,"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":3,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":4,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{"genOnOff":{"attributes":{"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":5,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":6,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":8,"profileID":260,"deviceID":83,"inputClusters":[12],"outputClusters":[],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"DC Source","_modelID":"lumi.ctrl_neutral1","_applicationVersion":1,"_stackVersion":2,"_zclVersion":0,"_hardwareVersion":38,"_dateCode":"04-25-2018","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1631717611797},"mapped":{"zigbeeModel":["lumi.ctrl_neutral1"],"model":"QBKG04LM","vendor":"Xiaomi","description":"Aqara single key wired wall switch without neutral wire. Doesn't work as a router and doesn't support power meter","fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genOnOff","type":["attributeReport"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"enum","name":"action","property":"action","access":1,"values":["single","release","hold"],"description":"Triggered action (e.g. a button click)"},{"type":"enum","name":"operation_mode","property":"operation_mode","access":7,"values":["control_relay","decoupled"],"description":"Decoupled mode"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["operation_mode"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"ota":{},"options":["[Circular]"]},"name":"0x00158d0002f8d76c"}	
2021-12-16 16:31:02.256 - info: zigbee.0 (26219) 0x00158d0002f8d76c (addr 10251): QBKG04LM - Xiaomi Aqara single key wired wall switch without neutral wire. Doesn't work as a router and doesn't support power meter (EndDevice)	
2021-12-16 16:31:02.257 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":9,"_type":"EndDevice","_ieeeAddr":"0x00158d000274f4de","_networkAddress":53691,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":53691,"deviceIeeeAddress":"0x00158d000274f4de","clusters":{"genBasic":{"attributes":{"65281":{"1":2995,"3":28,"4":17320,"5":37,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_magnet.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639668060686},"mapped":{"zigbeeModel":["lumi.sensor_magnet.aq2"],"model":"MCCGQ11LM","vendor":"Xiaomi","description":"Aqara door & window contact sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"binary","name":"contact","property":"contact","access":1,"value_on":false,"value_off":true,"description":"Indicates if the contact is closed (= true) or open (= false)"},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":["[Circular]","[Circular]"]},"name":"0x00158d000274f4de"}	
2021-12-16 16:31:02.258 - info: zigbee.0 (26219) 0x00158d000274f4de (addr 53691): MCCGQ11LM - Xiaomi Aqara door & window contact sensor (EndDevice)	
2021-12-16 16:31:02.258 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":10,"_type":"EndDevice","_ieeeAddr":"0x00158d0002135d9b","_networkAddress":45956,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":45956,"deviceIeeeAddress":"0x00158d0002135d9b","clusters":{"genBasic":{"attributes":{"65281":{"1":3015,"3":27,"4":17320,"5":77,"6":[0,1],"10":47504},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_switch.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639664787186},"mapped":{"zigbeeModel":["lumi.sensor_switch.aq2","lumi.remote.b1acn01"],"model":"WXKG11LM","vendor":"Xiaomi","description":"Aqara wireless switch","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"enum","name":"action","property":"action","access":1,"values":["single","double","triple","quadruple","hold","release"],"description":"Triggered action (e.g. a button click)"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genMultistateInput","type":["attributeReport"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genMultistateInput","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]}],"toZigbee":[],"options":["[Circular]"]},"name":"0x00158d0002135d9b"}	
2021-12-16 16:31:02.259 - info: zigbee.0 (26219) 0x00158d0002135d9b (addr 45956): WXKG11LM - Xiaomi Aqara wireless switch (EndDevice)	
2021-12-16 16:31:02.259 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":11,"_type":"EndDevice","_ieeeAddr":"0x00158d000274f4bf","_networkAddress":52827,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":52827,"deviceIeeeAddress":"0x00158d000274f4bf","clusters":{"genBasic":{"attributes":{"65281":{"1":2985,"3":24,"4":17320,"5":45,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_magnet.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639666026955},"mapped":{"zigbeeModel":["lumi.sensor_magnet.aq2"],"model":"MCCGQ11LM","vendor":"Xiaomi","description":"Aqara door & window contact sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"binary","name":"contact","property":"contact","access":1,"value_on":false,"value_off":true,"description":"Indicates if the contact is closed (= true) or open (= false)"},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":["[Circular]","[Circular]"]},"name":"0x00158d000274f4bf"}	
2021-12-16 16:31:02.260 - info: zigbee.0 (26219) 0x00158d000274f4bf (addr 52827): MCCGQ11LM - Xiaomi Aqara door & window contact sensor (EndDevice)	
2021-12-16 16:31:02.260 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":12,"_type":"EndDevice","_ieeeAddr":"0x00158d000271c4b7","_networkAddress":16037,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":1026,"inputClusters":[0,3,1],"outputClusters":[25],"deviceNetworkAddress":16037,"deviceIeeeAddress":"0x00158d000271c4b7","clusters":{"genBasic":{"attributes":{"65281":{"1":3025,"3":21,"4":17320,"5":10,"6":[0,1],"8":516,"10":47504,"100":1},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20170721","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_wleak.aq1","_applicationVersion":4,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20170721","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639666263071},"mapped":{"zigbeeModel":["lumi.sensor_wleak.aq1"],"model":"SJCGQ11LM","vendor":"Xiaomi","description":"Aqara water leak sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"ssIasZone","type":"commandStatusChangeNotification"},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"binary","name":"water_leak","property":"water_leak","access":1,"value_on":true,"value_off":false,"description":"Indicates whether the device detected a water leak"},{"type":"binary","name":"battery_low","property":"battery_low","access":1,"value_on":true,"value_off":false,"description":"Indicates if the battery of this device is almost empty"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":[]},"name":"0x00158d000271c4b7"}	
2021-12-16 16:31:02.261 - info: zigbee.0 (26219) 0x00158d000271c4b7 (addr 16037): SJCGQ11LM - Xiaomi Aqara water leak sensor (EndDevice)	
2021-12-16 16:31:02.262 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":13,"_type":"EndDevice","_ieeeAddr":"0x00158d0002f8d5b4","_networkAddress":29745,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":6,"inputClusters":[0,3,1,2,25,10],"outputClusters":[0,10,25],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{"genBasic":{"attributes":{"65281":{"1":3300,"3":29,"5":98,"8":9750,"10":0,"100":1,"101":0,"110":1,"111":255,"153":0,"155":0},"manufacturerName":"LUMI","powerSource":4,"zclVersion":0,"stackVersion":2,"hwVersion":38,"dateCode":"04-25-2018"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":2,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{"genOnOff":{"attributes":{"61440":57946368,"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":3,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":4,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{"genOnOff":{"attributes":{"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":5,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":6,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":8,"profileID":260,"deviceID":83,"inputClusters":[12],"outputClusters":[],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"DC Source","_modelID":"lumi.ctrl_neutral1","_applicationVersion":1,"_stackVersion":2,"_zclVersion":0,"_hardwareVersion":38,"_dateCode":"04-25-2018","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1631717587342},"mapped":{"zigbeeModel":["lumi.ctrl_neutral1"],"model":"QBKG04LM","vendor":"Xiaomi","description":"Aqara single key wired wall switch without neutral wire. Doesn't work as a router and doesn't support power meter","fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genOnOff","type":["attributeReport"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"enum","name":"action","property":"action","access":1,"values":["single","release","hold"],"description":"Triggered action (e.g. a button click)"},{"type":"enum","name":"operation_mode","property":"operation_mode","access":7,"values":["control_relay","decoupled"],"description":"Decoupled mode"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["operation_mode"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"ota":{},"options":["[Circular]"]},"name":"0x00158d0002f8d5b4"}	
2021-12-16 16:31:02.262 - info: zigbee.0 (26219) 0x00158d0002f8d5b4 (addr 29745): QBKG04LM - Xiaomi Aqara single key wired wall switch without neutral wire. Doesn't work as a router and doesn't support power meter (EndDevice)	
2021-12-16 16:31:02.263 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":14,"_type":"EndDevice","_ieeeAddr":"0x00158d0002e34b33","_networkAddress":5016,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":6,"inputClusters":[0,3,1,2,25,10],"outputClusters":[0,10,25],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{"genBasic":{"attributes":{"65281":{"1":3300,"3":28,"5":16,"8":9750,"10":0,"100":1,"101":0,"110":1,"111":255,"153":0,"155":0},"manufacturerName":"LUMI","powerSource":4,"zclVersion":0,"stackVersion":2,"hwVersion":38,"dateCode":"04-25-2018"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":2,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{"genOnOff":{"attributes":{"61440":51615981,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":3,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":4,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{"genOnOff":{"attributes":{"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":5,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":6,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":8,"profileID":260,"deviceID":83,"inputClusters":[12],"outputClusters":[],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"DC Source","_modelID":"lumi.ctrl_neutral1","_applicationVersion":1,"_stackVersion":2,"_zclVersion":0,"_hardwareVersion":38,"_dateCode":"04-25-2018","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1631717605447},"mapped":{"zigbeeModel":["lumi.ctrl_neutral1"],"model":"QBKG04LM","vendor":"Xiaomi","description":"Aqara single key wired wall switch without neutral wire. Doesn't work as a router and doesn't support power meter","fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genOnOff","type":["attributeReport"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"enum","name":"action","property":"action","access":1,"values":["single","release","hold"],"description":"Triggered action (e.g. a button click)"},{"type":"enum","name":"operation_mode","property":"operation_mode","access":7,"values":["control_relay","decoupled"],"description":"Decoupled mode"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["operation_mode"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"ota":{},"options":["[Circular]"]},"name":"0x00158d0002e34b33"}	
2021-12-16 16:31:02.264 - info: zigbee.0 (26219) 0x00158d0002e34b33 (addr 5016): QBKG04LM - Xiaomi Aqara single key wired wall switch without neutral wire. Doesn't work as a router and doesn't support power meter (EndDevice)	
2021-12-16 16:31:02.266 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":15,"_type":"EndDevice","_ieeeAddr":"0x00158d000521d656","_networkAddress":1024,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":6,"inputClusters":[0,3,1,2,25,10],"outputClusters":[0,10,25],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{"genBasic":{"attributes":{"65281":{"1":3300,"3":20,"5":14,"8":13850,"10":0,"100":0,"101":0,"110":0,"111":255,"153":0,"155":0},"manufacturerName":"LUMI","powerSource":4,"zclVersion":0,"stackVersion":2,"hwVersion":54,"dateCode":"03-20-2019"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":2,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{"genOnOff":{"attributes":{"61440":117440754,"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":3,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":4,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{"genOnOff":{"attributes":{"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":5,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":6,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":8,"profileID":260,"deviceID":83,"inputClusters":[12],"outputClusters":[],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"DC Source","_modelID":"lumi.switch.b1lacn02","_applicationVersion":1,"_stackVersion":2,"_zclVersion":0,"_hardwareVersion":54,"_dateCode":"03-20-2019","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1631717612335},"mapped":{"zigbeeModel":["lumi.switch.b1lacn02"],"model":"QBKG21LM","vendor":"Xiaomi","description":"Aqara D1 single gang smart wall switch (no neutral wire)","fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genOnOff","type":["attributeReport"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"enum","name":"action","property":"action","access":1,"values":["single","hold","release"],"description":"Triggered action (e.g. a button click)"},{"type":"enum","name":"operation_mode","property":"operation_mode","access":7,"values":["control_relay","decoupled"],"description":"Decoupled mode"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["operation_mode"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"options":["[Circular]"]},"name":"0x00158d000521d656"}	
2021-12-16 16:31:02.266 - info: zigbee.0 (26219) 0x00158d000521d656 (addr 1024): QBKG21LM - Xiaomi Aqara D1 single gang smart wall switch (no neutral wire) (EndDevice)	
2021-12-16 16:31:02.267 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":16,"_type":"Router","_ieeeAddr":"0x84182600000c7532","_networkAddress":56716,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":56716,"deviceIeeeAddress":"0x84182600000c7532","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":1}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668628742},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["Plug 01"],"model":"AB3257001NJ","description":"Smart+ plug","vendor":"OSRAM","whiteLabel":[{"vendor":"LEDVANCE","model":"AB3257001NJ"}],"ota":{},"options":[]},"name":"0x84182600000c7532"}	
2021-12-16 16:31:02.267 - info: zigbee.0 (26219) 0x84182600000c7532 (addr 56716): AB3257001NJ - OSRAM Smart+ plug (Router)	
2021-12-16 16:31:02.268 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":17,"_type":"Router","_ieeeAddr":"0x7cb03eaa0a025809","_networkAddress":18602,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":18602,"deviceIeeeAddress":"0x7cb03eaa0a025809","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668625910},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["Plug 01"],"model":"AB3257001NJ","description":"Smart+ plug","vendor":"OSRAM","whiteLabel":[{"vendor":"LEDVANCE","model":"AB3257001NJ"}],"ota":{},"options":[]},"name":"0x7cb03eaa0a025809"}	
2021-12-16 16:31:02.268 - info: zigbee.0 (26219) 0x7cb03eaa0a025809 (addr 18602): AB3257001NJ - OSRAM Smart+ plug (Router)	
2021-12-16 16:31:02.269 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":18,"_type":"EndDevice","_ieeeAddr":"0x00158d00028aee30","_networkAddress":54685,"_manufacturerID":4151,"_endpoints":[{"ID":1,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":54685,"deviceIeeeAddress":"0x00158d00028aee30","clusters":{"genBasic":{"attributes":{"65281":{"1":2965,"3":19,"4":17320,"5":264,"6":[0,1],"10":0,"151":1,"152":3918,"153":2933,"154":4}}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":2,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":54685,"deviceIeeeAddress":"0x00158d00028aee30","clusters":{"genMultistateInput":{"attributes":{"presentValue":2}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":3,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":54685,"deviceIeeeAddress":"0x00158d00028aee30","clusters":{"genAnalogInput":{"attributes":{"65285":500,"presentValue":12.239999771118164}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_cube.aqgl01","_applicationVersion":5,"_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639666386256},"mapped":{"zigbeeModel":["lumi.sensor_cube","lumi.sensor_cube.aqgl01"],"model":"MFKZQ01LM","vendor":"Xiaomi","description":"Mi/Aqara smart home cube","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genMultistateInput","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genAnalogInput","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]}],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"action_angle","property":"action_angle","access":1,"value_min":-360,"value_max":360},{"type":"numeric","name":"action_from_side","property":"action_from_side","access":1,"description":"Side of the cube","value_min":0,"value_max":6,"value_step":1},{"type":"numeric","name":"action_side","property":"action_side","access":1,"description":"Side of the cube","value_min":0,"value_max":6,"value_step":1},{"type":"numeric","name":"action_to_side","property":"action_to_side","access":1,"description":"Side of the cube","value_min":0,"value_max":6,"value_step":1},{"type":"enum","name":"action","property":"action","access":1,"values":["shake","wakeup","fall","tap","slide","flip180","flip90","rotate_left","rotate_right"],"description":"Triggered action (e.g. a button click)"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"toZigbee":[],"options":["[Circular]"]},"name":"0x00158d00028aee30"}	
2021-12-16 16:31:02.270 - info: zigbee.0 (26219) 0x00158d00028aee30 (addr 54685): MFKZQ01LM - Xiaomi Mi/Aqara smart home cube (EndDevice)	
2021-12-16 16:31:02.270 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":19,"_type":"EndDevice","_ieeeAddr":"0x00158d00021369f3","_networkAddress":4218,"_manufacturerID":4151,"_endpoints":[{"ID":1,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":4218,"deviceIeeeAddress":"0x00158d00021369f3","clusters":{"genBasic":{"attributes":{"65281":{"1":3025,"3":21,"4":17320,"5":23802,"6":[0,1],"10":47504},"modelId":"lumi.sensor_switch.aq2","appVersion":3}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_switch.aq2","_applicationVersion":3,"_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639666109455},"mapped":{"zigbeeModel":["lumi.sensor_switch.aq2","lumi.remote.b1acn01"],"model":"WXKG11LM","vendor":"Xiaomi","description":"Aqara wireless switch","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"enum","name":"action","property":"action","access":1,"values":["single","double","triple","quadruple","hold","release"],"description":"Triggered action (e.g. a button click)"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genMultistateInput","type":["attributeReport"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genMultistateInput","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]}],"toZigbee":[],"options":["[Circular]"]},"name":"0x00158d00021369f3"}	
2021-12-16 16:31:02.271 - info: zigbee.0 (26219) 0x00158d00021369f3 (addr 4218): WXKG11LM - Xiaomi Aqara wireless switch (EndDevice)	
2021-12-16 16:31:02.272 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":20,"_type":"EndDevice","_ieeeAddr":"0x00158d0002b54752","_networkAddress":39900,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":39900,"deviceIeeeAddress":"0x00158d0002b54752","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2131}},"msRelativeHumidity":{"attributes":{"measuredValue":5113}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10313}},"genBasic":{"attributes":{"65281":{"1":2915,"4":17320,"5":18,"6":[0,1],"10":18602,"100":2165,"101":5928,"102":102898},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.weather","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":30,"_dateCode":"20161129","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639667987037},"mapped":{"zigbeeModel":["lumi.weather"],"model":"WSDCGQ11LM","vendor":"Xiaomi","description":"Aqara temperature, humidity and pressure sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"msTemperatureMeasurement","options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}],"type":["attributeReport","readResponse"]},{"cluster":"msRelativeHumidity","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."}]},{"cluster":"msPressureMeasurement","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"humidity","property":"humidity","access":1,"unit":"%","description":"Measured relative humidity"},{"type":"numeric","name":"pressure","property":"pressure","access":1,"unit":"hPa","description":"The measured atmospheric pressure"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":["[Circular]","[Circular]","[Circular]","[Circular]","[Circular]","[Circular]"]},"name":"0x00158d0002b54752"}	
2021-12-16 16:31:02.272 - info: zigbee.0 (26219) 0x00158d0002b54752 (addr 39900): WSDCGQ11LM - Xiaomi Aqara temperature, humidity and pressure sensor (EndDevice)	
2021-12-16 16:31:02.273 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":21,"_type":"EndDevice","_ieeeAddr":"0x00158d000274f643","_networkAddress":43219,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":43219,"deviceIeeeAddress":"0x00158d000274f643","clusters":{"genBasic":{"attributes":{"65281":{"1":2995,"3":24,"4":17320,"5":32,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001","modelId":"lumi.sensor_magnet.aq2"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_magnet.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639665912300},"mapped":{"zigbeeModel":["lumi.sensor_magnet.aq2"],"model":"MCCGQ11LM","vendor":"Xiaomi","description":"Aqara door & window contact sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"binary","name":"contact","property":"contact","access":1,"value_on":false,"value_off":true,"description":"Indicates if the contact is closed (= true) or open (= false)"},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":["[Circular]","[Circular]"]},"name":"0x00158d000274f643"}	
2021-12-16 16:31:02.273 - info: zigbee.0 (26219) 0x00158d000274f643 (addr 43219): MCCGQ11LM - Xiaomi Aqara door & window contact sensor (EndDevice)	
2021-12-16 16:31:02.274 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":22,"_type":"EndDevice","_ieeeAddr":"0x00158d000274f64d","_networkAddress":61566,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":61566,"deviceIeeeAddress":"0x00158d000274f64d","clusters":{"genBasic":{"attributes":{"65281":{"1":3025,"3":17,"4":17320,"5":83,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_magnet.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639668558468},"mapped":{"zigbeeModel":["lumi.sensor_magnet.aq2"],"model":"MCCGQ11LM","vendor":"Xiaomi","description":"Aqara door & window contact sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"binary","name":"contact","property":"contact","access":1,"value_on":false,"value_off":true,"description":"Indicates if the contact is closed (= true) or open (= false)"},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":["[Circular]","[Circular]"]},"name":"0x00158d000274f64d"}	
2021-12-16 16:31:02.274 - info: zigbee.0 (26219) 0x00158d000274f64d (addr 61566): MCCGQ11LM - Xiaomi Aqara door & window contact sensor (EndDevice)	
2021-12-16 16:31:02.275 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":23,"_type":"EndDevice","_ieeeAddr":"0x00158d0002b51c42","_networkAddress":49773,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":49773,"deviceIeeeAddress":"0x00158d0002b51c42","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2152}},"msRelativeHumidity":{"attributes":{"measuredValue":4958}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10316}},"genBasic":{"attributes":{"65281":{"1":2905,"4":17320,"5":100,"6":[0,1],"10":47504,"100":2140,"101":4904,"102":103126},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001","modelId":"lumi.weather"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.weather","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":30,"_dateCode":"20161129","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668367804},"mapped":{"zigbeeModel":["lumi.weather"],"model":"WSDCGQ11LM","vendor":"Xiaomi","description":"Aqara temperature, humidity and pressure sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"msTemperatureMeasurement","options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}],"type":["attributeReport","readResponse"]},{"cluster":"msRelativeHumidity","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."}]},{"cluster":"msPressureMeasurement","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"humidity","property":"humidity","access":1,"unit":"%","description":"Measured relative humidity"},{"type":"numeric","name":"pressure","property":"pressure","access":1,"unit":"hPa","description":"The measured atmospheric pressure"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":["[Circular]","[Circular]","[Circular]","[Circular]","[Circular]","[Circular]"]},"name":"0x00158d0002b51c42"}	
2021-12-16 16:31:02.276 - info: zigbee.0 (26219) 0x00158d0002b51c42 (addr 49773): WSDCGQ11LM - Xiaomi Aqara temperature, humidity and pressure sensor (EndDevice)	
2021-12-16 16:31:02.276 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":24,"_type":"EndDevice","_ieeeAddr":"0x00158d000274f4f7","_networkAddress":17905,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":17905,"deviceIeeeAddress":"0x00158d000274f4f7","clusters":{"genBasic":{"attributes":{"65281":{"1":3005,"3":23,"4":17320,"5":34,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_magnet.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639663882017},"mapped":{"zigbeeModel":["lumi.sensor_magnet.aq2"],"model":"MCCGQ11LM","vendor":"Xiaomi","description":"Aqara door & window contact sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"binary","name":"contact","property":"contact","access":1,"value_on":false,"value_off":true,"description":"Indicates if the contact is closed (= true) or open (= false)"},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":["[Circular]","[Circular]"]},"name":"0x00158d000274f4f7"}	
2021-12-16 16:31:02.277 - info: zigbee.0 (26219) 0x00158d000274f4f7 (addr 17905): MCCGQ11LM - Xiaomi Aqara door & window contact sensor (EndDevice)	
2021-12-16 16:31:02.278 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":25,"_type":"Router","_ieeeAddr":"0x7cb03eaa00a36bed","_networkAddress":65448,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":65448,"deviceIeeeAddress":"0x7cb03eaa00a36bed","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1622654614413},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["Plug 01"],"model":"AB3257001NJ","description":"Smart+ plug","vendor":"OSRAM","whiteLabel":[{"vendor":"LEDVANCE","model":"AB3257001NJ"}],"ota":{},"options":[]},"name":"0x7cb03eaa00a36bed"}	
2021-12-16 16:31:02.278 - info: zigbee.0 (26219) 0x7cb03eaa00a36bed (addr 65448): AB3257001NJ - OSRAM Smart+ plug (Router)	
2021-12-16 16:31:02.279 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":26,"_type":"Router","_ieeeAddr":"0x7cb03eaa0a019e9d","_networkAddress":32268,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":32268,"deviceIeeeAddress":"0x7cb03eaa0a019e9d","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668629319},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["Plug 01"],"model":"AB3257001NJ","description":"Smart+ plug","vendor":"OSRAM","whiteLabel":[{"vendor":"LEDVANCE","model":"AB3257001NJ"}],"ota":{},"options":[]},"name":"0x7cb03eaa0a019e9d"}	
2021-12-16 16:31:02.280 - info: zigbee.0 (26219) 0x7cb03eaa0a019e9d (addr 32268): AB3257001NJ - OSRAM Smart+ plug (Router)	
2021-12-16 16:31:02.281 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":27,"_type":"Router","_ieeeAddr":"0x00158d0002b805e3","_networkAddress":39725,"_manufacturerID":4447,"_endpoints":[{"ID":1,"profileID":260,"deviceID":258,"inputClusters":[0,4,3,5,10,258,13,19,6,1,1030,8,768,1027,1029,1026],"outputClusters":[25,10,13,258,19,6,1,1030,8,768],"deviceNetworkAddress":39725,"deviceIeeeAddress":"0x00158d0002b805e3","clusters":{"genBasic":{"attributes":{"65281":{"3":69,"5":322,"7":"0x0000000000000000","8":278,"9":1792,"10":41267,"100":1,"101":254,"102":346},"manufacturerName":"LUMI","powerSource":4,"zclVersion":1,"stackVersion":2,"hwVersion":1,"dateCode":"09-30-2018","swBuildId":"1.22\u0000","modelId":"lumi.light.aqcn02"}},"genOnOff":{"attributes":{"61440":117440752,"onOff":1}},"lightingColorCtrl":{"attributes":{"colorTemperature":346,"tuyaRgbMode":10169600,"colorMode":1}},"genLevelCtrl":{"attributes":{"61440":10169600,"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"DC Source","_modelID":"lumi.light.aqcn02","_applicationVersion":22,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"09-30-2018","_softwareBuildID":"1.22\u0000","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639597212133},"mapped":{"zigbeeModel":["lumi.light.aqcn02"],"model":"ZNLDP12LM","vendor":"Xiaomi","description":"Aqara smart LED bulb","toZigbee":[{"key":["state","brightness","brightness_percent"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp","color_temp_percent"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."},{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["transition"],"attr":[]},{"key":["rate"],"attr":[]},{"key":["brightness_move","brightness_move_onoff"]},{"key":["colortemp_move","color_temp_move"]},{"key":["brightness_step","brightness_step_onoff"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_step"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["level_config"]},{"key":["power_on_behavior"]},{"key":["color_options"]},{"key":["color_mode"]},{"key":["effect","alert","flash"]},{"key":["power_outage_memory"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"fromZigbee":[{"cluster":"lightingColorCtrl","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"msOccupancySensing","type":["attributeReport","readResponse"]},{"cluster":"msRelativeHumidity","type":["attributeReport","readResponse"]},{"cluster":"msPressureMeasurement","type":["attributeReport","readResponse"]},{"cluster":"msTemperatureMeasurement","type":["attributeReport","readResponse"]}],"exposes":[{"type":"light","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","value_toggle":"TOGGLE","description":"On/off state of this light"},{"type":"numeric","name":"brightness","property":"brightness","access":7,"value_min":0,"value_max":254,"description":"Brightness of this light"},{"type":"numeric","name":"color_temp","property":"color_temp","access":7,"unit":"mired","value_min":150,"value_max":500,"description":"Color temperature of this light","presets":[{"name":"coolest","value":150,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":500,"description":"Warmest temperature supported"}]}]},{"type":"enum","name":"effect","property":"effect","access":2,"values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)"},{"type":"binary","name":"power_outage_memory","property":"power_outage_memory","access":3,"value_on":true,"value_off":false,"description":"Enable/disable the power outage memory, this recovers the on/off mode after power failure"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"ota":{},"options":["[Circular]","[Circular]"]},"name":"0x00158d0002b805e3"}	
2021-12-16 16:31:02.282 - info: zigbee.0 (26219) 0x00158d0002b805e3 (addr 39725): ZNLDP12LM - Xiaomi Aqara smart LED bulb (Router)	
2021-12-16 16:31:02.294 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":28,"_type":"Router","_ieeeAddr":"0x00158d0002b7d87c","_networkAddress":35436,"_manufacturerID":4447,"_endpoints":[{"ID":1,"profileID":260,"deviceID":258,"inputClusters":[0,4,3,5,10,258,13,19,6,1,1030,8,768,1027,1029,1026],"outputClusters":[25,10,13,258,19,6,1,1030,8,768],"deviceNetworkAddress":35436,"deviceIeeeAddress":"0x00158d0002b7d87c","clusters":{"genBasic":{"attributes":{"65281":{"3":76,"5":351,"7":"0x0000000000000000","8":278,"9":1792,"10":0,"100":1,"101":254,"102":346},"manufacturerName":"LUMI","powerSource":4,"zclVersion":1,"stackVersion":2,"hwVersion":1,"dateCode":"09-30-2018","swBuildId":"1.22\u0000","modelId":"lumi.light.aqcn02"}},"genOnOff":{"attributes":{"61440":117440752,"onOff":1}},"lightingColorCtrl":{"attributes":{"colorTemperature":346,"tuyaRgbMode":9071616,"colorMode":1}},"genLevelCtrl":{"attributes":{"61440":9071616,"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"DC Source","_modelID":"lumi.light.aqcn02","_applicationVersion":22,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"09-30-2018","_softwareBuildID":"1.22\u0000","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639597258122},"mapped":{"zigbeeModel":["lumi.light.aqcn02"],"model":"ZNLDP12LM","vendor":"Xiaomi","description":"Aqara smart LED bulb","toZigbee":[{"key":["state","brightness","brightness_percent"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp","color_temp_percent"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."},{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["transition"],"attr":[]},{"key":["rate"],"attr":[]},{"key":["brightness_move","brightness_move_onoff"]},{"key":["colortemp_move","color_temp_move"]},{"key":["brightness_step","brightness_step_onoff"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_step"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["level_config"]},{"key":["power_on_behavior"]},{"key":["color_options"]},{"key":["color_mode"]},{"key":["effect","alert","flash"]},{"key":["power_outage_memory"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"fromZigbee":[{"cluster":"lightingColorCtrl","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"msOccupancySensing","type":["attributeReport","readResponse"]},{"cluster":"msRelativeHumidity","type":["attributeReport","readResponse"]},{"cluster":"msPressureMeasurement","type":["attributeReport","readResponse"]},{"cluster":"msTemperatureMeasurement","type":["attributeReport","readResponse"]}],"exposes":[{"type":"light","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","value_toggle":"TOGGLE","description":"On/off state of this light"},{"type":"numeric","name":"brightness","property":"brightness","access":7,"value_min":0,"value_max":254,"description":"Brightness of this light"},{"type":"numeric","name":"color_temp","property":"color_temp","access":7,"unit":"mired","value_min":150,"value_max":500,"description":"Color temperature of this light","presets":[{"name":"coolest","value":150,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":500,"description":"Warmest temperature supported"}]}]},{"type":"enum","name":"effect","property":"effect","access":2,"values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)"},{"type":"binary","name":"power_outage_memory","property":"power_outage_memory","access":3,"value_on":true,"value_off":false,"description":"Enable/disable the power outage memory, this recovers the on/off mode after power failure"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"ota":{},"options":["[Circular]","[Circular]"]},"name":"0x00158d0002b7d87c"}	
2021-12-16 16:31:02.295 - info: zigbee.0 (26219) 0x00158d0002b7d87c (addr 35436): ZNLDP12LM - Xiaomi Aqara smart LED bulb (Router)	
2021-12-16 16:31:02.296 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":29,"_type":"Router","_ieeeAddr":"0x00158d0002b7d6a9","_networkAddress":19263,"_manufacturerID":4447,"_endpoints":[{"ID":1,"profileID":260,"deviceID":258,"inputClusters":[0,4,3,5,10,258,13,19,6,1,1030,8,768,1027,1029,1026],"outputClusters":[25,10,13,258,19,6,1,1030,8,768],"deviceNetworkAddress":19263,"deviceIeeeAddress":"0x00158d0002b7d6a9","clusters":{"genBasic":{"attributes":{"65281":{"3":74,"5":376,"7":"0x0000000000000000","8":278,"9":1792,"10":0,"100":1,"101":254,"102":346},"manufacturerName":"LUMI","powerSource":4,"zclVersion":1,"stackVersion":2,"hwVersion":1,"dateCode":"09-30-2018","swBuildId":"1.22\u0000","modelId":"lumi.light.aqcn02"}},"genOnOff":{"attributes":{"61440":117440752,"onOff":1}},"lightingColorCtrl":{"attributes":{"colorTemperature":346,"tuyaRgbMode":4931328,"colorMode":1}},"genLevelCtrl":{"attributes":{"61440":4931328,"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"DC Source","_modelID":"lumi.light.aqcn02","_applicationVersion":22,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"09-30-2018","_softwareBuildID":"1.22\u0000","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639597260119},"mapped":{"zigbeeModel":["lumi.light.aqcn02"],"model":"ZNLDP12LM","vendor":"Xiaomi","description":"Aqara smart LED bulb","toZigbee":[{"key":["state","brightness","brightness_percent"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp","color_temp_percent"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."},{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["transition"],"attr":[]},{"key":["rate"],"attr":[]},{"key":["brightness_move","brightness_move_onoff"]},{"key":["colortemp_move","color_temp_move"]},{"key":["brightness_step","brightness_step_onoff"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_step"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["level_config"]},{"key":["power_on_behavior"]},{"key":["color_options"]},{"key":["color_mode"]},{"key":["effect","alert","flash"]},{"key":["power_outage_memory"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"fromZigbee":[{"cluster":"lightingColorCtrl","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"msOccupancySensing","type":["attributeReport","readResponse"]},{"cluster":"msRelativeHumidity","type":["attributeReport","readResponse"]},{"cluster":"msPressureMeasurement","type":["attributeReport","readResponse"]},{"cluster":"msTemperatureMeasurement","type":["attributeReport","readResponse"]}],"exposes":[{"type":"light","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","value_toggle":"TOGGLE","description":"On/off state of this light"},{"type":"numeric","name":"brightness","property":"brightness","access":7,"value_min":0,"value_max":254,"description":"Brightness of this light"},{"type":"numeric","name":"color_temp","property":"color_temp","access":7,"unit":"mired","value_min":150,"value_max":500,"description":"Color temperature of this light","presets":[{"name":"coolest","value":150,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":500,"description":"Warmest temperature supported"}]}]},{"type":"enum","name":"effect","property":"effect","access":2,"values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)"},{"type":"binary","name":"power_outage_memory","property":"power_outage_memory","access":3,"value_on":true,"value_off":false,"description":"Enable/disable the power outage memory, this recovers the on/off mode after power failure"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"ota":{},"options":["[Circular]","[Circular]"]},"name":"0x00158d0002b7d6a9"}	
2021-12-16 16:31:02.297 - info: zigbee.0 (26219) 0x00158d0002b7d6a9 (addr 19263): ZNLDP12LM - Xiaomi Aqara smart LED bulb (Router)	
2021-12-16 16:31:02.298 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":31,"_type":"Router","_ieeeAddr":"0x000b57fffe4436b0","_networkAddress":57723,"_manufacturerID":4476,"_endpoints":[{"ID":1,"profileID":49246,"deviceID":544,"inputClusters":[0,3,4,5,6,8,768,2821,4096],"outputClusters":[5,25,32,4096],"deviceNetworkAddress":57723,"deviceIeeeAddress":"0x000b57fffe4436b0","clusters":{"genBasic":{"attributes":{"modelId":"TRADFRI bulb E27 WS opal 980lm","manufacturerName":"IKEA of Sweden","powerSource":1,"zclVersion":1,"appVersion":17,"stackVersion":87,"hwVersion":1,"dateCode":"20170331","swBuildId":"1.2.217"}},"lightingColorCtrl":{"attributes":{"colorCapabilities":16,"colorTempPhysicalMin":250,"colorTempPhysicalMax":454,"colorMode":2,"colorTemperature":278}},"genOnOff":{"attributes":{"onOff":1}},"genLevelCtrl":{"attributes":{"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"IKEA of Sweden","_powerSource":"Mains (single phase)","_modelID":"TRADFRI bulb E27 WS opal 980lm","_applicationVersion":17,"_stackVersion":87,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20170331","_softwareBuildID":"1.2.217","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":2},"_lastSeen":1639638516008},"mapped":{"exposes":[{"type":"light","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","value_toggle":"TOGGLE","description":"On/off state of this light"},{"type":"numeric","name":"brightness","property":"brightness","access":7,"value_min":0,"value_max":254,"description":"Brightness of this light"},{"type":"numeric","name":"color_temp","property":"color_temp","access":7,"unit":"mired","value_min":250,"value_max":454,"description":"Color temperature of this light","presets":[{"name":"coolest","value":250,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":454,"description":"Warmest temperature supported"}]},{"type":"numeric","name":"color_temp_startup","property":"color_temp_startup","access":7,"unit":"mired","value_min":250,"value_max":454,"description":"Color temperature after cold power on of this light","presets":[{"name":"coolest","value":250,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":454,"description":"Warmest temperature supported"},{"name":"previous","value":65535,"description":"Restore previous color_temp on cold power on"}]}]},{"type":"enum","name":"effect","property":"effect","access":2,"values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)"},{"type":"enum","name":"power_on_behavior","property":"power_on_behavior","access":7,"values":["off","previous","on"],"description":"Controls the behavior when the device is powered on"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"lightingColorCtrl","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","brightness","brightness_percent"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp","color_temp_percent"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."},{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["transition"],"attr":[]},{"key":["rate"],"attr":[]},{"key":["brightness_move","brightness_move_onoff"]},{"key":["colortemp_move","color_temp_move"]},{"key":["brightness_step","brightness_step_onoff"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_step"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_startup"]},{"key":["level_config"]},{"key":["power_on_behavior"]},{"key":["color_options"]},{"key":["color_mode"]},{"key":["effect","alert","flash"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"ota":{},"zigbeeModel":["TRADFRI bulb E27 WS opal 980lm","TRADFRI bulb E26 WS opal 980lm","TRADFRI bulb E27 WSopal 980lm"],"model":"LED1545G12","vendor":"IKEA","description":"TRADFRI LED bulb E26/E27 980 lumen, dimmable, white spectrum, opal white","options":["[Circular]","[Circular]"]},"name":"0x000b57fffe4436b0"}	
2021-12-16 16:31:02.300 - info: zigbee.0 (26219) 0x000b57fffe4436b0 (addr 57723): LED1545G12 - IKEA TRADFRI LED bulb E26/E27 980 lumen, dimmable, white spectrum, opal white (Router)	
2021-12-16 16:31:02.301 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":32,"_type":"Router","_ieeeAddr":"0x90fd9ffffe02c40f","_networkAddress":56799,"_manufacturerID":4476,"_endpoints":[{"ID":1,"profileID":49246,"deviceID":544,"inputClusters":[0,3,4,5,6,8,768,2821,4096],"outputClusters":[5,25,32,4096],"deviceNetworkAddress":56799,"deviceIeeeAddress":"0x90fd9ffffe02c40f","clusters":{"genBasic":{"attributes":{"modelId":"TRADFRI bulb E27 WS opal 980lm","manufacturerName":"IKEA of Sweden","powerSource":1,"zclVersion":1,"appVersion":17,"stackVersion":87,"hwVersion":1,"dateCode":"20170331","swBuildId":"1.2.217"}},"lightingColorCtrl":{"attributes":{"colorCapabilities":16,"colorTempPhysicalMin":250,"colorTempPhysicalMax":454,"colorMode":2,"colorTemperature":278}},"genOnOff":{"attributes":{"onOff":1}},"genLevelCtrl":{"attributes":{"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"IKEA of Sweden","_powerSource":"Mains (single phase)","_modelID":"TRADFRI bulb E27 WS opal 980lm","_applicationVersion":17,"_stackVersion":87,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20170331","_softwareBuildID":"1.2.217","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":2},"_lastSeen":1639638516035},"mapped":{"exposes":[{"type":"light","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","value_toggle":"TOGGLE","description":"On/off state of this light"},{"type":"numeric","name":"brightness","property":"brightness","access":7,"value_min":0,"value_max":254,"description":"Brightness of this light"},{"type":"numeric","name":"color_temp","property":"color_temp","access":7,"unit":"mired","value_min":250,"value_max":454,"description":"Color temperature of this light","presets":[{"name":"coolest","value":250,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":454,"description":"Warmest temperature supported"}]},{"type":"numeric","name":"color_temp_startup","property":"color_temp_startup","access":7,"unit":"mired","value_min":250,"value_max":454,"description":"Color temperature after cold power on of this light","presets":[{"name":"coolest","value":250,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":454,"description":"Warmest temperature supported"},{"name":"previous","value":65535,"description":"Restore previous color_temp on cold power on"}]}]},{"type":"enum","name":"effect","property":"effect","access":2,"values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)"},{"type":"enum","name":"power_on_behavior","property":"power_on_behavior","access":7,"values":["off","previous","on"],"description":"Controls the behavior when the device is powered on"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"lightingColorCtrl","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","brightness","brightness_percent"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp","color_temp_percent"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."},{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["transition"],"attr":[]},{"key":["rate"],"attr":[]},{"key":["brightness_move","brightness_move_onoff"]},{"key":["colortemp_move","color_temp_move"]},{"key":["brightness_step","brightness_step_onoff"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_step"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_startup"]},{"key":["level_config"]},{"key":["power_on_behavior"]},{"key":["color_options"]},{"key":["color_mode"]},{"key":["effect","alert","flash"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"ota":{},"zigbeeModel":["TRADFRI bulb E27 WS opal 980lm","TRADFRI bulb E26 WS opal 980lm","TRADFRI bulb E27 WSopal 980lm"],"model":"LED1545G12","vendor":"IKEA","description":"TRADFRI LED bulb E26/E27 980 lumen, dimmable, white spectrum, opal white","options":["[Circular]","[Circular]"]},"name":"0x90fd9ffffe02c40f"}	
2021-12-16 16:31:02.302 - info: zigbee.0 (26219) 0x90fd9ffffe02c40f (addr 56799): LED1545G12 - IKEA TRADFRI LED bulb E26/E27 980 lumen, dimmable, white spectrum, opal white (Router)	
2021-12-16 16:31:02.303 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":33,"_type":"Router","_ieeeAddr":"0x90fd9ffffe7fe8c9","_networkAddress":65244,"_manufacturerID":4476,"_endpoints":[{"ID":1,"profileID":49246,"deviceID":544,"inputClusters":[0,3,4,5,6,8,768,2821,4096],"outputClusters":[5,25,32,4096],"deviceNetworkAddress":65244,"deviceIeeeAddress":"0x90fd9ffffe7fe8c9","clusters":{"genBasic":{"attributes":{"modelId":"TRADFRI bulb E27 WS opal 980lm","manufacturerName":"IKEA of Sweden","powerSource":1,"zclVersion":1,"appVersion":17,"stackVersion":87,"hwVersion":1,"dateCode":"20170331","swBuildId":"1.2.217"}},"lightingColorCtrl":{"attributes":{"colorCapabilities":16,"colorTempPhysicalMin":250,"colorTempPhysicalMax":454,"colorMode":2,"colorTemperature":278}},"genOnOff":{"attributes":{"onOff":1}},"genLevelCtrl":{"attributes":{"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"IKEA of Sweden","_powerSource":"Mains (single phase)","_modelID":"TRADFRI bulb E27 WS opal 980lm","_applicationVersion":17,"_stackVersion":87,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20170331","_softwareBuildID":"1.2.217","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":2},"_lastSeen":1639638516041},"mapped":{"exposes":[{"type":"light","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","value_toggle":"TOGGLE","description":"On/off state of this light"},{"type":"numeric","name":"brightness","property":"brightness","access":7,"value_min":0,"value_max":254,"description":"Brightness of this light"},{"type":"numeric","name":"color_temp","property":"color_temp","access":7,"unit":"mired","value_min":250,"value_max":454,"description":"Color temperature of this light","presets":[{"name":"coolest","value":250,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":454,"description":"Warmest temperature supported"}]},{"type":"numeric","name":"color_temp_startup","property":"color_temp_startup","access":7,"unit":"mired","value_min":250,"value_max":454,"description":"Color temperature after cold power on of this light","presets":[{"name":"coolest","value":250,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":454,"description":"Warmest temperature supported"},{"name":"previous","value":65535,"description":"Restore previous color_temp on cold power on"}]}]},{"type":"enum","name":"effect","property":"effect","access":2,"values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)"},{"type":"enum","name":"power_on_behavior","property":"power_on_behavior","access":7,"values":["off","previous","on"],"description":"Controls the behavior when the device is powered on"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"lightingColorCtrl","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","brightness","brightness_percent"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp","color_temp_percent"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."},{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["transition"],"attr":[]},{"key":["rate"],"attr":[]},{"key":["brightness_move","brightness_move_onoff"]},{"key":["colortemp_move","color_temp_move"]},{"key":["brightness_step","brightness_step_onoff"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_step"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_startup"]},{"key":["level_config"]},{"key":["power_on_behavior"]},{"key":["color_options"]},{"key":["color_mode"]},{"key":["effect","alert","flash"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"ota":{},"zigbeeModel":["TRADFRI bulb E27 WS opal 980lm","TRADFRI bulb E26 WS opal 980lm","TRADFRI bulb E27 WSopal 980lm"],"model":"LED1545G12","vendor":"IKEA","description":"TRADFRI LED bulb E26/E27 980 lumen, dimmable, white spectrum, opal white","options":["[Circular]","[Circular]"]},"name":"0x90fd9ffffe7fe8c9"}	
2021-12-16 16:31:02.304 - info: zigbee.0 (26219) 0x90fd9ffffe7fe8c9 (addr 65244): LED1545G12 - IKEA TRADFRI LED bulb E26/E27 980 lumen, dimmable, white spectrum, opal white (Router)	
2021-12-16 16:31:02.305 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":34,"_type":"Router","_ieeeAddr":"0x90fd9ffffe88755e","_networkAddress":2953,"_manufacturerID":4476,"_endpoints":[{"ID":1,"profileID":49246,"deviceID":544,"inputClusters":[0,3,4,5,6,8,768,2821,4096],"outputClusters":[5,25,32,4096],"deviceNetworkAddress":2953,"deviceIeeeAddress":"0x90fd9ffffe88755e","clusters":{"genBasic":{"attributes":{"modelId":"TRADFRI bulb E27 WS opal 980lm","manufacturerName":"IKEA of Sweden","powerSource":1,"zclVersion":1,"appVersion":17,"stackVersion":87,"hwVersion":1,"dateCode":"20170331","swBuildId":"1.2.217"}},"lightingColorCtrl":{"attributes":{"colorCapabilities":16,"colorTempPhysicalMin":250,"colorTempPhysicalMax":454,"colorMode":2,"colorTemperature":278}},"genOnOff":{"attributes":{"onOff":1}},"genLevelCtrl":{"attributes":{"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"IKEA of Sweden","_powerSource":"Mains (single phase)","_modelID":"TRADFRI bulb E27 WS opal 980lm","_applicationVersion":17,"_stackVersion":87,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20170331","_softwareBuildID":"1.2.217","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":2},"_lastSeen":1639638516042},"mapped":{"exposes":[{"type":"light","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","value_toggle":"TOGGLE","description":"On/off state of this light"},{"type":"numeric","name":"brightness","property":"brightness","access":7,"value_min":0,"value_max":254,"description":"Brightness of this light"},{"type":"numeric","name":"color_temp","property":"color_temp","access":7,"unit":"mired","value_min":250,"value_max":454,"description":"Color temperature of this light","presets":[{"name":"coolest","value":250,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":454,"description":"Warmest temperature supported"}]},{"type":"numeric","name":"color_temp_startup","property":"color_temp_startup","access":7,"unit":"mired","value_min":250,"value_max":454,"description":"Color temperature after cold power on of this light","presets":[{"name":"coolest","value":250,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":454,"description":"Warmest temperature supported"},{"name":"previous","value":65535,"description":"Restore previous color_temp on cold power on"}]}]},{"type":"enum","name":"effect","property":"effect","access":2,"values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)"},{"type":"enum","name":"power_on_behavior","property":"power_on_behavior","access":7,"values":["off","previous","on"],"description":"Controls the behavior when the device is powered on"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"lightingColorCtrl","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","brightness","brightness_percent"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp","color_temp_percent"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."},{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["transition"],"attr":[]},{"key":["rate"],"attr":[]},{"key":["brightness_move","brightness_move_onoff"]},{"key":["colortemp_move","color_temp_move"]},{"key":["brightness_step","brightness_step_onoff"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_step"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_startup"]},{"key":["level_config"]},{"key":["power_on_behavior"]},{"key":["color_options"]},{"key":["color_mode"]},{"key":["effect","alert","flash"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"ota":{},"zigbeeModel":["TRADFRI bulb E27 WS opal 980lm","TRADFRI bulb E26 WS opal 980lm","TRADFRI bulb E27 WSopal 980lm"],"model":"LED1545G12","vendor":"IKEA","description":"TRADFRI LED bulb E26/E27 980 lumen, dimmable, white spectrum, opal white","options":["[Circular]","[Circular]"]},"name":"0x90fd9ffffe88755e"}	
2021-12-16 16:31:02.306 - info: zigbee.0 (26219) 0x90fd9ffffe88755e (addr 2953): LED1545G12 - IKEA TRADFRI LED bulb E26/E27 980 lumen, dimmable, white spectrum, opal white (Router)	
2021-12-16 16:31:02.306 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":36,"_type":"EndDevice","_ieeeAddr":"0x00158d000274f4d3","_networkAddress":44450,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":44450,"deviceIeeeAddress":"0x00158d000274f4d3","clusters":{"genBasic":{"attributes":{"65281":{"1":2995,"3":26,"4":5032,"5":69,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_magnet.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639667159723},"mapped":{"zigbeeModel":["lumi.sensor_magnet.aq2"],"model":"MCCGQ11LM","vendor":"Xiaomi","description":"Aqara door & window contact sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"binary","name":"contact","property":"contact","access":1,"value_on":false,"value_off":true,"description":"Indicates if the contact is closed (= true) or open (= false)"},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":["[Circular]","[Circular]"]},"name":"0x00158d000274f4d3"}	
2021-12-16 16:31:02.307 - info: zigbee.0 (26219) 0x00158d000274f4d3 (addr 44450): MCCGQ11LM - Xiaomi Aqara door & window contact sensor (EndDevice)	
2021-12-16 16:31:02.308 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":37,"_type":"EndDevice","_ieeeAddr":"0x00158d0002722af7","_networkAddress":45388,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":45388,"deviceIeeeAddress":"0x00158d0002722af7","clusters":{"genBasic":{"attributes":{"65281":{"1":3025,"3":18,"4":5032,"5":64,"6":[0,1],"10":47504,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_magnet.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639664567227},"mapped":{"zigbeeModel":["lumi.sensor_magnet.aq2"],"model":"MCCGQ11LM","vendor":"Xiaomi","description":"Aqara door & window contact sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"binary","name":"contact","property":"contact","access":1,"value_on":false,"value_off":true,"description":"Indicates if the contact is closed (= true) or open (= false)"},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":["[Circular]","[Circular]"]},"name":"0x00158d0002722af7"}	
2021-12-16 16:31:02.308 - info: zigbee.0 (26219) 0x00158d0002722af7 (addr 45388): MCCGQ11LM - Xiaomi Aqara door & window contact sensor (EndDevice)	
2021-12-16 16:31:02.309 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":38,"_type":"EndDevice","_ieeeAddr":"0x847127fffed62092","_networkAddress":16764,"_manufacturerID":4098,"_endpoints":[{"ID":1,"profileID":260,"deviceID":81,"inputClusters":[0,4,5,61184],"outputClusters":[25,10],"deviceNetworkAddress":16764,"deviceIeeeAddress":"0x847127fffed62092","clusters":{"genBasic":{"attributes":{"modelId":"TS0601","manufacturerName":"_TZE200_zah67ekd","powerSource":3,"zclVersion":3,"appVersion":71,"stackVersion":0,"hwVersion":1,"dateCode":""}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZE200_zah67ekd","_powerSource":"Battery","_modelID":"TS0601","_applicationVersion":71,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639665489166},"mapped":{"zigbeeModel":["owvfni3\u0000","owvfni3","u1rkty3","aabybja","mcdj3aq","mcdj3aq\u0000"],"fingerprint":[{"modelID":"TS0601","manufacturerName":"_TZE200_5zbp6j0u"},{"modelID":"TS0601","manufacturerName":"_TZE200_nkoabg8w"},{"modelID":"TS0601","manufacturerName":"_TZE200_xuzcvlku"},{"modelID":"TS0601","manufacturerName":"_TZE200_4vobcgd3"},{"modelID":"TS0601","manufacturerName":"_TZE200_nogaemzt"},{"modelID":"TS0601","manufacturerName":"_TZE200_pk0sfzvr"},{"modelID":"TS0601","manufacturerName":"_TZE200_fdtjuw7u"},{"modelID":"TS0601","manufacturerName":"_TZE200_zpzndjez"},{"modelID":"TS0601","manufacturerName":"_TZE200_wmcdj3aq"},{"modelID":"TS0601","manufacturerName":"_TZE200_cowvfni3"},{"modelID":"TS0601","manufacturerName":"_TZE200_rddyvrci"},{"modelID":"TS0601","manufacturerName":"_TZE200_nueqqe6k"},{"modelID":"TS0601","manufacturerName":"_TZE200_xaabybja"},{"modelID":"TS0601","manufacturerName":"_TZE200_rmymn92d"},{"modelID":"zo2pocs\u0000","manufacturerName":"_TYST11_fzo2pocs"},{"modelID":"TS0601","manufacturerName":"_TZE200_sbordckq"},{"modelID":"TS0601","manufacturerName":"_TZE200_fctwhugx"},{"modelID":"TS0601","manufacturerName":"_TZE200_zah67ekd"},{"modelID":"TS0601","manufacturerName":"_TZE200_g5wdnuow"},{"modelID":"TS0601","manufacturerName":"_TZE200_fzo2pocs"},{"modelID":"TS0601","manufacturerName":"_TZE200_5sbebbzs"},{"modelID":"TS0601","manufacturerName":"_TZE200_zuz7f94z"}],"model":"TS0601_cover","vendor":"TuYa","description":"Curtain motor/roller blind motor/window pusher/tubular motor","whiteLabel":[{"vendor":"Yushun","model":"YS-MT750"},{"vendor":"Zemismart","model":"ZM79E-DT"},{"vendor":"Binthen","model":"BCM100D"},{"vendor":"Binthen","model":"CV01A"},{"vendor":"Zemismart","model":"M515EGB"},{"vendor":"TuYa","model":"M515EGZT"},{"vendor":"TuYa","model":"DT82LEMA-1.2N"},{"vendor":"Moes","model":"AM43-0.45/40-ES-EB"},{"vendor":"Larkkey","model":"ZSTY-SM-1SRZG-EU"},{"vendor":"Zemismart","model":"ZM25TQ","description":"Tubular motor"},{"vendor":"Zemismart","model":"AM43","description":"Roller blind motor"},{"vendor":"Zemismart","model":"M2805EGBZTN","description":"Tubular motor"},{"vendor":"Zemismart","model":"BCM500DS-TYZ","description":"Curtain motor"},{"vendor":"A-OK","model":"AM25","description":"Tubular motor"}],"fromZigbee":[{"cluster":"manuSpecificTuya","type":["commandSetDataResponse","commandGetData"],"options":[{"type":"binary","name":"invert_cover","property":"invert_cover","access":2,"value_on":true,"value_off":false,"description":"Inverts the cover position, false: open=100,close=0, true: open=0,close=100 (default false)."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","position"],"options":[{"type":"binary","name":"invert_cover","property":"invert_cover","access":2,"value_on":true,"value_off":false,"description":"Inverts the cover position, false: open=100,close=0, true: open=0,close=100 (default false)."}]},{"key":["options"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"exposes":[{"type":"cover","features":[{"type":"enum","name":"state","property":"state","access":3,"values":["OPEN","CLOSE","STOP"]},{"type":"numeric","name":"position","property":"position","access":3,"value_min":0,"value_max":100,"description":"Position of this cover"}]},{"type":"composite","property":"options","name":"options","features":[{"type":"numeric","name":"motor_speed","property":"motor_speed","access":3,"value_min":0,"value_max":255,"description":"Motor speed"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":["[Circular]"]},"name":"0x847127fffed62092"}	
2021-12-16 16:31:02.310 - info: zigbee.0 (26219) 0x847127fffed62092 (addr 16764): TS0601_cover - TuYa Curtain motor/roller blind motor/window pusher/tubular motor (EndDevice)	
2021-12-16 16:31:02.310 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":39,"_type":"EndDevice","_ieeeAddr":"0x847127fffed0a598","_networkAddress":30072,"_manufacturerID":4098,"_endpoints":[{"ID":1,"profileID":260,"deviceID":81,"inputClusters":[0,4,5,61184],"outputClusters":[25,10],"deviceNetworkAddress":30072,"deviceIeeeAddress":"0x847127fffed0a598","clusters":{"genBasic":{"attributes":{"modelId":"TS0601","manufacturerName":"_TZE200_zah67ekd","powerSource":3,"zclVersion":3,"appVersion":71,"stackVersion":0,"hwVersion":1,"dateCode":""}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZE200_zah67ekd","_powerSource":"Battery","_modelID":"TS0601","_applicationVersion":71,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639667988665},"mapped":{"zigbeeModel":["owvfni3\u0000","owvfni3","u1rkty3","aabybja","mcdj3aq","mcdj3aq\u0000"],"fingerprint":[{"modelID":"TS0601","manufacturerName":"_TZE200_5zbp6j0u"},{"modelID":"TS0601","manufacturerName":"_TZE200_nkoabg8w"},{"modelID":"TS0601","manufacturerName":"_TZE200_xuzcvlku"},{"modelID":"TS0601","manufacturerName":"_TZE200_4vobcgd3"},{"modelID":"TS0601","manufacturerName":"_TZE200_nogaemzt"},{"modelID":"TS0601","manufacturerName":"_TZE200_pk0sfzvr"},{"modelID":"TS0601","manufacturerName":"_TZE200_fdtjuw7u"},{"modelID":"TS0601","manufacturerName":"_TZE200_zpzndjez"},{"modelID":"TS0601","manufacturerName":"_TZE200_wmcdj3aq"},{"modelID":"TS0601","manufacturerName":"_TZE200_cowvfni3"},{"modelID":"TS0601","manufacturerName":"_TZE200_rddyvrci"},{"modelID":"TS0601","manufacturerName":"_TZE200_nueqqe6k"},{"modelID":"TS0601","manufacturerName":"_TZE200_xaabybja"},{"modelID":"TS0601","manufacturerName":"_TZE200_rmymn92d"},{"modelID":"zo2pocs\u0000","manufacturerName":"_TYST11_fzo2pocs"},{"modelID":"TS0601","manufacturerName":"_TZE200_sbordckq"},{"modelID":"TS0601","manufacturerName":"_TZE200_fctwhugx"},{"modelID":"TS0601","manufacturerName":"_TZE200_zah67ekd"},{"modelID":"TS0601","manufacturerName":"_TZE200_g5wdnuow"},{"modelID":"TS0601","manufacturerName":"_TZE200_fzo2pocs"},{"modelID":"TS0601","manufacturerName":"_TZE200_5sbebbzs"},{"modelID":"TS0601","manufacturerName":"_TZE200_zuz7f94z"}],"model":"TS0601_cover","vendor":"TuYa","description":"Curtain motor/roller blind motor/window pusher/tubular motor","whiteLabel":[{"vendor":"Yushun","model":"YS-MT750"},{"vendor":"Zemismart","model":"ZM79E-DT"},{"vendor":"Binthen","model":"BCM100D"},{"vendor":"Binthen","model":"CV01A"},{"vendor":"Zemismart","model":"M515EGB"},{"vendor":"TuYa","model":"M515EGZT"},{"vendor":"TuYa","model":"DT82LEMA-1.2N"},{"vendor":"Moes","model":"AM43-0.45/40-ES-EB"},{"vendor":"Larkkey","model":"ZSTY-SM-1SRZG-EU"},{"vendor":"Zemismart","model":"ZM25TQ","description":"Tubular motor"},{"vendor":"Zemismart","model":"AM43","description":"Roller blind motor"},{"vendor":"Zemismart","model":"M2805EGBZTN","description":"Tubular motor"},{"vendor":"Zemismart","model":"BCM500DS-TYZ","description":"Curtain motor"},{"vendor":"A-OK","model":"AM25","description":"Tubular motor"}],"fromZigbee":[{"cluster":"manuSpecificTuya","type":["commandSetDataResponse","commandGetData"],"options":[{"type":"binary","name":"invert_cover","property":"invert_cover","access":2,"value_on":true,"value_off":false,"description":"Inverts the cover position, false: open=100,close=0, true: open=0,close=100 (default false)."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","position"],"options":[{"type":"binary","name":"invert_cover","property":"invert_cover","access":2,"value_on":true,"value_off":false,"description":"Inverts the cover position, false: open=100,close=0, true: open=0,close=100 (default false)."}]},{"key":["options"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"exposes":[{"type":"cover","features":[{"type":"enum","name":"state","property":"state","access":3,"values":["OPEN","CLOSE","STOP"]},{"type":"numeric","name":"position","property":"position","access":3,"value_min":0,"value_max":100,"description":"Position of this cover"}]},{"type":"composite","property":"options","name":"options","features":[{"type":"numeric","name":"motor_speed","property":"motor_speed","access":3,"value_min":0,"value_max":255,"description":"Motor speed"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":["[Circular]"]},"name":"0x847127fffed0a598"}	
2021-12-16 16:31:02.311 - info: zigbee.0 (26219) 0x847127fffed0a598 (addr 30072): TS0601_cover - TuYa Curtain motor/roller blind motor/window pusher/tubular motor (EndDevice)	
2021-12-16 16:31:02.312 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":40,"_type":"EndDevice","_ieeeAddr":"0x847127fffecfc657","_networkAddress":1896,"_manufacturerID":4098,"_endpoints":[{"ID":1,"profileID":260,"deviceID":81,"inputClusters":[0,4,5,61184],"outputClusters":[25,10],"deviceNetworkAddress":1896,"deviceIeeeAddress":"0x847127fffecfc657","clusters":{"genBasic":{"attributes":{"modelId":"TS0601","manufacturerName":"_TZE200_zah67ekd","powerSource":3,"zclVersion":3,"appVersion":71,"stackVersion":0,"hwVersion":1,"dateCode":""}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZE200_zah67ekd","_powerSource":"Battery","_modelID":"TS0601","_applicationVersion":71,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639668374974},"mapped":{"zigbeeModel":["owvfni3\u0000","owvfni3","u1rkty3","aabybja","mcdj3aq","mcdj3aq\u0000"],"fingerprint":[{"modelID":"TS0601","manufacturerName":"_TZE200_5zbp6j0u"},{"modelID":"TS0601","manufacturerName":"_TZE200_nkoabg8w"},{"modelID":"TS0601","manufacturerName":"_TZE200_xuzcvlku"},{"modelID":"TS0601","manufacturerName":"_TZE200_4vobcgd3"},{"modelID":"TS0601","manufacturerName":"_TZE200_nogaemzt"},{"modelID":"TS0601","manufacturerName":"_TZE200_pk0sfzvr"},{"modelID":"TS0601","manufacturerName":"_TZE200_fdtjuw7u"},{"modelID":"TS0601","manufacturerName":"_TZE200_zpzndjez"},{"modelID":"TS0601","manufacturerName":"_TZE200_wmcdj3aq"},{"modelID":"TS0601","manufacturerName":"_TZE200_cowvfni3"},{"modelID":"TS0601","manufacturerName":"_TZE200_rddyvrci"},{"modelID":"TS0601","manufacturerName":"_TZE200_nueqqe6k"},{"modelID":"TS0601","manufacturerName":"_TZE200_xaabybja"},{"modelID":"TS0601","manufacturerName":"_TZE200_rmymn92d"},{"modelID":"zo2pocs\u0000","manufacturerName":"_TYST11_fzo2pocs"},{"modelID":"TS0601","manufacturerName":"_TZE200_sbordckq"},{"modelID":"TS0601","manufacturerName":"_TZE200_fctwhugx"},{"modelID":"TS0601","manufacturerName":"_TZE200_zah67ekd"},{"modelID":"TS0601","manufacturerName":"_TZE200_g5wdnuow"},{"modelID":"TS0601","manufacturerName":"_TZE200_fzo2pocs"},{"modelID":"TS0601","manufacturerName":"_TZE200_5sbebbzs"},{"modelID":"TS0601","manufacturerName":"_TZE200_zuz7f94z"}],"model":"TS0601_cover","vendor":"TuYa","description":"Curtain motor/roller blind motor/window pusher/tubular motor","whiteLabel":[{"vendor":"Yushun","model":"YS-MT750"},{"vendor":"Zemismart","model":"ZM79E-DT"},{"vendor":"Binthen","model":"BCM100D"},{"vendor":"Binthen","model":"CV01A"},{"vendor":"Zemismart","model":"M515EGB"},{"vendor":"TuYa","model":"M515EGZT"},{"vendor":"TuYa","model":"DT82LEMA-1.2N"},{"vendor":"Moes","model":"AM43-0.45/40-ES-EB"},{"vendor":"Larkkey","model":"ZSTY-SM-1SRZG-EU"},{"vendor":"Zemismart","model":"ZM25TQ","description":"Tubular motor"},{"vendor":"Zemismart","model":"AM43","description":"Roller blind motor"},{"vendor":"Zemismart","model":"M2805EGBZTN","description":"Tubular motor"},{"vendor":"Zemismart","model":"BCM500DS-TYZ","description":"Curtain motor"},{"vendor":"A-OK","model":"AM25","description":"Tubular motor"}],"fromZigbee":[{"cluster":"manuSpecificTuya","type":["commandSetDataResponse","commandGetData"],"options":[{"type":"binary","name":"invert_cover","property":"invert_cover","access":2,"value_on":true,"value_off":false,"description":"Inverts the cover position, false: open=100,close=0, true: open=0,close=100 (default false)."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","position"],"options":[{"type":"binary","name":"invert_cover","property":"invert_cover","access":2,"value_on":true,"value_off":false,"description":"Inverts the cover position, false: open=100,close=0, true: open=0,close=100 (default false)."}]},{"key":["options"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"exposes":[{"type":"cover","features":[{"type":"enum","name":"state","property":"state","access":3,"values":["OPEN","CLOSE","STOP"]},{"type":"numeric","name":"position","property":"position","access":3,"value_min":0,"value_max":100,"description":"Position of this cover"}]},{"type":"composite","property":"options","name":"options","features":[{"type":"numeric","name":"motor_speed","property":"motor_speed","access":3,"value_min":0,"value_max":255,"description":"Motor speed"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":["[Circular]"]},"name":"0x847127fffecfc657"}	
2021-12-16 16:31:02.312 - info: zigbee.0 (26219) 0x847127fffecfc657 (addr 1896): TS0601_cover - TuYa Curtain motor/roller blind motor/window pusher/tubular motor (EndDevice)	
2021-12-16 16:31:02.313 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":42,"_type":"Router","_ieeeAddr":"0xa4c138934ce2822b","_networkAddress":25440,"_manufacturerID":4417,"_endpoints":[{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":25440,"deviceIeeeAddress":"0xa4c138934ce2822b","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":0,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}},"manuSpecificTuya_3":{"attributes":{"switchType":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":97,"inputClusters":[],"outputClusters":[33],"deviceNetworkAddress":25440,"deviceIeeeAddress":"0xa4c138934ce2822b","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZ3000_npzfdcof","_powerSource":"Mains (single phase)","_modelID":"TS0001","_applicationVersion":67,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639665984619},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["TS0001"],"model":"TS0001","vendor":"TuYa","description":"1 gang switch","whiteLabel":[{"vendor":"CR Smart Home","model":"TS0001","description":"Valve control"},{"vendor":"Lonsonho","model":"X701"},{"vendor":"Bandi","model":"BDS03G1"}],"options":[]},"name":"0xa4c138934ce2822b"}	
2021-12-16 16:31:02.313 - info: zigbee.0 (26219) 0xa4c138934ce2822b (addr 25440): TS0001 - TuYa 1 gang switch (Router)	
2021-12-16 16:31:02.314 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":43,"_type":"Router","_ieeeAddr":"0xa4c138ec0e4ef1cf","_networkAddress":60149,"_manufacturerID":4417,"_endpoints":[{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":0,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":97,"inputClusters":[],"outputClusters":[33],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZ3000_npzfdcof","_powerSource":"Mains (single phase)","_modelID":"TS0001","_applicationVersion":67,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668636848},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["TS0001"],"model":"TS0001","vendor":"TuYa","description":"1 gang switch","whiteLabel":[{"vendor":"CR Smart Home","model":"TS0001","description":"Valve control"},{"vendor":"Lonsonho","model":"X701"},{"vendor":"Bandi","model":"BDS03G1"}],"options":[]},"name":"0xa4c138ec0e4ef1cf"}	
2021-12-16 16:31:02.315 - info: zigbee.0 (26219) 0xa4c138ec0e4ef1cf (addr 60149): TS0001 - TuYa 1 gang switch (Router)	
2021-12-16 16:31:02.315 - debug: zigbee.0 (26219) New device event: {"type":"device","device":{"ID":44,"_type":"EndDevice","_ieeeAddr":"0x000d6ffffe2cd4b8","_networkAddress":935,"_manufacturerID":4476,"_endpoints":[{"ID":1,"profileID":260,"deviceID":514,"inputClusters":[0,1,3,4,5,32,258,4096,64636],"outputClusters":[25,4096],"deviceNetworkAddress":935,"deviceIeeeAddress":"0x000d6ffffe2cd4b8","clusters":{"genBasic":{"attributes":{"modelId":"FYRTUR block-out roller blind","manufacturerName":"IKEA of Sweden","powerSource":3,"zclVersion":3,"appVersion":33,"stackVersion":99,"hwVersion":1,"dateCode":"20190311","swBuildId":"2.3.073"}},"genPowerCfg":{"attributes":{"batteryPercentageRemaining":100}},"closuresWindowCovering":{"attributes":{"currentPositionLiftPercentage":0}}},"_binds":[{"cluster":1,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1},{"cluster":258,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":1,"attrId":33,"minRepIntval":3600,"maxRepIntval":62000,"repChange":0},{"cluster":258,"attrId":8,"minRepIntval":1,"maxRepIntval":62000,"repChange":1}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"IKEA of Sweden","_powerSource":"Battery","_modelID":"FYRTUR block-out roller blind","_applicationVersion":33,"_stackVersion":99,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"20190311","_softwareBuildID":"2.3.073","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":2},"_lastSeen":1638803854786,"useImplicitCheckin":true},"mapped":{"zigbeeModel":["FYRTUR block-out roller blind"],"model":"E1757","vendor":"IKEA","description":"FYRTUR roller blind","fromZigbee":[{"cluster":"closuresWindowCovering","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"invert_cover","property":"invert_cover","access":2,"value_on":true,"value_off":false,"description":"Inverts the cover position, false: open=100,close=0, true: open=0,close=100 (default false)."}]},{"cluster":"genPowerCfg","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state"]},{"key":["position","tilt"],"options":[{"type":"binary","name":"invert_cover","property":"invert_cover","access":2,"value_on":true,"value_off":false,"description":"Inverts the cover position, false: open=100,close=0, true: open=0,close=100 (default false)."}]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"meta":{"battery":{"dontDividePercentage":true}},"ota":{},"exposes":[{"type":"cover","features":[{"type":"enum","name":"state","property":"state","access":3,"values":["OPEN","CLOSE","STOP"]},{"type":"numeric","name":"position","property":"position","access":7,"value_min":0,"value_max":100,"description":"Position of this cover"}]},{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":["[Circular]"]},"name":"0x000d6ffffe2cd4b8"}	
2021-12-16 16:31:02.316 - info: zigbee.0 (26219) 0x000d6ffffe2cd4b8 (addr 935): E1757 - IKEA FYRTUR roller blind (EndDevice)	
2021-12-16 16:31:02.316 - info: zigbee.0 (26219) Zigbee started	
2021-12-16 16:31:02.458 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa00acb990/3 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:02.460 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00acb990:47504/3 (0,0,1)	
2021-12-16 16:31:02.463 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":47504,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":1,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,2,0,0,0]}}	
2021-12-16 16:31:02.464 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,144,185,3,1,6,0,1,0,30,5,16,2,0,0,0,15]	
2021-12-16 16:31:02.500 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:02.501 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:02.501 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:02.502 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:02.502 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:02.586 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,1,38]	
2021-12-16 16:31:02.588 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,1,38]	
2021-12-16 16:31:02.590 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,1] - 38	
2021-12-16 16:31:02.592 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":1}	
2021-12-16 16:31:02.594 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:02.595 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00acb990:47504,225,0)	
2021-12-16 16:31:02.665 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa0a00dfcb/3 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:02.666 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa0a00dfcb:34528/3 (0,0,2)	
2021-12-16 16:31:02.666 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":34528,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":2,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,3,0,0,0]}}	
2021-12-16 16:31:02.667 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,224,134,3,1,6,0,2,0,30,5,16,3,0,0,0,66]	
2021-12-16 16:31:02.694 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:02.695 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:02.695 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:02.696 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:02.697 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:02.866 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x00158d0002c65ed8/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:02.866 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002c65ed8:41267/1 (0,0,3)	
2021-12-16 16:31:02.867 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":41267,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":3,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,4,0,0,0]}}	
2021-12-16 16:31:02.867 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,51,161,1,1,6,0,3,0,30,5,16,4,0,0,0,178]	
2021-12-16 16:31:02.923 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:02.924 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:02.924 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:02.924 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:02.925 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:03.074 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x84182600000c7532/3 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:03.075 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x84182600000c7532:56716/3 (0,0,4)	
2021-12-16 16:31:03.076 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":56716,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":4,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,5,0,0,0]}}	
2021-12-16 16:31:03.077 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,140,221,3,1,6,0,4,0,30,5,16,5,0,0,0,117]	
2021-12-16 16:31:03.082 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:03.083 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:03.084 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:03.084 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:03.085 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:03.092 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,0,1,4,194]	
2021-12-16 16:31:03.093 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,0,1,4,194]	
2021-12-16 16:31:03.093 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [0,1,4] - 194	
2021-12-16 16:31:03.094 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":0,"endpoint":1,"transid":4}	
2021-12-16 16:31:03.094 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:03.132 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,28,68,129,0,0,6,0]	
2021-12-16 16:31:03.133 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,28,68,129,0,0,6,0]	
2021-12-16 16:31:03.134 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [140,221,3,1,0,78,0,121]	
2021-12-16 16:31:03.134 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,28,68,129,0,0,6,0,140,221,3,1,0,78,0,121]	
2021-12-16 16:31:03.136 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [13,66,0,0,8,24,5,1,0,0,0,16,1,245,234,28,242]	
2021-12-16 16:31:03.136 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,28,68,129,0,0,6,0,140,221,3,1,0,78,0,121,13,66,0,0,8,24,5,1,0,0,0,16,1,245,234,28,242]	
2021-12-16 16:31:03.137 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 28 - 2 - 4 - 129 - [0,0,6,0,140,221,3,1,0,78,0,121,13,66,0,0,8,24,5,1,0,0,0,16,1,245,234,28] - 242	
2021-12-16 16:31:03.138 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - incomingMsg - {"groupid":0,"clusterid":6,"srcaddr":56716,"srcendpoint":3,"dstendpoint":1,"wasbroadcast":0,"linkquality":78,"securityuse":0,"timestamp":4328825,"transseqnumber":0,"len":8,"data":{"type":"Buffer","data":[24,5,1,0,0,0,16,1]}}	
2021-12-16 16:31:03.141 - debug: zigbee.0 (26219) zigbee-herdsman:controller:log Received 'zcl' data '{"frame":{"Header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":5,"manufacturerCode":null,"commandIdentifier":1},"Payload":[{"attrId":0,"status":0,"dataType":16,"attrData":1}],"Command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}},"address":56716,"endpoint":3,"linkquality":78,"groupID":0,"wasBroadcast":false,"destinationEndpoint":1}'	
2021-12-16 16:31:03.143 - debug: zigbee.0 (26219) handleMessage. {"type":"readResponse","device":{"ID":16,"_type":"Router","_ieeeAddr":"0x84182600000c7532","_networkAddress":56716,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":56716,"deviceIeeeAddress":"0x84182600000c7532","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":1}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668663141,"_linkquality":78},"endpoint":"[Circular]","data":{"onOff":1},"linkquality":78,"groupID":0,"cluster":"genOnOff","meta":{"zclTransactionSequenceNumber":5,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:31:03.144 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:03.144 - debug: zigbee.0 (26219) Received Zigbee message from '0x84182600000c7532', type 'readResponse', cluster 'genOnOff', data '{"onOff":1}' from endpoint 3 with groupID 0	
2021-12-16 16:31:03.145 - debug: zigbee.0 (26219) Type readResponse device {"type":"device","device":{"ID":16,"_type":"Router","_ieeeAddr":"0x84182600000c7532","_networkAddress":56716,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":56716,"deviceIeeeAddress":"0x84182600000c7532","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":1}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668663141,"_linkquality":78},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["Plug 01"],"model":"AB3257001NJ","description":"Smart+ plug","vendor":"OSRAM","whiteLabel":[{"vendor":"LEDVANCE","model":"AB3257001NJ"}],"ota":{},"options":[]},"name":"0x84182600000c7532"} incoming event: {"type":"readResponse","device":{"ID":16,"_type":"Router","_ieeeAddr":"0x84182600000c7532","_networkAddress":56716,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":56716,"deviceIeeeAddress":"0x84182600000c7532","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":1}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668663141,"_linkquality":78},"endpoint":"[Circular]","data":{"onOff":1},"linkquality":78,"groupID":0,"cluster":"genOnOff","meta":{"zclTransactionSequenceNumber":5,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:31:03.147 - debug: zigbee.0 (26219) Publish available for 0x84182600000c7532 = true	
2021-12-16 16:31:03.148 - debug: zigbee.0 (26219) Publish LQ for 0x84182600000c7532 = 10	
2021-12-16 16:31:03.150 - debug: zigbee.0 (26219) Successful read state 'state' of '0x84182600000c7532' in stead of pinging	
2021-12-16 16:31:03.164 - debug: zigbee.0 (26219) Publish {"state":"ON"} to "84182600000c7532"	
2021-12-16 16:31:03.167 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,2,9]	
2021-12-16 16:31:03.167 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,2,9]	
2021-12-16 16:31:03.168 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,2] - 9	
2021-12-16 16:31:03.168 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":2}	
2021-12-16 16:31:03.168 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:03.169 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa0a00dfcb:34528,205,0)	
2021-12-16 16:31:03.169 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Wait 2000ms	
2021-12-16 16:31:03.240 - debug: zigbee.0 (26219) Publish available for 0x00158d0002b54a17 = true	
2021-12-16 16:31:03.241 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002b54a17 = 10	
2021-12-16 16:31:03.247 - debug: zigbee.0 (26219) Publish available for 0x00158d0002130d3b = true	
2021-12-16 16:31:03.249 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002130d3b = 10	
2021-12-16 16:31:03.252 - debug: zigbee.0 (26219) Publish available for 0x7cb03eaa00acb990 = true	
2021-12-16 16:31:03.253 - debug: zigbee.0 (26219) Publish LQ for 0x7cb03eaa00acb990 = 10	
2021-12-16 16:31:03.255 - debug: zigbee.0 (26219) Publish available for 0x7cb03eaa0a00dfcb = true	
2021-12-16 16:31:03.256 - debug: zigbee.0 (26219) Publish LQ for 0x7cb03eaa0a00dfcb = 10	
2021-12-16 16:31:03.260 - debug: zigbee.0 (26219) Publish available for 0x00158d0002c65ed8 = true	
2021-12-16 16:31:03.262 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002c65ed8 = 10	
2021-12-16 16:31:03.264 - debug: zigbee.0 (26219) Publish available for 0x00158d0002130f3a = true	
2021-12-16 16:31:03.265 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002130f3a = 10	
2021-12-16 16:31:03.266 - debug: zigbee.0 (26219) Publish available for 0x00158d0002f8d76c = true	
2021-12-16 16:31:03.268 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002f8d76c = 10	
2021-12-16 16:31:03.269 - debug: zigbee.0 (26219) Publish available for 0x00158d000274f4de = true	
2021-12-16 16:31:03.270 - debug: zigbee.0 (26219) Publish LQ for 0x00158d000274f4de = 10	
2021-12-16 16:31:03.272 - debug: zigbee.0 (26219) Publish available for 0x00158d0002135d9b = true	
2021-12-16 16:31:03.273 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002135d9b = 10	
2021-12-16 16:31:03.274 - debug: zigbee.0 (26219) Publish available for 0x00158d000274f4bf = true	
2021-12-16 16:31:03.276 - debug: zigbee.0 (26219) Publish LQ for 0x00158d000274f4bf = 10	
2021-12-16 16:31:03.277 - debug: zigbee.0 (26219) Publish available for 0x00158d000271c4b7 = true	
2021-12-16 16:31:03.279 - debug: zigbee.0 (26219) Publish LQ for 0x00158d000271c4b7 = 10	
2021-12-16 16:31:03.286 - debug: zigbee.0 (26219) Publish available for 0x00158d0002f8d5b4 = true	
2021-12-16 16:31:03.288 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002f8d5b4 = 10	
2021-12-16 16:31:03.290 - debug: zigbee.0 (26219) Publish available for 0x00158d0002e34b33 = true	
2021-12-16 16:31:03.292 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002e34b33 = 10	
2021-12-16 16:31:03.294 - debug: zigbee.0 (26219) Publish available for 0x00158d000521d656 = true	
2021-12-16 16:31:03.295 - debug: zigbee.0 (26219) Publish LQ for 0x00158d000521d656 = 10	
2021-12-16 16:31:03.296 - debug: zigbee.0 (26219) Publish available for 0x84182600000c7532 = true	
2021-12-16 16:31:03.298 - debug: zigbee.0 (26219) Publish LQ for 0x84182600000c7532 = 10	
2021-12-16 16:31:03.299 - debug: zigbee.0 (26219) Publish available for 0x7cb03eaa0a025809 = true	
2021-12-16 16:31:03.300 - debug: zigbee.0 (26219) Publish LQ for 0x7cb03eaa0a025809 = 10	
2021-12-16 16:31:03.302 - debug: zigbee.0 (26219) Publish available for 0x00158d00028aee30 = true	
2021-12-16 16:31:03.303 - debug: zigbee.0 (26219) Publish LQ for 0x00158d00028aee30 = 10	
2021-12-16 16:31:03.305 - debug: zigbee.0 (26219) Publish available for 0x00158d00021369f3 = true	
2021-12-16 16:31:03.306 - debug: zigbee.0 (26219) Publish LQ for 0x00158d00021369f3 = 10	
2021-12-16 16:31:03.307 - debug: zigbee.0 (26219) Publish available for 0x00158d0002b54752 = true	
2021-12-16 16:31:03.308 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002b54752 = 10	
2021-12-16 16:31:03.310 - debug: zigbee.0 (26219) Publish available for 0x00158d000274f643 = true	
2021-12-16 16:31:03.311 - debug: zigbee.0 (26219) Publish LQ for 0x00158d000274f643 = 10	
2021-12-16 16:31:03.312 - debug: zigbee.0 (26219) Publish available for 0x00158d000274f64d = true	
2021-12-16 16:31:03.314 - debug: zigbee.0 (26219) Publish LQ for 0x00158d000274f64d = 10	
2021-12-16 16:31:03.315 - debug: zigbee.0 (26219) Publish available for 0x00158d0002b51c42 = true	
2021-12-16 16:31:03.317 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002b51c42 = 10	
2021-12-16 16:31:03.318 - debug: zigbee.0 (26219) Publish available for 0x00158d000274f4f7 = true	
2021-12-16 16:31:03.320 - debug: zigbee.0 (26219) Publish LQ for 0x00158d000274f4f7 = 10	
2021-12-16 16:31:03.321 - debug: zigbee.0 (26219) Publish available for 0x7cb03eaa00a36bed = true	
2021-12-16 16:31:03.323 - debug: zigbee.0 (26219) Publish LQ for 0x7cb03eaa00a36bed = 10	
2021-12-16 16:31:03.324 - debug: zigbee.0 (26219) Publish available for 0x7cb03eaa0a019e9d = true	
2021-12-16 16:31:03.325 - debug: zigbee.0 (26219) Publish LQ for 0x7cb03eaa0a019e9d = 10	
2021-12-16 16:31:03.327 - debug: zigbee.0 (26219) Publish available for 0x00158d0002b805e3 = true	
2021-12-16 16:31:03.328 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002b805e3 = 10	
2021-12-16 16:31:03.329 - debug: zigbee.0 (26219) Publish available for 0x00158d0002b7d87c = true	
2021-12-16 16:31:03.331 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002b7d87c = 10	
2021-12-16 16:31:03.333 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa0a025809/3 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:03.333 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa0a025809:18602/3 (0,0,4)	
2021-12-16 16:31:03.334 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":18602,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":5,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,6,0,0,0]}}	
2021-12-16 16:31:03.334 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,170,72,3,1,6,0,5,0,30,5,16,6,0,0,0,196]	
2021-12-16 16:31:03.346 - debug: zigbee.0 (26219) Publish available for 0x00158d0002b7d6a9 = true	
2021-12-16 16:31:03.348 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002b7d6a9 = 10	
2021-12-16 16:31:03.350 - debug: zigbee.0 (26219) Publish available for 0x000b57fffe4436b0 = true	
2021-12-16 16:31:03.352 - debug: zigbee.0 (26219) Publish LQ for 0x000b57fffe4436b0 = 10	
2021-12-16 16:31:03.354 - debug: zigbee.0 (26219) Publish available for 0x90fd9ffffe02c40f = true	
2021-12-16 16:31:03.356 - debug: zigbee.0 (26219) Publish LQ for 0x90fd9ffffe02c40f = 10	
2021-12-16 16:31:03.358 - debug: zigbee.0 (26219) Publish available for 0x90fd9ffffe7fe8c9 = true	
2021-12-16 16:31:03.359 - debug: zigbee.0 (26219) Publish LQ for 0x90fd9ffffe7fe8c9 = 10	
2021-12-16 16:31:03.361 - debug: zigbee.0 (26219) Publish available for 0x90fd9ffffe88755e = true	
2021-12-16 16:31:03.363 - debug: zigbee.0 (26219) Publish LQ for 0x90fd9ffffe88755e = 10	
2021-12-16 16:31:03.366 - debug: zigbee.0 (26219) Publish available for 0x00158d000274f4d3 = true	
2021-12-16 16:31:03.368 - debug: zigbee.0 (26219) Publish LQ for 0x00158d000274f4d3 = 10	
2021-12-16 16:31:03.370 - debug: zigbee.0 (26219) Publish available for 0x00158d0002722af7 = true	
2021-12-16 16:31:03.371 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002722af7 = 10	
2021-12-16 16:31:03.376 - debug: zigbee.0 (26219) Publish available for 0x847127fffed62092 = true	
2021-12-16 16:31:03.377 - debug: zigbee.0 (26219) Publish LQ for 0x847127fffed62092 = 10	
2021-12-16 16:31:03.378 - debug: zigbee.0 (26219) Publish available for 0x847127fffed0a598 = true	
2021-12-16 16:31:03.380 - debug: zigbee.0 (26219) Publish LQ for 0x847127fffed0a598 = 10	
2021-12-16 16:31:03.381 - debug: zigbee.0 (26219) Publish available for 0x847127fffecfc657 = true	
2021-12-16 16:31:03.382 - debug: zigbee.0 (26219) Publish LQ for 0x847127fffecfc657 = 10	
2021-12-16 16:31:03.384 - debug: zigbee.0 (26219) Publish available for 0xa4c138934ce2822b = true	
2021-12-16 16:31:03.385 - debug: zigbee.0 (26219) Publish LQ for 0xa4c138934ce2822b = 10	
2021-12-16 16:31:03.387 - debug: zigbee.0 (26219) Publish available for 0xa4c138ec0e4ef1cf = true	
2021-12-16 16:31:03.388 - debug: zigbee.0 (26219) Publish LQ for 0xa4c138ec0e4ef1cf = 10	
2021-12-16 16:31:03.389 - debug: zigbee.0 (26219) Publish available for 0x000d6ffffe2cd4b8 = true	
2021-12-16 16:31:03.391 - debug: zigbee.0 (26219) Publish LQ for 0x000d6ffffe2cd4b8 = 10	
2021-12-16 16:31:03.406 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100,254,3,68,128,225,1,5,34]	
2021-12-16 16:31:03.407 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100,254,3,68,128,225,1,5,34]	
2021-12-16 16:31:03.407 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:03.408 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:03.408 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,5,34]	
2021-12-16 16:31:03.409 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,5] - 34	
2021-12-16 16:31:03.409 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":5}	
2021-12-16 16:31:03.410 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:03.410 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa0a025809:18602,225,0)	
2021-12-16 16:31:03.487 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,3,8]	
2021-12-16 16:31:03.488 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,3,8]	
2021-12-16 16:31:03.488 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,3] - 8	
2021-12-16 16:31:03.488 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":3}	
2021-12-16 16:31:03.489 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:03.489 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002c65ed8:41267,205,0)	
2021-12-16 16:31:03.490 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Wait 2000ms	
2021-12-16 16:31:03.536 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa00a36bed/3 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:03.537 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00a36bed:65448/3 (0,0,5)	
2021-12-16 16:31:03.538 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":65448,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":6,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,7,0,0,0]}}	
2021-12-16 16:31:03.540 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,168,255,3,1,6,0,6,0,30,5,16,7,0,0,0,115]	
2021-12-16 16:31:03.572 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:03.573 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:03.574 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:03.575 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:03.577 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:03.736 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa0a019e9d/3 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:03.736 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa0a019e9d:32268/3 (0,0,6)	
2021-12-16 16:31:03.737 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":32268,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":7,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,8,0,0,0]}}	
2021-12-16 16:31:03.737 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,12,126,3,1,6,0,7,0,30,5,16,8,0,0,0,88]	
2021-12-16 16:31:03.745 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:03.745 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:03.746 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:03.746 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:03.746 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:03.783 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,7,32]	
2021-12-16 16:31:03.783 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,7,32]	
2021-12-16 16:31:03.784 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,7] - 32	
2021-12-16 16:31:03.784 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":7}	
2021-12-16 16:31:03.784 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:03.785 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa0a019e9d:32268,225,0)	
2021-12-16 16:31:03.936 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x00158d0002b805e3/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:03.937 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002b805e3:39725/1 (0,0,7)	
2021-12-16 16:31:03.938 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":39725,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":8,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,9,0,0,0]}}	
2021-12-16 16:31:03.938 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,45,155,1,1,6,0,8,0,30,5,16,9,0,0,0,144]	
2021-12-16 16:31:03.946 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:03.947 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:03.947 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:03.947 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:03.947 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:04.007 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,6,13]	
2021-12-16 16:31:04.007 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,6,13]	
2021-12-16 16:31:04.007 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,6] - 13	
2021-12-16 16:31:04.008 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":6}	
2021-12-16 16:31:04.008 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:04.008 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00a36bed:65448,205,0)	
2021-12-16 16:31:04.008 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Wait 2000ms	
2021-12-16 16:31:04.137 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x00158d0002b7d87c/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:04.138 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002b7d87c:35436/1 (0,0,8)	
2021-12-16 16:31:04.138 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":35436,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":9,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,10,0,0,0]}}	
2021-12-16 16:31:04.139 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,108,138,1,1,6,0,9,0,30,5,16,10,0,0,0,194]	
2021-12-16 16:31:04.147 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:04.147 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:04.147 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:04.148 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:04.148 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:04.338 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x00158d0002b7d6a9/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:04.339 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002b7d6a9:19263/1 (0,0,9)	
2021-12-16 16:31:04.341 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":19263,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":10,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,11,0,0,0]}}	
2021-12-16 16:31:04.342 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,63,75,1,1,6,0,10,0,30,5,16,11,0,0,0,82]	
2021-12-16 16:31:04.351 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:04.352 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:04.353 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:04.355 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:04.356 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:04.415 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,8,3]	
2021-12-16 16:31:04.416 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,8,3]	
2021-12-16 16:31:04.416 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,8] - 3	
2021-12-16 16:31:04.417 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":8}	
2021-12-16 16:31:04.419 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:04.420 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002b805e3:39725,205,0)	
2021-12-16 16:31:04.420 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Wait 2000ms	
2021-12-16 16:31:04.537 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x000b57fffe4436b0/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:04.538 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x000b57fffe4436b0:57723/1 (0,0,10)	
2021-12-16 16:31:04.540 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":57723,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":11,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,12,0,0,0]}}	
2021-12-16 16:31:04.540 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,123,225,1,1,6,0,11,0,30,5,16,12,0,0,0,186]	
2021-12-16 16:31:04.549 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:04.550 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:04.551 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:04.551 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:04.552 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:04.596 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00acb990:47504/3 (0,1,10)	
2021-12-16 16:31:04.596 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":47504,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":12,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,2,0,0,0]}}	
2021-12-16 16:31:04.597 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,144,185,3,1,6,0,12,0,30,5,16,2,0,0,0,2]	
2021-12-16 16:31:04.607 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:04.608 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:04.608 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:04.609 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:04.609 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:04.651 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,12,43]	
2021-12-16 16:31:04.652 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,12,43]	
2021-12-16 16:31:04.652 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,12] - 43	
2021-12-16 16:31:04.652 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":12}	
2021-12-16 16:31:04.653 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:04.653 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00acb990:47504,225,1)	
2021-12-16 16:31:04.738 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x90fd9ffffe02c40f/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:04.739 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x90fd9ffffe02c40f:56799/1 (0,0,11)	
2021-12-16 16:31:04.739 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":56799,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":13,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,13,0,0,0]}}	
2021-12-16 16:31:04.740 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,223,221,1,1,6,0,13,0,30,5,16,13,0,0,0,37]	
2021-12-16 16:31:04.746 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:04.746 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:04.747 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:04.747 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:04.748 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:04.763 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,10,1]	
2021-12-16 16:31:04.764 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,10,1]	
2021-12-16 16:31:04.765 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,10] - 1	
2021-12-16 16:31:04.765 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":10}	
2021-12-16 16:31:04.766 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:04.766 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002b7d6a9:19263,205,0)	
2021-12-16 16:31:04.766 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Wait 2000ms	
2021-12-16 16:31:04.787 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,9,2]	
2021-12-16 16:31:04.788 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,9,2]	
2021-12-16 16:31:04.788 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,9] - 2	
2021-12-16 16:31:04.789 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":9}	
2021-12-16 16:31:04.789 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:04.790 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002b7d87c:35436,205,0)	
2021-12-16 16:31:04.790 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Wait 2000ms	
2021-12-16 16:31:04.937 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x90fd9ffffe7fe8c9/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:04.939 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x90fd9ffffe7fe8c9:65244/1 (0,0,12)	
2021-12-16 16:31:04.939 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":65244,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":14,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,14,0,0,0]}}	
2021-12-16 16:31:04.940 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,220,254,1,1,6,0,14,0,30,5,16,14,0,0,0,5]	
2021-12-16 16:31:04.947 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:04.948 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:04.948 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:04.949 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:04.950 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:04.952 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,14,5]	
2021-12-16 16:31:04.953 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,14,5]	
2021-12-16 16:31:04.954 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,14] - 5	
2021-12-16 16:31:04.955 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":14}	
2021-12-16 16:31:04.956 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:04.956 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x90fd9ffffe7fe8c9:65244,205,0)	
2021-12-16 16:31:04.957 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Wait 2000ms	
2021-12-16 16:31:05.138 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x90fd9ffffe88755e/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:05.139 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x90fd9ffffe88755e:2953/1 (0,0,13)	
2021-12-16 16:31:05.140 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":2953,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":15,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,15,0,0,0]}}	
2021-12-16 16:31:05.141 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,137,11,1,1,6,0,15,0,30,5,16,15,0,0,0,165]	
2021-12-16 16:31:05.147 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:05.148 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:05.149 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:05.150 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:05.150 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:05.153 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,15,4]	
2021-12-16 16:31:05.154 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,15,4]	
2021-12-16 16:31:05.155 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,15] - 4	
2021-12-16 16:31:05.156 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":15}	
2021-12-16 16:31:05.157 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:05.158 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x90fd9ffffe88755e:2953,205,0)	
2021-12-16 16:31:05.159 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Wait 2000ms	
2021-12-16 16:31:05.170 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa0a00dfcb:34528/3 (0,1,13)	
2021-12-16 16:31:05.171 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":34528,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":16,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,3,0,0,0]}}	
2021-12-16 16:31:05.172 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,224,134,3,1,6,0,16,0,30,5,16,3,0,0,0,80]	
2021-12-16 16:31:05.179 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:05.180 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:05.180 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:05.181 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:05.184 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:05.193 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,11,0]	
2021-12-16 16:31:05.195 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,11,0]	
2021-12-16 16:31:05.195 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,11] - 0	
2021-12-16 16:31:05.196 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":11}	
2021-12-16 16:31:05.197 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:05.197 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x000b57fffe4436b0:57723,205,0)	
2021-12-16 16:31:05.197 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Wait 2000ms	
2021-12-16 16:31:05.338 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0xa4c138934ce2822b/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:05.339 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0xa4c138934ce2822b:25440/1 (0,0,14)	
2021-12-16 16:31:05.341 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":25440,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":17,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,16,0,0,0]}}	
2021-12-16 16:31:05.342 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,96,99,1,1,6,0,17,0,30,5,16,16,0,0,0,37]	
2021-12-16 16:31:05.352 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:05.354 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:05.355 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:05.356 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:05.357 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:05.365 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,0,1,17,215]	
2021-12-16 16:31:05.366 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,0,1,17,215]	
2021-12-16 16:31:05.367 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [0,1,17] - 215	
2021-12-16 16:31:05.368 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":0,"endpoint":1,"transid":17}	
2021-12-16 16:31:05.369 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:05.395 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,69,196,96,99,0,129]	
2021-12-16 16:31:05.397 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,69,196,96,99,0,129]	
2021-12-16 16:31:05.398 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 5 - 196 - [96,99,0] - 129	
2021-12-16 16:31:05.399 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - srcRtgInd - {"dstaddr":25440,"relaycount":0,"relaylist":[]}	
2021-12-16 16:31:05.400 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:05.403 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,28,68,129,0,0,6,0,96,99,1,1,0,63,0,53,51,68,0,0,8,24,16,1,0,0,0,16,0,96,99,29,174]	
2021-12-16 16:31:05.404 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,28,68,129,0,0,6,0,96,99,1,1,0,63,0,53,51,68,0,0,8,24,16,1,0,0,0,16,0,96,99,29,174]	
2021-12-16 16:31:05.404 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 28 - 2 - 4 - 129 - [0,0,6,0,96,99,1,1,0,63,0,53,51,68,0,0,8,24,16,1,0,0,0,16,0,96,99,29] - 174	
2021-12-16 16:31:05.405 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - incomingMsg - {"groupid":0,"clusterid":6,"srcaddr":25440,"srcendpoint":1,"dstendpoint":1,"wasbroadcast":0,"linkquality":63,"securityuse":0,"timestamp":4469557,"transseqnumber":0,"len":8,"data":{"type":"Buffer","data":[24,16,1,0,0,0,16,0]}}	
2021-12-16 16:31:05.407 - debug: zigbee.0 (26219) zigbee-herdsman:controller:log Received 'zcl' data '{"frame":{"Header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":16,"manufacturerCode":null,"commandIdentifier":1},"Payload":[{"attrId":0,"status":0,"dataType":16,"attrData":0}],"Command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}},"address":25440,"endpoint":1,"linkquality":63,"groupID":0,"wasBroadcast":false,"destinationEndpoint":1}'	
2021-12-16 16:31:05.408 - debug: zigbee.0 (26219) handleMessage. {"type":"readResponse","device":{"ID":42,"_type":"Router","_ieeeAddr":"0xa4c138934ce2822b","_networkAddress":25440,"_manufacturerID":4417,"_endpoints":[{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":25440,"deviceIeeeAddress":"0xa4c138934ce2822b","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":0,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}},"manuSpecificTuya_3":{"attributes":{"switchType":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":97,"inputClusters":[],"outputClusters":[33],"deviceNetworkAddress":25440,"deviceIeeeAddress":"0xa4c138934ce2822b","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZ3000_npzfdcof","_powerSource":"Mains (single phase)","_modelID":"TS0001","_applicationVersion":67,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668665408,"_linkquality":63},"endpoint":"[Circular]","data":{"onOff":0},"linkquality":63,"groupID":0,"cluster":"genOnOff","meta":{"zclTransactionSequenceNumber":16,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:31:05.409 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:05.410 - debug: zigbee.0 (26219) Received Zigbee message from '0xa4c138934ce2822b', type 'readResponse', cluster 'genOnOff', data '{"onOff":0}' from endpoint 1 with groupID 0	
2021-12-16 16:31:05.410 - debug: zigbee.0 (26219) Type readResponse device {"type":"device","device":{"ID":42,"_type":"Router","_ieeeAddr":"0xa4c138934ce2822b","_networkAddress":25440,"_manufacturerID":4417,"_endpoints":[{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":25440,"deviceIeeeAddress":"0xa4c138934ce2822b","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":0,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}},"manuSpecificTuya_3":{"attributes":{"switchType":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":97,"inputClusters":[],"outputClusters":[33],"deviceNetworkAddress":25440,"deviceIeeeAddress":"0xa4c138934ce2822b","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZ3000_npzfdcof","_powerSource":"Mains (single phase)","_modelID":"TS0001","_applicationVersion":67,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668665408,"_linkquality":63},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["TS0001"],"model":"TS0001","vendor":"TuYa","description":"1 gang switch","whiteLabel":[{"vendor":"CR Smart Home","model":"TS0001","description":"Valve control"},{"vendor":"Lonsonho","model":"X701"},{"vendor":"Bandi","model":"BDS03G1"}],"options":[]},"name":"0xa4c138934ce2822b"} incoming event: {"type":"readResponse","device":{"ID":42,"_type":"Router","_ieeeAddr":"0xa4c138934ce2822b","_networkAddress":25440,"_manufacturerID":4417,"_endpoints":[{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":25440,"deviceIeeeAddress":"0xa4c138934ce2822b","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":0,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}},"manuSpecificTuya_3":{"attributes":{"switchType":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":97,"inputClusters":[],"outputClusters":[33],"deviceNetworkAddress":25440,"deviceIeeeAddress":"0xa4c138934ce2822b","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZ3000_npzfdcof","_powerSource":"Mains (single phase)","_modelID":"TS0001","_applicationVersion":67,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668665408,"_linkquality":63},"endpoint":"[Circular]","data":{"onOff":0},"linkquality":63,"groupID":0,"cluster":"genOnOff","meta":{"zclTransactionSequenceNumber":16,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:31:05.411 - debug: zigbee.0 (26219) Successful read state 'state' of '0xa4c138934ce2822b' in stead of pinging	
2021-12-16 16:31:05.413 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa0a025809:18602/3 (0,1,13)	
2021-12-16 16:31:05.414 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":18602,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":18,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,6,0,0,0]}}	
2021-12-16 16:31:05.415 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,170,72,3,1,6,0,18,0,30,5,16,6,0,0,0,211]	
2021-12-16 16:31:05.423 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:05.423 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:05.424 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:05.424 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:05.424 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:05.426 - debug: zigbee.0 (26219) Publish {"state":"OFF"} to "a4c138934ce2822b"	
2021-12-16 16:31:05.429 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,13,6]	
2021-12-16 16:31:05.430 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,13,6]	
2021-12-16 16:31:05.430 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,13] - 6	
2021-12-16 16:31:05.431 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":13}	
2021-12-16 16:31:05.431 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:05.431 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x90fd9ffffe02c40f:56799,205,0)	
2021-12-16 16:31:05.431 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Wait 2000ms	
2021-12-16 16:31:05.453 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,18,53]	
2021-12-16 16:31:05.453 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,18,53]	
2021-12-16 16:31:05.453 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,18] - 53	
2021-12-16 16:31:05.454 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":18}	
2021-12-16 16:31:05.454 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:05.454 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa0a025809:18602,225,1)	
2021-12-16 16:31:05.490 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002c65ed8:41267/1 (0,1,13)	
2021-12-16 16:31:05.491 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":41267,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":19,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,4,0,0,0]}}	
2021-12-16 16:31:05.491 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,51,161,1,1,6,0,19,0,30,5,16,4,0,0,0,162]	
2021-12-16 16:31:05.496 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:05.496 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:05.496 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:05.497 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:05.497 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:05.537 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0xa4c138ec0e4ef1cf/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:05.538 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0xa4c138ec0e4ef1cf:60149/1 (0,0,14)	
2021-12-16 16:31:05.538 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":60149,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":20,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,17,0,0,0]}}	
2021-12-16 16:31:05.538 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,245,234,1,1,6,0,20,0,30,5,16,17,0,0,0,61]	
2021-12-16 16:31:05.546 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:05.547 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:05.547 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:05.547 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:05.548 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:05.582 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,20,51]	
2021-12-16 16:31:05.584 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,20,51]	
2021-12-16 16:31:05.585 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,20] - 51	
2021-12-16 16:31:05.585 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":20}	
2021-12-16 16:31:05.586 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:05.586 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0xa4c138ec0e4ef1cf:60149,225,0)	
2021-12-16 16:31:05.785 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa0a019e9d:32268/3 (0,1,14)	
2021-12-16 16:31:05.785 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":32268,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":21,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,8,0,0,0]}}	
2021-12-16 16:31:05.786 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,12,126,3,1,6,0,21,0,30,5,16,8,0,0,0,74]	
2021-12-16 16:31:05.793 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:05.794 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:05.794 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:05.794 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:05.794 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:05.836 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,21,50]	
2021-12-16 16:31:05.836 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,21,50]	
2021-12-16 16:31:05.836 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,21] - 50	
2021-12-16 16:31:05.837 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":21}	
2021-12-16 16:31:05.837 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:05.837 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa0a019e9d:32268,225,1)	
2021-12-16 16:31:05.854 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,16,27]	
2021-12-16 16:31:05.854 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,16,27]	
2021-12-16 16:31:05.854 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,16] - 27	
2021-12-16 16:31:05.855 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":16}	
2021-12-16 16:31:05.855 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:05.855 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa0a00dfcb:34528,205,1)	
2021-12-16 16:31:05.856 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Discovering route to 34528	
2021-12-16 16:31:05.856 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - extRouteDisc - {"dstAddr":34528,"options":0,"radius":30}	
2021-12-16 16:31:05.856 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,4,37,69,224,134,0,30,28]	
2021-12-16 16:31:05.859 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,69,0,33]	
2021-12-16 16:31:05.860 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,69,0,33]	
2021-12-16 16:31:05.861 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 69 - [0] - 33	
2021-12-16 16:31:05.861 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - extRouteDisc - {"status":0}	
2021-12-16 16:31:05.862 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:06.009 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00a36bed:65448/3 (0,1,14)	
2021-12-16 16:31:06.009 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":65448,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":22,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,7,0,0,0]}}	
2021-12-16 16:31:06.010 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,168,255,3,1,6,0,22,0,30,5,16,7,0,0,0,99]	
2021-12-16 16:31:06.015 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:06.016 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:06.017 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:06.017 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:06.018 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:06.042 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,19,24]	
2021-12-16 16:31:06.042 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,19,24]	
2021-12-16 16:31:06.042 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,19] - 24	
2021-12-16 16:31:06.043 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":19}	
2021-12-16 16:31:06.043 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:06.044 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002c65ed8:41267,205,1)	
2021-12-16 16:31:06.044 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Discovering route to 41267	
2021-12-16 16:31:06.045 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - extRouteDisc - {"dstAddr":41267,"options":0,"radius":30}	
2021-12-16 16:31:06.045 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,4,37,69,51,161,0,30,232]	
2021-12-16 16:31:06.048 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,69,0,33]	
2021-12-16 16:31:06.049 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,69,0,33]	
2021-12-16 16:31:06.049 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 69 - [0] - 33	
2021-12-16 16:31:06.050 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - extRouteDisc - {"status":0}	
2021-12-16 16:31:06.050 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:06.421 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002b805e3:39725/1 (0,1,14)	
2021-12-16 16:31:06.422 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":39725,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":23,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,9,0,0,0]}}	
2021-12-16 16:31:06.422 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,45,155,1,1,6,0,23,0,30,5,16,9,0,0,0,143]	
2021-12-16 16:31:06.427 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:06.428 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:06.428 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:06.428 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:06.428 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:06.518 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,22,29]	
2021-12-16 16:31:06.518 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,22,29]	
2021-12-16 16:31:06.518 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,22] - 29	
2021-12-16 16:31:06.518 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":22}	
2021-12-16 16:31:06.519 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:06.519 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00a36bed:65448,205,1)	
2021-12-16 16:31:06.519 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Discovering route to 65448	
2021-12-16 16:31:06.520 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - extRouteDisc - {"dstAddr":65448,"options":0,"radius":30}	
2021-12-16 16:31:06.520 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,4,37,69,168,255,0,30,45]	
2021-12-16 16:31:06.524 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,69,0,33]	
2021-12-16 16:31:06.525 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,69,0,33]	
2021-12-16 16:31:06.526 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 69 - [0] - 33	
2021-12-16 16:31:06.526 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - extRouteDisc - {"status":0}	
2021-12-16 16:31:06.526 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:06.653 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00acb990:47504/3 (0,2,14)	
2021-12-16 16:31:06.654 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":47504,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":24,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,2,0,0,0]}}	
2021-12-16 16:31:06.655 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,144,185,3,1,6,0,24,0,30,5,16,2,0,0,0,22]	
2021-12-16 16:31:06.663 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:06.664 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:06.664 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:06.665 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:06.665 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:06.729 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,24,63]	
2021-12-16 16:31:06.729 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,24,63]	
2021-12-16 16:31:06.729 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,24] - 63	
2021-12-16 16:31:06.730 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":24}	
2021-12-16 16:31:06.730 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:06.730 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00acb990:47504,225,2)	
2021-12-16 16:31:06.767 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002b7d6a9:19263/1 (0,1,14)	
2021-12-16 16:31:06.768 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":19263,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":25,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,11,0,0,0]}}	
2021-12-16 16:31:06.768 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,63,75,1,1,6,0,25,0,30,5,16,11,0,0,0,65]	
2021-12-16 16:31:06.773 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:06.773 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:06.773 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:06.774 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:06.774 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:06.790 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002b7d87c:35436/1 (0,1,14)	
2021-12-16 16:31:06.791 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":35436,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":26,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,10,0,0,0]}}	
2021-12-16 16:31:06.791 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,108,138,1,1,6,0,26,0,30,5,16,10,0,0,0,209]	
2021-12-16 16:31:06.796 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:06.796 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:06.796 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:06.797 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:06.797 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:06.958 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x90fd9ffffe7fe8c9:65244/1 (0,1,14)	
2021-12-16 16:31:06.959 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":65244,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":27,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,14,0,0,0]}}	
2021-12-16 16:31:06.960 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,220,254,1,1,6,0,27,0,30,5,16,14,0,0,0,16]	
2021-12-16 16:31:06.968 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:06.968 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:06.971 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:06.971 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:06.972 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:06.977 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,23,28]	
2021-12-16 16:31:06.977 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,23,28]	
2021-12-16 16:31:06.978 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,23] - 28	
2021-12-16 16:31:06.979 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":23}	
2021-12-16 16:31:06.980 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:06.980 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002b805e3:39725,205,1)	
2021-12-16 16:31:06.981 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Discovering route to 39725	
2021-12-16 16:31:06.981 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - extRouteDisc - {"dstAddr":39725,"options":0,"radius":30}	
2021-12-16 16:31:06.982 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,4,37,69,45,155,0,30,204]	
2021-12-16 16:31:06.987 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,69,0,33]	
2021-12-16 16:31:06.988 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,69,0,33]	
2021-12-16 16:31:06.988 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 69 - [0] - 33	
2021-12-16 16:31:06.989 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - extRouteDisc - {"status":0}	
2021-12-16 16:31:06.990 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:07.160 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x90fd9ffffe88755e:2953/1 (0,1,14)	
2021-12-16 16:31:07.161 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":2953,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":28,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,15,0,0,0]}}	
2021-12-16 16:31:07.162 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,137,11,1,1,6,0,28,0,30,5,16,15,0,0,0,182]	
2021-12-16 16:31:07.169 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:07.170 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:07.171 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:07.172 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:07.173 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:07.198 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x000b57fffe4436b0:57723/1 (0,1,14)	
2021-12-16 16:31:07.199 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":57723,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":29,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,12,0,0,0]}}	
2021-12-16 16:31:07.200 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,123,225,1,1,6,0,29,0,30,5,16,12,0,0,0,172]	
2021-12-16 16:31:07.206 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:07.207 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:07.208 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:07.218 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:07.218 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:07.262 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,25,18]	
2021-12-16 16:31:07.263 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,25,18]	
2021-12-16 16:31:07.263 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,25] - 18	
2021-12-16 16:31:07.264 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":25}	
2021-12-16 16:31:07.264 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:07.265 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002b7d6a9:19263,205,1)	
2021-12-16 16:31:07.265 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Discovering route to 19263	
2021-12-16 16:31:07.266 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - extRouteDisc - {"dstAddr":19263,"options":0,"radius":30}	
2021-12-16 16:31:07.266 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,4,37,69,63,75,0,30,14]	
2021-12-16 16:31:07.270 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,69,0,33]	
2021-12-16 16:31:07.270 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,69,0,33]	
2021-12-16 16:31:07.271 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 69 - [0] - 33	
2021-12-16 16:31:07.272 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - extRouteDisc - {"status":0}	
2021-12-16 16:31:07.272 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:07.432 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x90fd9ffffe02c40f:56799/1 (0,1,14)	
2021-12-16 16:31:07.433 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":56799,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":30,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,13,0,0,0]}}	
2021-12-16 16:31:07.434 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,223,221,1,1,6,0,30,0,30,5,16,13,0,0,0,54]	
2021-12-16 16:31:07.440 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:07.441 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:07.442 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:07.442 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:07.443 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:07.455 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa0a025809:18602/3 (0,2,14)	
2021-12-16 16:31:07.456 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":18602,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":31,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,6,0,0,0]}}	
2021-12-16 16:31:07.457 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,170,72,3,1,6,0,31,0,30,5,16,6,0,0,0,222]	
2021-12-16 16:31:07.465 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:07.466 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:07.467 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:07.467 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:07.468 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:07.489 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,27,16]	
2021-12-16 16:31:07.490 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,27,16]	
2021-12-16 16:31:07.491 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,27] - 16	
2021-12-16 16:31:07.491 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":27}	
2021-12-16 16:31:07.492 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:07.493 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x90fd9ffffe7fe8c9:65244,205,1)	
2021-12-16 16:31:07.493 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Discovering route to 65244	
2021-12-16 16:31:07.494 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - extRouteDisc - {"dstAddr":65244,"options":0,"radius":30}	
2021-12-16 16:31:07.495 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,4,37,69,220,254,0,30,88]	
2021-12-16 16:31:07.500 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,69,0,33]	
2021-12-16 16:31:07.502 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,69,0,33]	
2021-12-16 16:31:07.502 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 69 - [0] - 33	
2021-12-16 16:31:07.503 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - extRouteDisc - {"status":0}	
2021-12-16 16:31:07.505 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:07.511 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,31,56]	
2021-12-16 16:31:07.512 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,31,56]	
2021-12-16 16:31:07.513 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,31] - 56	
2021-12-16 16:31:07.514 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":31}	
2021-12-16 16:31:07.514 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:07.516 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa0a025809:18602,225,2)	
2021-12-16 16:31:07.534 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,26,17]	
2021-12-16 16:31:07.534 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,26,17]	
2021-12-16 16:31:07.535 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,26] - 17	
2021-12-16 16:31:07.535 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":26}	
2021-12-16 16:31:07.535 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:07.535 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002b7d87c:35436,205,1)	
2021-12-16 16:31:07.536 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Discovering route to 35436	
2021-12-16 16:31:07.536 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - extRouteDisc - {"dstAddr":35436,"options":0,"radius":30}	
2021-12-16 16:31:07.536 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,4,37,69,108,138,0,30,156]	
2021-12-16 16:31:07.540 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,69,0,33]	
2021-12-16 16:31:07.540 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,69,0,33]	
2021-12-16 16:31:07.541 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 69 - [0] - 33	
2021-12-16 16:31:07.541 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - extRouteDisc - {"status":0}	
2021-12-16 16:31:07.542 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:07.587 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0xa4c138ec0e4ef1cf:60149/1 (0,1,14)	
2021-12-16 16:31:07.588 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":60149,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":32,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,17,0,0,0]}}	
2021-12-16 16:31:07.588 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,245,234,1,1,6,0,32,0,30,5,16,17,0,0,0,9]	
2021-12-16 16:31:07.596 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:07.596 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:07.597 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:07.597 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:07.597 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:07.648 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,32,7]	
2021-12-16 16:31:07.648 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,32,7]	
2021-12-16 16:31:07.648 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,32] - 7	
2021-12-16 16:31:07.649 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":32}	
2021-12-16 16:31:07.649 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:07.649 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0xa4c138ec0e4ef1cf:60149,225,1)	
2021-12-16 16:31:07.819 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,28,68,129,0,0,6,0]	
2021-12-16 16:31:07.820 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,28,68,129,0,0,6,0]	
2021-12-16 16:31:07.821 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [96,99,1,1,0,60,0,208]	
2021-12-16 16:31:07.821 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,28,68,129,0,0,6,0,96,99,1,1,0,60,0,208]	
2021-12-16 16:31:07.823 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [132,70,0,0,8,24,16,1,0,0,0,16,0,96,99,29,253]	
2021-12-16 16:31:07.823 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,28,68,129,0,0,6,0,96,99,1,1,0,60,0,208,132,70,0,0,8,24,16,1,0,0,0,16,0,96,99,29,253]	
2021-12-16 16:31:07.823 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 28 - 2 - 4 - 129 - [0,0,6,0,96,99,1,1,0,60,0,208,132,70,0,0,8,24,16,1,0,0,0,16,0,96,99,29] - 253	
2021-12-16 16:31:07.824 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - incomingMsg - {"groupid":0,"clusterid":6,"srcaddr":25440,"srcendpoint":1,"dstendpoint":1,"wasbroadcast":0,"linkquality":60,"securityuse":0,"timestamp":4621520,"transseqnumber":0,"len":8,"data":{"type":"Buffer","data":[24,16,1,0,0,0,16,0]}}	
2021-12-16 16:31:07.825 - debug: zigbee.0 (26219) zigbee-herdsman:controller:log Received 'zcl' data '{"frame":{"Header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":16,"manufacturerCode":null,"commandIdentifier":1},"Payload":[{"attrId":0,"status":0,"dataType":16,"attrData":0}],"Command":{"ID":1,"name":"readRsp","parameters":[{"name":"attrId","type":33},{"name":"status","type":32},{"name":"dataType","type":32,"conditions":[{"type":"statusEquals","value":0}]},{"name":"attrData","type":1000,"conditions":[{"type":"statusEquals","value":0}]}]}},"address":25440,"endpoint":1,"linkquality":60,"groupID":0,"wasBroadcast":false,"destinationEndpoint":1}'	
2021-12-16 16:31:07.826 - debug: zigbee.0 (26219) handleMessage. {"type":"readResponse","device":{"ID":42,"_type":"Router","_ieeeAddr":"0xa4c138934ce2822b","_networkAddress":25440,"_manufacturerID":4417,"_endpoints":[{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":25440,"deviceIeeeAddress":"0xa4c138934ce2822b","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":0,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}},"manuSpecificTuya_3":{"attributes":{"switchType":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":97,"inputClusters":[],"outputClusters":[33],"deviceNetworkAddress":25440,"deviceIeeeAddress":"0xa4c138934ce2822b","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZ3000_npzfdcof","_powerSource":"Mains (single phase)","_modelID":"TS0001","_applicationVersion":67,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668667825,"_linkquality":60},"endpoint":"[Circular]","data":{"onOff":0},"linkquality":60,"groupID":0,"cluster":"genOnOff","meta":{"zclTransactionSequenceNumber":16,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:31:07.826 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:07.826 - debug: zigbee.0 (26219) Received Zigbee message from '0xa4c138934ce2822b', type 'readResponse', cluster 'genOnOff', data '{"onOff":0}' from endpoint 1 with groupID 0	
2021-12-16 16:31:07.827 - debug: zigbee.0 (26219) Type readResponse device {"type":"device","device":{"ID":42,"_type":"Router","_ieeeAddr":"0xa4c138934ce2822b","_networkAddress":25440,"_manufacturerID":4417,"_endpoints":[{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":25440,"deviceIeeeAddress":"0xa4c138934ce2822b","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":0,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}},"manuSpecificTuya_3":{"attributes":{"switchType":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":97,"inputClusters":[],"outputClusters":[33],"deviceNetworkAddress":25440,"deviceIeeeAddress":"0xa4c138934ce2822b","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZ3000_npzfdcof","_powerSource":"Mains (single phase)","_modelID":"TS0001","_applicationVersion":67,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668667825,"_linkquality":60},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["TS0001"],"model":"TS0001","vendor":"TuYa","description":"1 gang switch","whiteLabel":[{"vendor":"CR Smart Home","model":"TS0001","description":"Valve control"},{"vendor":"Lonsonho","model":"X701"},{"vendor":"Bandi","model":"BDS03G1"}],"options":[]},"name":"0xa4c138934ce2822b"} incoming event: {"type":"readResponse","device":{"ID":42,"_type":"Router","_ieeeAddr":"0xa4c138934ce2822b","_networkAddress":25440,"_manufacturerID":4417,"_endpoints":[{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":25440,"deviceIeeeAddress":"0xa4c138934ce2822b","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":0,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}},"manuSpecificTuya_3":{"attributes":{"switchType":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":97,"inputClusters":[],"outputClusters":[33],"deviceNetworkAddress":25440,"deviceIeeeAddress":"0xa4c138934ce2822b","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZ3000_npzfdcof","_powerSource":"Mains (single phase)","_modelID":"TS0001","_applicationVersion":67,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668667825,"_linkquality":60},"endpoint":"[Circular]","data":{"onOff":0},"linkquality":60,"groupID":0,"cluster":"genOnOff","meta":{"zclTransactionSequenceNumber":16,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:31:07.837 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa0a019e9d:32268/3 (0,2,14)	
2021-12-16 16:31:07.838 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":32268,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":33,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,8,0,0,0]}}	
2021-12-16 16:31:07.838 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,12,126,3,1,6,0,33,0,30,5,16,8,0,0,0,126]	
2021-12-16 16:31:07.840 - debug: zigbee.0 (26219) Publish {"state":"OFF"} to "a4c138934ce2822b"	
2021-12-16 16:31:07.847 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:07.848 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:07.848 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:07.848 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:07.849 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:07.863 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,29,22]	
2021-12-16 16:31:07.863 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,29,22]	
2021-12-16 16:31:07.863 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,29] - 22	
2021-12-16 16:31:07.864 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":29}	
2021-12-16 16:31:07.864 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:07.864 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x000b57fffe4436b0:57723,205,1)	
2021-12-16 16:31:07.864 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Discovering route to 57723	
2021-12-16 16:31:07.865 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - extRouteDisc - {"dstAddr":57723,"options":0,"radius":30}	
2021-12-16 16:31:07.865 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,4,37,69,123,225,0,30,224]	
2021-12-16 16:31:07.868 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,69,0,33]	
2021-12-16 16:31:07.869 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,69,0,33]	
2021-12-16 16:31:07.869 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 69 - [0] - 33	
2021-12-16 16:31:07.870 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - extRouteDisc - {"status":0}	
2021-12-16 16:31:07.870 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:07.899 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,33,6]	
2021-12-16 16:31:07.899 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,33,6]	
2021-12-16 16:31:07.900 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,33] - 6	
2021-12-16 16:31:07.900 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":33}	
2021-12-16 16:31:07.900 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:07.901 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa0a019e9d:32268,225,2)	
2021-12-16 16:31:07.965 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,28,23]	
2021-12-16 16:31:07.967 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,28,23]	
2021-12-16 16:31:07.967 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,28] - 23	
2021-12-16 16:31:07.967 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":28}	
2021-12-16 16:31:07.968 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:07.968 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x90fd9ffffe88755e:2953,205,1)	
2021-12-16 16:31:07.968 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Discovering route to 2953	
2021-12-16 16:31:07.968 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - extRouteDisc - {"dstAddr":2953,"options":0,"radius":30}	
2021-12-16 16:31:07.969 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,4,37,69,137,11,0,30,248]	
2021-12-16 16:31:07.972 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,69,0,33]	
2021-12-16 16:31:07.973 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,69,0,33]	
2021-12-16 16:31:07.973 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 69 - [0] - 33	
2021-12-16 16:31:07.974 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - extRouteDisc - {"status":0}	
2021-12-16 16:31:07.974 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:08.036 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,30,21]	
2021-12-16 16:31:08.036 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,30,21]	
2021-12-16 16:31:08.036 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,30] - 21	
2021-12-16 16:31:08.037 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":30}	
2021-12-16 16:31:08.037 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:08.037 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x90fd9ffffe02c40f:56799,205,1)	
2021-12-16 16:31:08.037 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Discovering route to 56799	
2021-12-16 16:31:08.038 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - extRouteDisc - {"dstAddr":56799,"options":0,"radius":30}	
2021-12-16 16:31:08.038 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,4,37,69,223,221,0,30,120]	
2021-12-16 16:31:08.041 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,69,0,33]	
2021-12-16 16:31:08.042 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,69,0,33]	
2021-12-16 16:31:08.042 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 69 - [0] - 33	
2021-12-16 16:31:08.043 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - extRouteDisc - {"status":0}	
2021-12-16 16:31:08.043 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:08.731 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00acb990:47504/3 (0,3,14)	
2021-12-16 16:31:08.732 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":47504,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":34,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,2,0,0,0]}}	
2021-12-16 16:31:08.733 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,144,185,3,1,6,0,34,0,30,5,16,2,0,0,0,44]	
2021-12-16 16:31:08.744 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:08.745 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:08.746 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:08.746 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:08.747 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:08.788 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,34,5]	
2021-12-16 16:31:08.789 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,34,5]	
2021-12-16 16:31:08.789 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,34] - 5	
2021-12-16 16:31:08.790 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":34}	
2021-12-16 16:31:08.791 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:08.791 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00acb990:47504,225,3)	
2021-12-16 16:31:08.863 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa0a00dfcb:34528/3 (0,2,14)	
2021-12-16 16:31:08.867 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":34528,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":35,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,3,0,0,0]}}	
2021-12-16 16:31:08.868 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,224,134,3,1,6,0,35,0,30,5,16,3,0,0,0,99]	
2021-12-16 16:31:08.877 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:08.877 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:08.878 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:08.878 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:08.879 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:09.051 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002c65ed8:41267/1 (0,2,14)	
2021-12-16 16:31:09.053 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":41267,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":36,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,4,0,0,0]}}	
2021-12-16 16:31:09.054 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,51,161,1,1,6,0,36,0,30,5,16,4,0,0,0,149]	
2021-12-16 16:31:09.063 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:09.064 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:09.065 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:09.065 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:09.066 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:09.516 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa0a025809:18602/3 (0,3,14)	
2021-12-16 16:31:09.517 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":18602,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":37,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,6,0,0,0]}}	
2021-12-16 16:31:09.518 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,170,72,3,1,6,0,37,0,30,5,16,6,0,0,0,228]	
2021-12-16 16:31:09.526 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:09.526 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:09.527 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:09.527 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:09.528 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:09.529 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00a36bed:65448/3 (0,2,14)	
2021-12-16 16:31:09.530 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":65448,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":38,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,7,0,0,0]}}	
2021-12-16 16:31:09.531 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,168,255,3,1,6,0,38,0,30,5,16,7,0,0,0,83]	
2021-12-16 16:31:09.541 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100,254,3]	
2021-12-16 16:31:09.541 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100,254,3]	
2021-12-16 16:31:09.542 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:09.542 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:09.543 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3]	
2021-12-16 16:31:09.545 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [68,128,205,1,36,47]	
2021-12-16 16:31:09.546 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,36,47]	
2021-12-16 16:31:09.547 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,36] - 47	
2021-12-16 16:31:09.547 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":36}	
2021-12-16 16:31:09.548 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:09.549 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002c65ed8:41267,205,2)	
2021-12-16 16:31:09.550 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Request network address of '0x00158d0002c65ed8'	
2021-12-16 16:31:09.551 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - nwkAddrReq - {"ieeeaddr":"0x00158d0002c65ed8","reqtype":0,"startindex":0}	
2021-12-16 16:31:09.553 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,10,37,0,216,94,198,2,0,141,21,0,0,0,245]	
2021-12-16 16:31:09.561 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,0,0,100]	
2021-12-16 16:31:09.562 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,0,0,100]	
2021-12-16 16:31:09.562 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 0 - [0] - 100	
2021-12-16 16:31:09.563 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - nwkAddrReq - {"status":0}	
2021-12-16 16:31:09.564 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:09.576 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,37,2]	
2021-12-16 16:31:09.577 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,37,2]	
2021-12-16 16:31:09.577 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,37] - 2	
2021-12-16 16:31:09.578 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":37}	
2021-12-16 16:31:09.579 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:09.579 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa0a025809:18602,225,3)	
2021-12-16 16:31:09.650 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0xa4c138ec0e4ef1cf:60149/1 (0,2,14)	
2021-12-16 16:31:09.651 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":60149,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":39,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,17,0,0,0]}}	
2021-12-16 16:31:09.651 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,245,234,1,1,6,0,39,0,30,5,16,17,0,0,0,14]	
2021-12-16 16:31:09.659 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:09.660 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:09.660 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:09.660 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:09.661 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:09.713 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,39,0]	
2021-12-16 16:31:09.714 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,39,0]	
2021-12-16 16:31:09.714 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,39] - 0	
2021-12-16 16:31:09.715 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":39}	
2021-12-16 16:31:09.715 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:09.716 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0xa4c138ec0e4ef1cf:60149,225,2)	
2021-12-16 16:31:09.718 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,35,40]	
2021-12-16 16:31:09.718 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,35,40]	
2021-12-16 16:31:09.719 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,35] - 40	
2021-12-16 16:31:09.720 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":35}	
2021-12-16 16:31:09.720 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:09.721 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa0a00dfcb:34528,205,2)	
2021-12-16 16:31:09.721 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Request network address of '0x7cb03eaa0a00dfcb'	
2021-12-16 16:31:09.722 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - nwkAddrReq - {"ieeeaddr":"0x7cb03eaa0a00dfcb","reqtype":0,"startindex":0}	
2021-12-16 16:31:09.722 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,10,37,0,203,223,0,10,170,62,176,124,0,0,105]	
2021-12-16 16:31:09.730 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,0,0,100]	
2021-12-16 16:31:09.731 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,0,0,100]	
2021-12-16 16:31:09.732 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 0 - [0] - 100	
2021-12-16 16:31:09.732 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - nwkAddrReq - {"status":0}	
2021-12-16 16:31:09.733 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:09.901 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa0a019e9d:32268/3 (0,3,14)	
2021-12-16 16:31:09.902 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":32268,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":40,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,8,0,0,0]}}	
2021-12-16 16:31:09.903 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,12,126,3,1,6,0,40,0,30,5,16,8,0,0,0,119]	
2021-12-16 16:31:09.911 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:09.911 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:09.912 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:09.912 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:09.913 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:09.946 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,40,15]	
2021-12-16 16:31:09.947 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,40,15]	
2021-12-16 16:31:09.947 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,40] - 15	
2021-12-16 16:31:09.948 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":40}	
2021-12-16 16:31:09.949 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:09.949 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa0a019e9d:32268,225,3)	
2021-12-16 16:31:09.991 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002b805e3:39725/1 (0,2,14)	
2021-12-16 16:31:09.992 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":39725,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":41,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,9,0,0,0]}}	
2021-12-16 16:31:09.993 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,45,155,1,1,6,0,41,0,30,5,16,9,0,0,0,177]	
2021-12-16 16:31:10.002 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:10.002 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:10.003 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:10.003 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:10.004 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:10.184 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,38,45]	
2021-12-16 16:31:10.185 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,38,45]	
2021-12-16 16:31:10.185 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,38] - 45	
2021-12-16 16:31:10.186 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":38}	
2021-12-16 16:31:10.187 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:10.188 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00a36bed:65448,205,2)	
2021-12-16 16:31:10.189 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Request network address of '0x7cb03eaa00a36bed'	
2021-12-16 16:31:10.190 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - nwkAddrReq - {"ieeeaddr":"0x7cb03eaa00a36bed","reqtype":0,"startindex":0}	
2021-12-16 16:31:10.191 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,10,37,0,237,107,163,0,170,62,176,124,0,0,82]	
2021-12-16 16:31:10.200 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,0,0,100]	
2021-12-16 16:31:10.201 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,0,0,100]	
2021-12-16 16:31:10.202 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 0 - [0] - 100	
2021-12-16 16:31:10.203 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - nwkAddrReq - {"status":0}	
2021-12-16 16:31:10.205 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:10.274 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002b7d6a9:19263/1 (0,2,14)	
2021-12-16 16:31:10.275 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":19263,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":42,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,11,0,0,0]}}	
2021-12-16 16:31:10.275 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,63,75,1,1,6,0,42,0,30,5,16,11,0,0,0,114]	
2021-12-16 16:31:10.284 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:10.285 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:10.285 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:10.286 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:10.286 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:10.506 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x90fd9ffffe7fe8c9:65244/1 (0,2,14)	
2021-12-16 16:31:10.507 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":65244,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":43,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,14,0,0,0]}}	
2021-12-16 16:31:10.508 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,220,254,1,1,6,0,43,0,30,5,16,14,0,0,0,32]	
2021-12-16 16:31:10.517 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:10.518 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:10.518 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:10.519 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:10.520 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:10.543 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002b7d87c:35436/1 (0,2,14)	
2021-12-16 16:31:10.544 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":35436,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":44,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,10,0,0,0]}}	
2021-12-16 16:31:10.545 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,108,138,1,1,6,0,44,0,30,5,16,10,0,0,0,231]	
2021-12-16 16:31:10.554 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:10.555 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:10.555 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:10.556 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:10.556 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:10.734 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,41,34]	
2021-12-16 16:31:10.735 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,41,34]	
2021-12-16 16:31:10.736 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,41] - 34	
2021-12-16 16:31:10.736 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":41}	
2021-12-16 16:31:10.737 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:10.737 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002b805e3:39725,205,2)	
2021-12-16 16:31:10.738 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Request network address of '0x00158d0002b805e3'	
2021-12-16 16:31:10.738 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - nwkAddrReq - {"ieeeaddr":"0x00158d0002b805e3","reqtype":0,"startindex":0}	
2021-12-16 16:31:10.739 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,10,37,0,227,5,184,2,0,141,21,0,0,0,235]	
2021-12-16 16:31:10.751 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,0,0,100]	
2021-12-16 16:31:10.752 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,0,0,100]	
2021-12-16 16:31:10.753 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 0 - [0] - 100	
2021-12-16 16:31:10.754 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - nwkAddrReq - {"status":0}	
2021-12-16 16:31:10.755 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:10.792 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00acb990:47504/3 (0,4,14)	
2021-12-16 16:31:10.793 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":47504,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":45,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,2,0,0,0]}}	
2021-12-16 16:31:10.794 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,144,185,3,1,6,0,45,0,30,5,16,2,0,0,0,35]	
2021-12-16 16:31:10.803 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:10.804 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:10.805 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:10.806 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:10.807 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:10.862 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,45,10]	
2021-12-16 16:31:10.862 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,45,10]	
2021-12-16 16:31:10.862 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,45] - 10	
2021-12-16 16:31:10.863 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":45}	
2021-12-16 16:31:10.863 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:10.863 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00acb990:47504,225,4)	
2021-12-16 16:31:10.864 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa00acb990/3 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'MAC channel access failure' (225))	
2021-12-16 16:31:10.864 - debug: zigbee.0 (26219) Exception in readState of '0x7cb03eaa00acb990' - error : 'Error: Read 0x7cb03eaa00acb990/3 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'MAC channel access failure' (225))'	
2021-12-16 16:31:10.865 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa00acb990/3 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:10.866 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00acb990:47504/3 (0,0,14)	
2021-12-16 16:31:10.866 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":47504,"destendpoint":3,"srcendpoint":1,"clusterid":0,"transid":46,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,18,0,0,0]}}	
2021-12-16 16:31:10.866 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,144,185,3,1,0,0,46,0,30,5,16,18,0,0,0,54]	
2021-12-16 16:31:10.872 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x000b57fffe4436b0:57723/1 (0,2,14)	
2021-12-16 16:31:10.874 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:10.875 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:10.875 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:10.876 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:10.876 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:10.876 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":57723,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":47,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,12,0,0,0]}}	
2021-12-16 16:31:10.877 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,123,225,1,1,6,0,47,0,30,5,16,12,0,0,0,158]	
2021-12-16 16:31:10.885 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:10.886 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:10.886 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:10.886 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:10.887 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:10.948 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,46,9]	
2021-12-16 16:31:10.949 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,46,9]	
2021-12-16 16:31:10.949 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,46] - 9	
2021-12-16 16:31:10.949 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":46}	
2021-12-16 16:31:10.949 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:10.950 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00acb990:47504,225,0)	
2021-12-16 16:31:10.950 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa00acb990/3 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'MAC channel access failure' (225))	
2021-12-16 16:31:10.951 - warn: zigbee.0 (26219) Failed to ping 0x7cb03eaa00acb990 Plug 01	
2021-12-16 16:31:10.951 - debug: zigbee.0 (26219) Publish available for 0x7cb03eaa00acb990 = false	
2021-12-16 16:31:10.952 - debug: zigbee.0 (26219) Publish LQ for 0x7cb03eaa00acb990 = 0	
2021-12-16 16:31:10.976 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x90fd9ffffe88755e:2953/1 (0,2,13)	
2021-12-16 16:31:10.976 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":2953,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":48,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,15,0,0,0]}}	
2021-12-16 16:31:10.977 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,137,11,1,1,6,0,48,0,30,5,16,15,0,0,0,154]	
2021-12-16 16:31:10.982 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:10.982 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:10.982 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:10.983 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:10.983 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:10.985 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,48,59]	
2021-12-16 16:31:10.985 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,48,59]	
2021-12-16 16:31:10.986 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,48] - 59	
2021-12-16 16:31:10.986 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":48}	
2021-12-16 16:31:10.987 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:10.987 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x90fd9ffffe88755e:2953,205,2)	
2021-12-16 16:31:10.987 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Request network address of '0x90fd9ffffe88755e'	
2021-12-16 16:31:10.989 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - nwkAddrReq - {"ieeeaddr":"0x90fd9ffffe88755e","reqtype":0,"startindex":0}	
2021-12-16 16:31:10.989 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,10,37,0,94,117,136,254,255,159,253,144,0,0,127]	
2021-12-16 16:31:10.996 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,0,0,100]	
2021-12-16 16:31:10.997 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,0,0,100]	
2021-12-16 16:31:10.997 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 0 - [0] - 100	
2021-12-16 16:31:10.997 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - nwkAddrReq - {"status":0}	
2021-12-16 16:31:10.998 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:11.013 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,42,33]	
2021-12-16 16:31:11.013 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,42,33]	
2021-12-16 16:31:11.014 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,42] - 33	
2021-12-16 16:31:11.014 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":42}	
2021-12-16 16:31:11.014 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:11.014 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002b7d6a9:19263,205,2)	
2021-12-16 16:31:11.015 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Request network address of '0x00158d0002b7d6a9'	
2021-12-16 16:31:11.015 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - nwkAddrReq - {"ieeeaddr":"0x00158d0002b7d6a9","reqtype":0,"startindex":0}	
2021-12-16 16:31:11.015 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,10,37,0,169,214,183,2,0,141,21,0,0,0,125]	
2021-12-16 16:31:11.023 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,0,0,100]	
2021-12-16 16:31:11.023 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,0,0,100]	
2021-12-16 16:31:11.023 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 0 - [0] - 100	
2021-12-16 16:31:11.023 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - nwkAddrReq - {"status":0}	
2021-12-16 16:31:11.024 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:11.044 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x90fd9ffffe02c40f:56799/1 (0,2,13)	
2021-12-16 16:31:11.044 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":56799,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":49,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,13,0,0,0]}}	
2021-12-16 16:31:11.045 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,223,221,1,1,6,0,49,0,30,5,16,13,0,0,0,25]	
2021-12-16 16:31:11.050 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:11.050 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:11.050 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:11.051 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:11.051 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:11.053 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,49,58]	
2021-12-16 16:31:11.053 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,49,58]	
2021-12-16 16:31:11.054 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,49] - 58	
2021-12-16 16:31:11.054 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":49}	
2021-12-16 16:31:11.055 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:11.055 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x90fd9ffffe02c40f:56799,205,2)	
2021-12-16 16:31:11.055 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Request network address of '0x90fd9ffffe02c40f'	
2021-12-16 16:31:11.056 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - nwkAddrReq - {"ieeeaddr":"0x90fd9ffffe02c40f","reqtype":0,"startindex":0}	
2021-12-16 16:31:11.056 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,10,37,0,15,196,2,254,255,159,253,144,0,0,21]	
2021-12-16 16:31:11.066 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,0,0,100]	
2021-12-16 16:31:11.067 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,0,0,100]	
2021-12-16 16:31:11.067 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 0 - [0] - 100	
2021-12-16 16:31:11.067 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - nwkAddrReq - {"status":0}	
2021-12-16 16:31:11.067 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:11.147 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,43,32]	
2021-12-16 16:31:11.147 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,43,32]	
2021-12-16 16:31:11.147 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,43] - 32	
2021-12-16 16:31:11.148 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":43}	
2021-12-16 16:31:11.148 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:11.148 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x90fd9ffffe7fe8c9:65244,205,2)	
2021-12-16 16:31:11.148 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Request network address of '0x90fd9ffffe7fe8c9'	
2021-12-16 16:31:11.149 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - nwkAddrReq - {"ieeeaddr":"0x90fd9ffffe7fe8c9","reqtype":0,"startindex":0}	
2021-12-16 16:31:11.149 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,10,37,0,201,232,127,254,255,159,253,144,0,0,130]	
2021-12-16 16:31:11.156 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,0,0,100]	
2021-12-16 16:31:11.157 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,0,0,100]	
2021-12-16 16:31:11.157 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 0 - [0] - 100	
2021-12-16 16:31:11.157 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - nwkAddrReq - {"status":0}	
2021-12-16 16:31:11.158 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:11.173 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,44,39]	
2021-12-16 16:31:11.174 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,44,39]	
2021-12-16 16:31:11.174 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,44] - 39	
2021-12-16 16:31:11.174 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":44}	
2021-12-16 16:31:11.174 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:11.175 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002b7d87c:35436,205,2)	
2021-12-16 16:31:11.175 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Request network address of '0x00158d0002b7d87c'	
2021-12-16 16:31:11.175 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - nwkAddrReq - {"ieeeaddr":"0x00158d0002b7d87c","reqtype":0,"startindex":0}	
2021-12-16 16:31:11.175 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,10,37,0,124,216,183,2,0,141,21,0,0,0,166]	
2021-12-16 16:31:11.186 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,0,0,100]	
2021-12-16 16:31:11.186 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,0,0,100]	
2021-12-16 16:31:11.186 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 0 - [0] - 100	
2021-12-16 16:31:11.186 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - nwkAddrReq - {"status":0}	
2021-12-16 16:31:11.190 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:11.579 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa0a025809:18602/3 (0,4,13)	
2021-12-16 16:31:11.580 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":18602,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":50,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,6,0,0,0]}}	
2021-12-16 16:31:11.581 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,170,72,3,1,6,0,50,0,30,5,16,6,0,0,0,243]	
2021-12-16 16:31:11.590 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:11.590 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:11.591 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:11.591 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:11.592 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:11.608 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,47,36]	
2021-12-16 16:31:11.609 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,47,36]	
2021-12-16 16:31:11.609 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,47] - 36	
2021-12-16 16:31:11.610 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":47}	
2021-12-16 16:31:11.610 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:11.611 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x000b57fffe4436b0:57723,205,2)	
2021-12-16 16:31:11.611 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Request network address of '0x000b57fffe4436b0'	
2021-12-16 16:31:11.612 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - nwkAddrReq - {"ieeeaddr":"0x000b57fffe4436b0","reqtype":0,"startindex":0}	
2021-12-16 16:31:11.612 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,10,37,0,176,54,68,254,255,87,11,0,0,0,176]	
2021-12-16 16:31:11.621 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,0,0,100]	
2021-12-16 16:31:11.621 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,0,0,100]	
2021-12-16 16:31:11.622 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 0 - [0] - 100	
2021-12-16 16:31:11.623 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - nwkAddrReq - {"status":0}	
2021-12-16 16:31:11.624 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:11.669 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,50,21]	
2021-12-16 16:31:11.669 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,50,21]	
2021-12-16 16:31:11.669 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,50] - 21	
2021-12-16 16:31:11.670 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":50}	
2021-12-16 16:31:11.670 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:11.671 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa0a025809:18602,225,4)	
2021-12-16 16:31:11.671 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa0a025809/3 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'MAC channel access failure' (225))	
2021-12-16 16:31:11.672 - debug: zigbee.0 (26219) Exception in readState of '0x7cb03eaa0a025809' - error : 'Error: Read 0x7cb03eaa0a025809/3 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'MAC channel access failure' (225))'	
2021-12-16 16:31:11.673 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa0a025809/3 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:11.673 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa0a025809:18602/3 (0,0,13)	
2021-12-16 16:31:11.674 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":18602,"destendpoint":3,"srcendpoint":1,"clusterid":0,"transid":51,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,19,0,0,0]}}	
2021-12-16 16:31:11.674 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,170,72,3,1,0,0,51,0,30,5,16,19,0,0,0,225]	
2021-12-16 16:31:11.682 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:11.683 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:11.684 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:11.684 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:11.685 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:11.716 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0xa4c138ec0e4ef1cf:60149/1 (0,3,13)	
2021-12-16 16:31:11.716 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":60149,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":52,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,17,0,0,0]}}	
2021-12-16 16:31:11.717 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,245,234,1,1,6,0,52,0,30,5,16,17,0,0,0,29]	
2021-12-16 16:31:11.736 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:11.736 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:11.737 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:11.737 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:11.738 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:11.742 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,51,20]	
2021-12-16 16:31:11.742 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,51,20]	
2021-12-16 16:31:11.743 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,51] - 20	
2021-12-16 16:31:11.744 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":51}	
2021-12-16 16:31:11.745 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:11.745 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa0a025809:18602,225,0)	
2021-12-16 16:31:11.745 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa0a025809/3 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'MAC channel access failure' (225))	
2021-12-16 16:31:11.746 - warn: zigbee.0 (26219) Failed to ping 0x7cb03eaa0a025809 Plug 01	
2021-12-16 16:31:11.746 - debug: zigbee.0 (26219) Publish available for 0x7cb03eaa0a025809 = false	
2021-12-16 16:31:11.748 - debug: zigbee.0 (26219) Publish LQ for 0x7cb03eaa0a025809 = 0	
2021-12-16 16:31:11.772 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,52,19]	
2021-12-16 16:31:11.773 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,52,19]	
2021-12-16 16:31:11.773 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,52] - 19	
2021-12-16 16:31:11.773 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":52}	
2021-12-16 16:31:11.775 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:11.775 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0xa4c138ec0e4ef1cf:60149,225,3)	
2021-12-16 16:31:11.949 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa0a019e9d:32268/3 (0,4,12)	
2021-12-16 16:31:11.950 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":32268,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":53,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,8,0,0,0]}}	
2021-12-16 16:31:11.950 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,12,126,3,1,6,0,53,0,30,5,16,8,0,0,0,106]	
2021-12-16 16:31:11.961 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:11.961 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:11.961 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:11.961 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:11.962 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:12.009 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,53,18]	
2021-12-16 16:31:12.009 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,53,18]	
2021-12-16 16:31:12.009 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,53] - 18	
2021-12-16 16:31:12.009 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":53}	
2021-12-16 16:31:12.010 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:12.010 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa0a019e9d:32268,225,4)	
2021-12-16 16:31:12.010 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa0a019e9d/3 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'MAC channel access failure' (225))	
2021-12-16 16:31:12.010 - debug: zigbee.0 (26219) Exception in readState of '0x7cb03eaa0a019e9d' - error : 'Error: Read 0x7cb03eaa0a019e9d/3 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'MAC channel access failure' (225))'	
2021-12-16 16:31:12.011 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa0a019e9d/3 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:12.011 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa0a019e9d:32268/3 (0,0,12)	
2021-12-16 16:31:12.015 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":32268,"destendpoint":3,"srcendpoint":1,"clusterid":0,"transid":54,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,20,0,0,0]}}	
2021-12-16 16:31:12.016 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,12,126,3,1,0,0,54,0,30,5,16,20,0,0,0,115]	
2021-12-16 16:31:12.023 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:12.024 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:12.024 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:12.024 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:12.025 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:12.063 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,54,17]	
2021-12-16 16:31:12.063 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,54,17]	
2021-12-16 16:31:12.064 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,54] - 17	
2021-12-16 16:31:12.064 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":54}	
2021-12-16 16:31:12.064 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:12.064 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa0a019e9d:32268,225,0)	
2021-12-16 16:31:12.065 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa0a019e9d/3 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'MAC channel access failure' (225))	
2021-12-16 16:31:12.065 - warn: zigbee.0 (26219) Failed to ping 0x7cb03eaa0a019e9d Plug 01	
2021-12-16 16:31:12.065 - debug: zigbee.0 (26219) Publish available for 0x7cb03eaa0a019e9d = false	
2021-12-16 16:31:12.066 - debug: zigbee.0 (26219) Publish LQ for 0x7cb03eaa0a019e9d = 0	
2021-12-16 16:31:13.776 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0xa4c138ec0e4ef1cf:60149/1 (0,4,11)	
2021-12-16 16:31:13.777 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":60149,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":55,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,17,0,0,0]}}	
2021-12-16 16:31:13.778 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,245,234,1,1,6,0,55,0,30,5,16,17,0,0,0,30]	
2021-12-16 16:31:13.786 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:13.787 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:13.788 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:13.788 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:13.789 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:13.820 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,55,16]	
2021-12-16 16:31:13.821 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,55,16]	
2021-12-16 16:31:13.821 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,55] - 16	
2021-12-16 16:31:13.822 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":55}	
2021-12-16 16:31:13.823 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:13.823 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0xa4c138ec0e4ef1cf:60149,225,4)	
2021-12-16 16:31:13.824 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0xa4c138ec0e4ef1cf/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'MAC channel access failure' (225))	
2021-12-16 16:31:13.825 - debug: zigbee.0 (26219) Exception in readState of '0xa4c138ec0e4ef1cf' - error : 'Error: Read 0xa4c138ec0e4ef1cf/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'MAC channel access failure' (225))'	
2021-12-16 16:31:13.826 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0xa4c138ec0e4ef1cf/1 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:13.827 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0xa4c138ec0e4ef1cf:60149/1 (0,0,11)	
2021-12-16 16:31:13.828 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":60149,"destendpoint":1,"srcendpoint":1,"clusterid":0,"transid":56,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,21,0,0,0]}}	
2021-12-16 16:31:13.829 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,245,234,1,1,0,0,56,0,30,5,16,21,0,0,0,19]	
2021-12-16 16:31:13.840 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:13.841 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:13.844 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:13.845 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:13.846 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:13.898 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,56,31]	
2021-12-16 16:31:13.899 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,56,31]	
2021-12-16 16:31:13.899 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,56] - 31	
2021-12-16 16:31:13.902 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":56}	
2021-12-16 16:31:13.903 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:13.903 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0xa4c138ec0e4ef1cf:60149,225,0)	
2021-12-16 16:31:13.904 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0xa4c138ec0e4ef1cf/1 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'MAC channel access failure' (225))	
2021-12-16 16:31:13.904 - warn: zigbee.0 (26219) Failed to ping 0xa4c138ec0e4ef1cf TS0001	
2021-12-16 16:31:13.905 - debug: zigbee.0 (26219) Publish available for 0xa4c138ec0e4ef1cf = false	
2021-12-16 16:31:13.906 - debug: zigbee.0 (26219) Publish LQ for 0xa4c138ec0e4ef1cf = 0	
2021-12-16 16:31:19.567 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002c65ed8:41267/1 (0,3,10)	
2021-12-16 16:31:19.568 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":41267,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":57,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,4,0,0,0]}}	
2021-12-16 16:31:19.570 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,51,161,1,1,6,0,57,0,30,5,16,4,0,0,0,136]	
2021-12-16 16:31:19.579 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:19.580 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:19.581 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:19.581 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:19.582 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:19.734 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa0a00dfcb:34528/3 (0,3,10)	
2021-12-16 16:31:19.734 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":34528,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":58,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,3,0,0,0]}}	
2021-12-16 16:31:19.735 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,224,134,3,1,6,0,58,0,30,5,16,3,0,0,0,122]	
2021-12-16 16:31:19.743 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:19.743 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:19.743 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:19.743 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:19.744 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:20.207 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00a36bed:65448/3 (0,3,10)	
2021-12-16 16:31:20.208 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":65448,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":59,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,7,0,0,0]}}	
2021-12-16 16:31:20.208 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,168,255,3,1,6,0,59,0,30,5,16,7,0,0,0,78]	
2021-12-16 16:31:20.217 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:20.217 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:20.217 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:20.217 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:20.218 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:20.244 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,58,49]	
2021-12-16 16:31:20.245 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,58,49]	
2021-12-16 16:31:20.245 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,58] - 49	
2021-12-16 16:31:20.245 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":58}	
2021-12-16 16:31:20.245 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:20.246 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa0a00dfcb:34528,205,3)	
2021-12-16 16:31:20.246 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Wait 2000ms	
2021-12-16 16:31:20.267 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,57,50]	
2021-12-16 16:31:20.267 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,57,50]	
2021-12-16 16:31:20.267 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,57] - 50	
2021-12-16 16:31:20.268 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":57}	
2021-12-16 16:31:20.268 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:20.268 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002c65ed8:41267,205,3)	
2021-12-16 16:31:20.268 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Wait 2000ms	
2021-12-16 16:31:20.566 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,59,48]	
2021-12-16 16:31:20.567 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,59,48]	
2021-12-16 16:31:20.569 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,59] - 48	
2021-12-16 16:31:20.569 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":59}	
2021-12-16 16:31:20.572 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:20.572 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00a36bed:65448,205,3)	
2021-12-16 16:31:20.573 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Wait 2000ms	
2021-12-16 16:31:20.755 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002b805e3:39725/1 (0,3,10)	
2021-12-16 16:31:20.756 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":39725,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":60,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,9,0,0,0]}}	
2021-12-16 16:31:20.756 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,45,155,1,1,6,0,60,0,30,5,16,9,0,0,0,164]	
2021-12-16 16:31:20.764 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:20.764 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:20.765 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:20.765 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:20.765 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:20.999 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x90fd9ffffe88755e:2953/1 (0,3,10)	
2021-12-16 16:31:20.999 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":2953,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":61,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,15,0,0,0]}}	
2021-12-16 16:31:21.000 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,137,11,1,1,6,0,61,0,30,5,16,15,0,0,0,151]	
2021-12-16 16:31:21.008 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:21.008 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:21.008 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:21.009 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:21.009 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:21.024 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002b7d6a9:19263/1 (0,3,10)	
2021-12-16 16:31:21.025 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":19263,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":62,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,11,0,0,0]}}	
2021-12-16 16:31:21.025 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,63,75,1,1,6,0,62,0,30,5,16,11,0,0,0,102]	
2021-12-16 16:31:21.033 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:21.034 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:21.034 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:21.034 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:21.035 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:21.068 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x90fd9ffffe02c40f:56799/1 (0,3,10)	
2021-12-16 16:31:21.068 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":56799,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":63,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,13,0,0,0]}}	
2021-12-16 16:31:21.069 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,223,221,1,1,6,0,63,0,30,5,16,13,0,0,0,23]	
2021-12-16 16:31:21.077 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:21.077 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:21.078 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:21.078 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:21.078 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:21.158 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x90fd9ffffe7fe8c9:65244/1 (0,3,10)	
2021-12-16 16:31:21.159 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":65244,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":64,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,14,0,0,0]}}	
2021-12-16 16:31:21.159 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,220,254,1,1,6,0,64,0,30,5,16,14,0,0,0,75]	
2021-12-16 16:31:21.167 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:21.168 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:21.168 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:21.168 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:21.168 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:21.190 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002b7d87c:35436/1 (0,3,10)	
2021-12-16 16:31:21.191 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":35436,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":65,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,10,0,0,0]}}	
2021-12-16 16:31:21.191 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,108,138,1,1,6,0,65,0,30,5,16,10,0,0,0,138]	
2021-12-16 16:31:21.196 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:21.197 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:21.197 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:21.197 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:21.197 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:21.199 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,65,74]	
2021-12-16 16:31:21.199 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,65,74]	
2021-12-16 16:31:21.200 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,65] - 74	
2021-12-16 16:31:21.200 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":65}	
2021-12-16 16:31:21.200 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:21.201 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002b7d87c:35436,205,3)	
2021-12-16 16:31:21.201 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Wait 2000ms	
2021-12-16 16:31:21.315 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,61,54]	
2021-12-16 16:31:21.315 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,61,54]	
2021-12-16 16:31:21.316 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,61] - 54	
2021-12-16 16:31:21.316 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":61}	
2021-12-16 16:31:21.316 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:21.316 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x90fd9ffffe88755e:2953,205,3)	
2021-12-16 16:31:21.316 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Wait 2000ms	
2021-12-16 16:31:21.454 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,60,55]	
2021-12-16 16:31:21.454 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,60,55]	
2021-12-16 16:31:21.455 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,60] - 55	
2021-12-16 16:31:21.456 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":60}	
2021-12-16 16:31:21.456 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:21.457 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002b805e3:39725,205,3)	
2021-12-16 16:31:21.457 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Wait 2000ms	
2021-12-16 16:31:21.608 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,62,53]	
2021-12-16 16:31:21.608 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,62,53]	
2021-12-16 16:31:21.608 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,62] - 53	
2021-12-16 16:31:21.609 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":62}	
2021-12-16 16:31:21.609 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:21.609 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002b7d6a9:19263,205,3)	
2021-12-16 16:31:21.610 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Wait 2000ms	
2021-12-16 16:31:21.625 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x000b57fffe4436b0:57723/1 (0,3,10)	
2021-12-16 16:31:21.625 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":57723,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":66,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,12,0,0,0]}}	
2021-12-16 16:31:21.626 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,123,225,1,1,6,0,66,0,30,5,16,12,0,0,0,243]	
2021-12-16 16:31:21.631 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:21.632 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:21.633 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:21.633 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:21.634 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:21.636 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,66,73]	
2021-12-16 16:31:21.636 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,66,73]	
2021-12-16 16:31:21.637 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,66] - 73	
2021-12-16 16:31:21.637 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":66}	
2021-12-16 16:31:21.638 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:21.639 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x000b57fffe4436b0:57723,205,3)	
2021-12-16 16:31:21.639 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Wait 2000ms	
2021-12-16 16:31:21.644 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,64,75]	
2021-12-16 16:31:21.645 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,64,75]	
2021-12-16 16:31:21.646 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,64] - 75	
2021-12-16 16:31:21.646 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":64}	
2021-12-16 16:31:21.647 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:21.647 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x90fd9ffffe7fe8c9:65244,205,3)	
2021-12-16 16:31:21.647 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Wait 2000ms	
2021-12-16 16:31:21.750 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,63,52]	
2021-12-16 16:31:21.751 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,63,52]	
2021-12-16 16:31:21.751 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,63] - 52	
2021-12-16 16:31:21.752 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":63}	
2021-12-16 16:31:21.752 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:21.753 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x90fd9ffffe02c40f:56799,205,3)	
2021-12-16 16:31:21.753 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Wait 2000ms	
2021-12-16 16:31:22.247 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa0a00dfcb:34528/3 (0,4,10)	
2021-12-16 16:31:22.248 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":34528,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":67,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,3,0,0,0]}}	
2021-12-16 16:31:22.249 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,224,134,3,1,6,0,67,0,30,5,16,3,0,0,0,3]	
2021-12-16 16:31:22.255 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:22.256 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:22.256 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:22.257 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:22.258 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:22.269 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002c65ed8:41267/1 (0,4,10)	
2021-12-16 16:31:22.271 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":41267,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":68,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,4,0,0,0]}}	
2021-12-16 16:31:22.272 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,51,161,1,1,6,0,68,0,30,5,16,4,0,0,0,245]	
2021-12-16 16:31:22.278 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:22.279 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:22.280 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:22.281 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:22.281 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:22.575 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00a36bed:65448/3 (0,4,10)	
2021-12-16 16:31:22.575 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":65448,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":69,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,7,0,0,0]}}	
2021-12-16 16:31:22.576 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,168,255,3,1,6,0,69,0,30,5,16,7,0,0,0,48]	
2021-12-16 16:31:22.582 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:22.582 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:22.583 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:22.583 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:22.584 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:22.884 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,68,79]	
2021-12-16 16:31:22.884 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,68,79]	
2021-12-16 16:31:22.885 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,68] - 79	
2021-12-16 16:31:22.886 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":68}	
2021-12-16 16:31:22.886 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:22.887 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002c65ed8:41267,205,4)	
2021-12-16 16:31:22.887 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x00158d0002c65ed8/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))	
2021-12-16 16:31:22.888 - debug: zigbee.0 (26219) Exception in readState of '0x00158d0002c65ed8' - error : 'Error: Read 0x00158d0002c65ed8/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))'	
2021-12-16 16:31:22.889 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x00158d0002c65ed8/1 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:22.890 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002c65ed8:41267/1 (0,0,10)	
2021-12-16 16:31:22.891 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":41267,"destendpoint":1,"srcendpoint":1,"clusterid":0,"transid":70,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,22,0,0,0]}}	
2021-12-16 16:31:22.892 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,51,161,1,1,0,0,70,0,30,5,16,22,0,0,0,227]	
2021-12-16 16:31:22.897 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:22.898 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:22.899 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:22.899 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:22.900 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:22.920 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,69,78]	
2021-12-16 16:31:22.921 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,69,78]	
2021-12-16 16:31:22.922 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,69] - 78	
2021-12-16 16:31:22.922 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":69}	
2021-12-16 16:31:22.923 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:22.923 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00a36bed:65448,205,4)	
2021-12-16 16:31:22.928 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa00a36bed/3 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))	
2021-12-16 16:31:22.928 - debug: zigbee.0 (26219) Exception in readState of '0x7cb03eaa00a36bed' - error : 'Error: Read 0x7cb03eaa00a36bed/3 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))'	
2021-12-16 16:31:22.930 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa00a36bed/3 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:22.931 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00a36bed:65448/3 (0,0,10)	
2021-12-16 16:31:22.932 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":65448,"destendpoint":3,"srcendpoint":1,"clusterid":0,"transid":71,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,23,0,0,0]}}	
2021-12-16 16:31:22.932 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,168,255,3,1,0,0,71,0,30,5,16,23,0,0,0,36]	
2021-12-16 16:31:22.939 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:22.940 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:22.941 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:22.942 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:22.943 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:23.050 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,67,72]	
2021-12-16 16:31:23.051 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,67,72]	
2021-12-16 16:31:23.051 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,67] - 72	
2021-12-16 16:31:23.051 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":67}	
2021-12-16 16:31:23.052 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:23.052 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa0a00dfcb:34528,205,4)	
2021-12-16 16:31:23.052 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa0a00dfcb/3 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))	
2021-12-16 16:31:23.053 - debug: zigbee.0 (26219) Exception in readState of '0x7cb03eaa0a00dfcb' - error : 'Error: Read 0x7cb03eaa0a00dfcb/3 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))'	
2021-12-16 16:31:23.053 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa0a00dfcb/3 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:23.054 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa0a00dfcb:34528/3 (0,0,10)	
2021-12-16 16:31:23.054 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":34528,"destendpoint":3,"srcendpoint":1,"clusterid":0,"transid":72,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,24,0,0,0]}}	
2021-12-16 16:31:23.055 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,224,134,3,1,0,0,72,0,30,5,16,24,0,0,0,21]	
2021-12-16 16:31:23.060 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:23.061 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:23.062 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:23.062 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:23.063 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:23.202 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002b7d87c:35436/1 (0,4,10)	
2021-12-16 16:31:23.203 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":35436,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":73,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,10,0,0,0]}}	
2021-12-16 16:31:23.203 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,108,138,1,1,6,0,73,0,30,5,16,10,0,0,0,130]	
2021-12-16 16:31:23.209 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:23.210 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:23.210 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:23.211 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:23.211 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:23.317 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x90fd9ffffe88755e:2953/1 (0,4,10)	
2021-12-16 16:31:23.318 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":2953,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":74,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,15,0,0,0]}}	
2021-12-16 16:31:23.319 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,137,11,1,1,6,0,74,0,30,5,16,15,0,0,0,224]	
2021-12-16 16:31:23.324 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:23.325 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:23.326 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:23.326 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:23.327 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:23.458 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002b805e3:39725/1 (0,4,10)	
2021-12-16 16:31:23.459 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":39725,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":75,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,9,0,0,0]}}	
2021-12-16 16:31:23.460 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,45,155,1,1,6,0,75,0,30,5,16,9,0,0,0,211]	
2021-12-16 16:31:23.463 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,70,77]	
2021-12-16 16:31:23.465 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,70,77]	
2021-12-16 16:31:23.465 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,70] - 77	
2021-12-16 16:31:23.466 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":70}	
2021-12-16 16:31:23.467 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:23.468 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002c65ed8:41267,205,0)	
2021-12-16 16:31:23.469 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x00158d0002c65ed8/1 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))	
2021-12-16 16:31:23.469 - warn: zigbee.0 (26219) Failed to ping 0x00158d0002c65ed8 lumi.light.aqcn02	
2021-12-16 16:31:23.470 - debug: zigbee.0 (26219) Publish available for 0x00158d0002c65ed8 = false	
2021-12-16 16:31:23.472 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002c65ed8 = 0	
2021-12-16 16:31:23.481 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:23.481 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:23.482 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:23.483 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:23.484 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:23.513 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,71,76]	
2021-12-16 16:31:23.514 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,71,76]	
2021-12-16 16:31:23.515 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,71] - 76	
2021-12-16 16:31:23.515 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":71}	
2021-12-16 16:31:23.516 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:23.516 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00a36bed:65448,205,0)	
2021-12-16 16:31:23.517 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa00a36bed/3 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))	
2021-12-16 16:31:23.517 - warn: zigbee.0 (26219) Failed to ping 0x7cb03eaa00a36bed Plug 01	
2021-12-16 16:31:23.517 - debug: zigbee.0 (26219) Publish available for 0x7cb03eaa00a36bed = false	
2021-12-16 16:31:23.520 - debug: zigbee.0 (26219) Publish LQ for 0x7cb03eaa00a36bed = 0	
2021-12-16 16:31:23.610 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002b7d6a9:19263/1 (0,4,8)	
2021-12-16 16:31:23.610 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":19263,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":76,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,11,0,0,0]}}	
2021-12-16 16:31:23.610 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,63,75,1,1,6,0,76,0,30,5,16,11,0,0,0,20]	
2021-12-16 16:31:23.615 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:23.616 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:23.616 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:23.616 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:23.616 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:23.639 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x000b57fffe4436b0:57723/1 (0,4,8)	
2021-12-16 16:31:23.640 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":57723,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":77,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,12,0,0,0]}}	
2021-12-16 16:31:23.640 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,123,225,1,1,6,0,77,0,30,5,16,12,0,0,0,252]	
2021-12-16 16:31:23.645 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:23.645 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:23.645 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:23.646 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:23.646 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:23.649 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x90fd9ffffe7fe8c9:65244/1 (0,4,8)	
2021-12-16 16:31:23.650 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":65244,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":78,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,14,0,0,0]}}	
2021-12-16 16:31:23.650 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,220,254,1,1,6,0,78,0,30,5,16,14,0,0,0,69]	
2021-12-16 16:31:23.655 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,17,117]	
2021-12-16 16:31:23.655 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,17,117]	
2021-12-16 16:31:23.655 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [17] - 117	
2021-12-16 16:31:23.655 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":17}	
2021-12-16 16:31:23.656 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:23.656 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x90fd9ffffe7fe8c9/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (SREQ '--> AF - dataRequest - {"dstaddr":65244,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":78,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,14,0,0,0]}}' failed with status '(0x11: BUFFER_FULL)' (expected '(0x00: SUCCESS)'))	
2021-12-16 16:31:23.656 - debug: zigbee.0 (26219) Exception in readState of '0x90fd9ffffe7fe8c9' - error : 'Error: Read 0x90fd9ffffe7fe8c9/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (SREQ '--> AF - dataRequest - {"dstaddr":65244,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":78,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,14,0,0,0]}}' failed with status '(0x11: BUFFER_FULL)' (expected '(0x00: SUCCESS)'))'	
2021-12-16 16:31:23.657 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x90fd9ffffe7fe8c9/1 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:23.657 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x90fd9ffffe7fe8c9:65244/1 (0,0,8)	
2021-12-16 16:31:23.658 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":65244,"destendpoint":1,"srcendpoint":1,"clusterid":0,"transid":79,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,25,0,0,0]}}	
2021-12-16 16:31:23.658 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,220,254,1,1,0,0,79,0,30,5,16,25,0,0,0,85]	
2021-12-16 16:31:23.662 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,17,117]	
2021-12-16 16:31:23.663 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,17,117]	
2021-12-16 16:31:23.663 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [17] - 117	
2021-12-16 16:31:23.664 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":17}	
2021-12-16 16:31:23.664 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:23.665 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x90fd9ffffe7fe8c9/1 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (SREQ '--> AF - dataRequest - {"dstaddr":65244,"destendpoint":1,"srcendpoint":1,"clusterid":0,"transid":79,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,25,0,0,0]}}' failed with status '(0x11: BUFFER_FULL)' (expected '(0x00: SUCCESS)'))	
2021-12-16 16:31:23.665 - warn: zigbee.0 (26219) Failed to ping 0x90fd9ffffe7fe8c9 TRADFRI bulb E27 WS opal 980lm	
2021-12-16 16:31:23.665 - debug: zigbee.0 (26219) Publish available for 0x90fd9ffffe7fe8c9 = false	
2021-12-16 16:31:23.668 - debug: zigbee.0 (26219) Publish LQ for 0x90fd9ffffe7fe8c9 = 0	
2021-12-16 16:31:23.681 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,72,67]	
2021-12-16 16:31:23.681 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,72,67]	
2021-12-16 16:31:23.681 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,72] - 67	
2021-12-16 16:31:23.681 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":72}	
2021-12-16 16:31:23.682 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:23.682 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa0a00dfcb:34528,205,0)	
2021-12-16 16:31:23.682 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa0a00dfcb/3 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))	
2021-12-16 16:31:23.682 - warn: zigbee.0 (26219) Failed to ping 0x7cb03eaa0a00dfcb Plug 01	
2021-12-16 16:31:23.683 - debug: zigbee.0 (26219) Publish available for 0x7cb03eaa0a00dfcb = false	
2021-12-16 16:31:23.684 - debug: zigbee.0 (26219) Publish LQ for 0x7cb03eaa0a00dfcb = 0	
2021-12-16 16:31:23.714 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,73,66]	
2021-12-16 16:31:23.715 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,73,66]	
2021-12-16 16:31:23.715 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,73] - 66	
2021-12-16 16:31:23.716 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":73}	
2021-12-16 16:31:23.716 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:23.717 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002b7d87c:35436,205,4)	
2021-12-16 16:31:23.717 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x00158d0002b7d87c/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))	
2021-12-16 16:31:23.717 - debug: zigbee.0 (26219) Exception in readState of '0x00158d0002b7d87c' - error : 'Error: Read 0x00158d0002b7d87c/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))'	
2021-12-16 16:31:23.718 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x00158d0002b7d87c/1 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:23.718 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002b7d87c:35436/1 (0,0,6)	
2021-12-16 16:31:23.719 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":35436,"destendpoint":1,"srcendpoint":1,"clusterid":0,"transid":80,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,26,0,0,0]}}	
2021-12-16 16:31:23.719 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,108,138,1,1,0,0,80,0,30,5,16,26,0,0,0,141]	
2021-12-16 16:31:23.726 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:23.726 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:23.727 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:23.727 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:23.728 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:23.755 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x90fd9ffffe02c40f:56799/1 (0,4,6)	
2021-12-16 16:31:23.756 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":56799,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":81,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,13,0,0,0]}}	
2021-12-16 16:31:23.756 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,223,221,1,1,6,0,81,0,30,5,16,13,0,0,0,121]	
2021-12-16 16:31:23.761 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:23.761 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:23.761 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:23.761 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:23.762 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:23.793 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,74,65]	
2021-12-16 16:31:23.793 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,74,65]	
2021-12-16 16:31:23.794 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,74] - 65	
2021-12-16 16:31:23.794 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":74}	
2021-12-16 16:31:23.794 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:23.794 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x90fd9ffffe88755e:2953,205,4)	
2021-12-16 16:31:23.795 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x90fd9ffffe88755e/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))	
2021-12-16 16:31:23.795 - debug: zigbee.0 (26219) Exception in readState of '0x90fd9ffffe88755e' - error : 'Error: Read 0x90fd9ffffe88755e/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))'	
2021-12-16 16:31:23.795 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x90fd9ffffe88755e/1 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:23.796 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x90fd9ffffe88755e:2953/1 (0,0,6)	
2021-12-16 16:31:23.796 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":2953,"destendpoint":1,"srcendpoint":1,"clusterid":0,"transid":82,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,27,0,0,0]}}	
2021-12-16 16:31:23.797 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,137,11,1,1,0,0,82,0,30,5,16,27,0,0,0,234]	
2021-12-16 16:31:23.802 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:23.803 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:23.803 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:23.803 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:23.804 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:24.125 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,77,70]	
2021-12-16 16:31:24.125 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,77,70]	
2021-12-16 16:31:24.125 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,77] - 70	
2021-12-16 16:31:24.127 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":77}	
2021-12-16 16:31:24.127 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:24.127 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x000b57fffe4436b0:57723,205,4)	
2021-12-16 16:31:24.128 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x000b57fffe4436b0/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))	
2021-12-16 16:31:24.128 - debug: zigbee.0 (26219) Exception in readState of '0x000b57fffe4436b0' - error : 'Error: Read 0x000b57fffe4436b0/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))'	
2021-12-16 16:31:24.129 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x000b57fffe4436b0/1 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:24.129 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x000b57fffe4436b0:57723/1 (0,0,6)	
2021-12-16 16:31:24.129 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":57723,"destendpoint":1,"srcendpoint":1,"clusterid":0,"transid":83,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,28,0,0,0]}}	
2021-12-16 16:31:24.130 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,123,225,1,1,0,0,83,0,30,5,16,28,0,0,0,244]	
2021-12-16 16:31:24.135 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:24.135 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:24.136 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:24.136 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:24.137 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:24.182 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,75,64]	
2021-12-16 16:31:24.182 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,75,64]	
2021-12-16 16:31:24.182 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,75] - 64	
2021-12-16 16:31:24.183 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":75}	
2021-12-16 16:31:24.183 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:24.183 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002b805e3:39725,205,4)	
2021-12-16 16:31:24.183 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x00158d0002b805e3/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))	
2021-12-16 16:31:24.184 - debug: zigbee.0 (26219) Exception in readState of '0x00158d0002b805e3' - error : 'Error: Read 0x00158d0002b805e3/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))'	
2021-12-16 16:31:24.184 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x00158d0002b805e3/1 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:24.185 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002b805e3:39725/1 (0,0,6)	
2021-12-16 16:31:24.185 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":39725,"destendpoint":1,"srcendpoint":1,"clusterid":0,"transid":84,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,29,0,0,0]}}	
2021-12-16 16:31:24.185 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,45,155,1,1,0,0,84,0,30,5,16,29,0,0,0,222]	
2021-12-16 16:31:24.190 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:24.191 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:24.191 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:24.191 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:24.192 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:24.218 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,76,71]	
2021-12-16 16:31:24.219 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,76,71]	
2021-12-16 16:31:24.219 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,76] - 71	
2021-12-16 16:31:24.219 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":76}	
2021-12-16 16:31:24.219 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:24.219 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002b7d6a9:19263,205,4)	
2021-12-16 16:31:24.220 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x00158d0002b7d6a9/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))	
2021-12-16 16:31:24.220 - debug: zigbee.0 (26219) Exception in readState of '0x00158d0002b7d6a9' - error : 'Error: Read 0x00158d0002b7d6a9/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))'	
2021-12-16 16:31:24.220 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x00158d0002b7d6a9/1 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:24.221 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x00158d0002b7d6a9:19263/1 (0,0,6)	
2021-12-16 16:31:24.221 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":19263,"destendpoint":1,"srcendpoint":1,"clusterid":0,"transid":85,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,30,0,0,0]}}	
2021-12-16 16:31:24.221 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,63,75,1,1,0,0,85,0,30,5,16,30,0,0,0,30]	
2021-12-16 16:31:24.226 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:24.227 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:24.227 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:24.227 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:24.228 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:24.399 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,81,90]	
2021-12-16 16:31:24.401 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,81,90]	
2021-12-16 16:31:24.402 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,81] - 90	
2021-12-16 16:31:24.403 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":81}	
2021-12-16 16:31:24.405 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:24.407 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x90fd9ffffe02c40f:56799,205,4)	
2021-12-16 16:31:24.409 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x90fd9ffffe02c40f/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))	
2021-12-16 16:31:24.411 - debug: zigbee.0 (26219) Exception in readState of '0x90fd9ffffe02c40f' - error : 'Error: Read 0x90fd9ffffe02c40f/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))'	
2021-12-16 16:31:24.413 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x90fd9ffffe02c40f/1 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:31:24.414 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x90fd9ffffe02c40f:56799/1 (0,0,6)	
2021-12-16 16:31:24.415 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":56799,"destendpoint":1,"srcendpoint":1,"clusterid":0,"transid":86,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,31,0,0,0]}}	
2021-12-16 16:31:24.417 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,223,221,1,1,0,0,86,0,30,5,16,31,0,0,0,106]	
2021-12-16 16:31:24.425 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:31:24.426 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:31:24.427 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:31:24.428 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:31:24.429 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:24.491 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,82,89]	
2021-12-16 16:31:24.491 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,82,89]	
2021-12-16 16:31:24.491 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,82] - 89	
2021-12-16 16:31:24.492 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":82}	
2021-12-16 16:31:24.492 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:24.492 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x90fd9ffffe88755e:2953,205,0)	
2021-12-16 16:31:24.492 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x90fd9ffffe88755e/1 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))	
2021-12-16 16:31:24.492 - warn: zigbee.0 (26219) Failed to ping 0x90fd9ffffe88755e TRADFRI bulb E27 WS opal 980lm	
2021-12-16 16:31:24.493 - debug: zigbee.0 (26219) Publish available for 0x90fd9ffffe88755e = false	
2021-12-16 16:31:24.495 - debug: zigbee.0 (26219) Publish LQ for 0x90fd9ffffe88755e = 0	
2021-12-16 16:31:24.506 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,80,91]	
2021-12-16 16:31:24.506 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,80,91]	
2021-12-16 16:31:24.506 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,80] - 91	
2021-12-16 16:31:24.507 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":80}	
2021-12-16 16:31:24.510 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:24.511 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002b7d87c:35436,205,0)	
2021-12-16 16:31:24.511 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x00158d0002b7d87c/1 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))	
2021-12-16 16:31:24.511 - warn: zigbee.0 (26219) Failed to ping 0x00158d0002b7d87c lumi.light.aqcn02	
2021-12-16 16:31:24.511 - debug: zigbee.0 (26219) Publish available for 0x00158d0002b7d87c = false	
2021-12-16 16:31:24.513 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002b7d87c = 0	
2021-12-16 16:31:24.679 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,83,88]	
2021-12-16 16:31:24.679 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,83,88]	
2021-12-16 16:31:24.680 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,83] - 88	
2021-12-16 16:31:24.680 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":83}	
2021-12-16 16:31:24.680 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:24.680 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x000b57fffe4436b0:57723,205,0)	
2021-12-16 16:31:24.681 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x000b57fffe4436b0/1 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))	
2021-12-16 16:31:24.681 - warn: zigbee.0 (26219) Failed to ping 0x000b57fffe4436b0 TRADFRI bulb E27 WS opal 980lm	
2021-12-16 16:31:24.681 - debug: zigbee.0 (26219) Publish available for 0x000b57fffe4436b0 = false	
2021-12-16 16:31:24.682 - debug: zigbee.0 (26219) Publish LQ for 0x000b57fffe4436b0 = 0	
2021-12-16 16:31:24.724 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,85,94]	
2021-12-16 16:31:24.724 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,85,94]	
2021-12-16 16:31:24.724 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,85] - 94	
2021-12-16 16:31:24.724 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":85}	
2021-12-16 16:31:24.725 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:24.726 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002b7d6a9:19263,205,0)	
2021-12-16 16:31:24.726 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x00158d0002b7d6a9/1 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))	
2021-12-16 16:31:24.726 - warn: zigbee.0 (26219) Failed to ping 0x00158d0002b7d6a9 lumi.light.aqcn02	
2021-12-16 16:31:24.726 - debug: zigbee.0 (26219) Publish available for 0x00158d0002b7d6a9 = false	
2021-12-16 16:31:24.727 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002b7d6a9 = 0	
2021-12-16 16:31:24.988 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,86,93]	
2021-12-16 16:31:24.988 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,86,93]	
2021-12-16 16:31:24.989 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,86] - 93	
2021-12-16 16:31:24.989 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":86}	
2021-12-16 16:31:24.989 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:24.989 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x90fd9ffffe02c40f:56799,205,0)	
2021-12-16 16:31:24.989 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x90fd9ffffe02c40f/1 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))	
2021-12-16 16:31:24.990 - warn: zigbee.0 (26219) Failed to ping 0x90fd9ffffe02c40f TRADFRI bulb E27 WS opal 980lm	
2021-12-16 16:31:24.990 - debug: zigbee.0 (26219) Publish available for 0x90fd9ffffe02c40f = false	
2021-12-16 16:31:24.991 - debug: zigbee.0 (26219) Publish LQ for 0x90fd9ffffe02c40f = 0	
2021-12-16 16:31:25.018 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,205,1,84,95]	
2021-12-16 16:31:25.019 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,205,1,84,95]	
2021-12-16 16:31:25.019 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [205,1,84] - 95	
2021-12-16 16:31:25.019 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":205,"endpoint":1,"transid":84}	
2021-12-16 16:31:25.019 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:31:25.019 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x00158d0002b805e3:39725,205,0)	
2021-12-16 16:31:25.020 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x00158d0002b805e3/1 genBasic(["zclVersion"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":true,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'No network route' (205))	
2021-12-16 16:31:25.020 - warn: zigbee.0 (26219) Failed to ping 0x00158d0002b805e3 lumi.light.aqcn02	
2021-12-16 16:31:25.020 - debug: zigbee.0 (26219) Publish available for 0x00158d0002b805e3 = false	
2021-12-16 16:31:25.021 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002b805e3 = 0	
2021-12-16 16:32:02.144 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002b54a17 lumi.weather was last seen '425.632' seconds ago.	
2021-12-16 16:32:02.145 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002130d3b lumi.sensor_switch.aq2 was last seen '176.527' seconds ago.	
2021-12-16 16:32:02.146 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002130f3a lumi.sensor_switch.aq2 was last seen '2950.308' seconds ago.	
2021-12-16 16:32:02.146 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002f8d76c lumi.ctrl_neutral1 was last seen '7951110.349' seconds ago.	
2021-12-16 16:32:02.147 - debug: zigbee.0 (26219) Publish available for 0x00158d0002f8d76c = false	
2021-12-16 16:32:02.149 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002f8d76c = 0	
2021-12-16 16:32:02.151 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000274f4de lumi.sensor_magnet.aq2 was last seen '661.465' seconds ago.	
2021-12-16 16:32:02.152 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002135d9b lumi.sensor_switch.aq2 was last seen '3934.966' seconds ago.	
2021-12-16 16:32:02.152 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000274f4bf lumi.sensor_magnet.aq2 was last seen '2695.197' seconds ago.	
2021-12-16 16:32:02.153 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000271c4b7 lumi.sensor_wleak.aq1 was last seen '2459.082' seconds ago.	
2021-12-16 16:32:02.153 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002f8d5b4 lumi.ctrl_neutral1 was last seen '7951134.811' seconds ago.	
2021-12-16 16:32:02.153 - debug: zigbee.0 (26219) Publish available for 0x00158d0002f8d5b4 = false	
2021-12-16 16:32:02.155 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002f8d5b4 = 0	
2021-12-16 16:32:02.158 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002e34b33 lumi.ctrl_neutral1 was last seen '7951116.711' seconds ago.	
2021-12-16 16:32:02.158 - debug: zigbee.0 (26219) Publish available for 0x00158d0002e34b33 = false	
2021-12-16 16:32:02.160 - debug: zigbee.0 (26219) Publish LQ for 0x00158d0002e34b33 = 0	
2021-12-16 16:32:02.165 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000521d656 lumi.switch.b1lacn02 was last seen '7951109.829' seconds ago.	
2021-12-16 16:32:02.165 - debug: zigbee.0 (26219) Publish available for 0x00158d000521d656 = false	
2021-12-16 16:32:02.167 - debug: zigbee.0 (26219) Publish LQ for 0x00158d000521d656 = 0	
2021-12-16 16:32:02.170 - debug: zigbee.0 (26219) Non-pingable device 0x00158d00028aee30 lumi.sensor_cube.aqgl01 was last seen '2335.914' seconds ago.	
2021-12-16 16:32:02.176 - debug: zigbee.0 (26219) Non-pingable device 0x00158d00021369f3 lumi.sensor_switch.aq2 was last seen '2612.721' seconds ago.	
2021-12-16 16:32:02.176 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002b54752 lumi.weather was last seen '735.139' seconds ago.	
2021-12-16 16:32:02.177 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000274f643 lumi.sensor_magnet.aq2 was last seen '2809.877' seconds ago.	
2021-12-16 16:32:02.178 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000274f64d lumi.sensor_magnet.aq2 was last seen '163.71' seconds ago.	
2021-12-16 16:32:02.178 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002b51c42 lumi.weather was last seen '354.374' seconds ago.	
2021-12-16 16:32:02.178 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000274f4f7 lumi.sensor_magnet.aq2 was last seen '4840.161' seconds ago.	
2021-12-16 16:32:02.179 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000274f4d3 lumi.sensor_magnet.aq2 was last seen '1562.456' seconds ago.	
2021-12-16 16:32:02.187 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002722af7 lumi.sensor_magnet.aq2 was last seen '4154.959' seconds ago.	
2021-12-16 16:32:02.187 - debug: zigbee.0 (26219) Non-pingable device 0x847127fffed62092 TS0601 was last seen '3233.021' seconds ago.	
2021-12-16 16:32:02.188 - debug: zigbee.0 (26219) Non-pingable device 0x847127fffed0a598 TS0601 was last seen '733.523' seconds ago.	
2021-12-16 16:32:02.190 - debug: zigbee.0 (26219) Non-pingable device 0x847127fffecfc657 TS0601 was last seen '347.216' seconds ago.	
2021-12-16 16:32:02.191 - debug: zigbee.0 (26219) Non-pingable device 0x000d6ffffe2cd4b8 FYRTUR block-out roller blind was last seen '864867.405' seconds ago.	
2021-12-16 16:32:02.191 - debug: zigbee.0 (26219) Publish available for 0x000d6ffffe2cd4b8 = false	
2021-12-16 16:32:02.194 - debug: zigbee.0 (26219) Publish LQ for 0x000d6ffffe2cd4b8 = 0	
2021-12-16 16:32:20.854 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,31,68,129,0,0,6,0]	
2021-12-16 16:32:20.855 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,31,68,129,0,0,6,0]	
2021-12-16 16:32:20.857 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [142,241,1,1,0,78,0,184,44,140,0,0,11,24,216,10,0,0,16,0,0,0,16,1]	
2021-12-16 16:32:20.857 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,31,68,129,0,0,6,0,142,241,1,1,0,78,0,184,44,140,0,0,11,24,216,10,0,0,16,0,0,0,16,1]	
2021-12-16 16:32:20.859 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [245,234,27,49]	
2021-12-16 16:32:20.859 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,31,68,129,0,0,6,0,142,241,1,1,0,78,0,184,44,140,0,0,11,24,216,10,0,0,16,0,0,0,16,1,245,234,27,49]	
2021-12-16 16:32:20.860 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 31 - 2 - 4 - 129 - [0,0,6,0,142,241,1,1,0,78,0,184,44,140,0,0,11,24,216,10,0,0,16,0,0,0,16,1,245,234,27] - 49	
2021-12-16 16:32:20.861 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - incomingMsg - {"groupid":0,"clusterid":6,"srcaddr":61838,"srcendpoint":1,"dstendpoint":1,"wasbroadcast":0,"linkquality":78,"securityuse":0,"timestamp":9186488,"transseqnumber":0,"len":11,"data":{"type":"Buffer","data":[24,216,10,0,0,16,0,0,0,16,1]}}	
2021-12-16 16:32:20.862 - debug: zigbee.0 (26219) zigbee-herdsman:controller:log Received 'zcl' data '{"frame":{"Header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":216,"manufacturerCode":null,"commandIdentifier":10},"Payload":[{"attrId":0,"dataType":16,"attrData":0},{"attrId":0,"dataType":16,"attrData":1}],"Command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}},"address":61838,"endpoint":1,"linkquality":78,"groupID":0,"wasBroadcast":false,"destinationEndpoint":1}'	
2021-12-16 16:32:20.863 - debug: zigbee.0 (26219) handleMessage. {"type":"attributeReport","device":{"ID":3,"_type":"EndDevice","_ieeeAddr":"0x00158d0002130d3b","_networkAddress":61838,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":61838,"deviceIeeeAddress":"0x00158d0002130d3b","clusters":{"genBasic":{"attributes":{"65281":{"1":3005,"3":27,"4":17320,"5":48,"6":[0,1],"10":47504},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_switch.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639668740863,"_linkquality":78},"endpoint":"[Circular]","data":{"onOff":1},"linkquality":78,"groupID":0,"cluster":"genOnOff","meta":{"zclTransactionSequenceNumber":216,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:32:20.864 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:20.864 - debug: zigbee.0 (26219) Received Zigbee message from '0x00158d0002130d3b', type 'attributeReport', cluster 'genOnOff', data '{"onOff":1}' from endpoint 1 with groupID 0	
2021-12-16 16:32:20.865 - debug: zigbee.0 (26219) Type attributeReport device {"type":"device","device":{"ID":3,"_type":"EndDevice","_ieeeAddr":"0x00158d0002130d3b","_networkAddress":61838,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":61838,"deviceIeeeAddress":"0x00158d0002130d3b","clusters":{"genBasic":{"attributes":{"65281":{"1":3005,"3":27,"4":17320,"5":48,"6":[0,1],"10":47504},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_switch.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639668740863,"_linkquality":78},"mapped":{"zigbeeModel":["lumi.sensor_switch.aq2","lumi.remote.b1acn01"],"model":"WXKG11LM","vendor":"Xiaomi","description":"Aqara wireless switch","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"enum","name":"action","property":"action","access":1,"values":["single","double","triple","quadruple","hold","release"],"description":"Triggered action (e.g. a button click)"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genMultistateInput","type":["attributeReport"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genMultistateInput","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]}],"toZigbee":[],"options":["[Circular]"]},"name":"0x00158d0002130d3b"} incoming event: {"type":"attributeReport","device":{"ID":3,"_type":"EndDevice","_ieeeAddr":"0x00158d0002130d3b","_networkAddress":61838,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":61838,"deviceIeeeAddress":"0x00158d0002130d3b","clusters":{"genBasic":{"attributes":{"65281":{"1":3005,"3":27,"4":17320,"5":48,"6":[0,1],"10":47504},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_switch.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639668740863,"_linkquality":78},"endpoint":"[Circular]","data":{"onOff":1},"linkquality":78,"groupID":0,"cluster":"genOnOff","meta":{"zclTransactionSequenceNumber":216,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:32:20.880 - debug: zigbee.0 (26219) Publish {"action":"single"} to "00158d0002130d3b"	
2021-12-16 16:32:20.882 - debug: zigbee.0 (26219) Publish {"click":"single"} to "00158d0002130d3b"	
2021-12-16 16:32:20.896 - info: javascript.0 (25312) script.js.common.Lautsprecher: Knopf wurde gedrückt	
2021-12-16 16:32:20.906 - debug: zigbee.0 (26219) User stateChange zigbee.0.7cb03eaa00acb990.state {"val":true,"ack":false,"ts":1639668740902,"q":0,"c":"script.js.common.Lautsprecher","from":"system.adapter.javascript.0","user":"system.user.admin","lc":1639668740902}	
2021-12-16 16:32:20.913 - debug: zigbee.0 (26219) Change state 'state' at device 0x7cb03eaa00acb990 type 'AB3257001NJ'	
2021-12-16 16:32:20.916 - debug: zigbee.0 (26219) entity: {"type":"device","device":{"ID":4,"_type":"Router","_ieeeAddr":"0x7cb03eaa00acb990","_networkAddress":47504,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":47504,"deviceIeeeAddress":"0x7cb03eaa00acb990","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668554590},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["Plug 01"],"model":"AB3257001NJ","description":"Smart+ plug","vendor":"OSRAM","whiteLabel":[{"vendor":"LEDVANCE","model":"AB3257001NJ"}],"ota":{},"options":[]},"endpoint":"[Circular]","endpoints":"[Circular]","name":"0x7cb03eaa00acb990"}	
2021-12-16 16:32:20.916 - debug: zigbee.0 (26219) Mapped Model: {"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["Plug 01"],"model":"AB3257001NJ","description":"Smart+ plug","vendor":"OSRAM","whiteLabel":[{"vendor":"LEDVANCE","model":"AB3257001NJ"}],"ota":{},"options":[]}	
2021-12-16 16:32:20.917 - debug: zigbee.0 (26219) convert state, "ON", {"state":"ON"}	
2021-12-16 16:32:20.918 - debug: zigbee.0 (26219) target: {"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":47504,"deviceIeeeAddress":"0x7cb03eaa00acb990","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}	
2021-12-16 16:32:20.920 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Command 0x7cb03eaa00acb990/3 genOnOff.on({}, {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:32:20.920 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00acb990:47504/3 (0,0,1)	
2021-12-16 16:32:20.921 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":47504,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":87,"options":0,"radius":30,"len":3,"data":{"type":"Buffer","data":[1,32,1]}}	
2021-12-16 16:32:20.922 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,13,36,1,144,185,3,1,6,0,87,0,30,3,1,32,1,111]	
2021-12-16 16:32:20.931 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:32:20.931 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:32:20.932 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:32:20.932 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:32:20.933 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:20.958 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,87,112]	
2021-12-16 16:32:20.959 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,87,112]	
2021-12-16 16:32:20.959 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,87] - 112	
2021-12-16 16:32:20.959 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":87}	
2021-12-16 16:32:20.960 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:20.960 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00acb990:47504,225,0)	
2021-12-16 16:32:22.961 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00acb990:47504/3 (0,1,1)	
2021-12-16 16:32:22.962 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":47504,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":88,"options":0,"radius":30,"len":3,"data":{"type":"Buffer","data":[1,32,1]}}	
2021-12-16 16:32:22.964 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,13,36,1,144,185,3,1,6,0,88,0,30,3,1,32,1,96]	
2021-12-16 16:32:22.972 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:32:22.973 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:32:22.974 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:32:22.975 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:32:22.976 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:22.995 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,88,127]	
2021-12-16 16:32:22.996 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,88,127]	
2021-12-16 16:32:22.997 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,88] - 127	
2021-12-16 16:32:22.998 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":88}	
2021-12-16 16:32:22.998 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:22.999 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00acb990:47504,225,1)	
2021-12-16 16:32:25.003 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00acb990:47504/3 (0,2,1)	
2021-12-16 16:32:25.005 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":47504,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":89,"options":0,"radius":30,"len":3,"data":{"type":"Buffer","data":[1,32,1]}}	
2021-12-16 16:32:25.006 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,13,36,1,144,185,3,1,6,0,89,0,30,3,1,32,1,97]	
2021-12-16 16:32:25.014 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:32:25.015 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:32:25.016 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:32:25.017 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:32:25.018 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:25.057 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,89,126]	
2021-12-16 16:32:25.058 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,89,126]	
2021-12-16 16:32:25.059 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,89] - 126	
2021-12-16 16:32:25.060 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":89}	
2021-12-16 16:32:25.061 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:25.062 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00acb990:47504,225,2)	
2021-12-16 16:32:27.066 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00acb990:47504/3 (0,3,1)	
2021-12-16 16:32:27.067 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":47504,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":90,"options":0,"radius":30,"len":3,"data":{"type":"Buffer","data":[1,32,1]}}	
2021-12-16 16:32:27.068 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,13,36,1,144,185,3,1,6,0,90,0,30,3,1,32,1,98]	
2021-12-16 16:32:27.077 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:32:27.078 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:32:27.079 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:32:27.080 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:32:27.081 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:27.106 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,0,1,90,156]	
2021-12-16 16:32:27.107 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,0,1,90,156]	
2021-12-16 16:32:27.108 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [0,1,90] - 156	
2021-12-16 16:32:27.108 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":0,"endpoint":1,"transid":90}	
2021-12-16 16:32:27.109 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:27.150 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,25,68,129,0,0,6,0]	
2021-12-16 16:32:27.151 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,25,68,129,0,0,6,0]	
2021-12-16 16:32:27.153 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [144,185,3,1,0,75,0,199,45,146,0,0,5,24,32,11,1,0,245,234,28,246]	
2021-12-16 16:32:27.154 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,25,68,129,0,0,6,0,144,185,3,1,0,75,0,199,45,146,0,0,5,24,32,11,1,0,245,234,28,246]	
2021-12-16 16:32:27.155 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 25 - 2 - 4 - 129 - [0,0,6,0,144,185,3,1,0,75,0,199,45,146,0,0,5,24,32,11,1,0,245,234,28] - 246	
2021-12-16 16:32:27.156 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - incomingMsg - {"groupid":0,"clusterid":6,"srcaddr":47504,"srcendpoint":3,"dstendpoint":1,"wasbroadcast":0,"linkquality":75,"securityuse":0,"timestamp":9579975,"transseqnumber":0,"len":5,"data":{"type":"Buffer","data":[24,32,11,1,0]}}	
2021-12-16 16:32:27.158 - debug: zigbee.0 (26219) zigbee-herdsman:controller:log Received 'zcl' data '{"frame":{"Header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":32,"manufacturerCode":null,"commandIdentifier":11},"Payload":{"cmdId":1,"statusCode":0},"Command":{"ID":11,"name":"defaultRsp","parameters":[{"name":"cmdId","type":32},{"name":"statusCode","type":32}]}},"address":47504,"endpoint":3,"linkquality":75,"groupID":0,"wasBroadcast":false,"destinationEndpoint":1}'	
2021-12-16 16:32:27.159 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:27.159 - debug: zigbee.0 (26219) convert result {"state":{"state":"ON"}}	
2021-12-16 16:32:27.212 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,27,68,129,0,0,6,0]	
2021-12-16 16:32:27.213 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,27,68,129,0,0,6,0]	
2021-12-16 16:32:27.215 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [144,185,3,1,0,75,0,222,60,146,0,0,7,24,160,10,0,0,16,1,245,234,28,111]	
2021-12-16 16:32:27.216 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,27,68,129,0,0,6,0,144,185,3,1,0,75,0,222,60,146,0,0,7,24,160,10,0,0,16,1,245,234,28,111]	
2021-12-16 16:32:27.217 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 27 - 2 - 4 - 129 - [0,0,6,0,144,185,3,1,0,75,0,222,60,146,0,0,7,24,160,10,0,0,16,1,245,234,28] - 111	
2021-12-16 16:32:27.218 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - incomingMsg - {"groupid":0,"clusterid":6,"srcaddr":47504,"srcendpoint":3,"dstendpoint":1,"wasbroadcast":0,"linkquality":75,"securityuse":0,"timestamp":9583838,"transseqnumber":0,"len":7,"data":{"type":"Buffer","data":[24,160,10,0,0,16,1]}}	
2021-12-16 16:32:27.220 - debug: zigbee.0 (26219) zigbee-herdsman:controller:log Received 'zcl' data '{"frame":{"Header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":160,"manufacturerCode":null,"commandIdentifier":10},"Payload":[{"attrId":0,"dataType":16,"attrData":1}],"Command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}},"address":47504,"endpoint":3,"linkquality":75,"groupID":0,"wasBroadcast":false,"destinationEndpoint":1}'	
2021-12-16 16:32:27.221 - debug: zigbee.0 (26219) handleMessage. {"type":"attributeReport","device":{"ID":4,"_type":"Router","_ieeeAddr":"0x7cb03eaa00acb990","_networkAddress":47504,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":47504,"deviceIeeeAddress":"0x7cb03eaa00acb990","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":1}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668747220,"_linkquality":75},"endpoint":"[Circular]","data":{"onOff":1},"linkquality":75,"groupID":0,"cluster":"genOnOff","meta":{"zclTransactionSequenceNumber":160,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:32:27.222 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:27.223 - debug: zigbee.0 (26219) Received Zigbee message from '0x7cb03eaa00acb990', type 'attributeReport', cluster 'genOnOff', data '{"onOff":1}' from endpoint 3 with groupID 0	
2021-12-16 16:32:27.224 - debug: zigbee.0 (26219) Type attributeReport device {"type":"device","device":{"ID":4,"_type":"Router","_ieeeAddr":"0x7cb03eaa00acb990","_networkAddress":47504,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":47504,"deviceIeeeAddress":"0x7cb03eaa00acb990","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":1}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668747220,"_linkquality":75},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["Plug 01"],"model":"AB3257001NJ","description":"Smart+ plug","vendor":"OSRAM","whiteLabel":[{"vendor":"LEDVANCE","model":"AB3257001NJ"}],"ota":{},"options":[]},"name":"0x7cb03eaa00acb990"} incoming event: {"type":"attributeReport","device":{"ID":4,"_type":"Router","_ieeeAddr":"0x7cb03eaa00acb990","_networkAddress":47504,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":47504,"deviceIeeeAddress":"0x7cb03eaa00acb990","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":1}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668747220,"_linkquality":75},"endpoint":"[Circular]","data":{"onOff":1},"linkquality":75,"groupID":0,"cluster":"genOnOff","meta":{"zclTransactionSequenceNumber":160,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:32:27.226 - debug: zigbee.0 (26219) Publish available for 0x7cb03eaa00acb990 = true	
2021-12-16 16:32:27.229 - debug: zigbee.0 (26219) Publish LQ for 0x7cb03eaa00acb990 = 10	
2021-12-16 16:32:27.233 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa00acb990/3 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:32:27.233 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00acb990:47504/3 (0,0,1)	
2021-12-16 16:32:27.234 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":47504,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":91,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,33,0,0,0]}}	
2021-12-16 16:32:27.235 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,144,185,3,1,6,0,91,0,30,5,16,33,0,0,0,118]	
2021-12-16 16:32:27.248 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:32:27.250 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:32:27.250 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:32:27.251 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:32:27.252 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:27.276 - debug: zigbee.0 (26219) Publish {"state":"ON"} to "7cb03eaa00acb990"	
2021-12-16 16:32:27.294 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,91,124]	
2021-12-16 16:32:27.296 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,91,124]	
2021-12-16 16:32:27.297 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,91] - 124	
2021-12-16 16:32:27.297 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":91}	
2021-12-16 16:32:27.298 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:27.298 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00acb990:47504,225,0)	
2021-12-16 16:32:29.300 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00acb990:47504/3 (0,1,1)	
2021-12-16 16:32:29.302 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":47504,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":92,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,33,0,0,0]}}	
2021-12-16 16:32:29.314 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,144,185,3,1,6,0,92,0,30,5,16,33,0,0,0,113]	
2021-12-16 16:32:29.325 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:32:29.326 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:32:29.327 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:32:29.328 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:32:29.328 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:29.362 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,92,123]	
2021-12-16 16:32:29.363 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,92,123]	
2021-12-16 16:32:29.363 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,92] - 123	
2021-12-16 16:32:29.364 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":92}	
2021-12-16 16:32:29.365 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:29.365 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00acb990:47504,225,1)	
2021-12-16 16:32:31.367 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00acb990:47504/3 (0,2,1)	
2021-12-16 16:32:31.369 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":47504,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":93,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,33,0,0,0]}}	
2021-12-16 16:32:31.370 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,144,185,3,1,6,0,93,0,30,5,16,33,0,0,0,112]	
2021-12-16 16:32:31.379 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:32:31.380 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:32:31.381 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:32:31.382 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:32:31.383 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:31.426 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,93,122]	
2021-12-16 16:32:31.427 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,93,122]	
2021-12-16 16:32:31.428 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,93] - 122	
2021-12-16 16:32:31.429 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":93}	
2021-12-16 16:32:31.430 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:31.431 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00acb990:47504,225,2)	
2021-12-16 16:32:33.432 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00acb990:47504/3 (0,3,1)	
2021-12-16 16:32:33.434 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":47504,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":94,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,33,0,0,0]}}	
2021-12-16 16:32:33.435 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,144,185,3,1,6,0,94,0,30,5,16,33,0,0,0,115]	
2021-12-16 16:32:33.444 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:32:33.445 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:32:33.446 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:32:33.447 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:32:33.447 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:33.483 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,94,121]	
2021-12-16 16:32:33.483 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,94,121]	
2021-12-16 16:32:33.485 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,94] - 121	
2021-12-16 16:32:33.486 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":94}	
2021-12-16 16:32:33.487 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:33.487 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00acb990:47504,225,3)	
2021-12-16 16:32:35.489 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00acb990:47504/3 (0,4,1)	
2021-12-16 16:32:35.490 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":47504,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":95,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,33,0,0,0]}}	
2021-12-16 16:32:35.490 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,144,185,3,1,6,0,95,0,30,5,16,33,0,0,0,114]	
2021-12-16 16:32:35.498 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:32:35.499 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:32:35.499 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:32:35.499 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:32:35.500 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:35.529 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,95,120]	
2021-12-16 16:32:35.529 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,95,120]	
2021-12-16 16:32:35.530 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,95] - 120	
2021-12-16 16:32:35.530 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":95}	
2021-12-16 16:32:35.531 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:35.532 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00acb990:47504,225,4)	
2021-12-16 16:32:35.532 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0x7cb03eaa00acb990/3 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'MAC channel access failure' (225))	
2021-12-16 16:32:35.533 - debug: zigbee.0 (26219) Failed to read state of '0x7cb03eaa00acb990' after reconnect	
2021-12-16 16:32:41.902 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtLqiReq - {"dstaddr":0,"startindex":0}	
2021-12-16 16:32:41.903 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,49,0,0,0,23]	
2021-12-16 16:32:41.906 - debug: zigbee.0 (26219) sendTo "getLibData" to system.adapter.admin.0 from system.adapter.zigbee.0	
2021-12-16 16:32:41.913 - debug: zigbee.0 (26219) getGroups result: {"1":"Deckenleuchte (Schlafzimmer)","2":"Deckenleuchte (Wohnzimmer)"}	
2021-12-16 16:32:41.914 - debug: zigbee.0 (26219) sendTo "getGroups" to system.adapter.admin.0 from system.adapter.zigbee.0	
2021-12-16 16:32:41.916 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,49,0,85,254,50,69,177,0,0,0,26,0,2,47,212,221,66,221,45,212,221,23,74,181,2,0,141,21,0,148,248,18,2,1,170,47,212,221,66,221,45,212,221,59,13,19,2,0,141,21,0,142,241]	
2021-12-16 16:32:41.916 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,49,0,85,254,50,69,177,0,0,0,26,0,2,47,212,221,66,221,45,212,221,23,74,181,2,0,141,21,0,148,248,18,2,1,170,47,212,221,66,221,45,212,221,59,13,19,2,0,141,21,0,142,241]	
2021-12-16 16:32:41.917 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 49 - [0] - 85	
2021-12-16 16:32:41.917 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtLqiReq - {"status":0}	
2021-12-16 16:32:41.918 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50,69,177,0,0,0,26,0,2,47,212,221,66,221,45,212,221,23,74,181,2,0,141,21,0,148,248,18,2,1,170,47,212,221,66,221,45,212,221,59,13,19,2,0,141,21,0,142,241]	
2021-12-16 16:32:41.920 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [18,2,1,170,0]	
2021-12-16 16:32:41.921 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50,69,177,0,0,0,26,0,2,47,212,221,66,221,45,212,221,23,74,181,2,0,141,21,0,148,248,18,2,1,170,47,212,221,66,221,45,212,221,59,13,19,2,0,141,21,0,142,241,18,2,1,170,0]	
2021-12-16 16:32:41.921 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 50 - 2 - 5 - 177 - [0,0,0,26,0,2,47,212,221,66,221,45,212,221,23,74,181,2,0,141,21,0,148,248,18,2,1,170,47,212,221,66,221,45,212,221,59,13,19,2,0,141,21,0,142,241,18,2,1,170] - 0	
2021-12-16 16:32:41.923 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - mgmtLqiRsp - {"srcaddr":0,"status":0,"neighbortableentries":26,"startindex":0,"neighborlqilistcount":2,"neighborlqilist":[{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x00158d0002b54a17","nwkAddr":63636,"deviceType":2,"rxOnWhenIdle":0,"relationship":1,"permitJoin":2,"depth":1,"lqi":170},{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x00158d0002130d3b","nwkAddr":61838,"deviceType":2,"rxOnWhenIdle":0,"relationship":1,"permitJoin":2,"depth":1,"lqi":170}]}	
2021-12-16 16:32:41.923 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:41.924 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtLqiReq - {"dstaddr":0,"startindex":2}	
2021-12-16 16:32:41.925 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,49,0,0,2,21]	
2021-12-16 16:32:41.932 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,49,0,85,254,50]	
2021-12-16 16:32:41.933 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,49,0,85,254,50]	
2021-12-16 16:32:41.933 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 49 - [0] - 85	
2021-12-16 16:32:41.934 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtLqiReq - {"status":0}	
2021-12-16 16:32:41.935 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50]	
2021-12-16 16:32:41.938 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [69,177,0,0,0,26,2,2,47,212,221,66,221,45,212,221,247,244,116,2,0,141,21,0,241,69,18,2,1,111,47,212,221,66,221,45,212,221,108,215,248,2,0,141,21,0,11,40,18,2,1,170,186]	
2021-12-16 16:32:41.938 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50,69,177,0,0,0,26,2,2,47,212,221,66,221,45,212,221,247,244,116,2,0,141,21,0,241,69,18,2,1,111,47,212,221,66,221,45,212,221,108,215,248,2,0,141,21,0,11,40,18,2,1,170,186]	
2021-12-16 16:32:41.941 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 50 - 2 - 5 - 177 - [0,0,0,26,2,2,47,212,221,66,221,45,212,221,247,244,116,2,0,141,21,0,241,69,18,2,1,111,47,212,221,66,221,45,212,221,108,215,248,2,0,141,21,0,11,40,18,2,1,170] - 186	
2021-12-16 16:32:41.942 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - mgmtLqiRsp - {"srcaddr":0,"status":0,"neighbortableentries":26,"startindex":2,"neighborlqilistcount":2,"neighborlqilist":[{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x00158d000274f4f7","nwkAddr":17905,"deviceType":2,"rxOnWhenIdle":0,"relationship":1,"permitJoin":2,"depth":1,"lqi":111},{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x00158d0002f8d76c","nwkAddr":10251,"deviceType":2,"rxOnWhenIdle":0,"relationship":1,"permitJoin":2,"depth":1,"lqi":170}]}	
2021-12-16 16:32:41.943 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:41.943 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtLqiReq - {"dstaddr":0,"startindex":4}	
2021-12-16 16:32:41.944 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,49,0,0,4,19]	
2021-12-16 16:32:41.952 - debug: zigbee.0 (26219) getCoorinatorInfo result: {"installSource":"iobroker.zigbee@1.6.6","channel":"14","port":"/dev/serial/by-id/usb-Texas_Instruments_XDS110__03.00.00.13__Embed_with_CMSIS-DAP_L1100L0A-if00","type":"zStack3x0","revision":20201026,"version":"2-1.2.7.1."}	
2021-12-16 16:32:41.952 - debug: zigbee.0 (26219) sendTo "getCoordinatorInfo" to system.adapter.admin.0 from system.adapter.zigbee.0	
2021-12-16 16:32:41.957 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,49,0,85,254,50,69,177,0,0,0,26,4,2,47,212,221,66,221,45,212,221,58,15,19,2,0,141,21,0,144,237,18,2,1,170,47,212,221,66,221,45,212,221,155,93,19,2,0,141,21,0,132,179,18,2,1,170,99]	
2021-12-16 16:32:41.958 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,49,0,85,254,50,69,177,0,0,0,26,4,2,47,212,221,66,221,45,212,221,58,15,19,2,0,141,21,0,144,237,18,2,1,170,47,212,221,66,221,45,212,221,155,93,19,2,0,141,21,0,132,179,18,2,1,170,99]	
2021-12-16 16:32:41.959 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 49 - [0] - 85	
2021-12-16 16:32:41.959 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtLqiReq - {"status":0}	
2021-12-16 16:32:41.960 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50,69,177,0,0,0,26,4,2,47,212,221,66,221,45,212,221,58,15,19,2,0,141,21,0,144,237,18,2,1,170,47,212,221,66,221,45,212,221,155,93,19,2,0,141,21,0,132,179,18,2,1,170,99]	
2021-12-16 16:32:41.960 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 50 - 2 - 5 - 177 - [0,0,0,26,4,2,47,212,221,66,221,45,212,221,58,15,19,2,0,141,21,0,144,237,18,2,1,170,47,212,221,66,221,45,212,221,155,93,19,2,0,141,21,0,132,179,18,2,1,170] - 99	
2021-12-16 16:32:41.961 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - mgmtLqiRsp - {"srcaddr":0,"status":0,"neighbortableentries":26,"startindex":4,"neighborlqilistcount":2,"neighborlqilist":[{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x00158d0002130f3a","nwkAddr":60816,"deviceType":2,"rxOnWhenIdle":0,"relationship":1,"permitJoin":2,"depth":1,"lqi":170},{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x00158d0002135d9b","nwkAddr":45956,"deviceType":2,"rxOnWhenIdle":0,"relationship":1,"permitJoin":2,"depth":1,"lqi":170}]}	
2021-12-16 16:32:41.961 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:41.962 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtLqiReq - {"dstaddr":0,"startindex":6}	
2021-12-16 16:32:41.962 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,49,0,0,6,17]	
2021-12-16 16:32:41.969 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,49,0,85,254,50,69,177,0,0,0,26,6,2,47,212,221,66,221,45,212,221]	
2021-12-16 16:32:41.969 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,49,0,85,254,50,69,177,0,0,0,26,6,2,47,212,221,66,221,45,212,221]	
2021-12-16 16:32:41.970 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 49 - [0] - 85	
2021-12-16 16:32:41.971 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtLqiReq - {"status":0}	
2021-12-16 16:32:41.971 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50,69,177,0,0,0,26,6,2,47,212,221,66,221,45,212,221]	
2021-12-16 16:32:41.974 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [180,213,248,2,0,141,21,0,49,116,18,2,1,170,47,212,221,66,221,45,212,221,191,244,116,2,0,141,21,0,91,206,18,2,1,100,96]	
2021-12-16 16:32:41.975 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50,69,177,0,0,0,26,6,2,47,212,221,66,221,45,212,221,180,213,248,2,0,141,21,0,49,116,18,2,1,170,47,212,221,66,221,45,212,221,191,244,116,2,0,141,21,0,91,206,18,2,1,100,96]	
2021-12-16 16:32:41.976 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 50 - 2 - 5 - 177 - [0,0,0,26,6,2,47,212,221,66,221,45,212,221,180,213,248,2,0,141,21,0,49,116,18,2,1,170,47,212,221,66,221,45,212,221,191,244,116,2,0,141,21,0,91,206,18,2,1,100] - 96	
2021-12-16 16:32:41.977 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - mgmtLqiRsp - {"srcaddr":0,"status":0,"neighbortableentries":26,"startindex":6,"neighborlqilistcount":2,"neighborlqilist":[{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x00158d0002f8d5b4","nwkAddr":29745,"deviceType":2,"rxOnWhenIdle":0,"relationship":1,"permitJoin":2,"depth":1,"lqi":170},{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x00158d000274f4bf","nwkAddr":52827,"deviceType":2,"rxOnWhenIdle":0,"relationship":1,"permitJoin":2,"depth":1,"lqi":100}]}	
2021-12-16 16:32:41.977 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:41.978 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtLqiReq - {"dstaddr":0,"startindex":8}	
2021-12-16 16:32:41.978 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,49,0,0,8,31]	
2021-12-16 16:32:41.984 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,49,0,85,254,50,69,177,0,0,0,26,8,2]	
2021-12-16 16:32:41.985 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,49,0,85,254,50,69,177,0,0,0,26,8,2]	
2021-12-16 16:32:41.986 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 49 - [0] - 85	
2021-12-16 16:32:41.986 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtLqiReq - {"status":0}	
2021-12-16 16:32:41.987 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50,69,177,0,0,0,26,8,2]	
2021-12-16 16:32:41.990 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [47,212,221,66,221,45,212,221,183,196,113,2,0,141,21,0,165,62,18,2,1,170,47,212,221,66,221,45,212,221,48,238,138,2,0,141,21,0,157,213,18,2,1,83,170]	
2021-12-16 16:32:41.990 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50,69,177,0,0,0,26,8,2,47,212,221,66,221,45,212,221,183,196,113,2,0,141,21,0,165,62,18,2,1,170,47,212,221,66,221,45,212,221,48,238,138,2,0,141,21,0,157,213,18,2,1,83,170]	
2021-12-16 16:32:41.991 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 50 - 2 - 5 - 177 - [0,0,0,26,8,2,47,212,221,66,221,45,212,221,183,196,113,2,0,141,21,0,165,62,18,2,1,170,47,212,221,66,221,45,212,221,48,238,138,2,0,141,21,0,157,213,18,2,1,83] - 170	
2021-12-16 16:32:41.992 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - mgmtLqiRsp - {"srcaddr":0,"status":0,"neighbortableentries":26,"startindex":8,"neighborlqilistcount":2,"neighborlqilist":[{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x00158d000271c4b7","nwkAddr":16037,"deviceType":2,"rxOnWhenIdle":0,"relationship":1,"permitJoin":2,"depth":1,"lqi":170},{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x00158d00028aee30","nwkAddr":54685,"deviceType":2,"rxOnWhenIdle":0,"relationship":1,"permitJoin":2,"depth":1,"lqi":83}]}	
2021-12-16 16:32:41.993 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:41.993 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtLqiReq - {"dstaddr":0,"startindex":10}	
2021-12-16 16:32:41.994 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,49,0,0,10,29]	
2021-12-16 16:32:42.004 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,49,0,85,254,50,69,177,0,0,0,26,10,2,47,212,221,66,221,45,212,221,67,246,116,2,0,141,21,0,211,168,18,2,1,101,47,212,221,66,221,45,212,221,77,246,116,2,0,141,21,0,126,240,18,2,1,67,9]	
2021-12-16 16:32:42.005 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,49,0,85,254,50,69,177,0,0,0,26,10,2,47,212,221,66,221,45,212,221,67,246,116,2,0,141,21,0,211,168,18,2,1,101,47,212,221,66,221,45,212,221,77,246,116,2,0,141,21,0,126,240,18,2,1,67,9]	
2021-12-16 16:32:42.005 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 49 - [0] - 85	
2021-12-16 16:32:42.006 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtLqiReq - {"status":0}	
2021-12-16 16:32:42.006 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50,69,177,0,0,0,26,10,2,47,212,221,66,221,45,212,221,67,246,116,2,0,141,21,0,211,168,18,2,1,101,47,212,221,66,221,45,212,221,77,246,116,2,0,141,21,0,126,240,18,2,1,67,9]	
2021-12-16 16:32:42.007 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 50 - 2 - 5 - 177 - [0,0,0,26,10,2,47,212,221,66,221,45,212,221,67,246,116,2,0,141,21,0,211,168,18,2,1,101,47,212,221,66,221,45,212,221,77,246,116,2,0,141,21,0,126,240,18,2,1,67] - 9	
2021-12-16 16:32:42.008 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - mgmtLqiRsp - {"srcaddr":0,"status":0,"neighbortableentries":26,"startindex":10,"neighborlqilistcount":2,"neighborlqilist":[{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x00158d000274f643","nwkAddr":43219,"deviceType":2,"rxOnWhenIdle":0,"relationship":1,"permitJoin":2,"depth":1,"lqi":101},{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x00158d000274f64d","nwkAddr":61566,"deviceType":2,"rxOnWhenIdle":0,"relationship":1,"permitJoin":2,"depth":1,"lqi":67}]}	
2021-12-16 16:32:42.020 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:42.020 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtLqiReq - {"dstaddr":0,"startindex":12}	
2021-12-16 16:32:42.021 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,49,0,0,12,27]	
2021-12-16 16:32:42.077 - debug: zigbee.0 (26219) List of ports: [{"comName":"/dev/ttyACM0"},{"comName":"/dev/ttyACM1"},{"comName":"/dev/ttyS0"},{"comName":"/dev/ttyAMA0"}]	
2021-12-16 16:32:42.078 - debug: zigbee.0 (26219) sendTo "listUart" to system.adapter.admin.0 from system.adapter.zigbee.0	
2021-12-16 16:32:42.085 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,49,0,85,254,50,69,177,0,0,0,26,12,2,47,212,221,66,221,45,212,221,243,105,19,2,0,141,21,0,122,16,18,2,1,170,47,212,221,66,221,45,212,221,66,28,181,2,0,141,21,0,109,194,18,2,1,170,117]	
2021-12-16 16:32:42.086 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,49,0,85,254,50,69,177,0,0,0,26,12,2,47,212,221,66,221,45,212,221,243,105,19,2,0,141,21,0,122,16,18,2,1,170,47,212,221,66,221,45,212,221,66,28,181,2,0,141,21,0,109,194,18,2,1,170,117]	
2021-12-16 16:32:42.086 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 49 - [0] - 85	
2021-12-16 16:32:42.087 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtLqiReq - {"status":0}	
2021-12-16 16:32:42.087 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50,69,177,0,0,0,26,12,2,47,212,221,66,221,45,212,221,243,105,19,2,0,141,21,0,122,16,18,2,1,170,47,212,221,66,221,45,212,221,66,28,181,2,0,141,21,0,109,194,18,2,1,170,117]	
2021-12-16 16:32:42.088 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 50 - 2 - 5 - 177 - [0,0,0,26,12,2,47,212,221,66,221,45,212,221,243,105,19,2,0,141,21,0,122,16,18,2,1,170,47,212,221,66,221,45,212,221,66,28,181,2,0,141,21,0,109,194,18,2,1,170] - 117	
2021-12-16 16:32:42.088 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - mgmtLqiRsp - {"srcaddr":0,"status":0,"neighbortableentries":26,"startindex":12,"neighborlqilistcount":2,"neighborlqilist":[{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x00158d00021369f3","nwkAddr":4218,"deviceType":2,"rxOnWhenIdle":0,"relationship":1,"permitJoin":2,"depth":1,"lqi":170},{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x00158d0002b51c42","nwkAddr":49773,"deviceType":2,"rxOnWhenIdle":0,"relationship":1,"permitJoin":2,"depth":1,"lqi":170}]}	
2021-12-16 16:32:42.088 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:42.089 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtLqiReq - {"dstaddr":0,"startindex":14}	
2021-12-16 16:32:42.089 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,49,0,0,14,25]	
2021-12-16 16:32:42.099 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,49,0,85,254,50,69,177,0,0,0,26,14,2,47,212,221,66,221,45,212,221,222,244,116,2,0,141,21,0,187,209,18,2,1,134,47,212,221,66,221,45,212,221,211,244,116,2,0,141,21,0,162,173,18,2,1,112,78]	
2021-12-16 16:32:42.100 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,49,0,85,254,50,69,177,0,0,0,26,14,2,47,212,221,66,221,45,212,221,222,244,116,2,0,141,21,0,187,209,18,2,1,134,47,212,221,66,221,45,212,221,211,244,116,2,0,141,21,0,162,173,18,2,1,112,78]	
2021-12-16 16:32:42.100 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 49 - [0] - 85	
2021-12-16 16:32:42.100 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtLqiReq - {"status":0}	
2021-12-16 16:32:42.101 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50,69,177,0,0,0,26,14,2,47,212,221,66,221,45,212,221,222,244,116,2,0,141,21,0,187,209,18,2,1,134,47,212,221,66,221,45,212,221,211,244,116,2,0,141,21,0,162,173,18,2,1,112,78]	
2021-12-16 16:32:42.101 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 50 - 2 - 5 - 177 - [0,0,0,26,14,2,47,212,221,66,221,45,212,221,222,244,116,2,0,141,21,0,187,209,18,2,1,134,47,212,221,66,221,45,212,221,211,244,116,2,0,141,21,0,162,173,18,2,1,112] - 78	
2021-12-16 16:32:42.102 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - mgmtLqiRsp - {"srcaddr":0,"status":0,"neighbortableentries":26,"startindex":14,"neighborlqilistcount":2,"neighborlqilist":[{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x00158d000274f4de","nwkAddr":53691,"deviceType":2,"rxOnWhenIdle":0,"relationship":1,"permitJoin":2,"depth":1,"lqi":134},{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x00158d000274f4d3","nwkAddr":44450,"deviceType":2,"rxOnWhenIdle":0,"relationship":1,"permitJoin":2,"depth":1,"lqi":112}]}	
2021-12-16 16:32:42.102 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:42.103 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtLqiReq - {"dstaddr":0,"startindex":16}	
2021-12-16 16:32:42.103 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,49,0,0,16,7]	
2021-12-16 16:32:42.108 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,49,0,85,254,50,69,177,0,0,0,26,16,2]	
2021-12-16 16:32:42.109 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,49,0,85,254,50,69,177,0,0,0,26,16,2]	
2021-12-16 16:32:42.109 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 49 - [0] - 85	
2021-12-16 16:32:42.110 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtLqiReq - {"status":0}	
2021-12-16 16:32:42.110 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50,69,177,0,0,0,26,16,2]	
2021-12-16 16:32:42.113 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [47,212,221,66,221,45,212,221,157,158,1,10,170,62,176,124,12,126,41,2,255,54,47,212,221,66,221,45,212,221,144,185]	
2021-12-16 16:32:42.114 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50,69,177,0,0,0,26,16,2,47,212,221,66,221,45,212,221,157,158,1,10,170,62,176,124,12,126,41,2,255,54,47,212,221,66,221,45,212,221,144,185]	
2021-12-16 16:32:42.116 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [172,0,170,62,176,124,144,185,41,2,255,68,106]	
2021-12-16 16:32:42.117 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50,69,177,0,0,0,26,16,2,47,212,221,66,221,45,212,221,157,158,1,10,170,62,176,124,12,126,41,2,255,54,47,212,221,66,221,45,212,221,144,185,172,0,170,62,176,124,144,185,41,2,255,68,106]	
2021-12-16 16:32:42.118 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 50 - 2 - 5 - 177 - [0,0,0,26,16,2,47,212,221,66,221,45,212,221,157,158,1,10,170,62,176,124,12,126,41,2,255,54,47,212,221,66,221,45,212,221,144,185,172,0,170,62,176,124,144,185,41,2,255,68] - 106	
2021-12-16 16:32:42.119 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - mgmtLqiRsp - {"srcaddr":0,"status":0,"neighbortableentries":26,"startindex":16,"neighborlqilistcount":2,"neighborlqilist":[{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x7cb03eaa0a019e9d","nwkAddr":32268,"deviceType":1,"rxOnWhenIdle":2,"relationship":2,"permitJoin":2,"depth":255,"lqi":54},{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x7cb03eaa00acb990","nwkAddr":47504,"deviceType":1,"rxOnWhenIdle":2,"relationship":2,"permitJoin":2,"depth":255,"lqi":68}]}	
2021-12-16 16:32:42.120 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:42.120 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtLqiReq - {"dstaddr":0,"startindex":18}	
2021-12-16 16:32:42.125 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,49,0,0,18,5]	
2021-12-16 16:32:42.129 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,49,0,85,254,50]	
2021-12-16 16:32:42.130 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,49,0,85,254,50]	
2021-12-16 16:32:42.131 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 49 - [0] - 85	
2021-12-16 16:32:42.131 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtLqiReq - {"status":0}	
2021-12-16 16:32:42.132 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50]	
2021-12-16 16:32:42.135 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [69,177,0,0,0,26,18,2,47,212,221,66,221,45,212,221,207,241,78,14,236,56,193,164,245,234,41,2,255,75,47,212,221,66,221,45,212,221,43,130]	
2021-12-16 16:32:42.135 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50,69,177,0,0,0,26,18,2,47,212,221,66,221,45,212,221,207,241,78,14,236,56,193,164,245,234,41,2,255,75,47,212,221,66,221,45,212,221,43,130]	
2021-12-16 16:32:42.151 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [226,76,147,56,193,164,96,99,41,2,255,64,221]	
2021-12-16 16:32:42.151 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50,69,177,0,0,0,26,18,2,47,212,221,66,221,45,212,221,207,241,78,14,236,56,193,164,245,234,41,2,255,75,47,212,221,66,221,45,212,221,43,130,226,76,147,56,193,164,96,99,41,2,255,64,221]	
2021-12-16 16:32:42.152 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 50 - 2 - 5 - 177 - [0,0,0,26,18,2,47,212,221,66,221,45,212,221,207,241,78,14,236,56,193,164,245,234,41,2,255,75,47,212,221,66,221,45,212,221,43,130,226,76,147,56,193,164,96,99,41,2,255,64] - 221	
2021-12-16 16:32:42.152 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - mgmtLqiRsp - {"srcaddr":0,"status":0,"neighbortableentries":26,"startindex":18,"neighborlqilistcount":2,"neighborlqilist":[{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0xa4c138ec0e4ef1cf","nwkAddr":60149,"deviceType":1,"rxOnWhenIdle":2,"relationship":2,"permitJoin":2,"depth":255,"lqi":75},{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0xa4c138934ce2822b","nwkAddr":25440,"deviceType":1,"rxOnWhenIdle":2,"relationship":2,"permitJoin":2,"depth":255,"lqi":64}]}	
2021-12-16 16:32:42.152 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:42.153 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtLqiReq - {"dstaddr":0,"startindex":20}	
2021-12-16 16:32:42.153 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,49,0,0,20,3]	
2021-12-16 16:32:42.220 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,49,0,85,254,50,69,177,0,0,0,26,20,2,47,212,221,66,221,45,212,221,9,88,2,10,170,62,176,124,170,72,41,2,255,44,47,212,221,66,221,45,212,221,50,117,12,0,0,38,24,132,140,221,41,2,255,51,150]	
2021-12-16 16:32:42.221 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,49,0,85,254,50,69,177,0,0,0,26,20,2,47,212,221,66,221,45,212,221,9,88,2,10,170,62,176,124,170,72,41,2,255,44,47,212,221,66,221,45,212,221,50,117,12,0,0,38,24,132,140,221,41,2,255,51,150]	
2021-12-16 16:32:42.221 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 49 - [0] - 85	
2021-12-16 16:32:42.221 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtLqiReq - {"status":0}	
2021-12-16 16:32:42.222 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50,69,177,0,0,0,26,20,2,47,212,221,66,221,45,212,221,9,88,2,10,170,62,176,124,170,72,41,2,255,44,47,212,221,66,221,45,212,221,50,117,12,0,0,38,24,132,140,221,41,2,255,51,150]	
2021-12-16 16:32:42.222 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 50 - 2 - 5 - 177 - [0,0,0,26,20,2,47,212,221,66,221,45,212,221,9,88,2,10,170,62,176,124,170,72,41,2,255,44,47,212,221,66,221,45,212,221,50,117,12,0,0,38,24,132,140,221,41,2,255,51] - 150	
2021-12-16 16:32:42.223 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - mgmtLqiRsp - {"srcaddr":0,"status":0,"neighbortableentries":26,"startindex":20,"neighborlqilistcount":2,"neighborlqilist":[{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x7cb03eaa0a025809","nwkAddr":18602,"deviceType":1,"rxOnWhenIdle":2,"relationship":2,"permitJoin":2,"depth":255,"lqi":44},{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x84182600000c7532","nwkAddr":56716,"deviceType":1,"rxOnWhenIdle":2,"relationship":2,"permitJoin":2,"depth":255,"lqi":51}]}	
2021-12-16 16:32:42.223 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:42.223 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtLqiReq - {"dstaddr":0,"startindex":22}	
2021-12-16 16:32:42.224 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,49,0,0,22,1]	
2021-12-16 16:32:42.237 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,49,0,85,254,50,69,177,0,0,0,26,22,2,47,212,221,66,221,45,212,221,15,196,2,254,255,159,253,144,223,221,41,2,255,0,47,212,221,66,221,45,212,221,176,54,68,254,255,87,11,0,123,225,41,2,255,0,245]	
2021-12-16 16:32:42.237 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,49,0,85,254,50,69,177,0,0,0,26,22,2,47,212,221,66,221,45,212,221,15,196,2,254,255,159,253,144,223,221,41,2,255,0,47,212,221,66,221,45,212,221,176,54,68,254,255,87,11,0,123,225,41,2,255,0,245]	
2021-12-16 16:32:42.237 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 49 - [0] - 85	
2021-12-16 16:32:42.238 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtLqiReq - {"status":0}	
2021-12-16 16:32:42.238 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50,69,177,0,0,0,26,22,2,47,212,221,66,221,45,212,221,15,196,2,254,255,159,253,144,223,221,41,2,255,0,47,212,221,66,221,45,212,221,176,54,68,254,255,87,11,0,123,225,41,2,255,0,245]	
2021-12-16 16:32:42.238 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 50 - 2 - 5 - 177 - [0,0,0,26,22,2,47,212,221,66,221,45,212,221,15,196,2,254,255,159,253,144,223,221,41,2,255,0,47,212,221,66,221,45,212,221,176,54,68,254,255,87,11,0,123,225,41,2,255,0] - 245	
2021-12-16 16:32:42.239 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - mgmtLqiRsp - {"srcaddr":0,"status":0,"neighbortableentries":26,"startindex":22,"neighborlqilistcount":2,"neighborlqilist":[{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x90fd9ffffe02c40f","nwkAddr":56799,"deviceType":1,"rxOnWhenIdle":2,"relationship":2,"permitJoin":2,"depth":255,"lqi":0},{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x000b57fffe4436b0","nwkAddr":57723,"deviceType":1,"rxOnWhenIdle":2,"relationship":2,"permitJoin":2,"depth":255,"lqi":0}]}	
2021-12-16 16:32:42.239 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:42.239 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtLqiReq - {"dstaddr":0,"startindex":24}	
2021-12-16 16:32:42.240 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,49,0,0,24,15]	
2021-12-16 16:32:42.249 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,49,0,85,254,50,69,177,0,0,0,26,24,2,47,212,221,66,221,45,212,221,94,117,136,254,255,159,253,144,137,11,41,2,255,0,47,212,221,66,221,45,212,221,201,232,127,254,255,159,253,144,220,254,41,2,255,0,155]	
2021-12-16 16:32:42.249 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,49,0,85,254,50,69,177,0,0,0,26,24,2,47,212,221,66,221,45,212,221,94,117,136,254,255,159,253,144,137,11,41,2,255,0,47,212,221,66,221,45,212,221,201,232,127,254,255,159,253,144,220,254,41,2,255,0,155]	
2021-12-16 16:32:42.249 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 49 - [0] - 85	
2021-12-16 16:32:42.250 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtLqiReq - {"status":0}	
2021-12-16 16:32:42.250 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,50,69,177,0,0,0,26,24,2,47,212,221,66,221,45,212,221,94,117,136,254,255,159,253,144,137,11,41,2,255,0,47,212,221,66,221,45,212,221,201,232,127,254,255,159,253,144,220,254,41,2,255,0,155]	
2021-12-16 16:32:42.250 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 50 - 2 - 5 - 177 - [0,0,0,26,24,2,47,212,221,66,221,45,212,221,94,117,136,254,255,159,253,144,137,11,41,2,255,0,47,212,221,66,221,45,212,221,201,232,127,254,255,159,253,144,220,254,41,2,255,0] - 155	
2021-12-16 16:32:42.251 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - mgmtLqiRsp - {"srcaddr":0,"status":0,"neighbortableentries":26,"startindex":24,"neighborlqilistcount":2,"neighborlqilist":[{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x90fd9ffffe88755e","nwkAddr":2953,"deviceType":1,"rxOnWhenIdle":2,"relationship":2,"permitJoin":2,"depth":255,"lqi":0},{"extPandId":"0xddd42ddd42ddd42f","extAddr":"0x90fd9ffffe7fe8c9","nwkAddr":65244,"deviceType":1,"rxOnWhenIdle":2,"relationship":2,"permitJoin":2,"depth":255,"lqi":0}]}	
2021-12-16 16:32:42.251 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:42.252 - debug: zigbee.0 (26219) LQI succeeded for 'Coordinator'	
2021-12-16 16:32:42.253 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtRtgReq - {"dstaddr":0,"startindex":0}	
2021-12-16 16:32:42.253 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,50,0,0,0,20]	
2021-12-16 16:32:42.322 - debug: zigbee.0 (26219) group members: [{"device":"0x00158d0002b805e3","model":"lumi.light.aqcn02"},{"device":"0x00158d0002b7d6a9","model":"lumi.light.aqcn02"},{"device":"0x00158d0002b7d87c","model":"lumi.light.aqcn02"},{"device":"0x00158d0002c65ed8","model":"lumi.light.aqcn02"}]	
2021-12-16 16:32:42.323 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,50,0,86,254,21,69,178,0,0,0,3,0,3,140,221,0,245,234,170,72,0,245,234,144,185,0,245,234,103]	
2021-12-16 16:32:42.323 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,50,0,86,254,21,69,178,0,0,0,3,0,3,140,221,0,245,234,170,72,0,245,234,144,185,0,245,234,103]	
2021-12-16 16:32:42.323 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 50 - [0] - 86	
2021-12-16 16:32:42.324 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtRtgReq - {"status":0}	
2021-12-16 16:32:42.324 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,21,69,178,0,0,0,3,0,3,140,221,0,245,234,170,72,0,245,234,144,185,0,245,234,103]	
2021-12-16 16:32:42.324 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 21 - 2 - 5 - 178 - [0,0,0,3,0,3,140,221,0,245,234,170,72,0,245,234,144,185,0,245,234] - 103	
2021-12-16 16:32:42.325 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- ZDO - mgmtRtgRsp - {"srcaddr":0,"status":0,"routingtableentries":3,"startindex":0,"routingtablelistcount":3,"routingtablelist":[{"destNwkAddr":56716,"routeStatus":"ACTIVE","nextHopNwkAddr":60149},{"destNwkAddr":18602,"routeStatus":"ACTIVE","nextHopNwkAddr":60149},{"destNwkAddr":47504,"routeStatus":"ACTIVE","nextHopNwkAddr":60149}]}	
2021-12-16 16:32:42.325 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:42.326 - debug: zigbee.0 (26219) Routing for 'Coordinator': {"table":[{"destinationAddress":56716,"status":"ACTIVE","nextHop":60149},{"destinationAddress":18602,"status":"ACTIVE","nextHop":60149},{"destinationAddress":47504,"status":"ACTIVE","nextHop":60149}]}	
2021-12-16 16:32:42.326 - debug: zigbee.0 (26219) Routing table succeeded for 'Coordinator'	
2021-12-16 16:32:42.327 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtLqiReq - {"dstaddr":47504,"startindex":0}	
2021-12-16 16:32:42.327 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,49,144,185,0,62]	
2021-12-16 16:32:42.334 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,49,0,85]	
2021-12-16 16:32:42.334 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,49,0,85]	
2021-12-16 16:32:42.335 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 49 - [0] - 85	
2021-12-16 16:32:42.336 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtLqiReq - {"status":0}	
2021-12-16 16:32:42.336 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:32:42.342 - debug: zigbee.0 (26219) memberinfo: [{"name":"Deckenleuchte 1/4 (Schlafzimmer)","ieee":"0x00158d0002b805e3"},{"name":"Deckenleuchte 2/4 (Schlafzimmer)","ieee":"0x00158d0002b7d6a9"},{"name":"Deckenleuchte 3/4 (Schlafzimmer)","ieee":"0x00158d0002b7d87c"},{"name":"Deckenleuchte 4/4 (Schlafzimmer)","ieee":"0x00158d0002c65ed8"}]	
2021-12-16 16:32:42.343 - debug: zigbee.0 (26219) group members: [{"device":"0x000b57fffe4436b0","model":"TRADFRI bulb E27 WS opal 980lm"},{"device":"0x90fd9ffffe88755e","model":"TRADFRI bulb E27 WS opal 980lm"},{"device":"0x90fd9ffffe7fe8c9","model":"TRADFRI bulb E27 WS opal 980lm"},{"device":"0x90fd9ffffe02c40f","model":"TRADFRI bulb E27 WS opal 980lm"}]	
2021-12-16 16:32:42.348 - debug: zigbee.0 (26219) memberinfo: [{"name":"Deckenleuchte 1/4 (Wohnzimmer)","ieee":"0x000b57fffe4436b0"},{"name":"Deckenleuchte 2/4 (Wohnzimmer)","ieee":"0x90fd9ffffe88755e"},{"name":"Deckenleuchte 3/4 (Wohnzimmer)","ieee":"0x90fd9ffffe7fe8c9"},{"name":"Deckenleuchte 4/4 (Wohnzimmer)","ieee":"0x90fd9ffffe02c40f"}]	
2021-12-16 16:32:42.357 - debug: zigbee.0 (26219) getDevices result: [{"type":"device","common":{"name":"Deckenleuchte 1/4 (Wohnzimmer)","type":"LED1545G12","icon":"img/ikea_bulb_E27.png"},"native":{"id":"000b57fffe4436b0"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.000b57fffe4436b0","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":0,"link_quality_lc":1639668684695,"statesDef":[{"id":"zigbee.0.000b57fffe4436b0.brightness","name":"Brightness","type":"number","read":true,"write":true,"val":100,"role":"level.dimmer","unit":""},{"id":"zigbee.0.000b57fffe4436b0.colortemp","name":"Color temperature","type":"number","read":true,"write":true,"val":278,"role":"level.color.temperature"},{"id":"zigbee.0.000b57fffe4436b0.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":true,"role":"switch"},{"id":"zigbee.0.000b57fffe4436b0.transition_time","name":"Transition time","type":"number","read":false,"write":true,"role":"state","unit":"sec"}],"icon":"img/ikea_bulb_E27.png","info":{"type":"device","device":{"ID":31,"_type":"Router","_ieeeAddr":"0x000b57fffe4436b0","_networkAddress":57723,"_manufacturerID":4476,"_endpoints":[{"ID":1,"profileID":49246,"deviceID":544,"inputClusters":[0,3,4,5,6,8,768,2821,4096],"outputClusters":[5,25,32,4096],"deviceNetworkAddress":57723,"deviceIeeeAddress":"0x000b57fffe4436b0","clusters":{"genBasic":{"attributes":{"modelId":"TRADFRI bulb E27 WS opal 980lm","manufacturerName":"IKEA of Sweden","powerSource":1,"zclVersion":1,"appVersion":17,"stackVersion":87,"hwVersion":1,"dateCode":"20170331","swBuildId":"1.2.217"}},"lightingColorCtrl":{"attributes":{"colorCapabilities":16,"colorTempPhysicalMin":250,"colorTempPhysicalMax":454,"colorMode":2,"colorTemperature":278}},"genOnOff":{"attributes":{"onOff":1}},"genLevelCtrl":{"attributes":{"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"IKEA of Sweden","_powerSource":"Mains (single phase)","_modelID":"TRADFRI bulb E27 WS opal 980lm","_applicationVersion":17,"_stackVersion":87,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20170331","_softwareBuildID":"1.2.217","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":2},"_lastSeen":1639638516008},"mapped":{"exposes":[{"type":"light","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","value_toggle":"TOGGLE","description":"On/off state of this light"},{"type":"numeric","name":"brightness","property":"brightness","access":7,"value_min":0,"value_max":254,"description":"Brightness of this light"},{"type":"numeric","name":"color_temp","property":"color_temp","access":7,"unit":"mired","value_min":250,"value_max":454,"description":"Color temperature of this light","presets":[{"name":"coolest","value":250,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":454,"description":"Warmest temperature supported"}]},{"type":"numeric","name":"color_temp_startup","property":"color_temp_startup","access":7,"unit":"mired","value_min":250,"value_max":454,"description":"Color temperature after cold power on of this light","presets":[{"name":"coolest","value":250,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":454,"description":"Warmest temperature supported"},{"name":"previous","value":65535,"description":"Restore previous color_temp on cold power on"}]}]},{"type":"enum","name":"effect","property":"effect","access":2,"values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)"},{"type":"enum","name":"power_on_behavior","property":"power_on_behavior","access":7,"values":["off","previous","on"],"description":"Controls the behavior when the device is powered on"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"lightingColorCtrl","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","brightness","brightness_percent"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp","color_temp_percent"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."},{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["transition"],"attr":[]},{"key":["rate"],"attr":[]},{"key":["brightness_move","brightness_move_onoff"]},{"key":["colortemp_move","color_temp_move"]},{"key":["brightness_step","brightness_step_onoff"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_step"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_startup"]},{"key":["level_config"]},{"key":["power_on_behavior"]},{"key":["color_options"]},{"key":["color_mode"]},{"key":["effect","alert","flash"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"ota":{},"zigbeeModel":["TRADFRI bulb E27 WS opal 980lm","TRADFRI bulb E26 WS opal 980lm","TRADFRI bulb E27 WSopal 980lm"],"model":"LED1545G12","vendor":"IKEA","description":"TRADFRI LED bulb E26/E27 980 lumen, dimmable, white spectrum, opal white","options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."},{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},"endpoint":{"ID":1,"profileID":49246,"deviceID":544,"inputClusters":[0,3,4,5,6,8,768,2821,4096],"outputClusters":[5,25,32,4096],"deviceNetworkAddress":57723,"deviceIeeeAddress":"0x000b57fffe4436b0","clusters":{"genBasic":{"attributes":{"modelId":"TRADFRI bulb E27 WS opal 980lm","manufacturerName":"IKEA of Sweden","powerSource":1,"zclVersion":1,"appVersion":17,"stackVersion":87,"hwVersion":1,"dateCode":"20170331","swBuildId":"1.2.217"}},"lightingColorCtrl":{"attributes":{"colorCapabilities":16,"colorTempPhysicalMin":250,"colorTempPhysicalMax":454,"colorMode":2,"colorTemperature":278}},"genOnOff":{"attributes":{"onOff":1}},"genLevelCtrl":{"attributes":{"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":49246,"deviceID":544,"inputClusters":[0,3,4,5,6,8,768,2821,4096],"outputClusters":[5,25,32,4096],"deviceNetworkAddress":57723,"deviceIeeeAddress":"0x000b57fffe4436b0","clusters":{"genBasic":{"attributes":{"modelId":"TRADFRI bulb E27 WS opal 980lm","manufacturerName":"IKEA of Sweden","powerSource":1,"zclVersion":1,"appVersion":17,"stackVersion":87,"hwVersion":1,"dateCode":"20170331","swBuildId":"1.2.217"}},"lightingColorCtrl":{"attributes":{"colorCapabilities":16,"colorTempPhysicalMin":250,"colorTempPhysicalMax":454,"colorMode":2,"colorTemperature":278}},"genOnOff":{"attributes":{"onOff":1}},"genLevelCtrl":{"attributes":{"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x000b57fffe4436b0"},"rooms":[],"paired":true,"groups":["2"]},{"type":"device","common":{"name":"Rollo ( Wohnzimmer Tür)","type":"E1757","icon":"img/Ikea_fyrtur.png"},"native":{"id":"000d6ffffe2cd4b8"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.000d6ffffe2cd4b8","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":0,"link_quality_lc":1639668722241,"battery":100,"statesDef":[{"id":"zigbee.0.000d6ffffe2cd4b8.close","name":"Close blind","type":"boolean","read":true,"write":true,"val":false,"role":"button"},{"id":"zigbee.0.000d6ffffe2cd4b8.open","name":"Open blind","type":"boolean","read":true,"write":true,"val":false,"role":"button"},{"id":"zigbee.0.000d6ffffe2cd4b8.position","name":"Blind position","type":"number","read":true,"write":true,"val":100,"role":"state","unit":"%"},{"id":"zigbee.0.000d6ffffe2cd4b8.stop","name":"Stop blind","type":"boolean","read":true,"write":true,"val":false,"role":"button"}],"icon":"img/Ikea_fyrtur.png","info":{"type":"device","device":{"ID":44,"_type":"EndDevice","_ieeeAddr":"0x000d6ffffe2cd4b8","_networkAddress":935,"_manufacturerID":4476,"_endpoints":[{"ID":1,"profileID":260,"deviceID":514,"inputClusters":[0,1,3,4,5,32,258,4096,64636],"outputClusters":[25,4096],"deviceNetworkAddress":935,"deviceIeeeAddress":"0x000d6ffffe2cd4b8","clusters":{"genBasic":{"attributes":{"modelId":"FYRTUR block-out roller blind","manufacturerName":"IKEA of Sweden","powerSource":3,"zclVersion":3,"appVersion":33,"stackVersion":99,"hwVersion":1,"dateCode":"20190311","swBuildId":"2.3.073"}},"genPowerCfg":{"attributes":{"batteryPercentageRemaining":100}},"closuresWindowCovering":{"attributes":{"currentPositionLiftPercentage":0}}},"_binds":[{"cluster":1,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1},{"cluster":258,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":1,"attrId":33,"minRepIntval":3600,"maxRepIntval":62000,"repChange":0},{"cluster":258,"attrId":8,"minRepIntval":1,"maxRepIntval":62000,"repChange":1}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"IKEA of Sweden","_powerSource":"Battery","_modelID":"FYRTUR block-out roller blind","_applicationVersion":33,"_stackVersion":99,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"20190311","_softwareBuildID":"2.3.073","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":2},"_lastSeen":1638803854786,"useImplicitCheckin":true},"mapped":{"zigbeeModel":["FYRTUR block-out roller blind"],"model":"E1757","vendor":"IKEA","description":"FYRTUR roller blind","fromZigbee":[{"cluster":"closuresWindowCovering","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"invert_cover","property":"invert_cover","access":2,"value_on":true,"value_off":false,"description":"Inverts the cover position, false: open=100,close=0, true: open=0,close=100 (default false)."}]},{"cluster":"genPowerCfg","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state"]},{"key":["position","tilt"],"options":[{"type":"binary","name":"invert_cover","property":"invert_cover","access":2,"value_on":true,"value_off":false,"description":"Inverts the cover position, false: open=100,close=0, true: open=0,close=100 (default false)."}]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"meta":{"battery":{"dontDividePercentage":true}},"ota":{},"exposes":[{"type":"cover","features":[{"type":"enum","name":"state","property":"state","access":3,"values":["OPEN","CLOSE","STOP"]},{"type":"numeric","name":"position","property":"position","access":7,"value_min":0,"value_max":100,"description":"Position of this cover"}]},{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":[{"type":"binary","name":"invert_cover","property":"invert_cover","access":2,"value_on":true,"value_off":false,"description":"Inverts the cover position, false: open=100,close=0, true: open=0,close=100 (default false)."}]},"endpoint":{"ID":1,"profileID":260,"deviceID":514,"inputClusters":[0,1,3,4,5,32,258,4096,64636],"outputClusters":[25,4096],"deviceNetworkAddress":935,"deviceIeeeAddress":"0x000d6ffffe2cd4b8","clusters":{"genBasic":{"attributes":{"modelId":"FYRTUR block-out roller blind","manufacturerName":"IKEA of Sweden","powerSource":3,"zclVersion":3,"appVersion":33,"stackVersion":99,"hwVersion":1,"dateCode":"20190311","swBuildId":"2.3.073"}},"genPowerCfg":{"attributes":{"batteryPercentageRemaining":100}},"closuresWindowCovering":{"attributes":{"currentPositionLiftPercentage":0}}},"_binds":[{"cluster":1,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1},{"cluster":258,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":1,"attrId":33,"minRepIntval":3600,"maxRepIntval":62000,"repChange":0},{"cluster":258,"attrId":8,"minRepIntval":1,"maxRepIntval":62000,"repChange":1}],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":514,"inputClusters":[0,1,3,4,5,32,258,4096,64636],"outputClusters":[25,4096],"deviceNetworkAddress":935,"deviceIeeeAddress":"0x000d6ffffe2cd4b8","clusters":{"genBasic":{"attributes":{"modelId":"FYRTUR block-out roller blind","manufacturerName":"IKEA of Sweden","powerSource":3,"zclVersion":3,"appVersion":33,"stackVersion":99,"hwVersion":1,"dateCode":"20190311","swBuildId":"2.3.073"}},"genPowerCfg":{"attributes":{"batteryPercentageRemaining":100}},"closuresWindowCovering":{"attributes":{"currentPositionLiftPercentage":0}}},"_binds":[{"cluster":1,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1},{"cluster":258,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":1,"attrId":33,"minRepIntval":3600,"maxRepIntval":62000,"repChange":0},{"cluster":258,"attrId":8,"minRepIntval":1,"maxRepIntval":62000,"repChange":1}],"meta":{},"pendingRequests":[]}],"name":"0x000d6ffffe2cd4b8"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Lautsprecher","type":"WXKG11LM","icon":"img/aqara_switch.png"},"native":{"id":"00158d0002130d3b"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662545,"_id":"zigbee.0.00158d0002130d3b","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":78,"link_quality_lc":1639668740892,"battery":100,"statesDef":[{"id":"zigbee.0.00158d0002130d3b.click","name":"Click event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d0002130d3b.double_click","name":"Double click event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d0002130d3b.quad_click","name":"Quadruple click event","type":"boolean","read":true,"write":false,"role":"button"},{"id":"zigbee.0.00158d0002130d3b.triple_click","name":"Triple click event","type":"boolean","read":true,"write":false,"role":"button"},{"id":"zigbee.0.00158d0002130d3b.voltage","name":"Battery voltage","type":"number","read":true,"write":false,"val":3.005,"role":"battery.voltage","unit":"V"}],"icon":"img/aqara_switch.png","info":{"type":"device","device":{"ID":3,"_type":"EndDevice","_ieeeAddr":"0x00158d0002130d3b","_networkAddress":61838,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":61838,"deviceIeeeAddress":"0x00158d0002130d3b","clusters":{"genBasic":{"attributes":{"65281":{"1":3005,"3":27,"4":17320,"5":48,"6":[0,1],"10":47504},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_switch.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639668740863,"_linkquality":78},"mapped":{"zigbeeModel":["lumi.sensor_switch.aq2","lumi.remote.b1acn01"],"model":"WXKG11LM","vendor":"Xiaomi","description":"Aqara wireless switch","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"enum","name":"action","property":"action","access":1,"values":["single","double","triple","quadruple","hold","release"],"description":"Triggered action (e.g. a button click)"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genMultistateInput","type":["attributeReport"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genMultistateInput","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]}],"toZigbee":[],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},"endpoint":{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":61838,"deviceIeeeAddress":"0x00158d0002130d3b","clusters":{"genBasic":{"attributes":{"65281":{"1":3005,"3":27,"4":17320,"5":48,"6":[0,1],"10":47504},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":61838,"deviceIeeeAddress":"0x00158d0002130d3b","clusters":{"genBasic":{"attributes":{"65281":{"1":3005,"3":27,"4":17320,"5":48,"6":[0,1],"10":47504},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d0002130d3b"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Lüfter-Taster (Badezimmer)","type":"WXKG11LM","icon":"img/aqara_switch.png"},"native":{"id":"00158d0002130f3a"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d0002130f3a","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":10,"link_quality_lc":1639668662643,"battery":100,"statesDef":[{"id":"zigbee.0.00158d0002130f3a.click","name":"Click event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d0002130f3a.double_click","name":"Double click event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d0002130f3a.quad_click","name":"Quadruple click event","type":"boolean","read":true,"write":false,"role":"button"},{"id":"zigbee.0.00158d0002130f3a.triple_click","name":"Triple click event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d0002130f3a.voltage","name":"Battery voltage","type":"number","read":true,"write":false,"val":3.015,"role":"battery.voltage","unit":"V"}],"icon":"img/aqara_switch.png","info":{"type":"device","device":{"ID":7,"_type":"EndDevice","_ieeeAddr":"0x00158d0002130f3a","_networkAddress":60816,"_manufacturerID":4151,"_endpoints":[{"ID":1,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":60816,"deviceIeeeAddress":"0x00158d0002130f3a","clusters":{"genBasic":{"attributes":{"65281":{"1":3015,"3":26,"4":17320,"5":23,"6":[0,1],"10":47504},"modelId":"lumi.sensor_switch.aq2","appVersion":3}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_switch.aq2","_applicationVersion":3,"_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639665771838},"mapped":{"zigbeeModel":["lumi.sensor_switch.aq2","lumi.remote.b1acn01"],"model":"WXKG11LM","vendor":"Xiaomi","description":"Aqara wireless switch","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"enum","name":"action","property":"action","access":1,"values":["single","double","triple","quadruple","hold","release"],"description":"Triggered action (e.g. a button click)"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genMultistateInput","type":["attributeReport"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genMultistateInput","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]}],"toZigbee":[],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},"endpoint":{"ID":1,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":60816,"deviceIeeeAddress":"0x00158d0002130f3a","clusters":{"genBasic":{"attributes":{"65281":{"1":3015,"3":26,"4":17320,"5":23,"6":[0,1],"10":47504},"modelId":"lumi.sensor_switch.aq2","appVersion":3}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":60816,"deviceIeeeAddress":"0x00158d0002130f3a","clusters":{"genBasic":{"attributes":{"65281":{"1":3015,"3":26,"4":17320,"5":23,"6":[0,1],"10":47504},"modelId":"lumi.sensor_switch.aq2","appVersion":3}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d0002130f3a"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Schranklichtschalter (Badezimmer)","type":"WXKG11LM","icon":"img/aqara_switch.png"},"native":{"id":"00158d0002135d9b"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d0002135d9b","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":10,"link_quality_lc":1639668662669,"battery":100,"statesDef":[{"id":"zigbee.0.00158d0002135d9b.click","name":"Click event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d0002135d9b.double_click","name":"Double click event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d0002135d9b.quad_click","name":"Quadruple click event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d0002135d9b.triple_click","name":"Triple click event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d0002135d9b.voltage","name":"Battery voltage","type":"number","read":true,"write":false,"val":3.015,"role":"battery.voltage","unit":"V"}],"icon":"img/aqara_switch.png","info":{"type":"device","device":{"ID":10,"_type":"EndDevice","_ieeeAddr":"0x00158d0002135d9b","_networkAddress":45956,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":45956,"deviceIeeeAddress":"0x00158d0002135d9b","clusters":{"genBasic":{"attributes":{"65281":{"1":3015,"3":27,"4":17320,"5":77,"6":[0,1],"10":47504},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_switch.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639664787186},"mapped":{"zigbeeModel":["lumi.sensor_switch.aq2","lumi.remote.b1acn01"],"model":"WXKG11LM","vendor":"Xiaomi","description":"Aqara wireless switch","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"enum","name":"action","property":"action","access":1,"values":["single","double","triple","quadruple","hold","release"],"description":"Triggered action (e.g. a button click)"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genMultistateInput","type":["attributeReport"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genMultistateInput","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]}],"toZigbee":[],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},"endpoint":{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":45956,"deviceIeeeAddress":"0x00158d0002135d9b","clusters":{"genBasic":{"attributes":{"65281":{"1":3015,"3":27,"4":17320,"5":77,"6":[0,1],"10":47504},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":45956,"deviceIeeeAddress":"0x00158d0002135d9b","clusters":{"genBasic":{"attributes":{"65281":{"1":3015,"3":27,"4":17320,"5":77,"6":[0,1],"10":47504},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d0002135d9b"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Szenenbutton","type":"WXKG11LM","icon":"img/aqara_switch.png"},"native":{"id":"00158d00021369f3"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d00021369f3","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":10,"link_quality_lc":1639668662669,"battery":100,"statesDef":[{"id":"zigbee.0.00158d00021369f3.click","name":"Click event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d00021369f3.double_click","name":"Double click event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d00021369f3.quad_click","name":"Quadruple click event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d00021369f3.triple_click","name":"Triple click event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d00021369f3.voltage","name":"Battery voltage","type":"number","read":true,"write":false,"val":3.025,"role":"battery.voltage","unit":"V"}],"icon":"img/aqara_switch.png","info":{"type":"device","device":{"ID":19,"_type":"EndDevice","_ieeeAddr":"0x00158d00021369f3","_networkAddress":4218,"_manufacturerID":4151,"_endpoints":[{"ID":1,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":4218,"deviceIeeeAddress":"0x00158d00021369f3","clusters":{"genBasic":{"attributes":{"65281":{"1":3025,"3":21,"4":17320,"5":23802,"6":[0,1],"10":47504},"modelId":"lumi.sensor_switch.aq2","appVersion":3}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_switch.aq2","_applicationVersion":3,"_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639666109455},"mapped":{"zigbeeModel":["lumi.sensor_switch.aq2","lumi.remote.b1acn01"],"model":"WXKG11LM","vendor":"Xiaomi","description":"Aqara wireless switch","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"enum","name":"action","property":"action","access":1,"values":["single","double","triple","quadruple","hold","release"],"description":"Triggered action (e.g. a button click)"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genMultistateInput","type":["attributeReport"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genMultistateInput","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]}],"toZigbee":[],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},"endpoint":{"ID":1,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":4218,"deviceIeeeAddress":"0x00158d00021369f3","clusters":{"genBasic":{"attributes":{"65281":{"1":3025,"3":21,"4":17320,"5":23802,"6":[0,1],"10":47504},"modelId":"lumi.sensor_switch.aq2","appVersion":3}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":4218,"deviceIeeeAddress":"0x00158d00021369f3","clusters":{"genBasic":{"attributes":{"65281":{"1":3025,"3":21,"4":17320,"5":23802,"6":[0,1],"10":47504},"modelId":"lumi.sensor_switch.aq2","appVersion":3}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d00021369f3"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Schlafzimmerlicht (defekt)","type":"QBKG04LM","icon":"img/ctrl_neutral1.png"},"native":{"id":"00158d000257b84c"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1607357950370,"_id":"zigbee.0.00158d000257b84c","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":94,"link_quality_lc":1600110394294,"statesDef":[{"id":"zigbee.0.00158d000257b84c.click","name":"Click event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d000257b84c.decoupled","name":"Decoupled mode","type":"boolean","read":true,"write":true,"role":"state"},{"id":"zigbee.0.00158d000257b84c.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":false,"role":"switch"}],"icon":"img/ctrl_neutral1.png","rooms":[],"paired":false},{"type":"device","common":{"name":"Lecksensor","type":"SJCGQ11LM","icon":"img/sensor_wleak_aq1.png"},"native":{"id":"00158d000271c4b7"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d000271c4b7","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":10,"link_quality_lc":1639668662550,"battery":100,"statesDef":[{"id":"zigbee.0.00158d000271c4b7.detected","name":"Water leak detected","type":"boolean","read":true,"write":false,"val":false,"role":"indicator.leakage"},{"id":"zigbee.0.00158d000271c4b7.voltage","name":"Battery voltage","type":"number","read":true,"write":false,"val":3.025,"role":"battery.voltage","unit":"V"}],"icon":"img/sensor_wleak_aq1.png","info":{"type":"device","device":{"ID":12,"_type":"EndDevice","_ieeeAddr":"0x00158d000271c4b7","_networkAddress":16037,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":1026,"inputClusters":[0,3,1],"outputClusters":[25],"deviceNetworkAddress":16037,"deviceIeeeAddress":"0x00158d000271c4b7","clusters":{"genBasic":{"attributes":{"65281":{"1":3025,"3":21,"4":17320,"5":10,"6":[0,1],"8":516,"10":47504,"100":1},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20170721","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_wleak.aq1","_applicationVersion":4,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20170721","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639666263071},"mapped":{"zigbeeModel":["lumi.sensor_wleak.aq1"],"model":"SJCGQ11LM","vendor":"Xiaomi","description":"Aqara water leak sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"ssIasZone","type":"commandStatusChangeNotification"},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"binary","name":"water_leak","property":"water_leak","access":1,"value_on":true,"value_off":false,"description":"Indicates whether the device detected a water leak"},{"type":"binary","name":"battery_low","property":"battery_low","access":1,"value_on":true,"value_off":false,"description":"Indicates if the battery of this device is almost empty"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":[]},"endpoint":{"ID":1,"profileID":260,"deviceID":1026,"inputClusters":[0,3,1],"outputClusters":[25],"deviceNetworkAddress":16037,"deviceIeeeAddress":"0x00158d000271c4b7","clusters":{"genBasic":{"attributes":{"65281":{"1":3025,"3":21,"4":17320,"5":10,"6":[0,1],"8":516,"10":47504,"100":1},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20170721","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":1026,"inputClusters":[0,3,1],"outputClusters":[25],"deviceNetworkAddress":16037,"deviceIeeeAddress":"0x00158d000271c4b7","clusters":{"genBasic":{"attributes":{"65281":{"1":3025,"3":21,"4":17320,"5":10,"6":[0,1],"8":516,"10":47504,"100":1},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20170721","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d000271c4b7"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Fenster (Schlafzimmer klein)","type":"MCCGQ11LM","icon":"img/sensor_magnet_aq2.png"},"native":{"id":"00158d0002722af7"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d0002722af7","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":10,"link_quality_lc":1639668662558,"battery":100,"statesDef":[{"id":"zigbee.0.00158d0002722af7.contact","name":"Contact event","type":"boolean","read":true,"write":false,"val":true,"role":"state"},{"id":"zigbee.0.00158d0002722af7.opened","name":"Is open","type":"boolean","read":true,"write":false,"val":false,"role":"state"},{"id":"zigbee.0.00158d0002722af7.voltage","name":"Battery voltage","type":"number","read":true,"write":false,"val":3.025,"role":"battery.voltage","unit":"V"}],"icon":"img/sensor_magnet_aq2.png","info":{"type":"device","device":{"ID":37,"_type":"EndDevice","_ieeeAddr":"0x00158d0002722af7","_networkAddress":45388,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":45388,"deviceIeeeAddress":"0x00158d0002722af7","clusters":{"genBasic":{"attributes":{"65281":{"1":3025,"3":18,"4":5032,"5":64,"6":[0,1],"10":47504,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_magnet.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639664567227},"mapped":{"zigbeeModel":["lumi.sensor_magnet.aq2"],"model":"MCCGQ11LM","vendor":"Xiaomi","description":"Aqara door & window contact sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"binary","name":"contact","property":"contact","access":1,"value_on":false,"value_off":true,"description":"Indicates if the contact is closed (= true) or open (= false)"},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]},"endpoint":{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":45388,"deviceIeeeAddress":"0x00158d0002722af7","clusters":{"genBasic":{"attributes":{"65281":{"1":3025,"3":18,"4":5032,"5":64,"6":[0,1],"10":47504,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":45388,"deviceIeeeAddress":"0x00158d0002722af7","clusters":{"genBasic":{"attributes":{"65281":{"1":3025,"3":18,"4":5032,"5":64,"6":[0,1],"10":47504,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d0002722af7"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Fenster (Wohnzimmer rechts groß)","type":"MCCGQ11LM","icon":"img/sensor_magnet_aq2.png"},"native":{"id":"00158d000274f4bf"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d000274f4bf","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":10,"link_quality_lc":1639668662550,"battery":91,"statesDef":[{"id":"zigbee.0.00158d000274f4bf.contact","name":"Contact event","type":"boolean","read":true,"write":false,"val":true,"role":"state"},{"id":"zigbee.0.00158d000274f4bf.opened","name":"Is open","type":"boolean","read":true,"write":false,"val":false,"role":"state"},{"id":"zigbee.0.00158d000274f4bf.voltage","name":"Battery voltage","type":"number","read":true,"write":false,"val":2.985,"role":"battery.voltage","unit":"V"}],"icon":"img/sensor_magnet_aq2.png","info":{"type":"device","device":{"ID":11,"_type":"EndDevice","_ieeeAddr":"0x00158d000274f4bf","_networkAddress":52827,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":52827,"deviceIeeeAddress":"0x00158d000274f4bf","clusters":{"genBasic":{"attributes":{"65281":{"1":2985,"3":24,"4":17320,"5":45,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_magnet.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639666026955},"mapped":{"zigbeeModel":["lumi.sensor_magnet.aq2"],"model":"MCCGQ11LM","vendor":"Xiaomi","description":"Aqara door & window contact sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"binary","name":"contact","property":"contact","access":1,"value_on":false,"value_off":true,"description":"Indicates if the contact is closed (= true) or open (= false)"},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]},"endpoint":{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":52827,"deviceIeeeAddress":"0x00158d000274f4bf","clusters":{"genBasic":{"attributes":{"65281":{"1":2985,"3":24,"4":17320,"5":45,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":52827,"deviceIeeeAddress":"0x00158d000274f4bf","clusters":{"genBasic":{"attributes":{"65281":{"1":2985,"3":24,"4":17320,"5":45,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d000274f4bf"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Fenster (Küche)","type":"MCCGQ11LM","icon":"img/sensor_magnet_aq2.png"},"native":{"id":"00158d000274f4d3"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d000274f4d3","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":10,"link_quality_lc":1639668662557,"battery":97,"statesDef":[{"id":"zigbee.0.00158d000274f4d3.contact","name":"Contact event","type":"boolean","read":true,"write":false,"val":true,"role":"state"},{"id":"zigbee.0.00158d000274f4d3.opened","name":"Is open","type":"boolean","read":true,"write":false,"val":false,"role":"state"},{"id":"zigbee.0.00158d000274f4d3.voltage","name":"Battery voltage","type":"number","read":true,"write":false,"val":2.995,"role":"battery.voltage","unit":"V"}],"icon":"img/sensor_magnet_aq2.png","info":{"type":"device","device":{"ID":36,"_type":"EndDevice","_ieeeAddr":"0x00158d000274f4d3","_networkAddress":44450,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":44450,"deviceIeeeAddress":"0x00158d000274f4d3","clusters":{"genBasic":{"attributes":{"65281":{"1":2995,"3":26,"4":5032,"5":69,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_magnet.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639667159723},"mapped":{"zigbeeModel":["lumi.sensor_magnet.aq2"],"model":"MCCGQ11LM","vendor":"Xiaomi","description":"Aqara door & window contact sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"binary","name":"contact","property":"contact","access":1,"value_on":false,"value_off":true,"description":"Indicates if the contact is closed (= true) or open (= false)"},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]},"endpoint":{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":44450,"deviceIeeeAddress":"0x00158d000274f4d3","clusters":{"genBasic":{"attributes":{"65281":{"1":2995,"3":26,"4":5032,"5":69,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":44450,"deviceIeeeAddress":"0x00158d000274f4d3","clusters":{"genBasic":{"attributes":{"65281":{"1":2995,"3":26,"4":5032,"5":69,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d000274f4d3"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Haustuersensor","type":"MCCGQ11LM","icon":"img/sensor_magnet_aq2.png"},"native":{"id":"00158d000274f4de"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d000274f4de","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":10,"link_quality_lc":1639668662549,"battery":97,"statesDef":[{"id":"zigbee.0.00158d000274f4de.contact","name":"Contact event","type":"boolean","read":true,"write":false,"val":true,"role":"state"},{"id":"zigbee.0.00158d000274f4de.opened","name":"Is open","type":"boolean","read":true,"write":false,"val":false,"role":"state"},{"id":"zigbee.0.00158d000274f4de.voltage","name":"Battery voltage","type":"number","read":true,"write":false,"val":2.995,"role":"battery.voltage","unit":"V"}],"icon":"img/sensor_magnet_aq2.png","info":{"type":"device","device":{"ID":9,"_type":"EndDevice","_ieeeAddr":"0x00158d000274f4de","_networkAddress":53691,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":53691,"deviceIeeeAddress":"0x00158d000274f4de","clusters":{"genBasic":{"attributes":{"65281":{"1":2995,"3":28,"4":17320,"5":37,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_magnet.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639668060686},"mapped":{"zigbeeModel":["lumi.sensor_magnet.aq2"],"model":"MCCGQ11LM","vendor":"Xiaomi","description":"Aqara door & window contact sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"binary","name":"contact","property":"contact","access":1,"value_on":false,"value_off":true,"description":"Indicates if the contact is closed (= true) or open (= false)"},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]},"endpoint":{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":53691,"deviceIeeeAddress":"0x00158d000274f4de","clusters":{"genBasic":{"attributes":{"65281":{"1":2995,"3":28,"4":17320,"5":37,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":53691,"deviceIeeeAddress":"0x00158d000274f4de","clusters":{"genBasic":{"attributes":{"65281":{"1":2995,"3":28,"4":17320,"5":37,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d000274f4de"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Fenster (Wohnzimmer links groß)","type":"MCCGQ11LM","icon":"img/sensor_magnet_aq2.png"},"native":{"id":"00158d000274f4f7"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d000274f4f7","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":10,"link_quality_lc":1639668662556,"battery":100,"statesDef":[{"id":"zigbee.0.00158d000274f4f7.contact","name":"Contact event","type":"boolean","read":true,"write":false,"val":true,"role":"state"},{"id":"zigbee.0.00158d000274f4f7.opened","name":"Is open","type":"boolean","read":true,"write":false,"val":false,"role":"state"},{"id":"zigbee.0.00158d000274f4f7.voltage","name":"Battery voltage","type":"number","read":true,"write":false,"val":3.005,"role":"battery.voltage","unit":"V"}],"icon":"img/sensor_magnet_aq2.png","info":{"type":"device","device":{"ID":24,"_type":"EndDevice","_ieeeAddr":"0x00158d000274f4f7","_networkAddress":17905,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":17905,"deviceIeeeAddress":"0x00158d000274f4f7","clusters":{"genBasic":{"attributes":{"65281":{"1":3005,"3":23,"4":17320,"5":34,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_magnet.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639663882017},"mapped":{"zigbeeModel":["lumi.sensor_magnet.aq2"],"model":"MCCGQ11LM","vendor":"Xiaomi","description":"Aqara door & window contact sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"binary","name":"contact","property":"contact","access":1,"value_on":false,"value_off":true,"description":"Indicates if the contact is closed (= true) or open (= false)"},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]},"endpoint":{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":17905,"deviceIeeeAddress":"0x00158d000274f4f7","clusters":{"genBasic":{"attributes":{"65281":{"1":3005,"3":23,"4":17320,"5":34,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":17905,"deviceIeeeAddress":"0x00158d000274f4f7","clusters":{"genBasic":{"attributes":{"65281":{"1":3005,"3":23,"4":17320,"5":34,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d000274f4f7"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Fenster (Wohnzimmer rechts klein)","type":"MCCGQ11LM","icon":"img/sensor_magnet_aq2.png"},"native":{"id":"00158d000274f643"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d000274f643","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":10,"link_quality_lc":1639668662554,"battery":97,"statesDef":[{"id":"zigbee.0.00158d000274f643.contact","name":"Contact event","type":"boolean","read":true,"write":false,"val":true,"role":"state"},{"id":"zigbee.0.00158d000274f643.opened","name":"Is open","type":"boolean","read":true,"write":false,"val":false,"role":"state"},{"id":"zigbee.0.00158d000274f643.voltage","name":"Battery voltage","type":"number","read":true,"write":false,"val":2.995,"role":"battery.voltage","unit":"V"}],"icon":"img/sensor_magnet_aq2.png","info":{"type":"device","device":{"ID":21,"_type":"EndDevice","_ieeeAddr":"0x00158d000274f643","_networkAddress":43219,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":43219,"deviceIeeeAddress":"0x00158d000274f643","clusters":{"genBasic":{"attributes":{"65281":{"1":2995,"3":24,"4":17320,"5":32,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001","modelId":"lumi.sensor_magnet.aq2"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_magnet.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639665912300},"mapped":{"zigbeeModel":["lumi.sensor_magnet.aq2"],"model":"MCCGQ11LM","vendor":"Xiaomi","description":"Aqara door & window contact sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"binary","name":"contact","property":"contact","access":1,"value_on":false,"value_off":true,"description":"Indicates if the contact is closed (= true) or open (= false)"},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]},"endpoint":{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":43219,"deviceIeeeAddress":"0x00158d000274f643","clusters":{"genBasic":{"attributes":{"65281":{"1":2995,"3":24,"4":17320,"5":32,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001","modelId":"lumi.sensor_magnet.aq2"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":43219,"deviceIeeeAddress":"0x00158d000274f643","clusters":{"genBasic":{"attributes":{"65281":{"1":2995,"3":24,"4":17320,"5":32,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001","modelId":"lumi.sensor_magnet.aq2"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d000274f643"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Fenster (Wohnzimmer links klein)","type":"MCCGQ11LM","icon":"img/sensor_magnet_aq2.png"},"native":{"id":"00158d000274f64d"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d000274f64d","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":10,"link_quality_lc":1639668662554,"battery":100,"statesDef":[{"id":"zigbee.0.00158d000274f64d.contact","name":"Contact event","type":"boolean","read":true,"write":false,"val":true,"role":"state"},{"id":"zigbee.0.00158d000274f64d.opened","name":"Is open","type":"boolean","read":true,"write":false,"val":false,"role":"state"},{"id":"zigbee.0.00158d000274f64d.voltage","name":"Battery voltage","type":"number","read":true,"write":false,"val":3.025,"role":"battery.voltage","unit":"V"}],"icon":"img/sensor_magnet_aq2.png","info":{"type":"device","device":{"ID":22,"_type":"EndDevice","_ieeeAddr":"0x00158d000274f64d","_networkAddress":61566,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":61566,"deviceIeeeAddress":"0x00158d000274f64d","clusters":{"genBasic":{"attributes":{"65281":{"1":3025,"3":17,"4":17320,"5":83,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_magnet.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639668558468},"mapped":{"zigbeeModel":["lumi.sensor_magnet.aq2"],"model":"MCCGQ11LM","vendor":"Xiaomi","description":"Aqara door & window contact sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"binary","name":"contact","property":"contact","access":1,"value_on":false,"value_off":true,"description":"Indicates if the contact is closed (= true) or open (= false)"},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}]},"endpoint":{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":61566,"deviceIeeeAddress":"0x00158d000274f64d","clusters":{"genBasic":{"attributes":{"65281":{"1":3025,"3":17,"4":17320,"5":83,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":61566,"deviceIeeeAddress":"0x00158d000274f64d","clusters":{"genBasic":{"attributes":{"65281":{"1":3025,"3":17,"4":17320,"5":83,"6":[0,1],"10":0,"100":0},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d000274f64d"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Wuerfel","type":"MFKZQ01LM","icon":"img/cube.png"},"native":{"id":"00158d00028aee30"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d00028aee30","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":10,"link_quality_lc":1639668662552,"battery":80,"statesDef":[{"id":"zigbee.0.00158d00028aee30.fall","name":"Free fall event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d00028aee30.flip180","name":"Flip on 180°","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d00028aee30.flip180_side","name":"Top side on flip 180°","type":"number","read":true,"write":false,"val":1,"role":"state"},{"id":"zigbee.0.00158d00028aee30.flip90","name":"Flip on 90° event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d00028aee30.flip90_from","name":"From top side on flip 90°","type":"number","read":true,"write":false,"val":2,"role":"state"},{"id":"zigbee.0.00158d00028aee30.flip90_to","name":"To top side on flip 90°","type":"number","read":true,"write":false,"val":0,"role":"state"},{"id":"zigbee.0.00158d00028aee30.rotate_angle","name":"Rotate angle","type":"number","read":true,"write":false,"val":12.23,"role":"state"},{"id":"zigbee.0.00158d00028aee30.rotate_left","name":"Rotate left event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d00028aee30.rotate_right","name":"Rotate right event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d00028aee30.shake","name":"Shake event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d00028aee30.slide","name":"Slide event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d00028aee30.slide_side","name":"Top side on slide","type":"number","read":true,"write":false,"val":0,"role":"state"},{"id":"zigbee.0.00158d00028aee30.tap","name":"Tapped twice event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d00028aee30.tap_side","name":"Top side on tap","type":"number","read":true,"write":false,"val":1,"role":"state"},{"id":"zigbee.0.00158d00028aee30.voltage","name":"Battery voltage","type":"number","read":true,"write":false,"val":2.965,"role":"battery.voltage","unit":"V"},{"id":"zigbee.0.00158d00028aee30.wakeup","name":"Wakeup event","type":"boolean","read":true,"write":false,"val":false,"role":"button"}],"icon":"img/cube.png","info":{"type":"device","device":{"ID":18,"_type":"EndDevice","_ieeeAddr":"0x00158d00028aee30","_networkAddress":54685,"_manufacturerID":4151,"_endpoints":[{"ID":1,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":54685,"deviceIeeeAddress":"0x00158d00028aee30","clusters":{"genBasic":{"attributes":{"65281":{"1":2965,"3":19,"4":17320,"5":264,"6":[0,1],"10":0,"151":1,"152":3918,"153":2933,"154":4}}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":2,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":54685,"deviceIeeeAddress":"0x00158d00028aee30","clusters":{"genMultistateInput":{"attributes":{"presentValue":2}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":3,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":54685,"deviceIeeeAddress":"0x00158d00028aee30","clusters":{"genAnalogInput":{"attributes":{"65285":500,"presentValue":12.239999771118164}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_cube.aqgl01","_applicationVersion":5,"_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639666386256},"mapped":{"zigbeeModel":["lumi.sensor_cube","lumi.sensor_cube.aqgl01"],"model":"MFKZQ01LM","vendor":"Xiaomi","description":"Mi/Aqara smart home cube","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genMultistateInput","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genAnalogInput","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]}],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"action_angle","property":"action_angle","access":1,"value_min":-360,"value_max":360},{"type":"numeric","name":"action_from_side","property":"action_from_side","access":1,"description":"Side of the cube","value_min":0,"value_max":6,"value_step":1},{"type":"numeric","name":"action_side","property":"action_side","access":1,"description":"Side of the cube","value_min":0,"value_max":6,"value_step":1},{"type":"numeric","name":"action_to_side","property":"action_to_side","access":1,"description":"Side of the cube","value_min":0,"value_max":6,"value_step":1},{"type":"enum","name":"action","property":"action","access":1,"values":["shake","wakeup","fall","tap","slide","flip180","flip90","rotate_left","rotate_right"],"description":"Triggered action (e.g. a button click)"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"toZigbee":[],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},"endpoint":{"ID":1,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":54685,"deviceIeeeAddress":"0x00158d00028aee30","clusters":{"genBasic":{"attributes":{"65281":{"1":2965,"3":19,"4":17320,"5":264,"6":[0,1],"10":0,"151":1,"152":3918,"153":2933,"154":4}}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":54685,"deviceIeeeAddress":"0x00158d00028aee30","clusters":{"genBasic":{"attributes":{"65281":{"1":2965,"3":19,"4":17320,"5":264,"6":[0,1],"10":0,"151":1,"152":3918,"153":2933,"154":4}}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":2,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":54685,"deviceIeeeAddress":"0x00158d00028aee30","clusters":{"genMultistateInput":{"attributes":{"presentValue":2}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":3,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":54685,"deviceIeeeAddress":"0x00158d00028aee30","clusters":{"genAnalogInput":{"attributes":{"65285":500,"presentValue":12.239999771118164}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d00028aee30"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Temperatur (Wohnzimmer)","type":"WSDCGQ11LM","icon":"img/aqara_temperature_sensor.png"},"native":{"id":"00158d0002b51c42"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d0002b51c42","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":10,"link_quality_lc":1639668662555,"battery":45,"statesDef":[{"id":"zigbee.0.00158d0002b51c42.humidity","name":"Humidity","type":"number","read":true,"write":false,"val":49.58,"role":"value.humidity","unit":"%"},{"id":"zigbee.0.00158d0002b51c42.pressure","name":"Pressure","type":"number","read":true,"write":false,"val":1031.6,"role":"value.pressure","unit":"hPa"},{"id":"zigbee.0.00158d0002b51c42.temperature","name":"Temperature","type":"number","read":true,"write":false,"val":21.52,"role":"value.temperature","unit":"°C"},{"id":"zigbee.0.00158d0002b51c42.voltage","name":"Battery voltage","type":"number","read":true,"write":false,"val":2.905,"role":"battery.voltage","unit":"V"}],"icon":"img/aqara_temperature_sensor.png","info":{"type":"device","device":{"ID":23,"_type":"EndDevice","_ieeeAddr":"0x00158d0002b51c42","_networkAddress":49773,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":49773,"deviceIeeeAddress":"0x00158d0002b51c42","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2152}},"msRelativeHumidity":{"attributes":{"measuredValue":4958}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10316}},"genBasic":{"attributes":{"65281":{"1":2905,"4":17320,"5":100,"6":[0,1],"10":47504,"100":2140,"101":4904,"102":103126},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001","modelId":"lumi.weather"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.weather","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":30,"_dateCode":"20161129","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668367804},"mapped":{"zigbeeModel":["lumi.weather"],"model":"WSDCGQ11LM","vendor":"Xiaomi","description":"Aqara temperature, humidity and pressure sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"msTemperatureMeasurement","options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}],"type":["attributeReport","readResponse"]},{"cluster":"msRelativeHumidity","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."}]},{"cluster":"msPressureMeasurement","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"humidity","property":"humidity","access":1,"unit":"%","description":"Measured relative humidity"},{"type":"numeric","name":"pressure","property":"pressure","access":1,"unit":"hPa","description":"The measured atmospheric pressure"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."}]},"endpoint":{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":49773,"deviceIeeeAddress":"0x00158d0002b51c42","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2152}},"msRelativeHumidity":{"attributes":{"measuredValue":4958}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10316}},"genBasic":{"attributes":{"65281":{"1":2905,"4":17320,"5":100,"6":[0,1],"10":47504,"100":2140,"101":4904,"102":103126},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001","modelId":"lumi.weather"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":49773,"deviceIeeeAddress":"0x00158d0002b51c42","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2152}},"msRelativeHumidity":{"attributes":{"measuredValue":4958}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10316}},"genBasic":{"attributes":{"65281":{"1":2905,"4":17320,"5":100,"6":[0,1],"10":47504,"100":2140,"101":4904,"102":103126},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001","modelId":"lumi.weather"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d0002b51c42"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Temperatur (Schlafzimmer)","type":"WSDCGQ11LM","icon":"img/aqara_temperature_sensor.png"},"native":{"id":"00158d0002b54752"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d0002b54752","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":10,"link_quality_lc":1639668662553,"battery":51,"statesDef":[{"id":"zigbee.0.00158d0002b54752.humidity","name":"Humidity","type":"number","read":true,"write":false,"val":51.13,"role":"value.humidity","unit":"%"},{"id":"zigbee.0.00158d0002b54752.pressure","name":"Pressure","type":"number","read":true,"write":false,"val":1031.3,"role":"value.pressure","unit":"hPa"},{"id":"zigbee.0.00158d0002b54752.temperature","name":"Temperature","type":"number","read":true,"write":false,"val":21.31,"role":"value.temperature","unit":"°C"},{"id":"zigbee.0.00158d0002b54752.voltage","name":"Battery voltage","type":"number","read":true,"write":false,"val":2.915,"role":"battery.voltage","unit":"V"}],"icon":"img/aqara_temperature_sensor.png","info":{"type":"device","device":{"ID":20,"_type":"EndDevice","_ieeeAddr":"0x00158d0002b54752","_networkAddress":39900,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":39900,"deviceIeeeAddress":"0x00158d0002b54752","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2131}},"msRelativeHumidity":{"attributes":{"measuredValue":5113}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10313}},"genBasic":{"attributes":{"65281":{"1":2915,"4":17320,"5":18,"6":[0,1],"10":18602,"100":2165,"101":5928,"102":102898},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.weather","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":30,"_dateCode":"20161129","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639667987037},"mapped":{"zigbeeModel":["lumi.weather"],"model":"WSDCGQ11LM","vendor":"Xiaomi","description":"Aqara temperature, humidity and pressure sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"msTemperatureMeasurement","options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}],"type":["attributeReport","readResponse"]},{"cluster":"msRelativeHumidity","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."}]},{"cluster":"msPressureMeasurement","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"humidity","property":"humidity","access":1,"unit":"%","description":"Measured relative humidity"},{"type":"numeric","name":"pressure","property":"pressure","access":1,"unit":"hPa","description":"The measured atmospheric pressure"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."}]},"endpoint":{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":39900,"deviceIeeeAddress":"0x00158d0002b54752","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2131}},"msRelativeHumidity":{"attributes":{"measuredValue":5113}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10313}},"genBasic":{"attributes":{"65281":{"1":2915,"4":17320,"5":18,"6":[0,1],"10":18602,"100":2165,"101":5928,"102":102898},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":39900,"deviceIeeeAddress":"0x00158d0002b54752","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2131}},"msRelativeHumidity":{"attributes":{"measuredValue":5113}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10313}},"genBasic":{"attributes":{"65281":{"1":2915,"4":17320,"5":18,"6":[0,1],"10":18602,"100":2165,"101":5928,"102":102898},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d0002b54752"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Temperatur (Arbeitszimmer)","type":"WSDCGQ11LM","icon":"img/aqara_temperature_sensor.png"},"native":{"id":"00158d0002b54a17"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662545,"_id":"zigbee.0.00158d0002b54a17","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":10,"link_quality_lc":1639668662548,"battery":74,"statesDef":[{"id":"zigbee.0.00158d0002b54a17.humidity","name":"Humidity","type":"number","read":true,"write":false,"val":46.86,"role":"value.humidity","unit":"%"},{"id":"zigbee.0.00158d0002b54a17.pressure","name":"Pressure","type":"number","read":true,"write":false,"val":1031.4,"role":"value.pressure","unit":"hPa"},{"id":"zigbee.0.00158d0002b54a17.temperature","name":"Temperature","type":"number","read":true,"write":false,"val":22.11,"role":"value.temperature","unit":"°C"},{"id":"zigbee.0.00158d0002b54a17.voltage","name":"Battery voltage","type":"number","read":true,"write":false,"val":2.955,"role":"battery.voltage","unit":"V"}],"icon":"img/aqara_temperature_sensor.png","info":{"type":"device","device":{"ID":2,"_type":"EndDevice","_ieeeAddr":"0x00158d0002b54a17","_networkAddress":63636,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":63636,"deviceIeeeAddress":"0x00158d0002b54a17","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2211}},"msRelativeHumidity":{"attributes":{"measuredValue":4686}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10314}},"genBasic":{"attributes":{"65281":{"1":2955,"4":17320,"5":35,"6":[0,1],"10":32268,"100":2206,"101":4686,"102":103143},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.weather","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":30,"_dateCode":"20161129","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668296512},"mapped":{"zigbeeModel":["lumi.weather"],"model":"WSDCGQ11LM","vendor":"Xiaomi","description":"Aqara temperature, humidity and pressure sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"msTemperatureMeasurement","options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}],"type":["attributeReport","readResponse"]},{"cluster":"msRelativeHumidity","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."}]},{"cluster":"msPressureMeasurement","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"humidity","property":"humidity","access":1,"unit":"%","description":"Measured relative humidity"},{"type":"numeric","name":"pressure","property":"pressure","access":1,"unit":"hPa","description":"The measured atmospheric pressure"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."}]},"endpoint":{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":63636,"deviceIeeeAddress":"0x00158d0002b54a17","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2211}},"msRelativeHumidity":{"attributes":{"measuredValue":4686}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10314}},"genBasic":{"attributes":{"65281":{"1":2955,"4":17320,"5":35,"6":[0,1],"10":32268,"100":2206,"101":4686,"102":103143},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":63636,"deviceIeeeAddress":"0x00158d0002b54a17","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2211}},"msRelativeHumidity":{"attributes":{"measuredValue":4686}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10314}},"genBasic":{"attributes":{"65281":{"1":2955,"4":17320,"5":35,"6":[0,1],"10":32268,"100":2206,"101":4686,"102":103143},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d0002b54a17"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Deckenleuchte 2/4 (Schlafzimmer)","type":"ZNLDP12LM","icon":"img/aqara_bulb.png"},"native":{"id":"00158d0002b7d6a9"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d0002b7d6a9","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":0,"link_quality_lc":1639668684738,"statesDef":[{"id":"zigbee.0.00158d0002b7d6a9.brightness","name":"Brightness","type":"number","read":true,"write":true,"val":100,"role":"level.dimmer"},{"id":"zigbee.0.00158d0002b7d6a9.colortemp","name":"Color temperature","type":"number","read":true,"write":true,"val":346,"role":"level.color.temperature"},{"id":"zigbee.0.00158d0002b7d6a9.colortemp_move","name":"Colortemp change","type":"number","read":false,"write":true,"role":"state"},{"id":"zigbee.0.00158d0002b7d6a9.effect","name":"Triggers an effect on the light (e.g. make light blink for a few seconds)","type":"string","read":true,"write":true,"role":"state","states":"blink:blink;breathe:breathe;okay:okay;channel_change:channel_change;finish_effect:finish_effect;stop_effect:stop_effect"},{"id":"zigbee.0.00158d0002b7d6a9.power_outage_memory","name":"Enable/disable the power outage memory, this recovers the on/off mode after power failure","type":"boolean","read":true,"write":true,"role":"state"},{"id":"zigbee.0.00158d0002b7d6a9.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":true,"role":"switch"},{"id":"zigbee.0.00158d0002b7d6a9.transition_time","name":"Transition time","type":"number","read":false,"write":true,"role":"state","unit":"sec"}],"icon":"img/aqara_bulb.png","info":{"type":"device","device":{"ID":29,"_type":"Router","_ieeeAddr":"0x00158d0002b7d6a9","_networkAddress":19263,"_manufacturerID":4447,"_endpoints":[{"ID":1,"profileID":260,"deviceID":258,"inputClusters":[0,4,3,5,10,258,13,19,6,1,1030,8,768,1027,1029,1026],"outputClusters":[25,10,13,258,19,6,1,1030,8,768],"deviceNetworkAddress":19263,"deviceIeeeAddress":"0x00158d0002b7d6a9","clusters":{"genBasic":{"attributes":{"65281":{"3":74,"5":376,"7":"0x0000000000000000","8":278,"9":1792,"10":0,"100":1,"101":254,"102":346},"manufacturerName":"LUMI","powerSource":4,"zclVersion":1,"stackVersion":2,"hwVersion":1,"dateCode":"09-30-2018","swBuildId":"1.22\u0000","modelId":"lumi.light.aqcn02"}},"genOnOff":{"attributes":{"61440":117440752,"onOff":1}},"lightingColorCtrl":{"attributes":{"colorTemperature":346,"tuyaRgbMode":4931328,"colorMode":1}},"genLevelCtrl":{"attributes":{"61440":4931328,"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"DC Source","_modelID":"lumi.light.aqcn02","_applicationVersion":22,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"09-30-2018","_softwareBuildID":"1.22\u0000","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639597260119},"mapped":{"zigbeeModel":["lumi.light.aqcn02"],"model":"ZNLDP12LM","vendor":"Xiaomi","description":"Aqara smart LED bulb","toZigbee":[{"key":["state","brightness","brightness_percent"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp","color_temp_percent"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."},{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["transition"],"attr":[]},{"key":["rate"],"attr":[]},{"key":["brightness_move","brightness_move_onoff"]},{"key":["colortemp_move","color_temp_move"]},{"key":["brightness_step","brightness_step_onoff"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_step"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["level_config"]},{"key":["power_on_behavior"]},{"key":["color_options"]},{"key":["color_mode"]},{"key":["effect","alert","flash"]},{"key":["power_outage_memory"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"fromZigbee":[{"cluster":"lightingColorCtrl","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"msOccupancySensing","type":["attributeReport","readResponse"]},{"cluster":"msRelativeHumidity","type":["attributeReport","readResponse"]},{"cluster":"msPressureMeasurement","type":["attributeReport","readResponse"]},{"cluster":"msTemperatureMeasurement","type":["attributeReport","readResponse"]}],"exposes":[{"type":"light","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","value_toggle":"TOGGLE","description":"On/off state of this light"},{"type":"numeric","name":"brightness","property":"brightness","access":7,"value_min":0,"value_max":254,"description":"Brightness of this light"},{"type":"numeric","name":"color_temp","property":"color_temp","access":7,"unit":"mired","value_min":150,"value_max":500,"description":"Color temperature of this light","presets":[{"name":"coolest","value":150,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":500,"description":"Warmest temperature supported"}]}]},{"type":"enum","name":"effect","property":"effect","access":2,"values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)"},{"type":"binary","name":"power_outage_memory","property":"power_outage_memory","access":3,"value_on":true,"value_off":false,"description":"Enable/disable the power outage memory, this recovers the on/off mode after power failure"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"ota":{},"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."},{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},"endpoint":{"ID":1,"profileID":260,"deviceID":258,"inputClusters":[0,4,3,5,10,258,13,19,6,1,1030,8,768,1027,1029,1026],"outputClusters":[25,10,13,258,19,6,1,1030,8,768],"deviceNetworkAddress":19263,"deviceIeeeAddress":"0x00158d0002b7d6a9","clusters":{"genBasic":{"attributes":{"65281":{"3":74,"5":376,"7":"0x0000000000000000","8":278,"9":1792,"10":0,"100":1,"101":254,"102":346},"manufacturerName":"LUMI","powerSource":4,"zclVersion":1,"stackVersion":2,"hwVersion":1,"dateCode":"09-30-2018","swBuildId":"1.22\u0000","modelId":"lumi.light.aqcn02"}},"genOnOff":{"attributes":{"61440":117440752,"onOff":1}},"lightingColorCtrl":{"attributes":{"colorTemperature":346,"tuyaRgbMode":4931328,"colorMode":1}},"genLevelCtrl":{"attributes":{"61440":4931328,"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":258,"inputClusters":[0,4,3,5,10,258,13,19,6,1,1030,8,768,1027,1029,1026],"outputClusters":[25,10,13,258,19,6,1,1030,8,768],"deviceNetworkAddress":19263,"deviceIeeeAddress":"0x00158d0002b7d6a9","clusters":{"genBasic":{"attributes":{"65281":{"3":74,"5":376,"7":"0x0000000000000000","8":278,"9":1792,"10":0,"100":1,"101":254,"102":346},"manufacturerName":"LUMI","powerSource":4,"zclVersion":1,"stackVersion":2,"hwVersion":1,"dateCode":"09-30-2018","swBuildId":"1.22\u0000","modelId":"lumi.light.aqcn02"}},"genOnOff":{"attributes":{"61440":117440752,"onOff":1}},"lightingColorCtrl":{"attributes":{"colorTemperature":346,"tuyaRgbMode":4931328,"colorMode":1}},"genLevelCtrl":{"attributes":{"61440":4931328,"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d0002b7d6a9"},"rooms":[],"paired":true,"groups":["1"]},{"type":"device","common":{"name":"Deckenleuchte 3/4 (Schlafzimmer)","type":"ZNLDP12LM","icon":"img/aqara_bulb.png"},"native":{"id":"00158d0002b7d87c"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d0002b7d87c","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":0,"link_quality_lc":1639668684575,"statesDef":[{"id":"zigbee.0.00158d0002b7d87c.brightness","name":"Brightness","type":"number","read":true,"write":true,"val":100,"role":"level.dimmer"},{"id":"zigbee.0.00158d0002b7d87c.colortemp","name":"Color temperature","type":"number","read":true,"write":true,"val":346,"role":"level.color.temperature"},{"id":"zigbee.0.00158d0002b7d87c.colortemp_move","name":"Colortemp change","type":"number","read":false,"write":true,"role":"state"},{"id":"zigbee.0.00158d0002b7d87c.effect","name":"Triggers an effect on the light (e.g. make light blink for a few seconds)","type":"string","read":true,"write":true,"role":"state","states":"blink:blink;breathe:breathe;okay:okay;channel_change:channel_change;finish_effect:finish_effect;stop_effect:stop_effect"},{"id":"zigbee.0.00158d0002b7d87c.power_outage_memory","name":"Enable/disable the power outage memory, this recovers the on/off mode after power failure","type":"boolean","read":true,"write":true,"role":"state"},{"id":"zigbee.0.00158d0002b7d87c.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":true,"role":"switch"},{"id":"zigbee.0.00158d0002b7d87c.transition_time","name":"Transition time","type":"number","read":false,"write":true,"role":"state","unit":"sec"}],"icon":"img/aqara_bulb.png","info":{"type":"device","device":{"ID":28,"_type":"Router","_ieeeAddr":"0x00158d0002b7d87c","_networkAddress":35436,"_manufacturerID":4447,"_endpoints":[{"ID":1,"profileID":260,"deviceID":258,"inputClusters":[0,4,3,5,10,258,13,19,6,1,1030,8,768,1027,1029,1026],"outputClusters":[25,10,13,258,19,6,1,1030,8,768],"deviceNetworkAddress":35436,"deviceIeeeAddress":"0x00158d0002b7d87c","clusters":{"genBasic":{"attributes":{"65281":{"3":76,"5":351,"7":"0x0000000000000000","8":278,"9":1792,"10":0,"100":1,"101":254,"102":346},"manufacturerName":"LUMI","powerSource":4,"zclVersion":1,"stackVersion":2,"hwVersion":1,"dateCode":"09-30-2018","swBuildId":"1.22\u0000","modelId":"lumi.light.aqcn02"}},"genOnOff":{"attributes":{"61440":117440752,"onOff":1}},"lightingColorCtrl":{"attributes":{"colorTemperature":346,"tuyaRgbMode":9071616,"colorMode":1}},"genLevelCtrl":{"attributes":{"61440":9071616,"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"DC Source","_modelID":"lumi.light.aqcn02","_applicationVersion":22,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"09-30-2018","_softwareBuildID":"1.22\u0000","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639597258122},"mapped":{"zigbeeModel":["lumi.light.aqcn02"],"model":"ZNLDP12LM","vendor":"Xiaomi","description":"Aqara smart LED bulb","toZigbee":[{"key":["state","brightness","brightness_percent"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp","color_temp_percent"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."},{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["transition"],"attr":[]},{"key":["rate"],"attr":[]},{"key":["brightness_move","brightness_move_onoff"]},{"key":["colortemp_move","color_temp_move"]},{"key":["brightness_step","brightness_step_onoff"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_step"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["level_config"]},{"key":["power_on_behavior"]},{"key":["color_options"]},{"key":["color_mode"]},{"key":["effect","alert","flash"]},{"key":["power_outage_memory"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"fromZigbee":[{"cluster":"lightingColorCtrl","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"msOccupancySensing","type":["attributeReport","readResponse"]},{"cluster":"msRelativeHumidity","type":["attributeReport","readResponse"]},{"cluster":"msPressureMeasurement","type":["attributeReport","readResponse"]},{"cluster":"msTemperatureMeasurement","type":["attributeReport","readResponse"]}],"exposes":[{"type":"light","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","value_toggle":"TOGGLE","description":"On/off state of this light"},{"type":"numeric","name":"brightness","property":"brightness","access":7,"value_min":0,"value_max":254,"description":"Brightness of this light"},{"type":"numeric","name":"color_temp","property":"color_temp","access":7,"unit":"mired","value_min":150,"value_max":500,"description":"Color temperature of this light","presets":[{"name":"coolest","value":150,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":500,"description":"Warmest temperature supported"}]}]},{"type":"enum","name":"effect","property":"effect","access":2,"values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)"},{"type":"binary","name":"power_outage_memory","property":"power_outage_memory","access":3,"value_on":true,"value_off":false,"description":"Enable/disable the power outage memory, this recovers the on/off mode after power failure"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"ota":{},"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."},{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},"endpoint":{"ID":1,"profileID":260,"deviceID":258,"inputClusters":[0,4,3,5,10,258,13,19,6,1,1030,8,768,1027,1029,1026],"outputClusters":[25,10,13,258,19,6,1,1030,8,768],"deviceNetworkAddress":35436,"deviceIeeeAddress":"0x00158d0002b7d87c","clusters":{"genBasic":{"attributes":{"65281":{"3":76,"5":351,"7":"0x0000000000000000","8":278,"9":1792,"10":0,"100":1,"101":254,"102":346},"manufacturerName":"LUMI","powerSource":4,"zclVersion":1,"stackVersion":2,"hwVersion":1,"dateCode":"09-30-2018","swBuildId":"1.22\u0000","modelId":"lumi.light.aqcn02"}},"genOnOff":{"attributes":{"61440":117440752,"onOff":1}},"lightingColorCtrl":{"attributes":{"colorTemperature":346,"tuyaRgbMode":9071616,"colorMode":1}},"genLevelCtrl":{"attributes":{"61440":9071616,"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":258,"inputClusters":[0,4,3,5,10,258,13,19,6,1,1030,8,768,1027,1029,1026],"outputClusters":[25,10,13,258,19,6,1,1030,8,768],"deviceNetworkAddress":35436,"deviceIeeeAddress":"0x00158d0002b7d87c","clusters":{"genBasic":{"attributes":{"65281":{"3":76,"5":351,"7":"0x0000000000000000","8":278,"9":1792,"10":0,"100":1,"101":254,"102":346},"manufacturerName":"LUMI","powerSource":4,"zclVersion":1,"stackVersion":2,"hwVersion":1,"dateCode":"09-30-2018","swBuildId":"1.22\u0000","modelId":"lumi.light.aqcn02"}},"genOnOff":{"attributes":{"61440":117440752,"onOff":1}},"lightingColorCtrl":{"attributes":{"colorTemperature":346,"tuyaRgbMode":9071616,"colorMode":1}},"genLevelCtrl":{"attributes":{"61440":9071616,"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d0002b7d87c"},"rooms":[],"paired":true,"groups":["1"]},{"type":"device","common":{"name":"Deckenleuchte 1/4 (Schlafzimmer)","type":"ZNLDP12LM","icon":"img/aqara_bulb.png"},"native":{"id":"00158d0002b805e3"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d0002b805e3","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":0,"link_quality_lc":1639668685085,"statesDef":[{"id":"zigbee.0.00158d0002b805e3.brightness","name":"Brightness","type":"number","read":true,"write":true,"val":100,"role":"level.dimmer"},{"id":"zigbee.0.00158d0002b805e3.colortemp","name":"Color temperature","type":"number","read":true,"write":true,"val":346,"role":"level.color.temperature"},{"id":"zigbee.0.00158d0002b805e3.colortemp_move","name":"Colortemp change","type":"number","read":false,"write":true,"role":"state"},{"id":"zigbee.0.00158d0002b805e3.effect","name":"Triggers an effect on the light (e.g. make light blink for a few seconds)","type":"string","read":true,"write":true,"role":"state","states":"blink:blink;breathe:breathe;okay:okay;channel_change:channel_change;finish_effect:finish_effect;stop_effect:stop_effect"},{"id":"zigbee.0.00158d0002b805e3.power_outage_memory","name":"Enable/disable the power outage memory, this recovers the on/off mode after power failure","type":"boolean","read":true,"write":true,"role":"state"},{"id":"zigbee.0.00158d0002b805e3.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":true,"role":"switch"},{"id":"zigbee.0.00158d0002b805e3.transition_time","name":"Transition time","type":"number","read":false,"write":true,"role":"state","unit":"sec"}],"icon":"img/aqara_bulb.png","info":{"type":"device","device":{"ID":27,"_type":"Router","_ieeeAddr":"0x00158d0002b805e3","_networkAddress":39725,"_manufacturerID":4447,"_endpoints":[{"ID":1,"profileID":260,"deviceID":258,"inputClusters":[0,4,3,5,10,258,13,19,6,1,1030,8,768,1027,1029,1026],"outputClusters":[25,10,13,258,19,6,1,1030,8,768],"deviceNetworkAddress":39725,"deviceIeeeAddress":"0x00158d0002b805e3","clusters":{"genBasic":{"attributes":{"65281":{"3":69,"5":322,"7":"0x0000000000000000","8":278,"9":1792,"10":41267,"100":1,"101":254,"102":346},"manufacturerName":"LUMI","powerSource":4,"zclVersion":1,"stackVersion":2,"hwVersion":1,"dateCode":"09-30-2018","swBuildId":"1.22\u0000","modelId":"lumi.light.aqcn02"}},"genOnOff":{"attributes":{"61440":117440752,"onOff":1}},"lightingColorCtrl":{"attributes":{"colorTemperature":346,"tuyaRgbMode":10169600,"colorMode":1}},"genLevelCtrl":{"attributes":{"61440":10169600,"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"DC Source","_modelID":"lumi.light.aqcn02","_applicationVersion":22,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"09-30-2018","_softwareBuildID":"1.22\u0000","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639597212133},"mapped":{"zigbeeModel":["lumi.light.aqcn02"],"model":"ZNLDP12LM","vendor":"Xiaomi","description":"Aqara smart LED bulb","toZigbee":[{"key":["state","brightness","brightness_percent"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp","color_temp_percent"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."},{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["transition"],"attr":[]},{"key":["rate"],"attr":[]},{"key":["brightness_move","brightness_move_onoff"]},{"key":["colortemp_move","color_temp_move"]},{"key":["brightness_step","brightness_step_onoff"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_step"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["level_config"]},{"key":["power_on_behavior"]},{"key":["color_options"]},{"key":["color_mode"]},{"key":["effect","alert","flash"]},{"key":["power_outage_memory"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"fromZigbee":[{"cluster":"lightingColorCtrl","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"msOccupancySensing","type":["attributeReport","readResponse"]},{"cluster":"msRelativeHumidity","type":["attributeReport","readResponse"]},{"cluster":"msPressureMeasurement","type":["attributeReport","readResponse"]},{"cluster":"msTemperatureMeasurement","type":["attributeReport","readResponse"]}],"exposes":[{"type":"light","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","value_toggle":"TOGGLE","description":"On/off state of this light"},{"type":"numeric","name":"brightness","property":"brightness","access":7,"value_min":0,"value_max":254,"description":"Brightness of this light"},{"type":"numeric","name":"color_temp","property":"color_temp","access":7,"unit":"mired","value_min":150,"value_max":500,"description":"Color temperature of this light","presets":[{"name":"coolest","value":150,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":500,"description":"Warmest temperature supported"}]}]},{"type":"enum","name":"effect","property":"effect","access":2,"values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)"},{"type":"binary","name":"power_outage_memory","property":"power_outage_memory","access":3,"value_on":true,"value_off":false,"description":"Enable/disable the power outage memory, this recovers the on/off mode after power failure"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"ota":{},"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."},{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},"endpoint":{"ID":1,"profileID":260,"deviceID":258,"inputClusters":[0,4,3,5,10,258,13,19,6,1,1030,8,768,1027,1029,1026],"outputClusters":[25,10,13,258,19,6,1,1030,8,768],"deviceNetworkAddress":39725,"deviceIeeeAddress":"0x00158d0002b805e3","clusters":{"genBasic":{"attributes":{"65281":{"3":69,"5":322,"7":"0x0000000000000000","8":278,"9":1792,"10":41267,"100":1,"101":254,"102":346},"manufacturerName":"LUMI","powerSource":4,"zclVersion":1,"stackVersion":2,"hwVersion":1,"dateCode":"09-30-2018","swBuildId":"1.22\u0000","modelId":"lumi.light.aqcn02"}},"genOnOff":{"attributes":{"61440":117440752,"onOff":1}},"lightingColorCtrl":{"attributes":{"colorTemperature":346,"tuyaRgbMode":10169600,"colorMode":1}},"genLevelCtrl":{"attributes":{"61440":10169600,"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":258,"inputClusters":[0,4,3,5,10,258,13,19,6,1,1030,8,768,1027,1029,1026],"outputClusters":[25,10,13,258,19,6,1,1030,8,768],"deviceNetworkAddress":39725,"deviceIeeeAddress":"0x00158d0002b805e3","clusters":{"genBasic":{"attributes":{"65281":{"3":69,"5":322,"7":"0x0000000000000000","8":278,"9":1792,"10":41267,"100":1,"101":254,"102":346},"manufacturerName":"LUMI","powerSource":4,"zclVersion":1,"stackVersion":2,"hwVersion":1,"dateCode":"09-30-2018","swBuildId":"1.22\u0000","modelId":"lumi.light.aqcn02"}},"genOnOff":{"attributes":{"61440":117440752,"onOff":1}},"lightingColorCtrl":{"attributes":{"colorTemperature":346,"tuyaRgbMode":10169600,"colorMode":1}},"genLevelCtrl":{"attributes":{"61440":10169600,"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d0002b805e3"},"rooms":[],"paired":true,"groups":["1"]},{"type":"device","common":{"name":"Deckenleuchte 4/4 (Schlafzimmer)","type":"ZNLDP12LM","icon":"img/aqara_bulb.png"},"native":{"id":"00158d0002c65ed8"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662545,"_id":"zigbee.0.00158d0002c65ed8","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":0,"link_quality_lc":1639668683543,"statesDef":[{"id":"zigbee.0.00158d0002c65ed8.brightness","name":"Brightness","type":"number","read":true,"write":true,"val":100,"role":"level.dimmer","unit":""},{"id":"zigbee.0.00158d0002c65ed8.colortemp","name":"Color temperature","type":"number","read":true,"write":true,"val":346,"role":"level.color.temperature"},{"id":"zigbee.0.00158d0002c65ed8.colortemp_move","name":"Colortemp change","type":"number","read":false,"write":true,"role":"state"},{"id":"zigbee.0.00158d0002c65ed8.effect","name":"Triggers an effect on the light (e.g. make light blink for a few seconds)","type":"string","read":true,"write":true,"role":"state","states":"blink:blink;breathe:breathe;okay:okay;channel_change:channel_change;finish_effect:finish_effect;stop_effect:stop_effect"},{"id":"zigbee.0.00158d0002c65ed8.power_outage_memory","name":"Enable/disable the power outage memory, this recovers the on/off mode after power failure","type":"boolean","read":true,"write":true,"role":"state"},{"id":"zigbee.0.00158d0002c65ed8.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":true,"role":"switch"},{"id":"zigbee.0.00158d0002c65ed8.transition_time","name":"Transition time","type":"number","read":false,"write":true,"role":"state","unit":"sec"}],"icon":"img/aqara_bulb.png","info":{"type":"device","device":{"ID":6,"_type":"Router","_ieeeAddr":"0x00158d0002c65ed8","_networkAddress":41267,"_manufacturerID":4447,"_endpoints":[{"ID":1,"profileID":260,"deviceID":258,"inputClusters":[0,4,3,5,10,258,13,19,6,1,1030,8,768,1027,1029,1026],"outputClusters":[25,10,13,258,19,6,1,1030,8,768],"deviceNetworkAddress":41267,"deviceIeeeAddress":"0x00158d0002c65ed8","clusters":{"genBasic":{"attributes":{"65281":{"3":86,"5":430,"7":"0x0000000000000000","8":279,"9":1792,"10":0,"100":1,"101":254,"102":346},"modelId":"lumi.light.aqcn02","appVersion":23,"manufacturerName":"LUMI","powerSource":4,"zclVersion":1,"stackVersion":2,"hwVersion":1,"dateCode":"11-22-2018","swBuildId":"1.23\u0000"}},"genOnOff":{"attributes":{"61440":117440752,"onOff":1}},"msTemperatureMeasurement":{"attributes":{"measuredValue":2122}},"lightingColorCtrl":{"attributes":{"colorTemperature":346,"tuyaRgbMode":10564352,"colorMode":1}},"genLevelCtrl":{"attributes":{"61440":10564352,"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"DC Source","_modelID":"lumi.light.aqcn02","_applicationVersion":23,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"11-22-2018","_softwareBuildID":"1.23\u0000","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":2},"_lastSeen":1639597631149},"mapped":{"zigbeeModel":["lumi.light.aqcn02"],"model":"ZNLDP12LM","vendor":"Xiaomi","description":"Aqara smart LED bulb","toZigbee":[{"key":["state","brightness","brightness_percent"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp","color_temp_percent"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."},{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["transition"],"attr":[]},{"key":["rate"],"attr":[]},{"key":["brightness_move","brightness_move_onoff"]},{"key":["colortemp_move","color_temp_move"]},{"key":["brightness_step","brightness_step_onoff"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_step"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["level_config"]},{"key":["power_on_behavior"]},{"key":["color_options"]},{"key":["color_mode"]},{"key":["effect","alert","flash"]},{"key":["power_outage_memory"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"fromZigbee":[{"cluster":"lightingColorCtrl","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"msOccupancySensing","type":["attributeReport","readResponse"]},{"cluster":"msRelativeHumidity","type":["attributeReport","readResponse"]},{"cluster":"msPressureMeasurement","type":["attributeReport","readResponse"]},{"cluster":"msTemperatureMeasurement","type":["attributeReport","readResponse"]}],"exposes":[{"type":"light","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","value_toggle":"TOGGLE","description":"On/off state of this light"},{"type":"numeric","name":"brightness","property":"brightness","access":7,"value_min":0,"value_max":254,"description":"Brightness of this light"},{"type":"numeric","name":"color_temp","property":"color_temp","access":7,"unit":"mired","value_min":150,"value_max":500,"description":"Color temperature of this light","presets":[{"name":"coolest","value":150,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":500,"description":"Warmest temperature supported"}]}]},{"type":"enum","name":"effect","property":"effect","access":2,"values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)"},{"type":"binary","name":"power_outage_memory","property":"power_outage_memory","access":3,"value_on":true,"value_off":false,"description":"Enable/disable the power outage memory, this recovers the on/off mode after power failure"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"ota":{},"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."},{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},"endpoint":{"ID":1,"profileID":260,"deviceID":258,"inputClusters":[0,4,3,5,10,258,13,19,6,1,1030,8,768,1027,1029,1026],"outputClusters":[25,10,13,258,19,6,1,1030,8,768],"deviceNetworkAddress":41267,"deviceIeeeAddress":"0x00158d0002c65ed8","clusters":{"genBasic":{"attributes":{"65281":{"3":86,"5":430,"7":"0x0000000000000000","8":279,"9":1792,"10":0,"100":1,"101":254,"102":346},"modelId":"lumi.light.aqcn02","appVersion":23,"manufacturerName":"LUMI","powerSource":4,"zclVersion":1,"stackVersion":2,"hwVersion":1,"dateCode":"11-22-2018","swBuildId":"1.23\u0000"}},"genOnOff":{"attributes":{"61440":117440752,"onOff":1}},"msTemperatureMeasurement":{"attributes":{"measuredValue":2122}},"lightingColorCtrl":{"attributes":{"colorTemperature":346,"tuyaRgbMode":10564352,"colorMode":1}},"genLevelCtrl":{"attributes":{"61440":10564352,"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":258,"inputClusters":[0,4,3,5,10,258,13,19,6,1,1030,8,768,1027,1029,1026],"outputClusters":[25,10,13,258,19,6,1,1030,8,768],"deviceNetworkAddress":41267,"deviceIeeeAddress":"0x00158d0002c65ed8","clusters":{"genBasic":{"attributes":{"65281":{"3":86,"5":430,"7":"0x0000000000000000","8":279,"9":1792,"10":0,"100":1,"101":254,"102":346},"modelId":"lumi.light.aqcn02","appVersion":23,"manufacturerName":"LUMI","powerSource":4,"zclVersion":1,"stackVersion":2,"hwVersion":1,"dateCode":"11-22-2018","swBuildId":"1.23\u0000"}},"genOnOff":{"attributes":{"61440":117440752,"onOff":1}},"msTemperatureMeasurement":{"attributes":{"measuredValue":2122}},"lightingColorCtrl":{"attributes":{"colorTemperature":346,"tuyaRgbMode":10564352,"colorMode":1}},"genLevelCtrl":{"attributes":{"61440":10564352,"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d0002c65ed8"},"rooms":[],"paired":true,"groups":["1"]},{"type":"device","common":{"name":"Flurlicht","type":"QBKG04LM","icon":"img/ctrl_neutral1.png"},"native":{"id":"00158d0002e34b33"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d0002e34b33","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":0,"link_quality_lc":1639668722235,"statesDef":[{"id":"zigbee.0.00158d0002e34b33.click","name":"Click event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d0002e34b33.decoupled","name":"Decoupled mode","type":"boolean","read":true,"write":true,"role":"state"},{"id":"zigbee.0.00158d0002e34b33.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":false,"role":"switch"}],"icon":"img/ctrl_neutral1.png","info":{"type":"device","device":{"ID":14,"_type":"EndDevice","_ieeeAddr":"0x00158d0002e34b33","_networkAddress":5016,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":6,"inputClusters":[0,3,1,2,25,10],"outputClusters":[0,10,25],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{"genBasic":{"attributes":{"65281":{"1":3300,"3":28,"5":16,"8":9750,"10":0,"100":1,"101":0,"110":1,"111":255,"153":0,"155":0},"manufacturerName":"LUMI","powerSource":4,"zclVersion":0,"stackVersion":2,"hwVersion":38,"dateCode":"04-25-2018"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":2,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{"genOnOff":{"attributes":{"61440":51615981,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":3,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":4,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{"genOnOff":{"attributes":{"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":5,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":6,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":8,"profileID":260,"deviceID":83,"inputClusters":[12],"outputClusters":[],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"DC Source","_modelID":"lumi.ctrl_neutral1","_applicationVersion":1,"_stackVersion":2,"_zclVersion":0,"_hardwareVersion":38,"_dateCode":"04-25-2018","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1631717605447},"mapped":{"zigbeeModel":["lumi.ctrl_neutral1"],"model":"QBKG04LM","vendor":"Xiaomi","description":"Aqara single key wired wall switch without neutral wire. Doesn't work as a router and doesn't support power meter","fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genOnOff","type":["attributeReport"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"enum","name":"action","property":"action","access":1,"values":["single","release","hold"],"description":"Triggered action (e.g. a button click)"},{"type":"enum","name":"operation_mode","property":"operation_mode","access":7,"values":["control_relay","decoupled"],"description":"Decoupled mode"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["operation_mode"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"ota":{},"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},"endpoint":{"ID":2,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{"genOnOff":{"attributes":{"61440":51615981,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":6,"inputClusters":[0,3,1,2,25,10],"outputClusters":[0,10,25],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{"genBasic":{"attributes":{"65281":{"1":3300,"3":28,"5":16,"8":9750,"10":0,"100":1,"101":0,"110":1,"111":255,"153":0,"155":0},"manufacturerName":"LUMI","powerSource":4,"zclVersion":0,"stackVersion":2,"hwVersion":38,"dateCode":"04-25-2018"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":2,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{"genOnOff":{"attributes":{"61440":51615981,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":3,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":4,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{"genOnOff":{"attributes":{"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":5,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":6,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":8,"profileID":260,"deviceID":83,"inputClusters":[12],"outputClusters":[],"deviceNetworkAddress":5016,"deviceIeeeAddress":"0x00158d0002e34b33","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d0002e34b33"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Badezimmerlicht","type":"QBKG04LM","icon":"img/ctrl_neutral1.png"},"native":{"id":"00158d0002f8d5b4"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d0002f8d5b4","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":0,"link_quality_lc":1639668722230,"statesDef":[{"id":"zigbee.0.00158d0002f8d5b4.click","name":"Click event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d0002f8d5b4.decoupled","name":"Decoupled mode","type":"boolean","read":true,"write":true,"role":"state"},{"id":"zigbee.0.00158d0002f8d5b4.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":false,"role":"switch"}],"icon":"img/ctrl_neutral1.png","info":{"type":"device","device":{"ID":13,"_type":"EndDevice","_ieeeAddr":"0x00158d0002f8d5b4","_networkAddress":29745,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":6,"inputClusters":[0,3,1,2,25,10],"outputClusters":[0,10,25],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{"genBasic":{"attributes":{"65281":{"1":3300,"3":29,"5":98,"8":9750,"10":0,"100":1,"101":0,"110":1,"111":255,"153":0,"155":0},"manufacturerName":"LUMI","powerSource":4,"zclVersion":0,"stackVersion":2,"hwVersion":38,"dateCode":"04-25-2018"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":2,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{"genOnOff":{"attributes":{"61440":57946368,"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":3,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":4,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{"genOnOff":{"attributes":{"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":5,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":6,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":8,"profileID":260,"deviceID":83,"inputClusters":[12],"outputClusters":[],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"DC Source","_modelID":"lumi.ctrl_neutral1","_applicationVersion":1,"_stackVersion":2,"_zclVersion":0,"_hardwareVersion":38,"_dateCode":"04-25-2018","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1631717587342},"mapped":{"zigbeeModel":["lumi.ctrl_neutral1"],"model":"QBKG04LM","vendor":"Xiaomi","description":"Aqara single key wired wall switch without neutral wire. Doesn't work as a router and doesn't support power meter","fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genOnOff","type":["attributeReport"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"enum","name":"action","property":"action","access":1,"values":["single","release","hold"],"description":"Triggered action (e.g. a button click)"},{"type":"enum","name":"operation_mode","property":"operation_mode","access":7,"values":["control_relay","decoupled"],"description":"Decoupled mode"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["operation_mode"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"ota":{},"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},"endpoint":{"ID":2,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{"genOnOff":{"attributes":{"61440":57946368,"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":6,"inputClusters":[0,3,1,2,25,10],"outputClusters":[0,10,25],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{"genBasic":{"attributes":{"65281":{"1":3300,"3":29,"5":98,"8":9750,"10":0,"100":1,"101":0,"110":1,"111":255,"153":0,"155":0},"manufacturerName":"LUMI","powerSource":4,"zclVersion":0,"stackVersion":2,"hwVersion":38,"dateCode":"04-25-2018"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":2,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{"genOnOff":{"attributes":{"61440":57946368,"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":3,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":4,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{"genOnOff":{"attributes":{"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":5,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":6,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":8,"profileID":260,"deviceID":83,"inputClusters":[12],"outputClusters":[],"deviceNetworkAddress":29745,"deviceIeeeAddress":"0x00158d0002f8d5b4","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d0002f8d5b4"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Arbeitszimmerlicht","type":"QBKG04LM","icon":"img/ctrl_neutral1.png"},"native":{"id":"00158d0002f8d76c"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d0002f8d76c","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":0,"link_quality_lc":1639668722228,"statesDef":[{"id":"zigbee.0.00158d0002f8d76c.click","name":"Click event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d0002f8d76c.decoupled","name":"Decoupled mode","type":"boolean","read":true,"write":true,"role":"state"},{"id":"zigbee.0.00158d0002f8d76c.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":false,"role":"switch"}],"icon":"img/ctrl_neutral1.png","info":{"type":"device","device":{"ID":8,"_type":"EndDevice","_ieeeAddr":"0x00158d0002f8d76c","_networkAddress":10251,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":6,"inputClusters":[0,3,1,2,25,10],"outputClusters":[0,10,25],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{"genBasic":{"attributes":{"65281":{"1":3300,"3":29,"5":799,"8":9750,"10":0,"100":0,"101":0,"110":0,"111":255,"153":0,"155":0},"manufacturerName":"LUMI","powerSource":4,"zclVersion":0,"stackVersion":2,"hwVersion":38,"dateCode":"04-25-2018"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":2,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{"genOnOff":{"attributes":{"61440":52956144,"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":3,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":4,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{"genOnOff":{"attributes":{"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":5,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":6,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":8,"profileID":260,"deviceID":83,"inputClusters":[12],"outputClusters":[],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"DC Source","_modelID":"lumi.ctrl_neutral1","_applicationVersion":1,"_stackVersion":2,"_zclVersion":0,"_hardwareVersion":38,"_dateCode":"04-25-2018","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1631717611797},"mapped":{"zigbeeModel":["lumi.ctrl_neutral1"],"model":"QBKG04LM","vendor":"Xiaomi","description":"Aqara single key wired wall switch without neutral wire. Doesn't work as a router and doesn't support power meter","fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genOnOff","type":["attributeReport"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"enum","name":"action","property":"action","access":1,"values":["single","release","hold"],"description":"Triggered action (e.g. a button click)"},{"type":"enum","name":"operation_mode","property":"operation_mode","access":7,"values":["control_relay","decoupled"],"description":"Decoupled mode"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["operation_mode"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"ota":{},"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},"endpoint":{"ID":2,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{"genOnOff":{"attributes":{"61440":52956144,"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":6,"inputClusters":[0,3,1,2,25,10],"outputClusters":[0,10,25],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{"genBasic":{"attributes":{"65281":{"1":3300,"3":29,"5":799,"8":9750,"10":0,"100":0,"101":0,"110":0,"111":255,"153":0,"155":0},"manufacturerName":"LUMI","powerSource":4,"zclVersion":0,"stackVersion":2,"hwVersion":38,"dateCode":"04-25-2018"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":2,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{"genOnOff":{"attributes":{"61440":52956144,"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":3,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":4,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{"genOnOff":{"attributes":{"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":5,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":6,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":8,"profileID":260,"deviceID":83,"inputClusters":[12],"outputClusters":[],"deviceNetworkAddress":10251,"deviceIeeeAddress":"0x00158d0002f8d76c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d0002f8d76c"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Schlafzimmerlicht","type":"QBKG21LM","icon":"img/ctrl_neutral1.png"},"native":{"id":"00158d000521d656"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.00158d000521d656","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":0,"link_quality_lc":1639668722240,"statesDef":[{"id":"zigbee.0.00158d000521d656.click","name":"Click event","type":"boolean","read":true,"write":false,"val":false,"role":"button"},{"id":"zigbee.0.00158d000521d656.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":false,"role":"switch"}],"icon":"img/ctrl_neutral1.png","info":{"type":"device","device":{"ID":15,"_type":"EndDevice","_ieeeAddr":"0x00158d000521d656","_networkAddress":1024,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":6,"inputClusters":[0,3,1,2,25,10],"outputClusters":[0,10,25],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{"genBasic":{"attributes":{"65281":{"1":3300,"3":20,"5":14,"8":13850,"10":0,"100":0,"101":0,"110":0,"111":255,"153":0,"155":0},"manufacturerName":"LUMI","powerSource":4,"zclVersion":0,"stackVersion":2,"hwVersion":54,"dateCode":"03-20-2019"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":2,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{"genOnOff":{"attributes":{"61440":117440754,"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":3,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":4,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{"genOnOff":{"attributes":{"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":5,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":6,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":8,"profileID":260,"deviceID":83,"inputClusters":[12],"outputClusters":[],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"DC Source","_modelID":"lumi.switch.b1lacn02","_applicationVersion":1,"_stackVersion":2,"_zclVersion":0,"_hardwareVersion":54,"_dateCode":"03-20-2019","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1631717612335},"mapped":{"zigbeeModel":["lumi.switch.b1lacn02"],"model":"QBKG21LM","vendor":"Xiaomi","description":"Aqara D1 single gang smart wall switch (no neutral wire)","fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genOnOff","type":["attributeReport"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"enum","name":"action","property":"action","access":1,"values":["single","hold","release"],"description":"Triggered action (e.g. a button click)"},{"type":"enum","name":"operation_mode","property":"operation_mode","access":7,"values":["control_relay","decoupled"],"description":"Decoupled mode"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["operation_mode"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},"endpoint":{"ID":2,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{"genOnOff":{"attributes":{"61440":117440754,"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":6,"inputClusters":[0,3,1,2,25,10],"outputClusters":[0,10,25],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{"genBasic":{"attributes":{"65281":{"1":3300,"3":20,"5":14,"8":13850,"10":0,"100":0,"101":0,"110":0,"111":255,"153":0,"155":0},"manufacturerName":"LUMI","powerSource":4,"zclVersion":0,"stackVersion":2,"hwVersion":54,"dateCode":"03-20-2019"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":2,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{"genOnOff":{"attributes":{"61440":117440754,"onOff":0}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":3,"profileID":260,"deviceID":256,"inputClusters":[16,6,4,5],"outputClusters":[],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":4,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{"genOnOff":{"attributes":{"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":5,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":6,"profileID":260,"deviceID":0,"inputClusters":[18,6],"outputClusters":[],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":8,"profileID":260,"deviceID":83,"inputClusters":[12],"outputClusters":[],"deviceNetworkAddress":1024,"deviceIeeeAddress":"0x00158d000521d656","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00158d000521d656"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Arbeitszimmer (notInUse)","type":"AB3257001NJ","icon":"img/lightify-plug.png"},"native":{"id":"7cb03eaa00a36bed"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.7cb03eaa00a36bed","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":0,"link_quality_lc":1639668683612,"statesDef":[{"id":"zigbee.0.7cb03eaa00a36bed.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":false,"role":"switch"}],"icon":"img/lightify-plug.png","info":{"type":"device","device":{"ID":25,"_type":"Router","_ieeeAddr":"0x7cb03eaa00a36bed","_networkAddress":65448,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":65448,"deviceIeeeAddress":"0x7cb03eaa00a36bed","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1622654614413},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["Plug 01"],"model":"AB3257001NJ","description":"Smart+ plug","vendor":"OSRAM","whiteLabel":[{"vendor":"LEDVANCE","model":"AB3257001NJ"}],"ota":{},"options":[]},"endpoint":{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":65448,"deviceIeeeAddress":"0x7cb03eaa00a36bed","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":65448,"deviceIeeeAddress":"0x7cb03eaa00a36bed","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"name":"0x7cb03eaa00a36bed"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Lautsprecher","type":"AB3257001NJ","icon":"img/lightify-plug.png"},"native":{"id":"7cb03eaa00acb990"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662545,"_id":"zigbee.0.7cb03eaa00acb990","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":75,"link_quality_lc":1639668747283,"statesDef":[{"id":"zigbee.0.7cb03eaa00acb990.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":true,"role":"switch"}],"icon":"img/lightify-plug.png","info":{"type":"device","device":{"ID":4,"_type":"Router","_ieeeAddr":"0x7cb03eaa00acb990","_networkAddress":47504,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":47504,"deviceIeeeAddress":"0x7cb03eaa00acb990","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":1}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668747220,"_linkquality":75},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["Plug 01"],"model":"AB3257001NJ","description":"Smart+ plug","vendor":"OSRAM","whiteLabel":[{"vendor":"LEDVANCE","model":"AB3257001NJ"}],"ota":{},"options":[]},"endpoint":{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":47504,"deviceIeeeAddress":"0x7cb03eaa00acb990","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":1}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":47504,"deviceIeeeAddress":"0x7cb03eaa00acb990","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":1}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"name":"0x7cb03eaa00acb990"},"rooms":[],"paired":true},{"type":"device","common":{"name":"3D-Drucker","type":"AB3257001NJ","icon":"img/lightify-plug.png"},"native":{"id":"7cb03eaa0a00dfcb"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662545,"_id":"zigbee.0.7cb03eaa0a00dfcb","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":0,"link_quality_lc":1639668683711,"statesDef":[{"id":"zigbee.0.7cb03eaa0a00dfcb.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":false,"role":"switch"}],"icon":"img/lightify-plug.png","info":{"type":"device","device":{"ID":5,"_type":"Router","_ieeeAddr":"0x7cb03eaa0a00dfcb","_networkAddress":34528,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":34528,"deviceIeeeAddress":"0x7cb03eaa0a00dfcb","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1629886942483},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["Plug 01"],"model":"AB3257001NJ","description":"Smart+ plug","vendor":"OSRAM","whiteLabel":[{"vendor":"LEDVANCE","model":"AB3257001NJ"}],"ota":{},"options":[]},"endpoint":{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":34528,"deviceIeeeAddress":"0x7cb03eaa0a00dfcb","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":34528,"deviceIeeeAddress":"0x7cb03eaa0a00dfcb","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"name":"0x7cb03eaa0a00dfcb"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Luftbefeuchter (Schlafzimmer)","type":"AB3257001NJ","icon":"img/lightify-plug.png"},"native":{"id":"7cb03eaa0a019e9d"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.7cb03eaa0a019e9d","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":0,"link_quality_lc":1639668672082,"statesDef":[{"id":"zigbee.0.7cb03eaa0a019e9d.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":false,"role":"switch"}],"icon":"img/lightify-plug.png","info":{"type":"device","device":{"ID":26,"_type":"Router","_ieeeAddr":"0x7cb03eaa0a019e9d","_networkAddress":32268,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":32268,"deviceIeeeAddress":"0x7cb03eaa0a019e9d","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668629319},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["Plug 01"],"model":"AB3257001NJ","description":"Smart+ plug","vendor":"OSRAM","whiteLabel":[{"vendor":"LEDVANCE","model":"AB3257001NJ"}],"ota":{},"options":[]},"endpoint":{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":32268,"deviceIeeeAddress":"0x7cb03eaa0a019e9d","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":32268,"deviceIeeeAddress":"0x7cb03eaa0a019e9d","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"name":"0x7cb03eaa0a019e9d"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Stehlampe (Schlafzimmer)","type":"AB3257001NJ","icon":"img/lightify-plug.png"},"native":{"id":"7cb03eaa0a025809"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.7cb03eaa0a025809","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":0,"link_quality_lc":1639668671760,"statesDef":[{"id":"zigbee.0.7cb03eaa0a025809.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":false,"role":"switch"}],"icon":"img/lightify-plug.png","info":{"type":"device","device":{"ID":17,"_type":"Router","_ieeeAddr":"0x7cb03eaa0a025809","_networkAddress":18602,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":18602,"deviceIeeeAddress":"0x7cb03eaa0a025809","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668625910},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["Plug 01"],"model":"AB3257001NJ","description":"Smart+ plug","vendor":"OSRAM","whiteLabel":[{"vendor":"LEDVANCE","model":"AB3257001NJ"}],"ota":{},"options":[]},"endpoint":{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":18602,"deviceIeeeAddress":"0x7cb03eaa0a025809","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":18602,"deviceIeeeAddress":"0x7cb03eaa0a025809","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"name":"0x7cb03eaa0a025809"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Stehlampen (Wohnzimmer)","type":"AB3257001NJ","icon":"img/lightify-plug.png"},"native":{"id":"84182600000c7532"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.84182600000c7532","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":10,"link_quality_lc":1639668663511,"statesDef":[{"id":"zigbee.0.84182600000c7532.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":true,"role":"switch"}],"icon":"img/lightify-plug.png","info":{"type":"device","device":{"ID":16,"_type":"Router","_ieeeAddr":"0x84182600000c7532","_networkAddress":56716,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":56716,"deviceIeeeAddress":"0x84182600000c7532","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":1}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668663141,"_linkquality":78},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["Plug 01"],"model":"AB3257001NJ","description":"Smart+ plug","vendor":"OSRAM","whiteLabel":[{"vendor":"LEDVANCE","model":"AB3257001NJ"}],"ota":{},"options":[]},"endpoint":{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":56716,"deviceIeeeAddress":"0x84182600000c7532","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":1}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":56716,"deviceIeeeAddress":"0x84182600000c7532","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":1}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"name":"0x84182600000c7532"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Rollo (Wohnzimmer rechts)","type":"TS0601_cover"},"native":{"id":"847127fffecfc657"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.847127fffecfc657","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":10,"link_quality_lc":1639668662559,"statesDef":[{"id":"zigbee.0.847127fffecfc657.motor_speed","name":"Motor speed","type":"number","read":true,"write":true,"val":40,"role":"state"},{"id":"zigbee.0.847127fffecfc657.position","name":"Position of this cover","type":"number","read":true,"write":true,"val":0,"role":"state"},{"id":"zigbee.0.847127fffecfc657.state","name":"state","type":"string","read":true,"write":true,"val":"CLOSE","role":"switch","states":"OPEN:OPEN;CLOSE:CLOSE;STOP:STOP"}],"icon":"https://www.zigbee2mqtt.io/images/devices/TS0601_cover.jpg","info":{"type":"device","device":{"ID":40,"_type":"EndDevice","_ieeeAddr":"0x847127fffecfc657","_networkAddress":1896,"_manufacturerID":4098,"_endpoints":[{"ID":1,"profileID":260,"deviceID":81,"inputClusters":[0,4,5,61184],"outputClusters":[25,10],"deviceNetworkAddress":1896,"deviceIeeeAddress":"0x847127fffecfc657","clusters":{"genBasic":{"attributes":{"modelId":"TS0601","manufacturerName":"_TZE200_zah67ekd","powerSource":3,"zclVersion":3,"appVersion":71,"stackVersion":0,"hwVersion":1,"dateCode":""}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZE200_zah67ekd","_powerSource":"Battery","_modelID":"TS0601","_applicationVersion":71,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639668374974},"mapped":{"zigbeeModel":["owvfni3\u0000","owvfni3","u1rkty3","aabybja","mcdj3aq","mcdj3aq\u0000"],"fingerprint":[{"modelID":"TS0601","manufacturerName":"_TZE200_5zbp6j0u"},{"modelID":"TS0601","manufacturerName":"_TZE200_nkoabg8w"},{"modelID":"TS0601","manufacturerName":"_TZE200_xuzcvlku"},{"modelID":"TS0601","manufacturerName":"_TZE200_4vobcgd3"},{"modelID":"TS0601","manufacturerName":"_TZE200_nogaemzt"},{"modelID":"TS0601","manufacturerName":"_TZE200_pk0sfzvr"},{"modelID":"TS0601","manufacturerName":"_TZE200_fdtjuw7u"},{"modelID":"TS0601","manufacturerName":"_TZE200_zpzndjez"},{"modelID":"TS0601","manufacturerName":"_TZE200_wmcdj3aq"},{"modelID":"TS0601","manufacturerName":"_TZE200_cowvfni3"},{"modelID":"TS0601","manufacturerName":"_TZE200_rddyvrci"},{"modelID":"TS0601","manufacturerName":"_TZE200_nueqqe6k"},{"modelID":"TS0601","manufacturerName":"_TZE200_xaabybja"},{"modelID":"TS0601","manufacturerName":"_TZE200_rmymn92d"},{"modelID":"zo2pocs\u0000","manufacturerName":"_TYST11_fzo2pocs"},{"modelID":"TS0601","manufacturerName":"_TZE200_sbordckq"},{"modelID":"TS0601","manufacturerName":"_TZE200_fctwhugx"},{"modelID":"TS0601","manufacturerName":"_TZE200_zah67ekd"},{"modelID":"TS0601","manufacturerName":"_TZE200_g5wdnuow"},{"modelID":"TS0601","manufacturerName":"_TZE200_fzo2pocs"},{"modelID":"TS0601","manufacturerName":"_TZE200_5sbebbzs"},{"modelID":"TS0601","manufacturerName":"_TZE200_zuz7f94z"}],"model":"TS0601_cover","vendor":"TuYa","description":"Curtain motor/roller blind motor/window pusher/tubular motor","whiteLabel":[{"vendor":"Yushun","model":"YS-MT750"},{"vendor":"Zemismart","model":"ZM79E-DT"},{"vendor":"Binthen","model":"BCM100D"},{"vendor":"Binthen","model":"CV01A"},{"vendor":"Zemismart","model":"M515EGB"},{"vendor":"TuYa","model":"M515EGZT"},{"vendor":"TuYa","model":"DT82LEMA-1.2N"},{"vendor":"Moes","model":"AM43-0.45/40-ES-EB"},{"vendor":"Larkkey","model":"ZSTY-SM-1SRZG-EU"},{"vendor":"Zemismart","model":"ZM25TQ","description":"Tubular motor"},{"vendor":"Zemismart","model":"AM43","description":"Roller blind motor"},{"vendor":"Zemismart","model":"M2805EGBZTN","description":"Tubular motor"},{"vendor":"Zemismart","model":"BCM500DS-TYZ","description":"Curtain motor"},{"vendor":"A-OK","model":"AM25","description":"Tubular motor"}],"fromZigbee":[{"cluster":"manuSpecificTuya","type":["commandSetDataResponse","commandGetData"],"options":[{"type":"binary","name":"invert_cover","property":"invert_cover","access":2,"value_on":true,"value_off":false,"description":"Inverts the cover position, false: open=100,close=0, true: open=0,close=100 (default false)."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","position"],"options":[{"type":"binary","name":"invert_cover","property":"invert_cover","access":2,"value_on":true,"value_off":false,"description":"Inverts the cover position, false: open=100,close=0, true: open=0,close=100 (default false)."}]},{"key":["options"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"exposes":[{"type":"cover","features":[{"type":"enum","name":"state","property":"state","access":3,"values":["OPEN","CLOSE","STOP"]},{"type":"numeric","name":"position","property":"position","access":3,"value_min":0,"value_max":100,"description":"Position of this cover"}]},{"type":"composite","property":"options","name":"options","features":[{"type":"numeric","name":"motor_speed","property":"motor_speed","access":3,"value_min":0,"value_max":255,"description":"Motor speed"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":[{"type":"binary","name":"invert_cover","property":"invert_cover","access":2,"value_on":true,"value_off":false,"description":"Inverts the cover position, false: open=100,close=0, true: open=0,close=100 (default false)."}]},"endpoint":{"ID":1,"profileID":260,"deviceID":81,"inputClusters":[0,4,5,61184],"outputClusters":[25,10],"deviceNetworkAddress":1896,"deviceIeeeAddress":"0x847127fffecfc657","clusters":{"genBasic":{"attributes":{"modelId":"TS0601","manufacturerName":"_TZE200_zah67ekd","powerSource":3,"zclVersion":3,"appVersion":71,"stackVersion":0,"hwVersion":1,"dateCode":""}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":81,"inputClusters":[0,4,5,61184],"outputClusters":[25,10],"deviceNetworkAddress":1896,"deviceIeeeAddress":"0x847127fffecfc657","clusters":{"genBasic":{"attributes":{"modelId":"TS0601","manufacturerName":"_TZE200_zah67ekd","powerSource":3,"zclVersion":3,"appVersion":71,"stackVersion":0,"hwVersion":1,"dateCode":""}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x847127fffecfc657"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Rollo (Wohnzimmer links)","type":"TS0601_cover"},"native":{"id":"847127fffed0a598"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.847127fffed0a598","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":10,"link_quality_lc":1639668662558,"statesDef":[{"id":"zigbee.0.847127fffed0a598.motor_speed","name":"Motor speed","type":"number","read":true,"write":true,"val":40,"role":"state"},{"id":"zigbee.0.847127fffed0a598.position","name":"Position of this cover","type":"number","read":true,"write":true,"val":0,"role":"state"},{"id":"zigbee.0.847127fffed0a598.state","name":"state","type":"string","read":true,"write":true,"val":"CLOSE","role":"switch","states":"OPEN:OPEN;CLOSE:CLOSE;STOP:STOP"}],"icon":"https://www.zigbee2mqtt.io/images/devices/TS0601_cover.jpg","info":{"type":"device","device":{"ID":39,"_type":"EndDevice","_ieeeAddr":"0x847127fffed0a598","_networkAddress":30072,"_manufacturerID":4098,"_endpoints":[{"ID":1,"profileID":260,"deviceID":81,"inputClusters":[0,4,5,61184],"outputClusters":[25,10],"deviceNetworkAddress":30072,"deviceIeeeAddress":"0x847127fffed0a598","clusters":{"genBasic":{"attributes":{"modelId":"TS0601","manufacturerName":"_TZE200_zah67ekd","powerSource":3,"zclVersion":3,"appVersion":71,"stackVersion":0,"hwVersion":1,"dateCode":""}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZE200_zah67ekd","_powerSource":"Battery","_modelID":"TS0601","_applicationVersion":71,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639667988665},"mapped":{"zigbeeModel":["owvfni3\u0000","owvfni3","u1rkty3","aabybja","mcdj3aq","mcdj3aq\u0000"],"fingerprint":[{"modelID":"TS0601","manufacturerName":"_TZE200_5zbp6j0u"},{"modelID":"TS0601","manufacturerName":"_TZE200_nkoabg8w"},{"modelID":"TS0601","manufacturerName":"_TZE200_xuzcvlku"},{"modelID":"TS0601","manufacturerName":"_TZE200_4vobcgd3"},{"modelID":"TS0601","manufacturerName":"_TZE200_nogaemzt"},{"modelID":"TS0601","manufacturerName":"_TZE200_pk0sfzvr"},{"modelID":"TS0601","manufacturerName":"_TZE200_fdtjuw7u"},{"modelID":"TS0601","manufacturerName":"_TZE200_zpzndjez"},{"modelID":"TS0601","manufacturerName":"_TZE200_wmcdj3aq"},{"modelID":"TS0601","manufacturerName":"_TZE200_cowvfni3"},{"modelID":"TS0601","manufacturerName":"_TZE200_rddyvrci"},{"modelID":"TS0601","manufacturerName":"_TZE200_nueqqe6k"},{"modelID":"TS0601","manufacturerName":"_TZE200_xaabybja"},{"modelID":"TS0601","manufacturerName":"_TZE200_rmymn92d"},{"modelID":"zo2pocs\u0000","manufacturerName":"_TYST11_fzo2pocs"},{"modelID":"TS0601","manufacturerName":"_TZE200_sbordckq"},{"modelID":"TS0601","manufacturerName":"_TZE200_fctwhugx"},{"modelID":"TS0601","manufacturerName":"_TZE200_zah67ekd"},{"modelID":"TS0601","manufacturerName":"_TZE200_g5wdnuow"},{"modelID":"TS0601","manufacturerName":"_TZE200_fzo2pocs"},{"modelID":"TS0601","manufacturerName":"_TZE200_5sbebbzs"},{"modelID":"TS0601","manufacturerName":"_TZE200_zuz7f94z"}],"model":"TS0601_cover","vendor":"TuYa","description":"Curtain motor/roller blind motor/window pusher/tubular motor","whiteLabel":[{"vendor":"Yushun","model":"YS-MT750"},{"vendor":"Zemismart","model":"ZM79E-DT"},{"vendor":"Binthen","model":"BCM100D"},{"vendor":"Binthen","model":"CV01A"},{"vendor":"Zemismart","model":"M515EGB"},{"vendor":"TuYa","model":"M515EGZT"},{"vendor":"TuYa","model":"DT82LEMA-1.2N"},{"vendor":"Moes","model":"AM43-0.45/40-ES-EB"},{"vendor":"Larkkey","model":"ZSTY-SM-1SRZG-EU"},{"vendor":"Zemismart","model":"ZM25TQ","description":"Tubular motor"},{"vendor":"Zemismart","model":"AM43","description":"Roller blind motor"},{"vendor":"Zemismart","model":"M2805EGBZTN","description":"Tubular motor"},{"vendor":"Zemismart","model":"BCM500DS-TYZ","description":"Curtain motor"},{"vendor":"A-OK","model":"AM25","description":"Tubular motor"}],"fromZigbee":[{"cluster":"manuSpecificTuya","type":["commandSetDataResponse","commandGetData"],"options":[{"type":"binary","name":"invert_cover","property":"invert_cover","access":2,"value_on":true,"value_off":false,"description":"Inverts the cover position, false: open=100,close=0, true: open=0,close=100 (default false)."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","position"],"options":[{"type":"binary","name":"invert_cover","property":"invert_cover","access":2,"value_on":true,"value_off":false,"description":"Inverts the cover position, false: open=100,close=0, true: open=0,close=100 (default false)."}]},{"key":["options"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"exposes":[{"type":"cover","features":[{"type":"enum","name":"state","property":"state","access":3,"values":["OPEN","CLOSE","STOP"]},{"type":"numeric","name":"position","property":"position","access":3,"value_min":0,"value_max":100,"description":"Position of this cover"}]},{"type":"composite","property":"options","name":"options","features":[{"type":"numeric","name":"motor_speed","property":"motor_speed","access":3,"value_min":0,"value_max":255,"description":"Motor speed"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":[{"type":"binary","name":"invert_cover","property":"invert_cover","access":2,"value_on":true,"value_off":false,"description":"Inverts the cover position, false: open=100,close=0, true: open=0,close=100 (default false)."}]},"endpoint":{"ID":1,"profileID":260,"deviceID":81,"inputClusters":[0,4,5,61184],"outputClusters":[25,10],"deviceNetworkAddress":30072,"deviceIeeeAddress":"0x847127fffed0a598","clusters":{"genBasic":{"attributes":{"modelId":"TS0601","manufacturerName":"_TZE200_zah67ekd","powerSource":3,"zclVersion":3,"appVersion":71,"stackVersion":0,"hwVersion":1,"dateCode":""}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":81,"inputClusters":[0,4,5,61184],"outputClusters":[25,10],"deviceNetworkAddress":30072,"deviceIeeeAddress":"0x847127fffed0a598","clusters":{"genBasic":{"attributes":{"modelId":"TS0601","manufacturerName":"_TZE200_zah67ekd","powerSource":3,"zclVersion":3,"appVersion":71,"stackVersion":0,"hwVersion":1,"dateCode":""}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x847127fffed0a598"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Rollo (Schlafzimmer)","type":"TS0601_cover"},"native":{"id":"847127fffed62092"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.847127fffed62092","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":10,"link_quality_lc":1639668662558,"statesDef":[{"id":"zigbee.0.847127fffed62092.motor_speed","name":"Motor speed","type":"number","read":true,"write":true,"val":40,"role":"state"},{"id":"zigbee.0.847127fffed62092.position","name":"Position of this cover","type":"number","read":true,"write":true,"val":100,"role":"state"},{"id":"zigbee.0.847127fffed62092.state","name":"state","type":"string","read":true,"write":true,"val":true,"role":"switch","states":"OPEN:OPEN;CLOSE:CLOSE;STOP:STOP"}],"icon":"https://www.zigbee2mqtt.io/images/devices/TS0601_cover.jpg","info":{"type":"device","device":{"ID":38,"_type":"EndDevice","_ieeeAddr":"0x847127fffed62092","_networkAddress":16764,"_manufacturerID":4098,"_endpoints":[{"ID":1,"profileID":260,"deviceID":81,"inputClusters":[0,4,5,61184],"outputClusters":[25,10],"deviceNetworkAddress":16764,"deviceIeeeAddress":"0x847127fffed62092","clusters":{"genBasic":{"attributes":{"modelId":"TS0601","manufacturerName":"_TZE200_zah67ekd","powerSource":3,"zclVersion":3,"appVersion":71,"stackVersion":0,"hwVersion":1,"dateCode":""}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZE200_zah67ekd","_powerSource":"Battery","_modelID":"TS0601","_applicationVersion":71,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639665489166},"mapped":{"zigbeeModel":["owvfni3\u0000","owvfni3","u1rkty3","aabybja","mcdj3aq","mcdj3aq\u0000"],"fingerprint":[{"modelID":"TS0601","manufacturerName":"_TZE200_5zbp6j0u"},{"modelID":"TS0601","manufacturerName":"_TZE200_nkoabg8w"},{"modelID":"TS0601","manufacturerName":"_TZE200_xuzcvlku"},{"modelID":"TS0601","manufacturerName":"_TZE200_4vobcgd3"},{"modelID":"TS0601","manufacturerName":"_TZE200_nogaemzt"},{"modelID":"TS0601","manufacturerName":"_TZE200_pk0sfzvr"},{"modelID":"TS0601","manufacturerName":"_TZE200_fdtjuw7u"},{"modelID":"TS0601","manufacturerName":"_TZE200_zpzndjez"},{"modelID":"TS0601","manufacturerName":"_TZE200_wmcdj3aq"},{"modelID":"TS0601","manufacturerName":"_TZE200_cowvfni3"},{"modelID":"TS0601","manufacturerName":"_TZE200_rddyvrci"},{"modelID":"TS0601","manufacturerName":"_TZE200_nueqqe6k"},{"modelID":"TS0601","manufacturerName":"_TZE200_xaabybja"},{"modelID":"TS0601","manufacturerName":"_TZE200_rmymn92d"},{"modelID":"zo2pocs\u0000","manufacturerName":"_TYST11_fzo2pocs"},{"modelID":"TS0601","manufacturerName":"_TZE200_sbordckq"},{"modelID":"TS0601","manufacturerName":"_TZE200_fctwhugx"},{"modelID":"TS0601","manufacturerName":"_TZE200_zah67ekd"},{"modelID":"TS0601","manufacturerName":"_TZE200_g5wdnuow"},{"modelID":"TS0601","manufacturerName":"_TZE200_fzo2pocs"},{"modelID":"TS0601","manufacturerName":"_TZE200_5sbebbzs"},{"modelID":"TS0601","manufacturerName":"_TZE200_zuz7f94z"}],"model":"TS0601_cover","vendor":"TuYa","description":"Curtain motor/roller blind motor/window pusher/tubular motor","whiteLabel":[{"vendor":"Yushun","model":"YS-MT750"},{"vendor":"Zemismart","model":"ZM79E-DT"},{"vendor":"Binthen","model":"BCM100D"},{"vendor":"Binthen","model":"CV01A"},{"vendor":"Zemismart","model":"M515EGB"},{"vendor":"TuYa","model":"M515EGZT"},{"vendor":"TuYa","model":"DT82LEMA-1.2N"},{"vendor":"Moes","model":"AM43-0.45/40-ES-EB"},{"vendor":"Larkkey","model":"ZSTY-SM-1SRZG-EU"},{"vendor":"Zemismart","model":"ZM25TQ","description":"Tubular motor"},{"vendor":"Zemismart","model":"AM43","description":"Roller blind motor"},{"vendor":"Zemismart","model":"M2805EGBZTN","description":"Tubular motor"},{"vendor":"Zemismart","model":"BCM500DS-TYZ","description":"Curtain motor"},{"vendor":"A-OK","model":"AM25","description":"Tubular motor"}],"fromZigbee":[{"cluster":"manuSpecificTuya","type":["commandSetDataResponse","commandGetData"],"options":[{"type":"binary","name":"invert_cover","property":"invert_cover","access":2,"value_on":true,"value_off":false,"description":"Inverts the cover position, false: open=100,close=0, true: open=0,close=100 (default false)."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","position"],"options":[{"type":"binary","name":"invert_cover","property":"invert_cover","access":2,"value_on":true,"value_off":false,"description":"Inverts the cover position, false: open=100,close=0, true: open=0,close=100 (default false)."}]},{"key":["options"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"exposes":[{"type":"cover","features":[{"type":"enum","name":"state","property":"state","access":3,"values":["OPEN","CLOSE","STOP"]},{"type":"numeric","name":"position","property":"position","access":3,"value_min":0,"value_max":100,"description":"Position of this cover"}]},{"type":"composite","property":"options","name":"options","features":[{"type":"numeric","name":"motor_speed","property":"motor_speed","access":3,"value_min":0,"value_max":255,"description":"Motor speed"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":[{"type":"binary","name":"invert_cover","property":"invert_cover","access":2,"value_on":true,"value_off":false,"description":"Inverts the cover position, false: open=100,close=0, true: open=0,close=100 (default false)."}]},"endpoint":{"ID":1,"profileID":260,"deviceID":81,"inputClusters":[0,4,5,61184],"outputClusters":[25,10],"deviceNetworkAddress":16764,"deviceIeeeAddress":"0x847127fffed62092","clusters":{"genBasic":{"attributes":{"modelId":"TS0601","manufacturerName":"_TZE200_zah67ekd","powerSource":3,"zclVersion":3,"appVersion":71,"stackVersion":0,"hwVersion":1,"dateCode":""}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":81,"inputClusters":[0,4,5,61184],"outputClusters":[25,10],"deviceNetworkAddress":16764,"deviceIeeeAddress":"0x847127fffed62092","clusters":{"genBasic":{"attributes":{"modelId":"TS0601","manufacturerName":"_TZE200_zah67ekd","powerSource":3,"zclVersion":3,"appVersion":71,"stackVersion":0,"hwVersion":1,"dateCode":""}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x847127fffed62092"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Deckenleuchte 4/4 (Wohnzimmer)","type":"LED1545G12","icon":"img/ikea_bulb_E27.png"},"native":{"id":"90fd9ffffe02c40f"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.90fd9ffffe02c40f","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":0,"link_quality_lc":1639668685003,"statesDef":[{"id":"zigbee.0.90fd9ffffe02c40f.brightness","name":"Brightness","type":"number","read":true,"write":true,"val":100,"role":"level.dimmer","unit":""},{"id":"zigbee.0.90fd9ffffe02c40f.colortemp","name":"Color temperature","type":"number","read":true,"write":true,"val":278,"role":"level.color.temperature"},{"id":"zigbee.0.90fd9ffffe02c40f.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":true,"role":"switch"},{"id":"zigbee.0.90fd9ffffe02c40f.transition_time","name":"Transition time","type":"number","read":false,"write":true,"role":"state","unit":"sec"}],"icon":"img/ikea_bulb_E27.png","info":{"type":"device","device":{"ID":32,"_type":"Router","_ieeeAddr":"0x90fd9ffffe02c40f","_networkAddress":56799,"_manufacturerID":4476,"_endpoints":[{"ID":1,"profileID":49246,"deviceID":544,"inputClusters":[0,3,4,5,6,8,768,2821,4096],"outputClusters":[5,25,32,4096],"deviceNetworkAddress":56799,"deviceIeeeAddress":"0x90fd9ffffe02c40f","clusters":{"genBasic":{"attributes":{"modelId":"TRADFRI bulb E27 WS opal 980lm","manufacturerName":"IKEA of Sweden","powerSource":1,"zclVersion":1,"appVersion":17,"stackVersion":87,"hwVersion":1,"dateCode":"20170331","swBuildId":"1.2.217"}},"lightingColorCtrl":{"attributes":{"colorCapabilities":16,"colorTempPhysicalMin":250,"colorTempPhysicalMax":454,"colorMode":2,"colorTemperature":278}},"genOnOff":{"attributes":{"onOff":1}},"genLevelCtrl":{"attributes":{"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"IKEA of Sweden","_powerSource":"Mains (single phase)","_modelID":"TRADFRI bulb E27 WS opal 980lm","_applicationVersion":17,"_stackVersion":87,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20170331","_softwareBuildID":"1.2.217","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":2},"_lastSeen":1639638516035},"mapped":{"exposes":[{"type":"light","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","value_toggle":"TOGGLE","description":"On/off state of this light"},{"type":"numeric","name":"brightness","property":"brightness","access":7,"value_min":0,"value_max":254,"description":"Brightness of this light"},{"type":"numeric","name":"color_temp","property":"color_temp","access":7,"unit":"mired","value_min":250,"value_max":454,"description":"Color temperature of this light","presets":[{"name":"coolest","value":250,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":454,"description":"Warmest temperature supported"}]},{"type":"numeric","name":"color_temp_startup","property":"color_temp_startup","access":7,"unit":"mired","value_min":250,"value_max":454,"description":"Color temperature after cold power on of this light","presets":[{"name":"coolest","value":250,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":454,"description":"Warmest temperature supported"},{"name":"previous","value":65535,"description":"Restore previous color_temp on cold power on"}]}]},{"type":"enum","name":"effect","property":"effect","access":2,"values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)"},{"type":"enum","name":"power_on_behavior","property":"power_on_behavior","access":7,"values":["off","previous","on"],"description":"Controls the behavior when the device is powered on"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"lightingColorCtrl","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","brightness","brightness_percent"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp","color_temp_percent"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."},{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["transition"],"attr":[]},{"key":["rate"],"attr":[]},{"key":["brightness_move","brightness_move_onoff"]},{"key":["colortemp_move","color_temp_move"]},{"key":["brightness_step","brightness_step_onoff"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_step"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_startup"]},{"key":["level_config"]},{"key":["power_on_behavior"]},{"key":["color_options"]},{"key":["color_mode"]},{"key":["effect","alert","flash"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"ota":{},"zigbeeModel":["TRADFRI bulb E27 WS opal 980lm","TRADFRI bulb E26 WS opal 980lm","TRADFRI bulb E27 WSopal 980lm"],"model":"LED1545G12","vendor":"IKEA","description":"TRADFRI LED bulb E26/E27 980 lumen, dimmable, white spectrum, opal white","options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."},{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},"endpoint":{"ID":1,"profileID":49246,"deviceID":544,"inputClusters":[0,3,4,5,6,8,768,2821,4096],"outputClusters":[5,25,32,4096],"deviceNetworkAddress":56799,"deviceIeeeAddress":"0x90fd9ffffe02c40f","clusters":{"genBasic":{"attributes":{"modelId":"TRADFRI bulb E27 WS opal 980lm","manufacturerName":"IKEA of Sweden","powerSource":1,"zclVersion":1,"appVersion":17,"stackVersion":87,"hwVersion":1,"dateCode":"20170331","swBuildId":"1.2.217"}},"lightingColorCtrl":{"attributes":{"colorCapabilities":16,"colorTempPhysicalMin":250,"colorTempPhysicalMax":454,"colorMode":2,"colorTemperature":278}},"genOnOff":{"attributes":{"onOff":1}},"genLevelCtrl":{"attributes":{"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":49246,"deviceID":544,"inputClusters":[0,3,4,5,6,8,768,2821,4096],"outputClusters":[5,25,32,4096],"deviceNetworkAddress":56799,"deviceIeeeAddress":"0x90fd9ffffe02c40f","clusters":{"genBasic":{"attributes":{"modelId":"TRADFRI bulb E27 WS opal 980lm","manufacturerName":"IKEA of Sweden","powerSource":1,"zclVersion":1,"appVersion":17,"stackVersion":87,"hwVersion":1,"dateCode":"20170331","swBuildId":"1.2.217"}},"lightingColorCtrl":{"attributes":{"colorCapabilities":16,"colorTempPhysicalMin":250,"colorTempPhysicalMax":454,"colorMode":2,"colorTemperature":278}},"genOnOff":{"attributes":{"onOff":1}},"genLevelCtrl":{"attributes":{"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x90fd9ffffe02c40f"},"rooms":[],"paired":true,"groups":["2"]},{"type":"device","common":{"name":"Deckenleuchte 3/4 (Wohnzimmer)","type":"LED1545G12","icon":"img/ikea_bulb_E27.png"},"native":{"id":"90fd9ffffe7fe8c9"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.90fd9ffffe7fe8c9","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":0,"link_quality_lc":1639668683694,"statesDef":[{"id":"zigbee.0.90fd9ffffe7fe8c9.brightness","name":"Brightness","type":"number","read":true,"write":true,"val":100,"role":"level.dimmer","unit":""},{"id":"zigbee.0.90fd9ffffe7fe8c9.colortemp","name":"Color temperature","type":"number","read":true,"write":true,"val":278,"role":"level.color.temperature"},{"id":"zigbee.0.90fd9ffffe7fe8c9.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":true,"role":"switch"},{"id":"zigbee.0.90fd9ffffe7fe8c9.transition_time","name":"Transition time","type":"number","read":false,"write":true,"role":"state","unit":"sec"}],"icon":"img/ikea_bulb_E27.png","info":{"type":"device","device":{"ID":33,"_type":"Router","_ieeeAddr":"0x90fd9ffffe7fe8c9","_networkAddress":65244,"_manufacturerID":4476,"_endpoints":[{"ID":1,"profileID":49246,"deviceID":544,"inputClusters":[0,3,4,5,6,8,768,2821,4096],"outputClusters":[5,25,32,4096],"deviceNetworkAddress":65244,"deviceIeeeAddress":"0x90fd9ffffe7fe8c9","clusters":{"genBasic":{"attributes":{"modelId":"TRADFRI bulb E27 WS opal 980lm","manufacturerName":"IKEA of Sweden","powerSource":1,"zclVersion":1,"appVersion":17,"stackVersion":87,"hwVersion":1,"dateCode":"20170331","swBuildId":"1.2.217"}},"lightingColorCtrl":{"attributes":{"colorCapabilities":16,"colorTempPhysicalMin":250,"colorTempPhysicalMax":454,"colorMode":2,"colorTemperature":278}},"genOnOff":{"attributes":{"onOff":1}},"genLevelCtrl":{"attributes":{"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"IKEA of Sweden","_powerSource":"Mains (single phase)","_modelID":"TRADFRI bulb E27 WS opal 980lm","_applicationVersion":17,"_stackVersion":87,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20170331","_softwareBuildID":"1.2.217","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":2},"_lastSeen":1639638516041},"mapped":{"exposes":[{"type":"light","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","value_toggle":"TOGGLE","description":"On/off state of this light"},{"type":"numeric","name":"brightness","property":"brightness","access":7,"value_min":0,"value_max":254,"description":"Brightness of this light"},{"type":"numeric","name":"color_temp","property":"color_temp","access":7,"unit":"mired","value_min":250,"value_max":454,"description":"Color temperature of this light","presets":[{"name":"coolest","value":250,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":454,"description":"Warmest temperature supported"}]},{"type":"numeric","name":"color_temp_startup","property":"color_temp_startup","access":7,"unit":"mired","value_min":250,"value_max":454,"description":"Color temperature after cold power on of this light","presets":[{"name":"coolest","value":250,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":454,"description":"Warmest temperature supported"},{"name":"previous","value":65535,"description":"Restore previous color_temp on cold power on"}]}]},{"type":"enum","name":"effect","property":"effect","access":2,"values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)"},{"type":"enum","name":"power_on_behavior","property":"power_on_behavior","access":7,"values":["off","previous","on"],"description":"Controls the behavior when the device is powered on"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"lightingColorCtrl","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","brightness","brightness_percent"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp","color_temp_percent"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."},{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["transition"],"attr":[]},{"key":["rate"],"attr":[]},{"key":["brightness_move","brightness_move_onoff"]},{"key":["colortemp_move","color_temp_move"]},{"key":["brightness_step","brightness_step_onoff"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_step"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_startup"]},{"key":["level_config"]},{"key":["power_on_behavior"]},{"key":["color_options"]},{"key":["color_mode"]},{"key":["effect","alert","flash"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"ota":{},"zigbeeModel":["TRADFRI bulb E27 WS opal 980lm","TRADFRI bulb E26 WS opal 980lm","TRADFRI bulb E27 WSopal 980lm"],"model":"LED1545G12","vendor":"IKEA","description":"TRADFRI LED bulb E26/E27 980 lumen, dimmable, white spectrum, opal white","options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."},{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},"endpoint":{"ID":1,"profileID":49246,"deviceID":544,"inputClusters":[0,3,4,5,6,8,768,2821,4096],"outputClusters":[5,25,32,4096],"deviceNetworkAddress":65244,"deviceIeeeAddress":"0x90fd9ffffe7fe8c9","clusters":{"genBasic":{"attributes":{"modelId":"TRADFRI bulb E27 WS opal 980lm","manufacturerName":"IKEA of Sweden","powerSource":1,"zclVersion":1,"appVersion":17,"stackVersion":87,"hwVersion":1,"dateCode":"20170331","swBuildId":"1.2.217"}},"lightingColorCtrl":{"attributes":{"colorCapabilities":16,"colorTempPhysicalMin":250,"colorTempPhysicalMax":454,"colorMode":2,"colorTemperature":278}},"genOnOff":{"attributes":{"onOff":1}},"genLevelCtrl":{"attributes":{"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":49246,"deviceID":544,"inputClusters":[0,3,4,5,6,8,768,2821,4096],"outputClusters":[5,25,32,4096],"deviceNetworkAddress":65244,"deviceIeeeAddress":"0x90fd9ffffe7fe8c9","clusters":{"genBasic":{"attributes":{"modelId":"TRADFRI bulb E27 WS opal 980lm","manufacturerName":"IKEA of Sweden","powerSource":1,"zclVersion":1,"appVersion":17,"stackVersion":87,"hwVersion":1,"dateCode":"20170331","swBuildId":"1.2.217"}},"lightingColorCtrl":{"attributes":{"colorCapabilities":16,"colorTempPhysicalMin":250,"colorTempPhysicalMax":454,"colorMode":2,"colorTemperature":278}},"genOnOff":{"attributes":{"onOff":1}},"genLevelCtrl":{"attributes":{"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x90fd9ffffe7fe8c9"},"rooms":[],"paired":true,"groups":["2"]},{"type":"device","common":{"name":"Deckenleuchte 2/4 (Wohnzimmer)","type":"LED1545G12","icon":"img/ikea_bulb_E27.png"},"native":{"id":"90fd9ffffe88755e"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.90fd9ffffe88755e","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":0,"link_quality_lc":1639668684521,"statesDef":[{"id":"zigbee.0.90fd9ffffe88755e.brightness","name":"Brightness","type":"number","read":true,"write":true,"val":100,"role":"level.dimmer","unit":""},{"id":"zigbee.0.90fd9ffffe88755e.colortemp","name":"Color temperature","type":"number","read":true,"write":true,"val":278,"role":"level.color.temperature"},{"id":"zigbee.0.90fd9ffffe88755e.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":true,"role":"switch"},{"id":"zigbee.0.90fd9ffffe88755e.transition_time","name":"Transition time","type":"number","read":false,"write":true,"role":"state","unit":"sec"}],"icon":"img/ikea_bulb_E27.png","info":{"type":"device","device":{"ID":34,"_type":"Router","_ieeeAddr":"0x90fd9ffffe88755e","_networkAddress":2953,"_manufacturerID":4476,"_endpoints":[{"ID":1,"profileID":49246,"deviceID":544,"inputClusters":[0,3,4,5,6,8,768,2821,4096],"outputClusters":[5,25,32,4096],"deviceNetworkAddress":2953,"deviceIeeeAddress":"0x90fd9ffffe88755e","clusters":{"genBasic":{"attributes":{"modelId":"TRADFRI bulb E27 WS opal 980lm","manufacturerName":"IKEA of Sweden","powerSource":1,"zclVersion":1,"appVersion":17,"stackVersion":87,"hwVersion":1,"dateCode":"20170331","swBuildId":"1.2.217"}},"lightingColorCtrl":{"attributes":{"colorCapabilities":16,"colorTempPhysicalMin":250,"colorTempPhysicalMax":454,"colorMode":2,"colorTemperature":278}},"genOnOff":{"attributes":{"onOff":1}},"genLevelCtrl":{"attributes":{"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"IKEA of Sweden","_powerSource":"Mains (single phase)","_modelID":"TRADFRI bulb E27 WS opal 980lm","_applicationVersion":17,"_stackVersion":87,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20170331","_softwareBuildID":"1.2.217","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":2},"_lastSeen":1639638516042},"mapped":{"exposes":[{"type":"light","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","value_toggle":"TOGGLE","description":"On/off state of this light"},{"type":"numeric","name":"brightness","property":"brightness","access":7,"value_min":0,"value_max":254,"description":"Brightness of this light"},{"type":"numeric","name":"color_temp","property":"color_temp","access":7,"unit":"mired","value_min":250,"value_max":454,"description":"Color temperature of this light","presets":[{"name":"coolest","value":250,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":454,"description":"Warmest temperature supported"}]},{"type":"numeric","name":"color_temp_startup","property":"color_temp_startup","access":7,"unit":"mired","value_min":250,"value_max":454,"description":"Color temperature after cold power on of this light","presets":[{"name":"coolest","value":250,"description":"Coolest temperature supported"},{"name":"cool","value":250,"description":"Cool temperature (250 mireds / 4000 Kelvin)"},{"name":"neutral","value":370,"description":"Neutral temperature (370 mireds / 2700 Kelvin)"},{"name":"warm","value":454,"description":"Warm temperature (454 mireds / 2200 Kelvin)"},{"name":"warmest","value":454,"description":"Warmest temperature supported"},{"name":"previous","value":65535,"description":"Restore previous color_temp on cold power on"}]}]},{"type":"enum","name":"effect","property":"effect","access":2,"values":["blink","breathe","okay","channel_change","finish_effect","stop_effect"],"description":"Triggers an effect on the light (e.g. make light blink for a few seconds)"},{"type":"enum","name":"power_on_behavior","property":"power_on_behavior","access":7,"values":["off","previous","on"],"description":"Controls the behavior when the device is powered on"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"lightingColorCtrl","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genLevelCtrl","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","brightness","brightness_percent"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp","color_temp_percent"],"options":[{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."},{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["transition"],"attr":[]},{"key":["rate"],"attr":[]},{"key":["brightness_move","brightness_move_onoff"]},{"key":["colortemp_move","color_temp_move"]},{"key":["brightness_step","brightness_step_onoff"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_step"],"options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."}]},{"key":["color_temp_startup"]},{"key":["level_config"]},{"key":["power_on_behavior"]},{"key":["color_options"]},{"key":["color_mode"]},{"key":["effect","alert","flash"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"ota":{},"zigbeeModel":["TRADFRI bulb E27 WS opal 980lm","TRADFRI bulb E26 WS opal 980lm","TRADFRI bulb E27 WSopal 980lm"],"model":"LED1545G12","vendor":"IKEA","description":"TRADFRI LED bulb E26/E27 980 lumen, dimmable, white spectrum, opal white","options":[{"type":"numeric","name":"transition","property":"transition","access":2,"value_min":0,"description":"Controls the transition time (in seconds) of on/off, brightness, color temperature (if applicable) and color (if applicable) changes. Defaults to `0` (no transition)."},{"type":"binary","name":"color_sync","property":"color_sync","access":2,"value_on":true,"value_off":false,"description":"When enabled colors will be synced, e.g. if the light supports both color x/y and color temperature a conversion from color x/y to color temperature will be done when setting the x/y color (default true)."}]},"endpoint":{"ID":1,"profileID":49246,"deviceID":544,"inputClusters":[0,3,4,5,6,8,768,2821,4096],"outputClusters":[5,25,32,4096],"deviceNetworkAddress":2953,"deviceIeeeAddress":"0x90fd9ffffe88755e","clusters":{"genBasic":{"attributes":{"modelId":"TRADFRI bulb E27 WS opal 980lm","manufacturerName":"IKEA of Sweden","powerSource":1,"zclVersion":1,"appVersion":17,"stackVersion":87,"hwVersion":1,"dateCode":"20170331","swBuildId":"1.2.217"}},"lightingColorCtrl":{"attributes":{"colorCapabilities":16,"colorTempPhysicalMin":250,"colorTempPhysicalMax":454,"colorMode":2,"colorTemperature":278}},"genOnOff":{"attributes":{"onOff":1}},"genLevelCtrl":{"attributes":{"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":49246,"deviceID":544,"inputClusters":[0,3,4,5,6,8,768,2821,4096],"outputClusters":[5,25,32,4096],"deviceNetworkAddress":2953,"deviceIeeeAddress":"0x90fd9ffffe88755e","clusters":{"genBasic":{"attributes":{"modelId":"TRADFRI bulb E27 WS opal 980lm","manufacturerName":"IKEA of Sweden","powerSource":1,"zclVersion":1,"appVersion":17,"stackVersion":87,"hwVersion":1,"dateCode":"20170331","swBuildId":"1.2.217"}},"lightingColorCtrl":{"attributes":{"colorCapabilities":16,"colorTempPhysicalMin":250,"colorTempPhysicalMax":454,"colorMode":2,"colorTemperature":278}},"genOnOff":{"attributes":{"onOff":1}},"genLevelCtrl":{"attributes":{"currentLevel":254}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x90fd9ffffe88755e"},"rooms":[],"paired":true,"groups":["2"]},{"type":"device","common":{"name":"Lüfter (Badezimmer)","type":"TS0001","icon":"img/tuya_switch_1.png"},"native":{"id":"a4c138934ce2822b"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.a4c138934ce2822b","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":60,"link_quality_lc":1639668667846,"statesDef":[{"id":"zigbee.0.a4c138934ce2822b.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":false,"role":"switch"}],"icon":"img/tuya_switch_1.png","info":{"type":"device","device":{"ID":42,"_type":"Router","_ieeeAddr":"0xa4c138934ce2822b","_networkAddress":25440,"_manufacturerID":4417,"_endpoints":[{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":25440,"deviceIeeeAddress":"0xa4c138934ce2822b","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":0,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}},"manuSpecificTuya_3":{"attributes":{"switchType":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":97,"inputClusters":[],"outputClusters":[33],"deviceNetworkAddress":25440,"deviceIeeeAddress":"0xa4c138934ce2822b","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZ3000_npzfdcof","_powerSource":"Mains (single phase)","_modelID":"TS0001","_applicationVersion":67,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668667825,"_linkquality":60},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["TS0001"],"model":"TS0001","vendor":"TuYa","description":"1 gang switch","whiteLabel":[{"vendor":"CR Smart Home","model":"TS0001","description":"Valve control"},{"vendor":"Lonsonho","model":"X701"},{"vendor":"Bandi","model":"BDS03G1"}],"options":[]},"endpoint":{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":25440,"deviceIeeeAddress":"0xa4c138934ce2822b","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":0,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}},"manuSpecificTuya_3":{"attributes":{"switchType":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":25440,"deviceIeeeAddress":"0xa4c138934ce2822b","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":0,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}},"manuSpecificTuya_3":{"attributes":{"switchType":0}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":97,"inputClusters":[],"outputClusters":[33],"deviceNetworkAddress":25440,"deviceIeeeAddress":"0xa4c138934ce2822b","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0xa4c138934ce2822b"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Schranklicht (Badezimmer)","type":"TS0001","icon":"img/tuya_switch_1.png"},"native":{"id":"a4c138ec0e4ef1cf"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.a4c138ec0e4ef1cf","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"link_quality":0,"link_quality_lc":1639668673926,"statesDef":[{"id":"zigbee.0.a4c138ec0e4ef1cf.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":false,"role":"switch"}],"icon":"img/tuya_switch_1.png","info":{"type":"device","device":{"ID":43,"_type":"Router","_ieeeAddr":"0xa4c138ec0e4ef1cf","_networkAddress":60149,"_manufacturerID":4417,"_endpoints":[{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":0,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":97,"inputClusters":[],"outputClusters":[33],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZ3000_npzfdcof","_powerSource":"Mains (single phase)","_modelID":"TS0001","_applicationVersion":67,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668636848},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["TS0001"],"model":"TS0001","vendor":"TuYa","description":"1 gang switch","whiteLabel":[{"vendor":"CR Smart Home","model":"TS0001","description":"Valve control"},{"vendor":"Lonsonho","model":"X701"},{"vendor":"Bandi","model":"BDS03G1"}],"options":[]},"endpoint":{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":0,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":0,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":97,"inputClusters":[],"outputClusters":[33],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0xa4c138ec0e4ef1cf"},"rooms":[],"paired":true},{"type":"device","common":{"name":"Deckenleuchte (Schlafzimmer)","type":"group"},"native":{"id":"group_1"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662546,"_id":"zigbee.0.group_1","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"statesDef":[{"id":"zigbee.0.group_1.brightness","name":"Brightness","type":"number","read":true,"write":true,"val":100,"role":"level.dimmer","unit":""},{"id":"zigbee.0.group_1.color","name":"Color","type":"string","read":true,"write":true,"role":"level.color.rgb"},{"id":"zigbee.0.group_1.colortemp","name":"Color temperature","type":"number","read":true,"write":true,"val":346,"role":"level.color.temperature"},{"id":"zigbee.0.group_1.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":true,"role":"switch"},{"id":"zigbee.0.group_1.transition_time","name":"Transition time","type":"number","read":false,"write":true,"role":"state","unit":"sec"}],"icon":"img/group.png","vendor":"ioBroker","memberinfo":[{"name":"Deckenleuchte 1/4 (Schlafzimmer)","ieee":"0x00158d0002b805e3"},{"name":"Deckenleuchte 2/4 (Schlafzimmer)","ieee":"0x00158d0002b7d6a9"},{"name":"Deckenleuchte 3/4 (Schlafzimmer)","ieee":"0x00158d0002b7d87c"},{"name":"Deckenleuchte 4/4 (Schlafzimmer)","ieee":"0x00158d0002c65ed8"}],"rooms":[],"paired":false},{"type":"device","common":{"name":"Deckenleuchte (Wohnzimmer)","type":"group"},"native":{"id":"group_2"},"from":"system.adapter.zigbee.0","user":"system.user.admin","ts":1639668662547,"_id":"zigbee.0.group_2","acl":{"object":1636,"owner":"system.user.admin","ownerGroup":"system.group.administrator"},"statesDef":[{"id":"zigbee.0.group_2.brightness","name":"Brightness","type":"number","read":true,"write":true,"val":100,"role":"level.dimmer","unit":""},{"id":"zigbee.0.group_2.color","name":"Color","type":"string","read":true,"write":true,"role":"level.color.rgb"},{"id":"zigbee.0.group_2.colortemp","name":"Color temperature","type":"number","read":true,"write":true,"val":278,"role":"level.color.temperature"},{"id":"zigbee.0.group_2.state","name":"Switch state","type":"boolean","read":true,"write":true,"val":true,"role":"switch"},{"id":"zigbee.0.group_2.transition_time","name":"Transition time","type":"number","read":false,"write":true,"role":"state","unit":"sec"}],"icon":"img/group.png","vendor":"ioBroker","memberinfo":[{"name":"Deckenleuchte 1/4 (Wohnzimmer)","ieee":"0x000b57fffe4436b0"},{"name":"Deckenleuchte 2/4 (Wohnzimmer)","ieee":"0x90fd9ffffe88755e"},{"name":"Deckenleuchte 3/4 (Wohnzimmer)","ieee":"0x90fd9ffffe7fe8c9"},{"name":"Deckenleuchte 4/4 (Wohnzimmer)","ieee":"0x90fd9ffffe02c40f"}],"rooms":[],"paired":false},{"_id":"0x00124b00219fc18c","icon":"img/unknown.png","paired":true,"info":{"type":"device","device":{"ID":1,"_type":"Coordinator","_ieeeAddr":"0x00124b00219fc18c","_networkAddress":0,"_manufacturerID":0,"_endpoints":[{"ID":1,"profileID":260,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":2,"profileID":257,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":3,"profileID":261,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":4,"profileID":263,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":5,"profileID":264,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":6,"profileID":265,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":8,"profileID":260,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":10,"profileID":260,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":11,"profileID":260,"deviceID":1024,"inputClusters":[1281],"outputClusters":[1280,1282],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":12,"profileID":49246,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":13,"profileID":260,"deviceID":5,"inputClusters":[25],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":47,"profileID":260,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":110,"profileID":260,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":null},"mapped":null,"endpoint":{"ID":1,"profileID":260,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},"endpoints":[{"ID":1,"profileID":260,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":2,"profileID":257,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":3,"profileID":261,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":4,"profileID":263,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":5,"profileID":264,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":6,"profileID":265,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":8,"profileID":260,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":10,"profileID":260,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":11,"profileID":260,"deviceID":1024,"inputClusters":[1281],"outputClusters":[1280,1282],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":12,"profileID":49246,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":13,"profileID":260,"deviceID":5,"inputClusters":[25],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":47,"profileID":260,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":110,"profileID":260,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":5,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":0,"deviceIeeeAddress":"0x00124b00219fc18c","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"name":"0x00124b00219fc18c"},"common":{},"native":{}}]	
2021-12-16 16:32:42.379 - debug: zigbee.0 (26219) sendTo "getDevices" to system.adapter.admin.0 from system.adapter.zigbee.0	
2021-12-16 16:32:42.885 - debug: zigbee.0 (26219) getExclude result: []	
2021-12-16 16:32:42.886 - debug: zigbee.0 (26219) getBinding result: []	
2021-12-16 16:32:42.887 - debug: zigbee.0 (26219) sendTo "getBinding" to system.adapter.admin.0 from system.adapter.zigbee.0	
2021-12-16 16:32:42.894 - debug: zigbee.0 (26219) sendTo "getExclude" to system.adapter.admin.0 from system.adapter.zigbee.0	
2021-12-16 16:32:52.339 - debug: zigbee.0 (26219) Failed to execute LQI for '0x7cb03eaa00acb990'. "Error: AREQ - ZDO - mgmtLqiRsp after 10000ms\n at Timeout._onTimeout (/opt/iobroker/node_modules/zigbee-herdsman/dist/utils/waitress.js:37:35)\n at listOnTimeout (internal/timers.js:557:17)\n at processTimers (internal/timers.js:500:7)"	
2021-12-16 16:32:52.340 - debug: zigbee.0 (26219) LQI succeeded for '0x7cb03eaa00acb990'	
2021-12-16 16:32:52.340 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtRtgReq - {"dstaddr":47504,"startindex":0}	
2021-12-16 16:32:52.341 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,50,144,185,0,61]	
2021-12-16 16:32:52.349 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,50,0,86]	
2021-12-16 16:32:52.350 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,50,0,86]	
2021-12-16 16:32:52.351 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 50 - [0] - 86	
2021-12-16 16:32:52.351 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtRtgReq - {"status":0}	
2021-12-16 16:32:52.352 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:00.882 - debug: zigbee.0 (26219) User stateChange zigbee.0.a4c138ec0e4ef1cf.state {"val":true,"ack":false,"ts":1639668780872,"q":0,"from":"system.adapter.zigbee.0","user":"system.user.admin","lc":1639668780872}	
2021-12-16 16:33:00.892 - debug: zigbee.0 (26219) Change state 'state' at device 0xa4c138ec0e4ef1cf type 'TS0001'	
2021-12-16 16:33:00.898 - debug: zigbee.0 (26219) entity: {"type":"device","device":{"ID":43,"_type":"Router","_ieeeAddr":"0xa4c138ec0e4ef1cf","_networkAddress":60149,"_manufacturerID":4417,"_endpoints":[{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":0,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":97,"inputClusters":[],"outputClusters":[33],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZ3000_npzfdcof","_powerSource":"Mains (single phase)","_modelID":"TS0001","_applicationVersion":67,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668636848},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["TS0001"],"model":"TS0001","vendor":"TuYa","description":"1 gang switch","whiteLabel":[{"vendor":"CR Smart Home","model":"TS0001","description":"Valve control"},{"vendor":"Lonsonho","model":"X701"},{"vendor":"Bandi","model":"BDS03G1"}],"options":[]},"endpoint":"[Circular]","endpoints":"[Circular]","name":"0xa4c138ec0e4ef1cf"}	
2021-12-16 16:33:00.899 - debug: zigbee.0 (26219) Mapped Model: {"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["TS0001"],"model":"TS0001","vendor":"TuYa","description":"1 gang switch","whiteLabel":[{"vendor":"CR Smart Home","model":"TS0001","description":"Valve control"},{"vendor":"Lonsonho","model":"X701"},{"vendor":"Bandi","model":"BDS03G1"}],"options":[]}	
2021-12-16 16:33:00.900 - debug: zigbee.0 (26219) convert state, "ON", {"state":"ON"}	
2021-12-16 16:33:00.901 - debug: zigbee.0 (26219) target: {"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":0,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]}	
2021-12-16 16:33:00.904 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Command 0xa4c138ec0e4ef1cf/1 genOnOff.on({}, {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:33:00.905 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0xa4c138ec0e4ef1cf:60149/1 (0,0,2)	
2021-12-16 16:33:00.906 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":60149,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":96,"options":0,"radius":30,"len":3,"data":{"type":"Buffer","data":[1,34,1]}}	
2021-12-16 16:33:00.907 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,13,36,1,245,234,1,1,6,0,96,0,30,3,1,34,1,110]	
2021-12-16 16:33:00.919 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:33:00.920 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:33:00.920 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:33:00.921 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:33:00.922 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:00.959 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,96,71]	
2021-12-16 16:33:00.959 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,96,71]	
2021-12-16 16:33:00.960 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,96] - 71	
2021-12-16 16:33:00.961 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":96}	
2021-12-16 16:33:00.962 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:00.962 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0xa4c138ec0e4ef1cf:60149,225,0)	
2021-12-16 16:33:02.144 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002b54a17 lumi.weather was last seen '485.632' seconds ago.	
2021-12-16 16:33:02.146 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002130d3b lumi.sensor_switch.aq2 was last seen '41.283' seconds ago.	
2021-12-16 16:33:02.148 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002130f3a lumi.sensor_switch.aq2 was last seen '3010.31' seconds ago.	
2021-12-16 16:33:02.149 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002f8d76c lumi.ctrl_neutral1 was last seen '7951170.352' seconds ago.	
2021-12-16 16:33:02.152 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000274f4de lumi.sensor_magnet.aq2 was last seen '721.466' seconds ago.	
2021-12-16 16:33:02.153 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002135d9b lumi.sensor_switch.aq2 was last seen '3994.967' seconds ago.	
2021-12-16 16:33:02.154 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000274f4bf lumi.sensor_magnet.aq2 was last seen '2755.199' seconds ago.	
2021-12-16 16:33:02.159 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000271c4b7 lumi.sensor_wleak.aq1 was last seen '2519.088' seconds ago.	
2021-12-16 16:33:02.162 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002f8d5b4 lumi.ctrl_neutral1 was last seen '7951194.82' seconds ago.	
2021-12-16 16:33:02.164 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002e34b33 lumi.ctrl_neutral1 was last seen '7951176.716' seconds ago.	
2021-12-16 16:33:02.167 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000521d656 lumi.switch.b1lacn02 was last seen '7951169.832' seconds ago.	
2021-12-16 16:33:02.170 - debug: zigbee.0 (26219) Non-pingable device 0x00158d00028aee30 lumi.sensor_cube.aqgl01 was last seen '2395.914' seconds ago.	
2021-12-16 16:33:02.177 - debug: zigbee.0 (26219) Non-pingable device 0x00158d00021369f3 lumi.sensor_switch.aq2 was last seen '2672.722' seconds ago.	
2021-12-16 16:33:02.178 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002b54752 lumi.weather was last seen '795.141' seconds ago.	
2021-12-16 16:33:02.181 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000274f643 lumi.sensor_magnet.aq2 was last seen '2869.881' seconds ago.	
2021-12-16 16:33:02.182 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000274f64d lumi.sensor_magnet.aq2 was last seen '223.714' seconds ago.	
2021-12-16 16:33:02.183 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002b51c42 lumi.weather was last seen '414.379' seconds ago.	
2021-12-16 16:33:02.184 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000274f4f7 lumi.sensor_magnet.aq2 was last seen '4900.167' seconds ago.	
2021-12-16 16:33:02.185 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000274f4d3 lumi.sensor_magnet.aq2 was last seen '1622.462' seconds ago.	
2021-12-16 16:33:02.189 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002722af7 lumi.sensor_magnet.aq2 was last seen '4214.962' seconds ago.	
2021-12-16 16:33:02.191 - debug: zigbee.0 (26219) Non-pingable device 0x847127fffed62092 TS0601 was last seen '3293.025' seconds ago.	
2021-12-16 16:33:02.192 - debug: zigbee.0 (26219) Non-pingable device 0x847127fffed0a598 TS0601 was last seen '793.527' seconds ago.	
2021-12-16 16:33:02.199 - debug: zigbee.0 (26219) Non-pingable device 0x847127fffecfc657 TS0601 was last seen '407.225' seconds ago.	
2021-12-16 16:33:02.200 - debug: zigbee.0 (26219) Non-pingable device 0x000d6ffffe2cd4b8 FYRTUR block-out roller blind was last seen '864927.414' seconds ago.	
2021-12-16 16:33:02.354 - debug: zigbee.0 (26219) Failed to execute routing table for '0x7cb03eaa00acb990'. "Error: AREQ - ZDO - mgmtRtgRsp after 10000ms\n at Timeout._onTimeout (/opt/iobroker/node_modules/zigbee-herdsman/dist/utils/waitress.js:37:35)\n at listOnTimeout (internal/timers.js:557:17)\n at processTimers (internal/timers.js:500:7)"	
2021-12-16 16:33:02.354 - debug: zigbee.0 (26219) Routing for '0x7cb03eaa00acb990': undefined	
2021-12-16 16:33:02.354 - debug: zigbee.0 (26219) Routing table succeeded for '0x7cb03eaa00acb990'	
2021-12-16 16:33:02.355 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtLqiReq - {"dstaddr":34528,"startindex":0}	
2021-12-16 16:33:02.355 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,49,224,134,0,113]	
2021-12-16 16:33:02.362 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,49,0,85]	
2021-12-16 16:33:02.362 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,49,0,85]	
2021-12-16 16:33:02.362 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 49 - [0] - 85	
2021-12-16 16:33:02.363 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtLqiReq - {"status":0}	
2021-12-16 16:33:02.363 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:02.963 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0xa4c138ec0e4ef1cf:60149/1 (0,1,2)	
2021-12-16 16:33:02.964 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":60149,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":97,"options":0,"radius":30,"len":3,"data":{"type":"Buffer","data":[1,34,1]}}	
2021-12-16 16:33:02.965 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,13,36,1,245,234,1,1,6,0,97,0,30,3,1,34,1,111]	
2021-12-16 16:33:02.974 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:33:02.975 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:33:02.976 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:33:02.977 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:33:02.977 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:03.019 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,0,1,97,167]	
2021-12-16 16:33:03.020 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,0,1,97,167]	
2021-12-16 16:33:03.021 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [0,1,97] - 167	
2021-12-16 16:33:03.021 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":0,"endpoint":1,"transid":97}	
2021-12-16 16:33:03.022 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:03.054 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,25,68,129,0,0,6,0]	
2021-12-16 16:33:03.055 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,25,68,129,0,0,6,0]	
2021-12-16 16:33:03.057 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [245,234,1,1,0,75,0,208,106,180,0,0,5,24,34,11]	
2021-12-16 16:33:03.058 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,25,68,129,0,0,6,0,245,234,1,1,0,75,0,208,106,180,0,0,5,24,34,11]	
2021-12-16 16:33:03.060 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [1,0,245,234,29,183,254,27,68,129,0,0,6,0,245,234,1,1,0,72,0,135,107,180,0,0,7,24,30,10,0,0]	
2021-12-16 16:33:03.061 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,25,68,129,0,0,6,0,245,234,1,1,0,75,0,208,106,180,0,0,5,24,34,11,1,0,245,234,29,183,254,27,68,129,0,0,6,0,245,234,1,1,0,72,0,135,107,180,0,0,7,24,30,10,0,0]	
2021-12-16 16:33:03.061 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 25 - 2 - 4 - 129 - [0,0,6,0,245,234,1,1,0,75,0,208,106,180,0,0,5,24,34,11,1,0,245,234,29] - 183	
2021-12-16 16:33:03.062 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - incomingMsg - {"groupid":0,"clusterid":6,"srcaddr":60149,"srcendpoint":1,"dstendpoint":1,"wasbroadcast":0,"linkquality":75,"securityuse":0,"timestamp":11823824,"transseqnumber":0,"len":5,"data":{"type":"Buffer","data":[24,34,11,1,0]}}	
2021-12-16 16:33:03.064 - debug: zigbee.0 (26219) zigbee-herdsman:controller:log Received 'zcl' data '{"frame":{"Header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":34,"manufacturerCode":null,"commandIdentifier":11},"Payload":{"cmdId":1,"statusCode":0},"Command":{"ID":11,"name":"defaultRsp","parameters":[{"name":"cmdId","type":32},{"name":"statusCode","type":32}]}},"address":60149,"endpoint":1,"linkquality":75,"groupID":0,"wasBroadcast":false,"destinationEndpoint":1}'	
2021-12-16 16:33:03.065 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,27,68,129,0,0,6,0,245,234,1,1,0,72,0,135,107,180,0,0,7,24,30,10,0,0]	
2021-12-16 16:33:03.065 - debug: zigbee.0 (26219) convert result {"state":{"state":"ON"}}	
2021-12-16 16:33:03.069 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [16,1,245,234,29,207]	
2021-12-16 16:33:03.070 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,27,68,129,0,0,6,0,245,234,1,1,0,72,0,135,107,180,0,0,7,24,30,10,0,0,16,1,245,234,29,207]	
2021-12-16 16:33:03.071 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 27 - 2 - 4 - 129 - [0,0,6,0,245,234,1,1,0,72,0,135,107,180,0,0,7,24,30,10,0,0,16,1,245,234,29] - 207	
2021-12-16 16:33:03.071 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - incomingMsg - {"groupid":0,"clusterid":6,"srcaddr":60149,"srcendpoint":1,"dstendpoint":1,"wasbroadcast":0,"linkquality":72,"securityuse":0,"timestamp":11824007,"transseqnumber":0,"len":7,"data":{"type":"Buffer","data":[24,30,10,0,0,16,1]}}	
2021-12-16 16:33:03.073 - debug: zigbee.0 (26219) zigbee-herdsman:controller:log Received 'zcl' data '{"frame":{"Header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":30,"manufacturerCode":null,"commandIdentifier":10},"Payload":[{"attrId":0,"dataType":16,"attrData":1}],"Command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}},"address":60149,"endpoint":1,"linkquality":72,"groupID":0,"wasBroadcast":false,"destinationEndpoint":1}'	
2021-12-16 16:33:03.076 - debug: zigbee.0 (26219) handleMessage. {"type":"attributeReport","device":{"ID":43,"_type":"Router","_ieeeAddr":"0xa4c138ec0e4ef1cf","_networkAddress":60149,"_manufacturerID":4417,"_endpoints":[{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":1,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":97,"inputClusters":[],"outputClusters":[33],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZ3000_npzfdcof","_powerSource":"Mains (single phase)","_modelID":"TS0001","_applicationVersion":67,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668783075,"_linkquality":72},"endpoint":"[Circular]","data":{"onOff":1},"linkquality":72,"groupID":0,"cluster":"genOnOff","meta":{"zclTransactionSequenceNumber":30,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:33:03.077 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:03.078 - debug: zigbee.0 (26219) Received Zigbee message from '0xa4c138ec0e4ef1cf', type 'attributeReport', cluster 'genOnOff', data '{"onOff":1}' from endpoint 1 with groupID 0	
2021-12-16 16:33:03.080 - debug: zigbee.0 (26219) Type attributeReport device {"type":"device","device":{"ID":43,"_type":"Router","_ieeeAddr":"0xa4c138ec0e4ef1cf","_networkAddress":60149,"_manufacturerID":4417,"_endpoints":[{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":1,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":97,"inputClusters":[],"outputClusters":[33],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZ3000_npzfdcof","_powerSource":"Mains (single phase)","_modelID":"TS0001","_applicationVersion":67,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668783075,"_linkquality":72},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["TS0001"],"model":"TS0001","vendor":"TuYa","description":"1 gang switch","whiteLabel":[{"vendor":"CR Smart Home","model":"TS0001","description":"Valve control"},{"vendor":"Lonsonho","model":"X701"},{"vendor":"Bandi","model":"BDS03G1"}],"options":[]},"name":"0xa4c138ec0e4ef1cf"} incoming event: {"type":"attributeReport","device":{"ID":43,"_type":"Router","_ieeeAddr":"0xa4c138ec0e4ef1cf","_networkAddress":60149,"_manufacturerID":4417,"_endpoints":[{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":1,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":97,"inputClusters":[],"outputClusters":[33],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZ3000_npzfdcof","_powerSource":"Mains (single phase)","_modelID":"TS0001","_applicationVersion":67,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668783075,"_linkquality":72},"endpoint":"[Circular]","data":{"onOff":1},"linkquality":72,"groupID":0,"cluster":"genOnOff","meta":{"zclTransactionSequenceNumber":30,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:33:03.083 - debug: zigbee.0 (26219) Publish available for 0xa4c138ec0e4ef1cf = true	
2021-12-16 16:33:03.087 - debug: zigbee.0 (26219) Publish LQ for 0xa4c138ec0e4ef1cf = 10	
2021-12-16 16:33:03.090 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0xa4c138ec0e4ef1cf/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:33:03.091 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0xa4c138ec0e4ef1cf:60149/1 (0,0,2)	
2021-12-16 16:33:03.092 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":60149,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":98,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,35,0,0,0]}}	
2021-12-16 16:33:03.093 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,245,234,1,1,6,0,98,0,30,5,16,35,0,0,0,121]	
2021-12-16 16:33:03.111 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:33:03.112 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:33:03.112 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:33:03.113 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:33:03.114 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:03.142 - debug: zigbee.0 (26219) Publish {"state":"ON"} to "a4c138ec0e4ef1cf"	
2021-12-16 16:33:03.158 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,98,69]	
2021-12-16 16:33:03.158 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,98,69]	
2021-12-16 16:33:03.159 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,98] - 69	
2021-12-16 16:33:03.159 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":98}	
2021-12-16 16:33:03.160 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:03.160 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0xa4c138ec0e4ef1cf:60149,225,0)	
2021-12-16 16:33:03.608 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,55,68,129,0,0,0,0]	
2021-12-16 16:33:03.608 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,55,68,129,0,0,0,0]	
2021-12-16 16:33:03.609 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [144,237,1,1,0,60,0,116,242,180,0,0,35,28,95,17]	
2021-12-16 16:33:03.610 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,55,68,129,0,0,0,0,144,237,1,1,0,60,0,116,242,180,0,0,35,28,95,17]	
2021-12-16 16:33:03.611 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [221,10,1,255,66,26,1,33,199,11,3,40,26,4,33,168]	
2021-12-16 16:33:03.612 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,55,68,129,0,0,0,0,144,237,1,1,0,60,0,116,242,180,0,0,35,28,95,17,221,10,1,255,66,26,1,33,199,11,3,40,26,4,33,168]	
2021-12-16 16:33:03.614 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [67,5,33,23,0,6,36,1,0,0,0,0,10,33,144,185,245,234,27,132]	
2021-12-16 16:33:03.614 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,55,68,129,0,0,0,0,144,237,1,1,0,60,0,116,242,180,0,0,35,28,95,17,221,10,1,255,66,26,1,33,199,11,3,40,26,4,33,168,67,5,33,23,0,6,36,1,0,0,0,0,10,33,144,185,245,234,27,132]	
2021-12-16 16:33:03.615 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 55 - 2 - 4 - 129 - [0,0,0,0,144,237,1,1,0,60,0,116,242,180,0,0,35,28,95,17,221,10,1,255,66,26,1,33,199,11,3,40,26,4,33,168,67,5,33,23,0,6,36,1,0,0,0,0,10,33,144,185,245,234,27] - 132	
2021-12-16 16:33:03.616 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - incomingMsg - {"groupid":0,"clusterid":0,"srcaddr":60816,"srcendpoint":1,"dstendpoint":1,"wasbroadcast":0,"linkquality":60,"securityuse":0,"timestamp":11858548,"transseqnumber":0,"len":35,"data":{"type":"Buffer","data":[28,95,17,221,10,1,255,66,26,1,33,199,11,3,40,26,4,33,168,67,5,33,23,0,6,36,1,0,0,0,0,10,33,144,185]}}	
2021-12-16 16:33:03.618 - debug: zigbee.0 (26219) zigbee-herdsman:controller:log Received 'zcl' data '{"frame":{"Header":{"frameControl":{"frameType":0,"manufacturerSpecific":true,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":221,"manufacturerCode":4447,"commandIdentifier":10},"Payload":[{"attrId":65281,"dataType":66,"attrData":{"1":3015,"3":26,"4":17320,"5":23,"6":[0,1],"10":47504}}],"Command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}},"address":60816,"endpoint":1,"linkquality":60,"groupID":0,"wasBroadcast":false,"destinationEndpoint":1}'	
2021-12-16 16:33:03.619 - debug: zigbee.0 (26219) handleMessage. {"type":"attributeReport","device":{"ID":7,"_type":"EndDevice","_ieeeAddr":"0x00158d0002130f3a","_networkAddress":60816,"_manufacturerID":4151,"_endpoints":[{"ID":1,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":60816,"deviceIeeeAddress":"0x00158d0002130f3a","clusters":{"genBasic":{"attributes":{"65281":{"1":3015,"3":26,"4":17320,"5":23,"6":[0,1],"10":47504},"modelId":"lumi.sensor_switch.aq2","appVersion":3}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_switch.aq2","_applicationVersion":3,"_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639668783618,"_linkquality":60},"endpoint":"[Circular]","data":{"65281":"[Circular]"},"linkquality":60,"groupID":0,"cluster":"genBasic","meta":{"zclTransactionSequenceNumber":221,"manufacturerCode":4447,"frameControl":{"frameType":0,"manufacturerSpecific":true,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:33:03.619 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:03.620 - debug: zigbee.0 (26219) Received Zigbee message from '0x00158d0002130f3a', type 'attributeReport', cluster 'genBasic', data '{"65281":{"1":3015,"3":26,"4":17320,"5":23,"6":[0,1],"10":47504}}' from endpoint 1 with groupID 0	
2021-12-16 16:33:03.621 - debug: zigbee.0 (26219) Type attributeReport device {"type":"device","device":{"ID":7,"_type":"EndDevice","_ieeeAddr":"0x00158d0002130f3a","_networkAddress":60816,"_manufacturerID":4151,"_endpoints":[{"ID":1,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":60816,"deviceIeeeAddress":"0x00158d0002130f3a","clusters":{"genBasic":{"attributes":{"65281":{"1":3015,"3":26,"4":17320,"5":23,"6":[0,1],"10":47504},"modelId":"lumi.sensor_switch.aq2","appVersion":3}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_switch.aq2","_applicationVersion":3,"_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639668783618,"_linkquality":60},"mapped":{"zigbeeModel":["lumi.sensor_switch.aq2","lumi.remote.b1acn01"],"model":"WXKG11LM","vendor":"Xiaomi","description":"Aqara wireless switch","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"enum","name":"action","property":"action","access":1,"values":["single","double","triple","quadruple","hold","release"],"description":"Triggered action (e.g. a button click)"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genMultistateInput","type":["attributeReport"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genMultistateInput","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]}],"toZigbee":[],"options":["[Circular]"]},"name":"0x00158d0002130f3a"} incoming event: {"type":"attributeReport","device":{"ID":7,"_type":"EndDevice","_ieeeAddr":"0x00158d0002130f3a","_networkAddress":60816,"_manufacturerID":4151,"_endpoints":[{"ID":1,"inputClusters":[],"outputClusters":[],"deviceNetworkAddress":60816,"deviceIeeeAddress":"0x00158d0002130f3a","clusters":{"genBasic":{"attributes":{"65281":{"1":3015,"3":26,"4":17320,"5":23,"6":[0,1],"10":47504},"modelId":"lumi.sensor_switch.aq2","appVersion":3}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_switch.aq2","_applicationVersion":3,"_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639668783618,"_linkquality":60},"endpoint":"[Circular]","data":{"65281":"[Circular]"},"linkquality":60,"groupID":0,"cluster":"genBasic","meta":{"zclTransactionSequenceNumber":221,"manufacturerCode":4447,"frameControl":{"frameType":0,"manufacturerSpecific":true,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:33:03.637 - debug: zigbee.0 (26219) Publish {"voltage":3015,"battery":100} to "00158d0002130f3a"	
2021-12-16 16:33:05.162 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0xa4c138ec0e4ef1cf:60149/1 (0,1,2)	
2021-12-16 16:33:05.163 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":60149,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":99,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,35,0,0,0]}}	
2021-12-16 16:33:05.164 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,245,234,1,1,6,0,99,0,30,5,16,35,0,0,0,120]	
2021-12-16 16:33:05.173 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:33:05.174 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:33:05.175 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:33:05.176 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:33:05.176 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:05.206 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,99,68]	
2021-12-16 16:33:05.207 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,99,68]	
2021-12-16 16:33:05.207 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,99] - 68	
2021-12-16 16:33:05.208 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":99}	
2021-12-16 16:33:05.209 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:05.209 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0xa4c138ec0e4ef1cf:60149,225,1)	
2021-12-16 16:33:07.211 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0xa4c138ec0e4ef1cf:60149/1 (0,2,2)	
2021-12-16 16:33:07.212 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":60149,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":100,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,35,0,0,0]}}	
2021-12-16 16:33:07.213 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,245,234,1,1,6,0,100,0,30,5,16,35,0,0,0,127]	
2021-12-16 16:33:07.223 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:33:07.224 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:33:07.224 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:33:07.225 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:33:07.226 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:07.278 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,100,67]	
2021-12-16 16:33:07.279 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,100,67]	
2021-12-16 16:33:07.280 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,100] - 67	
2021-12-16 16:33:07.281 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":100}	
2021-12-16 16:33:07.283 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:07.284 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0xa4c138ec0e4ef1cf:60149,225,2)	
2021-12-16 16:33:08.865 - debug: zigbee.0 (26219) User stateChange zigbee.0.a4c138ec0e4ef1cf.state {"val":false,"ack":false,"ts":1639668788862,"q":0,"from":"system.adapter.zigbee.0","user":"system.user.admin","lc":1639668788862}	
2021-12-16 16:33:08.869 - debug: zigbee.0 (26219) Change state 'state' at device 0xa4c138ec0e4ef1cf type 'TS0001'	
2021-12-16 16:33:08.871 - debug: zigbee.0 (26219) entity: {"type":"device","device":{"ID":43,"_type":"Router","_ieeeAddr":"0xa4c138ec0e4ef1cf","_networkAddress":60149,"_manufacturerID":4417,"_endpoints":[{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":1,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":97,"inputClusters":[],"outputClusters":[33],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZ3000_npzfdcof","_powerSource":"Mains (single phase)","_modelID":"TS0001","_applicationVersion":67,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668783075,"_linkquality":72},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["TS0001"],"model":"TS0001","vendor":"TuYa","description":"1 gang switch","whiteLabel":[{"vendor":"CR Smart Home","model":"TS0001","description":"Valve control"},{"vendor":"Lonsonho","model":"X701"},{"vendor":"Bandi","model":"BDS03G1"}],"options":[]},"endpoint":"[Circular]","endpoints":"[Circular]","name":"0xa4c138ec0e4ef1cf"}	
2021-12-16 16:33:08.872 - debug: zigbee.0 (26219) Mapped Model: {"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["TS0001"],"model":"TS0001","vendor":"TuYa","description":"1 gang switch","whiteLabel":[{"vendor":"CR Smart Home","model":"TS0001","description":"Valve control"},{"vendor":"Lonsonho","model":"X701"},{"vendor":"Bandi","model":"BDS03G1"}],"options":[]}	
2021-12-16 16:33:08.872 - debug: zigbee.0 (26219) convert state, "OFF", {"state":"OFF"}	
2021-12-16 16:33:08.872 - debug: zigbee.0 (26219) target: {"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":1,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]}	
2021-12-16 16:33:08.873 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Command 0xa4c138ec0e4ef1cf/1 genOnOff.off({}, {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:33:09.285 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0xa4c138ec0e4ef1cf:60149/1 (0,3,3)	
2021-12-16 16:33:09.285 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":60149,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":101,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,35,0,0,0]}}	
2021-12-16 16:33:09.286 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,245,234,1,1,6,0,101,0,30,5,16,35,0,0,0,126]	
2021-12-16 16:33:09.294 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:33:09.295 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:33:09.295 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:33:09.295 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:33:09.295 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:09.321 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,101,66]	
2021-12-16 16:33:09.322 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,101,66]	
2021-12-16 16:33:09.323 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,101] - 66	
2021-12-16 16:33:09.324 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":101}	
2021-12-16 16:33:09.325 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:09.325 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0xa4c138ec0e4ef1cf:60149,225,3)	
2021-12-16 16:33:11.326 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0xa4c138ec0e4ef1cf:60149/1 (0,4,3)	
2021-12-16 16:33:11.327 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":60149,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":102,"options":0,"radius":30,"len":5,"data":{"type":"Buffer","data":[16,35,0,0,0]}}	
2021-12-16 16:33:11.329 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,15,36,1,245,234,1,1,6,0,102,0,30,5,16,35,0,0,0,125]	
2021-12-16 16:33:11.337 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:33:11.339 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:33:11.340 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:33:11.340 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:33:11.341 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:11.372 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,102,65]	
2021-12-16 16:33:11.373 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,102,65]	
2021-12-16 16:33:11.374 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,102] - 65	
2021-12-16 16:33:11.374 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":102}	
2021-12-16 16:33:11.375 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:11.376 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0xa4c138ec0e4ef1cf:60149,225,4)	
2021-12-16 16:33:11.377 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0xa4c138ec0e4ef1cf:60149/1 (0,0,2)	
2021-12-16 16:33:11.378 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":60149,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":103,"options":0,"radius":30,"len":3,"data":{"type":"Buffer","data":[1,36,0]}}	
2021-12-16 16:33:11.379 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,13,36,1,245,234,1,1,6,0,103,0,30,3,1,36,0,110]	
2021-12-16 16:33:11.380 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Read 0xa4c138ec0e4ef1cf/1 genOnOff(["onOff"], {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":true,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'MAC channel access failure' (225))	
2021-12-16 16:33:11.381 - debug: zigbee.0 (26219) Failed to read state of '0xa4c138ec0e4ef1cf' after reconnect	
2021-12-16 16:33:11.389 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:33:11.390 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:33:11.391 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:33:11.392 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:33:11.394 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:11.421 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,103,64]	
2021-12-16 16:33:11.422 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,103,64]	
2021-12-16 16:33:11.425 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,103] - 64	
2021-12-16 16:33:11.426 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":103}	
2021-12-16 16:33:11.427 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:11.428 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0xa4c138ec0e4ef1cf:60149,225,0)	
2021-12-16 16:33:12.365 - debug: zigbee.0 (26219) Failed to execute LQI for '0x7cb03eaa0a00dfcb'. "Error: AREQ - ZDO - mgmtLqiRsp after 10000ms\n at Timeout._onTimeout (/opt/iobroker/node_modules/zigbee-herdsman/dist/utils/waitress.js:37:35)\n at listOnTimeout (internal/timers.js:557:17)\n at processTimers (internal/timers.js:500:7)"	
2021-12-16 16:33:12.366 - debug: zigbee.0 (26219) LQI succeeded for '0x7cb03eaa0a00dfcb'	
2021-12-16 16:33:12.367 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtRtgReq - {"dstaddr":34528,"startindex":0}	
2021-12-16 16:33:12.368 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,50,224,134,0,114]	
2021-12-16 16:33:12.377 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,50,0,86]	
2021-12-16 16:33:12.378 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,50,0,86]	
2021-12-16 16:33:12.379 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 50 - [0] - 86	
2021-12-16 16:33:12.380 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtRtgReq - {"status":0}	
2021-12-16 16:33:12.381 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:13.430 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0xa4c138ec0e4ef1cf:60149/1 (0,1,2)	
2021-12-16 16:33:13.432 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":60149,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":104,"options":0,"radius":30,"len":3,"data":{"type":"Buffer","data":[1,36,0]}}	
2021-12-16 16:33:13.433 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,13,36,1,245,234,1,1,6,0,104,0,30,3,1,36,0,97]	
2021-12-16 16:33:13.441 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:33:13.442 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:33:13.443 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:33:13.444 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:33:13.445 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:13.473 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,104,79]	
2021-12-16 16:33:13.474 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,104,79]	
2021-12-16 16:33:13.474 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,104] - 79	
2021-12-16 16:33:13.475 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":104}	
2021-12-16 16:33:13.476 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:13.476 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0xa4c138ec0e4ef1cf:60149,225,1)	
2021-12-16 16:33:15.478 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0xa4c138ec0e4ef1cf:60149/1 (0,2,2)	
2021-12-16 16:33:15.481 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":60149,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":105,"options":0,"radius":30,"len":3,"data":{"type":"Buffer","data":[1,36,0]}}	
2021-12-16 16:33:15.482 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,13,36,1,245,234,1,1,6,0,105,0,30,3,1,36,0,96]	
2021-12-16 16:33:15.491 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:33:15.493 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:33:15.493 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:33:15.494 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:33:15.495 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:15.534 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,105,78]	
2021-12-16 16:33:15.535 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,105,78]	
2021-12-16 16:33:15.536 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,105] - 78	
2021-12-16 16:33:15.537 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":105}	
2021-12-16 16:33:15.537 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:15.538 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0xa4c138ec0e4ef1cf:60149,225,2)	
2021-12-16 16:33:17.539 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0xa4c138ec0e4ef1cf:60149/1 (0,3,2)	
2021-12-16 16:33:17.541 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":60149,"destendpoint":1,"srcendpoint":1,"clusterid":6,"transid":106,"options":0,"radius":30,"len":3,"data":{"type":"Buffer","data":[1,36,0]}}	
2021-12-16 16:33:17.542 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,13,36,1,245,234,1,1,6,0,106,0,30,3,1,36,0,99]	
2021-12-16 16:33:17.551 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:33:17.552 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:33:17.552 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:33:17.553 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:33:17.554 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:17.568 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,0,1,106,172]	
2021-12-16 16:33:17.569 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,0,1,106,172]	
2021-12-16 16:33:17.570 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [0,1,106] - 172	
2021-12-16 16:33:17.570 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":0,"endpoint":1,"transid":106}	
2021-12-16 16:33:17.571 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:17.612 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,25,68,129,0,0,6,0]	
2021-12-16 16:33:17.613 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,25,68,129,0,0,6,0]	
2021-12-16 16:33:17.615 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [245,234,1,1,0,63,0,240,76,194,0,0,5,24,36,11,0,0,245,234,29,180,254,27]	
2021-12-16 16:33:17.617 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,25,68,129,0,0,6,0,245,234,1,1,0,63,0,240,76,194,0,0,5,24,36,11,0,0,245,234,29,180,254,27]	
2021-12-16 16:33:17.617 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 25 - 2 - 4 - 129 - [0,0,6,0,245,234,1,1,0,63,0,240,76,194,0,0,5,24,36,11,0,0,245,234,29] - 180	
2021-12-16 16:33:17.619 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - incomingMsg - {"groupid":0,"clusterid":6,"srcaddr":60149,"srcendpoint":1,"dstendpoint":1,"wasbroadcast":0,"linkquality":63,"securityuse":0,"timestamp":12733680,"transseqnumber":0,"len":5,"data":{"type":"Buffer","data":[24,36,11,0,0]}}	
2021-12-16 16:33:17.620 - debug: zigbee.0 (26219) zigbee-herdsman:controller:log Received 'zcl' data '{"frame":{"Header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":36,"manufacturerCode":null,"commandIdentifier":11},"Payload":{"cmdId":0,"statusCode":0},"Command":{"ID":11,"name":"defaultRsp","parameters":[{"name":"cmdId","type":32},{"name":"statusCode","type":32}]}},"address":60149,"endpoint":1,"linkquality":63,"groupID":0,"wasBroadcast":false,"destinationEndpoint":1}'	
2021-12-16 16:33:17.621 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,27]	
2021-12-16 16:33:17.622 - debug: zigbee.0 (26219) convert result {"state":{"state":"OFF"}}	
2021-12-16 16:33:17.628 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [68,129,0,0,6,0,245,234,1,1,0,60,0,167,77,194,0,0,7,24,31,10,0,0,16,0,245,234,29,203]	
2021-12-16 16:33:17.629 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,27,68,129,0,0,6,0,245,234,1,1,0,60,0,167,77,194,0,0,7,24,31,10,0,0,16,0,245,234,29,203]	
2021-12-16 16:33:17.630 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 27 - 2 - 4 - 129 - [0,0,6,0,245,234,1,1,0,60,0,167,77,194,0,0,7,24,31,10,0,0,16,0,245,234,29] - 203	
2021-12-16 16:33:17.631 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - incomingMsg - {"groupid":0,"clusterid":6,"srcaddr":60149,"srcendpoint":1,"dstendpoint":1,"wasbroadcast":0,"linkquality":60,"securityuse":0,"timestamp":12733863,"transseqnumber":0,"len":7,"data":{"type":"Buffer","data":[24,31,10,0,0,16,0]}}	
2021-12-16 16:33:17.634 - debug: zigbee.0 (26219) zigbee-herdsman:controller:log Received 'zcl' data '{"frame":{"Header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":31,"manufacturerCode":null,"commandIdentifier":10},"Payload":[{"attrId":0,"dataType":16,"attrData":0}],"Command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}},"address":60149,"endpoint":1,"linkquality":60,"groupID":0,"wasBroadcast":false,"destinationEndpoint":1}'	
2021-12-16 16:33:17.636 - debug: zigbee.0 (26219) handleMessage. {"type":"attributeReport","device":{"ID":43,"_type":"Router","_ieeeAddr":"0xa4c138ec0e4ef1cf","_networkAddress":60149,"_manufacturerID":4417,"_endpoints":[{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":0,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":97,"inputClusters":[],"outputClusters":[33],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZ3000_npzfdcof","_powerSource":"Mains (single phase)","_modelID":"TS0001","_applicationVersion":67,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668797635,"_linkquality":60},"endpoint":"[Circular]","data":{"onOff":0},"linkquality":60,"groupID":0,"cluster":"genOnOff","meta":{"zclTransactionSequenceNumber":31,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:33:17.637 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:17.637 - debug: zigbee.0 (26219) Received Zigbee message from '0xa4c138ec0e4ef1cf', type 'attributeReport', cluster 'genOnOff', data '{"onOff":0}' from endpoint 1 with groupID 0	
2021-12-16 16:33:17.639 - debug: zigbee.0 (26219) Type attributeReport device {"type":"device","device":{"ID":43,"_type":"Router","_ieeeAddr":"0xa4c138ec0e4ef1cf","_networkAddress":60149,"_manufacturerID":4417,"_endpoints":[{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":0,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":97,"inputClusters":[],"outputClusters":[33],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZ3000_npzfdcof","_powerSource":"Mains (single phase)","_modelID":"TS0001","_applicationVersion":67,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668797635,"_linkquality":60},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["TS0001"],"model":"TS0001","vendor":"TuYa","description":"1 gang switch","whiteLabel":[{"vendor":"CR Smart Home","model":"TS0001","description":"Valve control"},{"vendor":"Lonsonho","model":"X701"},{"vendor":"Bandi","model":"BDS03G1"}],"options":[]},"name":"0xa4c138ec0e4ef1cf"} incoming event: {"type":"attributeReport","device":{"ID":43,"_type":"Router","_ieeeAddr":"0xa4c138ec0e4ef1cf","_networkAddress":60149,"_manufacturerID":4417,"_endpoints":[{"ID":1,"profileID":260,"deviceID":256,"inputClusters":[3,4,5,6,57344,57345,0],"outputClusters":[25,10],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{"genBasic":{"attributes":{"modelId":"TS0001","manufacturerName":"_TZ3000_npzfdcof","powerSource":1,"zclVersion":3,"appVersion":67,"stackVersion":0,"hwVersion":1,"dateCode":""}},"genOnOff":{"attributes":{"onOff":0,"onTime":0,"offWaitTime":0,"moesStartUpOnOff":2}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[],"meta":{},"pendingRequests":[]},{"ID":242,"profileID":41440,"deviceID":97,"inputClusters":[],"outputClusters":[33],"deviceNetworkAddress":60149,"deviceIeeeAddress":"0xa4c138ec0e4ef1cf","clusters":{},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"_TZ3000_npzfdcof","_powerSource":"Mains (single phase)","_modelID":"TS0001","_applicationVersion":67,"_stackVersion":0,"_zclVersion":3,"_hardwareVersion":1,"_dateCode":"","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668797635,"_linkquality":60},"endpoint":"[Circular]","data":{"onOff":0},"linkquality":60,"groupID":0,"cluster":"genOnOff","meta":{"zclTransactionSequenceNumber":31,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:33:17.661 - debug: zigbee.0 (26219) Publish {"state":"OFF"} to "a4c138ec0e4ef1cf"	
2021-12-16 16:33:22.392 - debug: zigbee.0 (26219) Failed to execute routing table for '0x7cb03eaa0a00dfcb'. "Error: AREQ - ZDO - mgmtRtgRsp after 10000ms\n at Timeout._onTimeout (/opt/iobroker/node_modules/zigbee-herdsman/dist/utils/waitress.js:37:35)\n at listOnTimeout (internal/timers.js:557:17)\n at processTimers (internal/timers.js:500:7)"	
2021-12-16 16:33:22.392 - debug: zigbee.0 (26219) Routing for '0x7cb03eaa0a00dfcb': undefined	
2021-12-16 16:33:22.393 - debug: zigbee.0 (26219) Routing table succeeded for '0x7cb03eaa0a00dfcb'	
2021-12-16 16:33:22.393 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtLqiReq - {"dstaddr":41267,"startindex":0}	
2021-12-16 16:33:22.394 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,49,51,161,0,133]	
2021-12-16 16:33:22.402 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,49,0,85]	
2021-12-16 16:33:22.404 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,49,0,85]	
2021-12-16 16:33:22.405 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 49 - [0] - 85	
2021-12-16 16:33:22.406 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtLqiReq - {"status":0}	
2021-12-16 16:33:22.406 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:32.408 - debug: zigbee.0 (26219) Failed to execute LQI for '0x00158d0002c65ed8'. "Error: AREQ - ZDO - mgmtLqiRsp after 10000ms\n at Timeout._onTimeout (/opt/iobroker/node_modules/zigbee-herdsman/dist/utils/waitress.js:37:35)\n at listOnTimeout (internal/timers.js:557:17)\n at processTimers (internal/timers.js:500:7)"	
2021-12-16 16:33:32.409 - debug: zigbee.0 (26219) LQI succeeded for '0x00158d0002c65ed8'	
2021-12-16 16:33:32.410 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtRtgReq - {"dstaddr":41267,"startindex":0}	
2021-12-16 16:33:32.411 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,50,51,161,0,134]	
2021-12-16 16:33:32.420 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,50,0,86]	
2021-12-16 16:33:32.420 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,50,0,86]	
2021-12-16 16:33:32.421 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 50 - [0] - 86	
2021-12-16 16:33:32.422 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtRtgReq - {"status":0}	
2021-12-16 16:33:32.425 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:42.427 - debug: zigbee.0 (26219) Failed to execute routing table for '0x00158d0002c65ed8'. "Error: AREQ - ZDO - mgmtRtgRsp after 10000ms\n at Timeout._onTimeout (/opt/iobroker/node_modules/zigbee-herdsman/dist/utils/waitress.js:37:35)\n at listOnTimeout (internal/timers.js:557:17)\n at processTimers (internal/timers.js:500:7)"	
2021-12-16 16:33:42.428 - debug: zigbee.0 (26219) Routing for '0x00158d0002c65ed8': undefined	
2021-12-16 16:33:42.428 - debug: zigbee.0 (26219) Routing table succeeded for '0x00158d0002c65ed8'	
2021-12-16 16:33:42.429 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtLqiReq - {"dstaddr":56716,"startindex":0}	
2021-12-16 16:33:42.430 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,49,140,221,0,70]	
2021-12-16 16:33:42.438 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,49,0,85]	
2021-12-16 16:33:42.439 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,49,0,85]	
2021-12-16 16:33:42.440 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 49 - [0] - 85	
2021-12-16 16:33:42.441 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtLqiReq - {"status":0}	
2021-12-16 16:33:42.442 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:33:52.444 - debug: zigbee.0 (26219) Failed to execute LQI for '0x84182600000c7532'. "Error: AREQ - ZDO - mgmtLqiRsp after 10000ms\n at Timeout._onTimeout (/opt/iobroker/node_modules/zigbee-herdsman/dist/utils/waitress.js:37:35)\n at listOnTimeout (internal/timers.js:557:17)\n at processTimers (internal/timers.js:500:7)"	
2021-12-16 16:33:52.445 - debug: zigbee.0 (26219) LQI succeeded for '0x84182600000c7532'	
2021-12-16 16:33:52.446 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtRtgReq - {"dstaddr":56716,"startindex":0}	
2021-12-16 16:33:52.446 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,50,140,221,0,69]	
2021-12-16 16:33:52.454 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,50,0,86]	
2021-12-16 16:33:52.455 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,50,0,86]	
2021-12-16 16:33:52.455 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 50 - [0] - 86	
2021-12-16 16:33:52.456 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtRtgReq - {"status":0}	
2021-12-16 16:33:52.456 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:02.145 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002b54a17 lumi.weather was last seen '545.633' seconds ago.	
2021-12-16 16:34:02.147 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002130d3b lumi.sensor_switch.aq2 was last seen '101.284' seconds ago.	
2021-12-16 16:34:02.148 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002130f3a lumi.sensor_switch.aq2 was last seen '58.53' seconds ago.	
2021-12-16 16:34:02.151 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002f8d76c lumi.ctrl_neutral1 was last seen '7951230.354' seconds ago.	
2021-12-16 16:34:02.153 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000274f4de lumi.sensor_magnet.aq2 was last seen '781.467' seconds ago.	
2021-12-16 16:34:02.155 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002135d9b lumi.sensor_switch.aq2 was last seen '4054.969' seconds ago.	
2021-12-16 16:34:02.156 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000274f4bf lumi.sensor_magnet.aq2 was last seen '2815.201' seconds ago.	
2021-12-16 16:34:02.159 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000271c4b7 lumi.sensor_wleak.aq1 was last seen '2579.088' seconds ago.	
2021-12-16 16:34:02.162 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002f8d5b4 lumi.ctrl_neutral1 was last seen '7951254.82' seconds ago.	
2021-12-16 16:34:02.165 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002e34b33 lumi.ctrl_neutral1 was last seen '7951236.718' seconds ago.	
2021-12-16 16:34:02.167 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000521d656 lumi.switch.b1lacn02 was last seen '7951229.832' seconds ago.	
2021-12-16 16:34:02.170 - debug: zigbee.0 (26219) Non-pingable device 0x00158d00028aee30 lumi.sensor_cube.aqgl01 was last seen '2455.913' seconds ago.	
2021-12-16 16:34:02.177 - debug: zigbee.0 (26219) Non-pingable device 0x00158d00021369f3 lumi.sensor_switch.aq2 was last seen '2732.722' seconds ago.	
2021-12-16 16:34:02.178 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002b54752 lumi.weather was last seen '855.141' seconds ago.	
2021-12-16 16:34:02.180 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000274f643 lumi.sensor_magnet.aq2 was last seen '2929.88' seconds ago.	
2021-12-16 16:34:02.183 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000274f64d lumi.sensor_magnet.aq2 was last seen '283.715' seconds ago.	
2021-12-16 16:34:02.185 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002b51c42 lumi.weather was last seen '474.381' seconds ago.	
2021-12-16 16:34:02.186 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000274f4f7 lumi.sensor_magnet.aq2 was last seen '4960.169' seconds ago.	
2021-12-16 16:34:02.189 - debug: zigbee.0 (26219) Non-pingable device 0x00158d000274f4d3 lumi.sensor_magnet.aq2 was last seen '1682.466' seconds ago.	
2021-12-16 16:34:02.191 - debug: zigbee.0 (26219) Non-pingable device 0x00158d0002722af7 lumi.sensor_magnet.aq2 was last seen '4274.964' seconds ago.	
2021-12-16 16:34:02.192 - debug: zigbee.0 (26219) Non-pingable device 0x847127fffed62092 TS0601 was last seen '3353.026' seconds ago.	
2021-12-16 16:34:02.195 - debug: zigbee.0 (26219) Non-pingable device 0x847127fffed0a598 TS0601 was last seen '853.53' seconds ago.	
2021-12-16 16:34:02.198 - debug: zigbee.0 (26219) Non-pingable device 0x847127fffecfc657 TS0601 was last seen '467.224' seconds ago.	
2021-12-16 16:34:02.201 - debug: zigbee.0 (26219) Non-pingable device 0x000d6ffffe2cd4b8 FYRTUR block-out roller blind was last seen '864987.415' seconds ago.	
2021-12-16 16:34:02.457 - debug: zigbee.0 (26219) Failed to execute routing table for '0x84182600000c7532'. "Error: AREQ - ZDO - mgmtRtgRsp after 10000ms\n at Timeout._onTimeout (/opt/iobroker/node_modules/zigbee-herdsman/dist/utils/waitress.js:37:35)\n at listOnTimeout (internal/timers.js:557:17)\n at processTimers (internal/timers.js:500:7)"	
2021-12-16 16:34:02.457 - debug: zigbee.0 (26219) Routing for '0x84182600000c7532': undefined	
2021-12-16 16:34:02.457 - debug: zigbee.0 (26219) Routing table succeeded for '0x84182600000c7532'	
2021-12-16 16:34:02.458 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtLqiReq - {"dstaddr":18602,"startindex":0}	
2021-12-16 16:34:02.458 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,49,170,72,0,245]	
2021-12-16 16:34:02.464 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,49,0,85]	
2021-12-16 16:34:02.465 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,49,0,85]	
2021-12-16 16:34:02.465 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 49 - [0] - 85	
2021-12-16 16:34:02.465 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtLqiReq - {"status":0}	
2021-12-16 16:34:02.466 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:10.434 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,31,68,129,0,0,6,0]	
2021-12-16 16:34:10.435 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,31,68,129,0,0,6,0]	
2021-12-16 16:34:10.437 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [142,241,1,1,0,75,0,167,173,4,0,0,11,24,217,10,0,0,16,0,0,0,16,1,245,234,27,35]	
2021-12-16 16:34:10.439 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,31,68,129,0,0,6,0,142,241,1,1,0,75,0,167,173,4,0,0,11,24,217,10,0,0,16,0,0,0,16,1,245,234,27,35]	
2021-12-16 16:34:10.440 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 31 - 2 - 4 - 129 - [0,0,6,0,142,241,1,1,0,75,0,167,173,4,0,0,11,24,217,10,0,0,16,0,0,0,16,1,245,234,27] - 35	
2021-12-16 16:34:10.441 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - incomingMsg - {"groupid":0,"clusterid":6,"srcaddr":61838,"srcendpoint":1,"dstendpoint":1,"wasbroadcast":0,"linkquality":75,"securityuse":0,"timestamp":306599,"transseqnumber":0,"len":11,"data":{"type":"Buffer","data":[24,217,10,0,0,16,0,0,0,16,1]}}	
2021-12-16 16:34:10.443 - debug: zigbee.0 (26219) zigbee-herdsman:controller:log Received 'zcl' data '{"frame":{"Header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":217,"manufacturerCode":null,"commandIdentifier":10},"Payload":[{"attrId":0,"dataType":16,"attrData":0},{"attrId":0,"dataType":16,"attrData":1}],"Command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}},"address":61838,"endpoint":1,"linkquality":75,"groupID":0,"wasBroadcast":false,"destinationEndpoint":1}'	
2021-12-16 16:34:10.446 - debug: zigbee.0 (26219) handleMessage. {"type":"attributeReport","device":{"ID":3,"_type":"EndDevice","_ieeeAddr":"0x00158d0002130d3b","_networkAddress":61838,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":61838,"deviceIeeeAddress":"0x00158d0002130d3b","clusters":{"genBasic":{"attributes":{"65281":{"1":3005,"3":27,"4":17320,"5":48,"6":[0,1],"10":47504},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_switch.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639668850444,"_linkquality":75},"endpoint":"[Circular]","data":{"onOff":1},"linkquality":75,"groupID":0,"cluster":"genOnOff","meta":{"zclTransactionSequenceNumber":217,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:34:10.447 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:10.447 - debug: zigbee.0 (26219) Received Zigbee message from '0x00158d0002130d3b', type 'attributeReport', cluster 'genOnOff', data '{"onOff":1}' from endpoint 1 with groupID 0	
2021-12-16 16:34:10.449 - debug: zigbee.0 (26219) Type attributeReport device {"type":"device","device":{"ID":3,"_type":"EndDevice","_ieeeAddr":"0x00158d0002130d3b","_networkAddress":61838,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":61838,"deviceIeeeAddress":"0x00158d0002130d3b","clusters":{"genBasic":{"attributes":{"65281":{"1":3005,"3":27,"4":17320,"5":48,"6":[0,1],"10":47504},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_switch.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639668850444,"_linkquality":75},"mapped":{"zigbeeModel":["lumi.sensor_switch.aq2","lumi.remote.b1acn01"],"model":"WXKG11LM","vendor":"Xiaomi","description":"Aqara wireless switch","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"enum","name":"action","property":"action","access":1,"values":["single","double","triple","quadruple","hold","release"],"description":"Triggered action (e.g. a button click)"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genMultistateInput","type":["attributeReport"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"genOnOff","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]},{"cluster":"genMultistateInput","type":["attributeReport","readResponse"],"options":[{"type":"binary","name":"legacy","property":"legacy","access":2,"value_on":true,"value_off":false,"description":"Set to false to disable the legacy integration (highly recommended), will change structure of the published payload (default true)."}]}],"toZigbee":[],"options":["[Circular]"]},"name":"0x00158d0002130d3b"} incoming event: {"type":"attributeReport","device":{"ID":3,"_type":"EndDevice","_ieeeAddr":"0x00158d0002130d3b","_networkAddress":61838,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,65535,6],"outputClusters":[0,4,65535],"deviceNetworkAddress":61838,"deviceIeeeAddress":"0x00158d0002130d3b","clusters":{"genBasic":{"attributes":{"65281":{"1":3005,"3":27,"4":17320,"5":48,"6":[0,1],"10":47504},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":2,"dateCode":"20161128","swBuildId":"3000-0001"}},"genOnOff":{"attributes":{"32768":2,"onOff":1}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.sensor_switch.aq2","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":2,"_dateCode":"20161128","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{},"_lastSeen":1639668850444,"_linkquality":75},"endpoint":"[Circular]","data":{"onOff":1},"linkquality":75,"groupID":0,"cluster":"genOnOff","meta":{"zclTransactionSequenceNumber":217,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:34:10.483 - debug: zigbee.0 (26219) Publish {"action":"single"} to "00158d0002130d3b"	
2021-12-16 16:34:10.487 - debug: zigbee.0 (26219) Publish {"click":"single"} to "00158d0002130d3b"	
2021-12-16 16:34:10.517 - info: javascript.0 (25312) script.js.common.Lautsprecher: Knopf wurde gedrückt	
2021-12-16 16:34:10.522 - debug: zigbee.0 (26219) User stateChange zigbee.0.7cb03eaa00acb990.state {"val":false,"ack":false,"ts":1639668850520,"q":0,"c":"script.js.common.Lautsprecher","from":"system.adapter.javascript.0","user":"system.user.admin","lc":1639668850520}	
2021-12-16 16:34:10.574 - debug: zigbee.0 (26219) Change state 'state' at device 0x7cb03eaa00acb990 type 'AB3257001NJ'	
2021-12-16 16:34:10.576 - debug: zigbee.0 (26219) entity: {"type":"device","device":{"ID":4,"_type":"Router","_ieeeAddr":"0x7cb03eaa00acb990","_networkAddress":47504,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":47504,"deviceIeeeAddress":"0x7cb03eaa00acb990","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":1}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668747220,"_linkquality":75},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["Plug 01"],"model":"AB3257001NJ","description":"Smart+ plug","vendor":"OSRAM","whiteLabel":[{"vendor":"LEDVANCE","model":"AB3257001NJ"}],"ota":{},"options":[]},"endpoint":"[Circular]","endpoints":"[Circular]","name":"0x7cb03eaa00acb990"}	
2021-12-16 16:34:10.577 - debug: zigbee.0 (26219) Mapped Model: {"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["Plug 01"],"model":"AB3257001NJ","description":"Smart+ plug","vendor":"OSRAM","whiteLabel":[{"vendor":"LEDVANCE","model":"AB3257001NJ"}],"ota":{},"options":[]}	
2021-12-16 16:34:10.577 - debug: zigbee.0 (26219) convert state, "OFF", {"state":"OFF"}	
2021-12-16 16:34:10.577 - debug: zigbee.0 (26219) target: {"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":47504,"deviceIeeeAddress":"0x7cb03eaa00acb990","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":1}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}	
2021-12-16 16:34:10.579 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Command 0x7cb03eaa00acb990/3 genOnOff.off({}, {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false})	
2021-12-16 16:34:10.579 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00acb990:47504/3 (0,0,2)	
2021-12-16 16:34:10.579 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":47504,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":107,"options":0,"radius":30,"len":3,"data":{"type":"Buffer","data":[1,37,0]}}	
2021-12-16 16:34:10.580 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,13,36,1,144,185,3,1,6,0,107,0,30,3,1,37,0,87]	
2021-12-16 16:34:10.587 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:34:10.588 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:34:10.588 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:34:10.588 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:34:10.589 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:10.621 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,107,76]	
2021-12-16 16:34:10.622 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,107,76]	
2021-12-16 16:34:10.622 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,107] - 76	
2021-12-16 16:34:10.622 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":107}	
2021-12-16 16:34:10.622 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:10.623 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00acb990:47504,225,0)	
2021-12-16 16:34:10.650 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,28,68,129,0,0,2,4]	
2021-12-16 16:34:10.651 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,28,68,129,0,0,2,4]	
2021-12-16 16:34:10.652 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [220,155,1,1,0,75,0,180,226,4,0,0,8,24,63,10]	
2021-12-16 16:34:10.653 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,28,68,129,0,0,2,4,220,155,1,1,0,75,0,180,226,4,0,0,8,24,63,10]	
2021-12-16 16:34:10.655 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [0,0,41,92,8,245,234,26,220]	
2021-12-16 16:34:10.655 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,28,68,129,0,0,2,4,220,155,1,1,0,75,0,180,226,4,0,0,8,24,63,10,0,0,41,92,8,245,234,26,220]	
2021-12-16 16:34:10.656 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 28 - 2 - 4 - 129 - [0,0,2,4,220,155,1,1,0,75,0,180,226,4,0,0,8,24,63,10,0,0,41,92,8,245,234,26] - 220	
2021-12-16 16:34:10.656 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - incomingMsg - {"groupid":0,"clusterid":1026,"srcaddr":39900,"srcendpoint":1,"dstendpoint":1,"wasbroadcast":0,"linkquality":75,"securityuse":0,"timestamp":320180,"transseqnumber":0,"len":8,"data":{"type":"Buffer","data":[24,63,10,0,0,41,92,8]}}	
2021-12-16 16:34:10.658 - debug: zigbee.0 (26219) zigbee-herdsman:controller:log Received 'zcl' data '{"frame":{"Header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":63,"manufacturerCode":null,"commandIdentifier":10},"Payload":[{"attrId":0,"dataType":41,"attrData":2140}],"Command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}},"address":39900,"endpoint":1,"linkquality":75,"groupID":0,"wasBroadcast":false,"destinationEndpoint":1}'	
2021-12-16 16:34:10.659 - debug: zigbee.0 (26219) handleMessage. {"type":"attributeReport","device":{"ID":20,"_type":"EndDevice","_ieeeAddr":"0x00158d0002b54752","_networkAddress":39900,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":39900,"deviceIeeeAddress":"0x00158d0002b54752","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2140}},"msRelativeHumidity":{"attributes":{"measuredValue":5113}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10313}},"genBasic":{"attributes":{"65281":{"1":2915,"4":17320,"5":18,"6":[0,1],"10":18602,"100":2165,"101":5928,"102":102898},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.weather","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":30,"_dateCode":"20161129","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668850658,"_linkquality":75},"endpoint":"[Circular]","data":{"measuredValue":2140},"linkquality":75,"groupID":0,"cluster":"msTemperatureMeasurement","meta":{"zclTransactionSequenceNumber":63,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:34:10.659 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:10.660 - debug: zigbee.0 (26219) Received Zigbee message from '0x00158d0002b54752', type 'attributeReport', cluster 'msTemperatureMeasurement', data '{"measuredValue":2140}' from endpoint 1 with groupID 0	
2021-12-16 16:34:10.661 - debug: zigbee.0 (26219) Type attributeReport device {"type":"device","device":{"ID":20,"_type":"EndDevice","_ieeeAddr":"0x00158d0002b54752","_networkAddress":39900,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":39900,"deviceIeeeAddress":"0x00158d0002b54752","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2140}},"msRelativeHumidity":{"attributes":{"measuredValue":5113}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10313}},"genBasic":{"attributes":{"65281":{"1":2915,"4":17320,"5":18,"6":[0,1],"10":18602,"100":2165,"101":5928,"102":102898},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.weather","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":30,"_dateCode":"20161129","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668850658,"_linkquality":75},"mapped":{"zigbeeModel":["lumi.weather"],"model":"WSDCGQ11LM","vendor":"Xiaomi","description":"Aqara temperature, humidity and pressure sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"msTemperatureMeasurement","options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}],"type":["attributeReport","readResponse"]},{"cluster":"msRelativeHumidity","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."}]},{"cluster":"msPressureMeasurement","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"humidity","property":"humidity","access":1,"unit":"%","description":"Measured relative humidity"},{"type":"numeric","name":"pressure","property":"pressure","access":1,"unit":"hPa","description":"The measured atmospheric pressure"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":["[Circular]","[Circular]","[Circular]","[Circular]","[Circular]","[Circular]"]},"name":"0x00158d0002b54752"} incoming event: {"type":"attributeReport","device":{"ID":20,"_type":"EndDevice","_ieeeAddr":"0x00158d0002b54752","_networkAddress":39900,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":39900,"deviceIeeeAddress":"0x00158d0002b54752","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2140}},"msRelativeHumidity":{"attributes":{"measuredValue":5113}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10313}},"genBasic":{"attributes":{"65281":{"1":2915,"4":17320,"5":18,"6":[0,1],"10":18602,"100":2165,"101":5928,"102":102898},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.weather","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":30,"_dateCode":"20161129","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668850658,"_linkquality":75},"endpoint":"[Circular]","data":{"measuredValue":2140},"linkquality":75,"groupID":0,"cluster":"msTemperatureMeasurement","meta":{"zclTransactionSequenceNumber":63,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:34:10.674 - debug: zigbee.0 (26219) Publish {"temperature":21.4} to "00158d0002b54752"	
2021-12-16 16:34:10.694 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,28,68,129,0,0,5,4]	
2021-12-16 16:34:10.695 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,28,68,129,0,0,5,4]	
2021-12-16 16:34:10.697 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [220,155,1,1,0,75,0,119,237,4,0,0,8,24,64,10]	
2021-12-16 16:34:10.697 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,28,68,129,0,0,5,4,220,155,1,1,0,75,0,119,237,4,0,0,8,24,64,10]	
2021-12-16 16:34:10.698 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [0,0,33,251,19,245,234,26,220]	
2021-12-16 16:34:10.699 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,28,68,129,0,0,5,4,220,155,1,1,0,75,0,119,237,4,0,0,8,24,64,10,0,0,33,251,19,245,234,26,220]	
2021-12-16 16:34:10.699 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 28 - 2 - 4 - 129 - [0,0,5,4,220,155,1,1,0,75,0,119,237,4,0,0,8,24,64,10,0,0,33,251,19,245,234,26] - 220	
2021-12-16 16:34:10.700 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - incomingMsg - {"groupid":0,"clusterid":1029,"srcaddr":39900,"srcendpoint":1,"dstendpoint":1,"wasbroadcast":0,"linkquality":75,"securityuse":0,"timestamp":322935,"transseqnumber":0,"len":8,"data":{"type":"Buffer","data":[24,64,10,0,0,33,251,19]}}	
2021-12-16 16:34:10.701 - debug: zigbee.0 (26219) zigbee-herdsman:controller:log Received 'zcl' data '{"frame":{"Header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":64,"manufacturerCode":null,"commandIdentifier":10},"Payload":[{"attrId":0,"dataType":33,"attrData":5115}],"Command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}},"address":39900,"endpoint":1,"linkquality":75,"groupID":0,"wasBroadcast":false,"destinationEndpoint":1}'	
2021-12-16 16:34:10.701 - debug: zigbee.0 (26219) handleMessage. {"type":"attributeReport","device":{"ID":20,"_type":"EndDevice","_ieeeAddr":"0x00158d0002b54752","_networkAddress":39900,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":39900,"deviceIeeeAddress":"0x00158d0002b54752","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2140}},"msRelativeHumidity":{"attributes":{"measuredValue":5115}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10313}},"genBasic":{"attributes":{"65281":{"1":2915,"4":17320,"5":18,"6":[0,1],"10":18602,"100":2165,"101":5928,"102":102898},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.weather","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":30,"_dateCode":"20161129","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668850701,"_linkquality":75},"endpoint":"[Circular]","data":{"measuredValue":5115},"linkquality":75,"groupID":0,"cluster":"msRelativeHumidity","meta":{"zclTransactionSequenceNumber":64,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:34:10.702 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:10.702 - debug: zigbee.0 (26219) Received Zigbee message from '0x00158d0002b54752', type 'attributeReport', cluster 'msRelativeHumidity', data '{"measuredValue":5115}' from endpoint 1 with groupID 0	
2021-12-16 16:34:10.705 - debug: zigbee.0 (26219) Type attributeReport device {"type":"device","device":{"ID":20,"_type":"EndDevice","_ieeeAddr":"0x00158d0002b54752","_networkAddress":39900,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":39900,"deviceIeeeAddress":"0x00158d0002b54752","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2140}},"msRelativeHumidity":{"attributes":{"measuredValue":5115}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10313}},"genBasic":{"attributes":{"65281":{"1":2915,"4":17320,"5":18,"6":[0,1],"10":18602,"100":2165,"101":5928,"102":102898},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.weather","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":30,"_dateCode":"20161129","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668850701,"_linkquality":75},"mapped":{"zigbeeModel":["lumi.weather"],"model":"WSDCGQ11LM","vendor":"Xiaomi","description":"Aqara temperature, humidity and pressure sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"msTemperatureMeasurement","options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}],"type":["attributeReport","readResponse"]},{"cluster":"msRelativeHumidity","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."}]},{"cluster":"msPressureMeasurement","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"humidity","property":"humidity","access":1,"unit":"%","description":"Measured relative humidity"},{"type":"numeric","name":"pressure","property":"pressure","access":1,"unit":"hPa","description":"The measured atmospheric pressure"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":["[Circular]","[Circular]","[Circular]","[Circular]","[Circular]","[Circular]"]},"name":"0x00158d0002b54752"} incoming event: {"type":"attributeReport","device":{"ID":20,"_type":"EndDevice","_ieeeAddr":"0x00158d0002b54752","_networkAddress":39900,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":39900,"deviceIeeeAddress":"0x00158d0002b54752","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2140}},"msRelativeHumidity":{"attributes":{"measuredValue":5115}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10313}},"genBasic":{"attributes":{"65281":{"1":2915,"4":17320,"5":18,"6":[0,1],"10":18602,"100":2165,"101":5928,"102":102898},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.weather","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":30,"_dateCode":"20161129","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668850701,"_linkquality":75},"endpoint":"[Circular]","data":{"measuredValue":5115},"linkquality":75,"groupID":0,"cluster":"msRelativeHumidity","meta":{"zclTransactionSequenceNumber":64,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:34:10.717 - debug: zigbee.0 (26219) Publish {"humidity":51.15} to "00158d0002b54752"	
2021-12-16 16:34:10.733 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,37,68,129,0,0,3,4,220,155,1,1,0,75,0,128]	
2021-12-16 16:34:10.733 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,37,68,129,0,0,3,4,220,155,1,1,0,75,0,128]	
2021-12-16 16:34:10.734 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [246,4,0,0,17,24,65,10,0,0,41,7,4,20,0,40]	
2021-12-16 16:34:10.735 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,37,68,129,0,0,3,4,220,155,1,1,0,75,0,128,246,4,0,0,17,24,65,10,0,0,41,7,4,20,0,40]	
2021-12-16 16:34:10.736 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [255,16,0,41,75,40,245,234,26,109]	
2021-12-16 16:34:10.737 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,37,68,129,0,0,3,4,220,155,1,1,0,75,0,128,246,4,0,0,17,24,65,10,0,0,41,7,4,20,0,40,255,16,0,41,75,40,245,234,26,109]	
2021-12-16 16:34:10.737 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 37 - 2 - 4 - 129 - [0,0,3,4,220,155,1,1,0,75,0,128,246,4,0,0,17,24,65,10,0,0,41,7,4,20,0,40,255,16,0,41,75,40,245,234,26] - 109	
2021-12-16 16:34:10.738 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - incomingMsg - {"groupid":0,"clusterid":1027,"srcaddr":39900,"srcendpoint":1,"dstendpoint":1,"wasbroadcast":0,"linkquality":75,"securityuse":0,"timestamp":325248,"transseqnumber":0,"len":17,"data":{"type":"Buffer","data":[24,65,10,0,0,41,7,4,20,0,40,255,16,0,41,75,40]}}	
2021-12-16 16:34:10.739 - debug: zigbee.0 (26219) zigbee-herdsman:controller:log Received 'zcl' data '{"frame":{"Header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":65,"manufacturerCode":null,"commandIdentifier":10},"Payload":[{"attrId":0,"dataType":41,"attrData":1031},{"attrId":20,"dataType":40,"attrData":-1},{"attrId":16,"dataType":41,"attrData":10315}],"Command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}},"address":39900,"endpoint":1,"linkquality":75,"groupID":0,"wasBroadcast":false,"destinationEndpoint":1}'	
2021-12-16 16:34:10.740 - debug: zigbee.0 (26219) handleMessage. {"type":"attributeReport","device":{"ID":20,"_type":"EndDevice","_ieeeAddr":"0x00158d0002b54752","_networkAddress":39900,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":39900,"deviceIeeeAddress":"0x00158d0002b54752","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2140}},"msRelativeHumidity":{"attributes":{"measuredValue":5115}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10315}},"genBasic":{"attributes":{"65281":{"1":2915,"4":17320,"5":18,"6":[0,1],"10":18602,"100":2165,"101":5928,"102":102898},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.weather","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":30,"_dateCode":"20161129","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668850739,"_linkquality":75},"endpoint":"[Circular]","data":{"measuredValue":1031,"scale":-1,"scaledValue":10315},"linkquality":75,"groupID":0,"cluster":"msPressureMeasurement","meta":{"zclTransactionSequenceNumber":65,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:34:10.740 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:10.740 - debug: zigbee.0 (26219) Received Zigbee message from '0x00158d0002b54752', type 'attributeReport', cluster 'msPressureMeasurement', data '{"measuredValue":1031,"scale":-1,"scaledValue":10315}' from endpoint 1 with groupID 0	
2021-12-16 16:34:10.741 - debug: zigbee.0 (26219) Type attributeReport device {"type":"device","device":{"ID":20,"_type":"EndDevice","_ieeeAddr":"0x00158d0002b54752","_networkAddress":39900,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":39900,"deviceIeeeAddress":"0x00158d0002b54752","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2140}},"msRelativeHumidity":{"attributes":{"measuredValue":5115}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10315}},"genBasic":{"attributes":{"65281":{"1":2915,"4":17320,"5":18,"6":[0,1],"10":18602,"100":2165,"101":5928,"102":102898},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.weather","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":30,"_dateCode":"20161129","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668850739,"_linkquality":75},"mapped":{"zigbeeModel":["lumi.weather"],"model":"WSDCGQ11LM","vendor":"Xiaomi","description":"Aqara temperature, humidity and pressure sensor","meta":{"battery":{"voltageToPercentage":"3V_2100"}},"fromZigbee":[{"cluster":"genBasic","type":["attributeReport","readResponse"]},{"cluster":"msTemperatureMeasurement","options":[{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."}],"type":["attributeReport","readResponse"]},{"cluster":"msRelativeHumidity","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."}]},{"cluster":"msPressureMeasurement","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."}]},{"cluster":"genBasic","type":["attributeReport","readResponse"],"options":[{"type":"numeric","name":"pressure_precision","property":"pressure_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for pressure, takes into effect on next report of device."},{"type":"numeric","name":"pressure_calibration","property":"pressure_calibration","access":2,"description":"Calibrates the pressure value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"temperature_precision","property":"temperature_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for temperature, takes into effect on next report of device."},{"type":"numeric","name":"temperature_calibration","property":"temperature_calibration","access":2,"description":"Calibrates the temperature value (absolute offset), takes into effect on next report of device."},{"type":"numeric","name":"humidity_precision","property":"humidity_precision","access":2,"value_min":0,"value_max":3,"description":"Number of digits after decimal point for humidity, takes into effect on next report of device."},{"type":"numeric","name":"humidity_calibration","property":"humidity_calibration","access":2,"description":"Calibrates the humidity value (absolute offset), takes into effect on next report of device."}]}],"toZigbee":[],"exposes":[{"type":"numeric","name":"battery","property":"battery","access":1,"unit":"%","description":"Remaining battery in %","value_min":0,"value_max":100},{"type":"numeric","name":"temperature","property":"temperature","access":1,"unit":"°C","description":"Measured temperature value"},{"type":"numeric","name":"humidity","property":"humidity","access":1,"unit":"%","description":"Measured relative humidity"},{"type":"numeric","name":"pressure","property":"pressure","access":1,"unit":"hPa","description":"The measured atmospheric pressure"},{"type":"numeric","name":"voltage","property":"voltage","access":1,"unit":"mV","description":"Voltage of the battery in millivolts"},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"options":["[Circular]","[Circular]","[Circular]","[Circular]","[Circular]","[Circular]"]},"name":"0x00158d0002b54752"} incoming event: {"type":"attributeReport","device":{"ID":20,"_type":"EndDevice","_ieeeAddr":"0x00158d0002b54752","_networkAddress":39900,"_manufacturerID":4151,"_endpoints":[{"ID":1,"profileID":260,"deviceID":24321,"inputClusters":[0,3,65535,1026,1027,1029],"outputClusters":[0,4,65535],"deviceNetworkAddress":39900,"deviceIeeeAddress":"0x00158d0002b54752","clusters":{"msTemperatureMeasurement":{"attributes":{"measuredValue":2140}},"msRelativeHumidity":{"attributes":{"measuredValue":5115}},"msPressureMeasurement":{"attributes":{"measuredValue":1031,"scale":-1,"scaledValue":10315}},"genBasic":{"attributes":{"65281":{"1":2915,"4":17320,"5":18,"6":[0,1],"10":18602,"100":2165,"101":5928,"102":102898},"manufacturerName":"LUMI","powerSource":3,"zclVersion":1,"stackVersion":2,"hwVersion":30,"dateCode":"20161129","swBuildId":"3000-0001"}}},"_binds":[],"_configuredReportings":[],"meta":{},"pendingRequests":[]}],"_manufacturerName":"LUMI","_powerSource":"Battery","_modelID":"lumi.weather","_applicationVersion":3,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":30,"_dateCode":"20161129","_softwareBuildID":"3000-0001","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668850739,"_linkquality":75},"endpoint":"[Circular]","data":{"measuredValue":1031,"scale":-1,"scaledValue":10315},"linkquality":75,"groupID":0,"cluster":"msPressureMeasurement","meta":{"zclTransactionSequenceNumber":65,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:34:10.753 - debug: zigbee.0 (26219) Publish {"pressure":1031.5} to "00158d0002b54752"	
2021-12-16 16:34:12.467 - debug: zigbee.0 (26219) Failed to execute LQI for '0x7cb03eaa0a025809'. "Error: AREQ - ZDO - mgmtLqiRsp after 10000ms\n at Timeout._onTimeout (/opt/iobroker/node_modules/zigbee-herdsman/dist/utils/waitress.js:37:35)\n at listOnTimeout (internal/timers.js:557:17)\n at processTimers (internal/timers.js:500:7)"	
2021-12-16 16:34:12.468 - debug: zigbee.0 (26219) LQI succeeded for '0x7cb03eaa0a025809'	
2021-12-16 16:34:12.469 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtRtgReq - {"dstaddr":18602,"startindex":0}	
2021-12-16 16:34:12.470 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,50,170,72,0,246]	
2021-12-16 16:34:12.478 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,50,0,86]	
2021-12-16 16:34:12.480 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,50,0,86]	
2021-12-16 16:34:12.480 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 50 - [0] - 86	
2021-12-16 16:34:12.481 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtRtgReq - {"status":0}	
2021-12-16 16:34:12.482 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:12.624 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00acb990:47504/3 (0,1,2)	
2021-12-16 16:34:12.625 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":47504,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":108,"options":0,"radius":30,"len":3,"data":{"type":"Buffer","data":[1,37,0]}}	
2021-12-16 16:34:12.627 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,13,36,1,144,185,3,1,6,0,108,0,30,3,1,37,0,80]	
2021-12-16 16:34:12.635 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:34:12.636 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:34:12.637 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:34:12.638 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:34:12.639 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:12.687 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,108,75]	
2021-12-16 16:34:12.688 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,108,75]	
2021-12-16 16:34:12.689 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,108] - 75	
2021-12-16 16:34:12.690 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":108}	
2021-12-16 16:34:12.691 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:12.692 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00acb990:47504,225,1)	
2021-12-16 16:34:14.698 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00acb990:47504/3 (0,2,2)	
2021-12-16 16:34:14.699 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":47504,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":109,"options":0,"radius":30,"len":3,"data":{"type":"Buffer","data":[1,37,0]}}	
2021-12-16 16:34:14.700 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,13,36,1,144,185,3,1,6,0,109,0,30,3,1,37,0,81]	
2021-12-16 16:34:14.708 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:34:14.708 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:34:14.709 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:34:14.709 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:34:14.710 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:14.753 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,109,74]	
2021-12-16 16:34:14.754 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,109,74]	
2021-12-16 16:34:14.755 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,109] - 74	
2021-12-16 16:34:14.755 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":109}	
2021-12-16 16:34:14.756 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:14.756 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00acb990:47504,225,2)	
2021-12-16 16:34:16.757 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00acb990:47504/3 (0,3,2)	
2021-12-16 16:34:16.758 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":47504,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":110,"options":0,"radius":30,"len":3,"data":{"type":"Buffer","data":[1,37,0]}}	
2021-12-16 16:34:16.759 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,13,36,1,144,185,3,1,6,0,110,0,30,3,1,37,0,82]	
2021-12-16 16:34:16.767 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:34:16.768 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:34:16.768 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:34:16.769 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:34:16.770 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:16.809 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,110,73]	
2021-12-16 16:34:16.810 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,110,73]	
2021-12-16 16:34:16.811 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,110] - 73	
2021-12-16 16:34:16.811 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":110}	
2021-12-16 16:34:16.812 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:16.813 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00acb990:47504,225,3)	
2021-12-16 16:34:18.813 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter sendZclFrameToEndpointInternal 0x7cb03eaa00acb990:47504/3 (0,4,2)	
2021-12-16 16:34:18.815 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> AF - dataRequest - {"dstaddr":47504,"destendpoint":3,"srcendpoint":1,"clusterid":6,"transid":111,"options":0,"radius":30,"len":3,"data":{"type":"Buffer","data":[1,37,0]}}	
2021-12-16 16:34:18.816 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,13,36,1,144,185,3,1,6,0,111,0,30,3,1,37,0,83]	
2021-12-16 16:34:18.824 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,100,1,0,100]	
2021-12-16 16:34:18.824 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,100,1,0,100]	
2021-12-16 16:34:18.825 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 4 - 1 - [0] - 100	
2021-12-16 16:34:18.825 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- AF - dataRequest - {"status":0}	
2021-12-16 16:34:18.826 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:18.877 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,3,68,128,225,1,111,72]	
2021-12-16 16:34:18.879 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,3,68,128,225,1,111,72]	
2021-12-16 16:34:18.879 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 3 - 2 - 4 - 128 - [225,1,111] - 72	
2021-12-16 16:34:18.881 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - dataConfirm - {"status":225,"endpoint":1,"transid":111}	
2021-12-16 16:34:18.882 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:18.882 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:adapter Data confirm error (0x7cb03eaa00acb990:47504,225,4)	
2021-12-16 16:34:18.883 - debug: zigbee.0 (26219) zigbee-herdsman:controller:endpoint Command 0x7cb03eaa00acb990/3 genOnOff.off({}, {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'MAC channel access failure' (225))	
2021-12-16 16:34:18.885 - error: zigbee.0 (26219) Error 225 on send command to 0x7cb03eaa00acb990. Error: Error: Command 0x7cb03eaa00acb990/3 genOnOff.off({}, {"sendWhenActive":false,"timeout":10000,"disableResponse":false,"disableRecovery":false,"disableDefaultResponse":false,"direction":0,"srcEndpoint":null,"reservedBits":0,"manufacturerCode":null,"transactionSequenceNumber":null,"writeUndiv":false}) failed (Data request failed with error: 'MAC channel access failure' (225))	
at ZStackAdapter.sendZclFrameToEndpointInternal (/opt/iobroker/node_modules/zigbee-herdsman/dist/adapter/z-stack/adapter/zStackAdapter.js:310:23)	
at async Queue.executeNext (/opt/iobroker/node_modules/zigbee-herdsman/dist/utils/queue.js:19:32)	
2021-12-16 16:34:22.484 - debug: zigbee.0 (26219) Failed to execute routing table for '0x7cb03eaa0a025809'. "Error: AREQ - ZDO - mgmtRtgRsp after 10000ms\n at Timeout._onTimeout (/opt/iobroker/node_modules/zigbee-herdsman/dist/utils/waitress.js:37:35)\n at listOnTimeout (internal/timers.js:557:17)\n at processTimers (internal/timers.js:500:7)"	
2021-12-16 16:34:22.485 - debug: zigbee.0 (26219) Routing for '0x7cb03eaa0a025809': undefined	
2021-12-16 16:34:22.485 - debug: zigbee.0 (26219) Routing table succeeded for '0x7cb03eaa0a025809'	
2021-12-16 16:34:22.485 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtLqiReq - {"dstaddr":65448,"startindex":0}	
2021-12-16 16:34:22.486 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,49,168,255,0,64]	
2021-12-16 16:34:22.493 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,49,0,85]	
2021-12-16 16:34:22.493 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,49,0,85]	
2021-12-16 16:34:22.493 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 49 - [0] - 85	
2021-12-16 16:34:22.494 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtLqiReq - {"status":0}	
2021-12-16 16:34:22.494 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:32.496 - debug: zigbee.0 (26219) Failed to execute LQI for '0x7cb03eaa00a36bed'. "Error: AREQ - ZDO - mgmtLqiRsp after 10000ms\n at Timeout._onTimeout (/opt/iobroker/node_modules/zigbee-herdsman/dist/utils/waitress.js:37:35)\n at listOnTimeout (internal/timers.js:557:17)\n at processTimers (internal/timers.js:500:7)"	
2021-12-16 16:34:32.497 - debug: zigbee.0 (26219) LQI succeeded for '0x7cb03eaa00a36bed'	
2021-12-16 16:34:32.498 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtRtgReq - {"dstaddr":65448,"startindex":0}	
2021-12-16 16:34:32.499 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,50,168,255,0,67]	
2021-12-16 16:34:32.508 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,50,0,86]	
2021-12-16 16:34:32.509 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,50,0,86]	
2021-12-16 16:34:32.510 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 50 - [0] - 86	
2021-12-16 16:34:32.510 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtRtgReq - {"status":0}	
2021-12-16 16:34:32.512 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:42.514 - debug: zigbee.0 (26219) Failed to execute routing table for '0x7cb03eaa00a36bed'. "Error: AREQ - ZDO - mgmtRtgRsp after 10000ms\n at Timeout._onTimeout (/opt/iobroker/node_modules/zigbee-herdsman/dist/utils/waitress.js:37:35)\n at listOnTimeout (internal/timers.js:557:17)\n at processTimers (internal/timers.js:500:7)"	
2021-12-16 16:34:42.515 - debug: zigbee.0 (26219) Routing for '0x7cb03eaa00a36bed': undefined	
2021-12-16 16:34:42.516 - debug: zigbee.0 (26219) Routing table succeeded for '0x7cb03eaa00a36bed'	
2021-12-16 16:34:42.517 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SREQ --> ZDO - mgmtLqiReq - {"dstaddr":32268,"startindex":0}	
2021-12-16 16:34:42.518 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:writer --> frame [254,3,37,49,12,126,0,101]	
2021-12-16 16:34:42.526 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,1,101,49,0,85]	
2021-12-16 16:34:42.528 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,1,101,49,0,85]	
2021-12-16 16:34:42.528 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 1 - 3 - 5 - 49 - [0] - 85	
2021-12-16 16:34:42.529 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:SRSP <-- ZDO - mgmtLqiReq - {"status":0}	
2021-12-16 16:34:42.530 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:48.405 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [254,27,68,129,0,0,6,0]	
2021-12-16 16:34:48.406 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,27,68,129,0,0,6,0]	
2021-12-16 16:34:48.409 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser <-- [140,221,3,1,0,75,0,10,228,40,0,0,7,24,88,10,0,0,16,1,245,234,28,89]	
2021-12-16 16:34:48.410 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext [254,27,68,129,0,0,6,0,140,221,3,1,0,75,0,10,228,40,0,0,7,24,88,10,0,0,16,1,245,234,28,89]	
2021-12-16 16:34:48.411 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --> parsed 27 - 2 - 4 - 129 - [0,0,6,0,140,221,3,1,0,75,0,10,228,40,0,0,7,24,88,10,0,0,16,1,245,234,28] - 89	
2021-12-16 16:34:48.412 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:znp:AREQ <-- AF - incomingMsg - {"groupid":0,"clusterid":6,"srcaddr":56716,"srcendpoint":3,"dstendpoint":1,"wasbroadcast":0,"linkquality":75,"securityuse":0,"timestamp":2679818,"transseqnumber":0,"len":7,"data":{"type":"Buffer","data":[24,88,10,0,0,16,1]}}	
2021-12-16 16:34:48.413 - debug: zigbee.0 (26219) zigbee-herdsman:controller:log Received 'zcl' data '{"frame":{"Header":{"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0},"transactionSequenceNumber":88,"manufacturerCode":null,"commandIdentifier":10},"Payload":[{"attrId":0,"dataType":16,"attrData":1}],"Command":{"ID":10,"name":"report","parameters":[{"name":"attrId","type":33},{"name":"dataType","type":32},{"name":"attrData","type":1000}]}},"address":56716,"endpoint":3,"linkquality":75,"groupID":0,"wasBroadcast":false,"destinationEndpoint":1}'	
2021-12-16 16:34:48.418 - debug: zigbee.0 (26219) handleMessage. {"type":"attributeReport","device":{"ID":16,"_type":"Router","_ieeeAddr":"0x84182600000c7532","_networkAddress":56716,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":56716,"deviceIeeeAddress":"0x84182600000c7532","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":1}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668888417,"_linkquality":75},"endpoint":"[Circular]","data":{"onOff":1},"linkquality":75,"groupID":0,"cluster":"genOnOff","meta":{"zclTransactionSequenceNumber":88,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:34:48.419 - debug: zigbee.0 (26219) zigbee-herdsman:adapter:zStack:unpi:parser --- parseNext []	
2021-12-16 16:34:48.419 - debug: zigbee.0 (26219) Received Zigbee message from '0x84182600000c7532', type 'attributeReport', cluster 'genOnOff', data '{"onOff":1}' from endpoint 3 with groupID 0	
2021-12-16 16:34:48.420 - debug: zigbee.0 (26219) Type attributeReport device {"type":"device","device":{"ID":16,"_type":"Router","_ieeeAddr":"0x84182600000c7532","_networkAddress":56716,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":56716,"deviceIeeeAddress":"0x84182600000c7532","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":1}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668888417,"_linkquality":75},"mapped":{"exposes":[{"type":"switch","features":[{"type":"binary","name":"state","property":"state","access":7,"value_on":"ON","value_off":"OFF","description":"On/off state of the switch","value_toggle":"TOGGLE"}]},{"type":"numeric","name":"linkquality","property":"linkquality","access":1,"unit":"lqi","description":"Link quality (signal strength)","value_min":0,"value_max":255}],"fromZigbee":[{"cluster":"genOnOff","type":["attributeReport","readResponse"]},{"cluster":"genBasic","type":["attributeReport","readResponse"]}],"toZigbee":[{"key":["state","on_time","off_wait_time"]},{"key":["scene_store"]},{"key":["scene_recall"]},{"key":["scene_add"]},{"key":["scene_remove"]},{"key":["scene_remove_all"]},{"key":["read"]},{"key":["write"]}],"zigbeeModel":["Plug 01"],"model":"AB3257001NJ","description":"Smart+ plug","vendor":"OSRAM","whiteLabel":[{"vendor":"LEDVANCE","model":"AB3257001NJ"}],"ota":{},"options":[]},"name":"0x84182600000c7532"} incoming event: {"type":"attributeReport","device":{"ID":16,"_type":"Router","_ieeeAddr":"0x84182600000c7532","_networkAddress":56716,"_manufacturerID":48042,"_endpoints":[{"ID":3,"profileID":49246,"deviceID":16,"inputClusters":[4096,0,3,4,5,6,2820,64527],"outputClusters":[25],"deviceNetworkAddress":56716,"deviceIeeeAddress":"0x84182600000c7532","clusters":{"genBasic":{"attributes":{"modelId":"Plug 01","manufacturerName":"OSRAM","powerSource":1,"zclVersion":1,"appVersion":12,"stackVersion":2,"hwVersion":1,"dateCode":"20140331DEOS****","swBuildId":"V1.04.12"}},"genOnOff":{"attributes":{"onOff":1}}},"_binds":[{"cluster":6,"type":"endpoint","deviceIeeeAddress":"0x00124b00219fc18c","endpointID":1}],"_configuredReportings":[{"cluster":6,"attrId":0,"minRepIntval":0,"maxRepIntval":3600,"repChange":0}],"meta":{},"pendingRequests":[]}],"_manufacturerName":"OSRAM","_powerSource":"Mains (single phase)","_modelID":"Plug 01","_applicationVersion":12,"_stackVersion":2,"_zclVersion":1,"_hardwareVersion":1,"_dateCode":"20140331DEOS****","_softwareBuildID":"V1.04.12","_interviewCompleted":true,"_interviewing":false,"_skipDefaultResponse":false,"_skipTimeResponse":false,"meta":{"configured":1},"_lastSeen":1639668888417,"_linkquality":75},"endpoint":"[Circular]","data":{"onOff":1},"linkquality":75,"groupID":0,"cluster":"genOnOff","meta":{"zclTransactionSequenceNumber":88,"manufacturerCode":null,"frameControl":{"frameType":0,"manufacturerSpecific":false,"direction":1,"disableDefaultResponse":true,"reservedBits":0}}}	
2021-12-16 16:34:48.446 - debug: zigbee.0 (26219) Publish {"state":"ON"} to "84182600000c7532"